From 8bf21a7f5449fde59e4c9772db0696b3dc4cfaef Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 20 Feb 2019 08:49:39 +0000
Subject: [PATCH] arm: bcm2835: Fix FIQ early ioremap

The ioremapping creates mappings within the vmalloc area. The
equivalent early function, create_mapping, now checks that the
requested explicit virtual address is between VMALLOC_START and
VMALLOC_END. As there is no reason to have any correlation between
the physical and virtual addresses, put the required mappings at
VMALLOC_START and above.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/mach-bcm/board_bcm2835.c | 21 +++++++++++++++------
 1 file changed, 15 insertions(+), 6 deletions(-)

--- a/arch/arm/mach-bcm/board_bcm2835.c
+++ b/arch/arm/mach-bcm/board_bcm2835.c
@@ -5,17 +5,20 @@
 
 #include <linux/init.h>
 #include <linux/irqchip.h>
+#include <linux/mm.h>
 #include <linux/of_address.h>
 #include <linux/of_fdt.h>
 #include <asm/system_info.h>
 
 #include <asm/mach/arch.h>
 #include <asm/mach/map.h>
+#include <asm/memory.h>
+#include <asm/pgtable.h>
 
 #include "platsmp.h"
 
-#define BCM2835_USB_VIRT_BASE   0xf0980000
-#define BCM2835_USB_VIRT_MPHI   0xf0006000
+#define BCM2835_USB_VIRT_BASE   (VMALLOC_START)
+#define BCM2835_USB_VIRT_MPHI   (VMALLOC_START + 0x10000)
 
 static void __init bcm2835_init(void)
 {
@@ -74,20 +77,26 @@ static int __init bcm2835_map_usb(unsign
 
 static void __init bcm2835_map_io(void)
 {
-	const __be32 *ranges;
+	const __be32 *ranges, *address_cells;
+	unsigned long root, addr_cells;
 	int soc, len;
 	unsigned long p2b_offset;
 
 	debug_ll_io_init();
 
+	root = of_get_flat_dt_root();
 	/* Find out how to map bus to physical address first from soc/ranges */
-	soc = of_get_flat_dt_subnode_by_name(of_get_flat_dt_root(), "soc");
+	soc = of_get_flat_dt_subnode_by_name(root, "soc");
 	if (soc < 0)
 		return;
+	address_cells = of_get_flat_dt_prop(root, "#address-cells", &len);
+	if (!address_cells || len < (sizeof(unsigned long)))
+		return;
+	addr_cells = be32_to_cpu(address_cells[0]);
 	ranges = of_get_flat_dt_prop(soc, "ranges", &len);
-	if (!ranges || len < (sizeof(unsigned long) * 3))
+	if (!ranges || len < (sizeof(unsigned long) * (2 + addr_cells)))
 		return;
-	p2b_offset = be32_to_cpu(ranges[0]) - be32_to_cpu(ranges[1]);
+	p2b_offset = be32_to_cpu(ranges[0]) - be32_to_cpu(ranges[addr_cells]);
 
 	/* Now search for bcm2708-usb node in device tree */
 	of_scan_flat_dt(bcm2835_map_usb, &p2b_offset);
