// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "tplink,eap225-wall-v2", "qca,qca9561";
	model = "TP-Link EAP225-Wall v2";

	aliases {
		label-mac-device = &eth1;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		led {
			label = "LED button";
			linux,code = <KEY_LIGHTS_TOGGLE>;
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status: status {
			label = "white:status";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};

	gpio-export {
		compatible = "gpio-export";

		poe_passthrough {
			gpio-export,name = "tp-link:poe-passthrough:enable";
			gpio-export,output = <0>;
			gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
		};
	};
};

&pcie {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "partition-table";
				reg = <0x020000 0x010000>;
				read-only;
			};

			info: partition@30000 {
				label = "info";
				reg = <0x030000 0x010000>;
				read-only;
			};

			partition@40000 {
				compatible = "openwrt,elf";
				label = "firmware";
				reg = <0x040000 0xd80000>;
			};

			partition@dc0000 {
				label = "config";
				reg = <0xdc0000 0x030000>;
				read-only;
			};

			/* df0000-f30000 undefined in vendor firmware */

			partition@f30000 {
				label = "mutil-log";
				reg = <0xf30000 0x080000>;
				read-only;
			};

			partition@fb0000 {
				label = "oops";
				reg = <0xfb0000 0x040000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&info {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_info_8: macaddr@8 {
		reg = <0x8 0x6>;
	};
};
