--- a/hostapd/Makefile
+++ b/hostapd/Makefile
@@ -221,6 +221,9 @@ endif
 ifdef CONFIG_NO_CTRL_IFACE
 CFLAGS += -DCONFIG_NO_CTRL_IFACE
 else
+ifdef CONFIG_CTRL_IFACE_MIB
+CFLAGS += -DCONFIG_CTRL_IFACE_MIB
+endif
 ifeq ($(CONFIG_CTRL_IFACE), udp)
 CFLAGS += -DCONFIG_CTRL_IFACE_UDP
 else
--- a/hostapd/ctrl_iface.c
+++ b/hostapd/ctrl_iface.c
@@ -3569,6 +3569,7 @@ static int hostapd_ctrl_iface_receive_pr
 						      reply_size);
 	} else if (os_strcmp(buf, "STATUS-DRIVER") == 0) {
 		reply_len = hostapd_drv_status(hapd, reply, reply_size);
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strcmp(buf, "MIB") == 0) {
 		reply_len = ieee802_11_get_mib(hapd, reply, reply_size);
 		if (reply_len >= 0) {
@@ -3610,6 +3611,7 @@ static int hostapd_ctrl_iface_receive_pr
 	} else if (os_strncmp(buf, "STA-NEXT ", 9) == 0) {
 		reply_len = hostapd_ctrl_iface_sta_next(hapd, buf + 9, reply,
 							reply_size);
+#endif
 	} else if (os_strcmp(buf, "ATTACH") == 0) {
 		if (hostapd_ctrl_iface_attach(hapd, from, fromlen, NULL))
 			reply_len = -1;
--- a/wpa_supplicant/Makefile
+++ b/wpa_supplicant/Makefile
@@ -955,6 +955,9 @@ ifdef CONFIG_FILS
 OBJS += ../src/ap/fils_hlp.o
 endif
 ifdef CONFIG_CTRL_IFACE
+ifdef CONFIG_CTRL_IFACE_MIB
+CFLAGS += -DCONFIG_CTRL_IFACE_MIB
+endif
 OBJS += ../src/ap/ctrl_iface_ap.o
 endif
 
--- a/wpa_supplicant/ctrl_iface.c
+++ b/wpa_supplicant/ctrl_iface.c
@@ -2308,7 +2308,7 @@ static int wpa_supplicant_ctrl_iface_sta
 			pos += ret;
 		}
 
-#ifdef CONFIG_AP
+#if defined(CONFIG_AP) && defined(CONFIG_CTRL_IFACE_MIB)
 		if (wpa_s->ap_iface) {
 			pos += ap_ctrl_iface_wpa_get_status(wpa_s, pos,
 							    end - pos,
@@ -10919,6 +10919,7 @@ char * wpa_supplicant_ctrl_iface_process
 			reply_len = -1;
 	} else if (os_strncmp(buf, "NOTE ", 5) == 0) {
 		wpa_printf(MSG_INFO, "NOTE: %s", buf + 5);
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strcmp(buf, "MIB") == 0) {
 		reply_len = wpa_sm_get_mib(wpa_s->wpa, reply, reply_size);
 		if (reply_len >= 0) {
@@ -10931,6 +10932,7 @@ char * wpa_supplicant_ctrl_iface_process
 				reply_size - reply_len);
 #endif /* CONFIG_MACSEC */
 		}
+#endif
 	} else if (os_strncmp(buf, "STATUS", 6) == 0) {
 		reply_len = wpa_supplicant_ctrl_iface_status(
 			wpa_s, buf + 6, reply, reply_size);
@@ -11419,6 +11421,7 @@ char * wpa_supplicant_ctrl_iface_process
 		reply_len = wpa_supplicant_ctrl_iface_bss(
 			wpa_s, buf + 4, reply, reply_size);
 #ifdef CONFIG_AP
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strcmp(buf, "STA-FIRST") == 0) {
 		reply_len = ap_ctrl_iface_sta_first(wpa_s, reply, reply_size);
 	} else if (os_strncmp(buf, "STA ", 4) == 0) {
@@ -11427,12 +11430,15 @@ char * wpa_supplicant_ctrl_iface_process
 	} else if (os_strncmp(buf, "STA-NEXT ", 9) == 0) {
 		reply_len = ap_ctrl_iface_sta_next(wpa_s, buf + 9, reply,
 						   reply_size);
+#endif
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strncmp(buf, "DEAUTHENTICATE ", 15) == 0) {
 		if (ap_ctrl_iface_sta_deauthenticate(wpa_s, buf + 15))
 			reply_len = -1;
 	} else if (os_strncmp(buf, "DISASSOCIATE ", 13) == 0) {
 		if (ap_ctrl_iface_sta_disassociate(wpa_s, buf + 13))
 			reply_len = -1;
+#endif
 	} else if (os_strncmp(buf, "CHAN_SWITCH ", 12) == 0) {
 		if (ap_ctrl_iface_chanswitch(wpa_s, buf + 12))
 			reply_len = -1;
--- a/src/ap/ctrl_iface_ap.c
+++ b/src/ap/ctrl_iface_ap.c
@@ -25,6 +25,7 @@
 #include "mbo_ap.h"
 #include "taxonomy.h"
 
+#ifdef CONFIG_CTRL_IFACE_MIB
 
 static size_t hostapd_write_ht_mcs_bitmask(char *buf, size_t buflen,
 					   size_t curr_len, const u8 *mcs_set)
@@ -451,6 +452,7 @@ int hostapd_ctrl_iface_sta_next(struct h
 	return hostapd_ctrl_iface_sta_mib(hapd, sta->next, buf, buflen);
 }
 
+#endif
 
 #ifdef CONFIG_P2P_MANAGER
 static int p2p_manager_disconnect(struct hostapd_data *hapd, u16 stype,
@@ -807,12 +809,12 @@ int hostapd_ctrl_iface_status(struct hos
 			return len;
 		len += ret;
 	}
-
+#ifdef CONFIG_CTRL_IFACE_MIB
 	if (iface->conf->ieee80211n && !hapd->conf->disable_11n && mode) {
 		len = hostapd_write_ht_mcs_bitmask(buf, buflen, len,
 						   mode->mcs_set);
 	}
-
+#endif /* CONFIG_CTRL_IFACE_MIB */
 	if (iface->current_rates && iface->num_rates) {
 		ret = os_snprintf(buf + len, buflen - len, "supported_rates=");
 		if (os_snprintf_error(buflen - len, ret))
--- a/src/ap/ieee802_1x.c
+++ b/src/ap/ieee802_1x.c
@@ -2712,6 +2712,7 @@ static const char * bool_txt(bool val)
 	return val ? "TRUE" : "FALSE";
 }
 
+#ifdef CONFIG_CTRL_IFACE_MIB
 
 int ieee802_1x_get_mib(struct hostapd_data *hapd, char *buf, size_t buflen)
 {
@@ -2898,6 +2899,7 @@ int ieee802_1x_get_mib_sta(struct hostap
 	return len;
 }
 
+#endif
 
 #ifdef CONFIG_HS20
 static void ieee802_1x_wnm_notif_send(void *eloop_ctx, void *timeout_ctx)
--- a/src/ap/wpa_auth.c
+++ b/src/ap/wpa_auth.c
@@ -4519,6 +4519,7 @@ static const char * wpa_bool_txt(int val
 	return val ? "TRUE" : "FALSE";
 }
 
+#ifdef CONFIG_CTRL_IFACE_MIB
 
 #define RSN_SUITE "%02x-%02x-%02x-%d"
 #define RSN_SUITE_ARG(s) \
@@ -4669,7 +4670,7 @@ int wpa_get_mib_sta(struct wpa_state_mac
 
 	return len;
 }
-
+#endif
 
 void wpa_auth_countermeasures_start(struct wpa_authenticator *wpa_auth)
 {
--- a/src/rsn_supp/wpa.c
+++ b/src/rsn_supp/wpa.c
@@ -2767,6 +2767,8 @@ static u32 wpa_key_mgmt_suite(struct wpa
 }
 
 
+#ifdef CONFIG_CTRL_IFACE_MIB
+
 #define RSN_SUITE "%02x-%02x-%02x-%d"
 #define RSN_SUITE_ARG(s) \
 ((s) >> 24) & 0xff, ((s) >> 16) & 0xff, ((s) >> 8) & 0xff, (s) & 0xff
@@ -2848,6 +2850,7 @@ int wpa_sm_get_mib(struct wpa_sm *sm, ch
 
 	return (int) len;
 }
+#endif
 #endif /* CONFIG_CTRL_IFACE */
 
 
--- a/wpa_supplicant/ap.c
+++ b/wpa_supplicant/ap.c
@@ -1364,7 +1364,7 @@ int wpas_ap_wps_nfc_report_handover(stru
 #endif /* CONFIG_WPS */
 
 
-#ifdef CONFIG_CTRL_IFACE
+#if defined(CONFIG_CTRL_IFACE) && defined(CONFIG_CTRL_IFACE_MIB)
 
 int ap_ctrl_iface_sta_first(struct wpa_supplicant *wpa_s,
 			    char *buf, size_t buflen)
