From 0e4fe4adfd9a9cd36220b79a8eecce4d24a9fd02 Mon Sep 17 00:00:00 2001
From: Dong Aisheng <aisheng.dong@nxp.com>
Date: Tue, 7 May 2019 11:01:08 +0800
Subject: [PATCH] ASoC: fsl: sai: fix build failture due to 5.1 RC7 upgrade

Signed-off-by: Dong Aisheng <aisheng.dong@nxp.com>
---
 sound/soc/fsl/fsl_sai.c | 10 ----------
 1 file changed, 10 deletions(-)

--- a/sound/soc/fsl/fsl_sai.c
+++ b/sound/soc/fsl/fsl_sai.c
@@ -418,14 +418,12 @@ static int fsl_sai_set_dai_fmt_tr(struct
 	case SND_SOC_DAIFMT_CBS_CFS:
 		val_cr2 |= FSL_SAI_CR2_BCD_MSTR;
 		val_cr4 |= FSL_SAI_CR4_FSD_MSTR;
-		sai->is_slave_mode = false;
 		break;
 	case SND_SOC_DAIFMT_CBM_CFM:
 		sai->slave_mode[tx] = true;
 		break;
 	case SND_SOC_DAIFMT_CBS_CFM:
 		val_cr2 |= FSL_SAI_CR2_BCD_MSTR;
-		sai->is_slave_mode = false;
 		break;
 	case SND_SOC_DAIFMT_CBM_CFS:
 		val_cr4 |= FSL_SAI_CR4_FSD_MSTR;
@@ -1575,14 +1573,6 @@ static int fsl_sai_remove(struct platfor
 	return 0;
 }
 
-static const struct of_device_id fsl_sai_ids[] = {
-	{ .compatible = "fsl,vf610-sai", },
-	{ .compatible = "fsl,imx6sx-sai", },
-	{ .compatible = "fsl,imx6ul-sai", },
-	{ /* sentinel */ }
-};
-MODULE_DEVICE_TABLE(of, fsl_sai_ids);
-
 #ifdef CONFIG_PM
 static int fsl_sai_runtime_suspend(struct device *dev)
 {
