From: Birger Koblitz <git@birger-koblitz.de>
Date: Sun, 5 Sep 2021 15:13:10 +0200
Subject: [PATCH] kernel: Add AQR113C and AQR813 support

This hack adds support for the Aquantia 4th generation, 10GBit
PHYs AQR113C and AQR813.

Signed-off-by: Birger Koblitz <git@birger-koblitz.de>

--- a/drivers/net/phy/aquantia_main.c
+++ b/drivers/net/phy/aquantia_main.c
@@ -20,8 +20,10 @@
 #define PHY_ID_AQR105	0x03a1b4a2
 #define PHY_ID_AQR106	0x03a1b4d0
 #define PHY_ID_AQR107	0x03a1b4e0
+#define PHY_ID_AQR113C	0x31c31c12
 #define PHY_ID_AQCS109	0x03a1b5c2
 #define PHY_ID_AQR405	0x03a1b4b0
+#define PHY_ID_AQR813	0x31c31cb2
 
 #define MDIO_PHYXS_VEND_IF_STATUS		0xe812
 #define MDIO_PHYXS_VEND_IF_STATUS_TYPE_MASK	GENMASK(7, 3)
@@ -330,6 +332,49 @@ static int aqr107_read_rate(struct phy_d
 	return 0;
 }
 
+static int aqr113c_read_status(struct phy_device *phydev)
+{
+	int val, ret;
+
+	ret = aqr_read_status(phydev);
+	if (ret)
+		return ret;
+
+	if (!phydev->link || phydev->autoneg == AUTONEG_DISABLE)
+		return 0;
+
+	// On AQR113C, the speed returned by aqr_read_status is wrong
+	aqr107_read_rate(phydev);
+
+	val = phy_read_mmd(phydev, MDIO_MMD_PHYXS, MDIO_PHYXS_VEND_IF_STATUS);
+	if (val < 0)
+		return val;
+
+	switch (FIELD_GET(MDIO_PHYXS_VEND_IF_STATUS_TYPE_MASK, val)) {
+	case MDIO_PHYXS_VEND_IF_STATUS_TYPE_KR:
+		phydev->interface = PHY_INTERFACE_MODE_10GKR;
+		break;
+	case MDIO_PHYXS_VEND_IF_STATUS_TYPE_XFI:
+		phydev->interface = PHY_INTERFACE_MODE_10GBASER;
+		break;
+	case MDIO_PHYXS_VEND_IF_STATUS_TYPE_USXGMII:
+		phydev->interface = PHY_INTERFACE_MODE_USXGMII;
+		break;
+	case MDIO_PHYXS_VEND_IF_STATUS_TYPE_SGMII:
+		phydev->interface = PHY_INTERFACE_MODE_SGMII;
+		break;
+	case MDIO_PHYXS_VEND_IF_STATUS_TYPE_OCSGMII:
+		phydev->interface = PHY_INTERFACE_MODE_2500BASEX;
+		break;
+	default:
+		phydev->interface = PHY_INTERFACE_MODE_NA;
+		break;
+	}
+
+	/* Read downshifted rate from vendor register */
+	return aqr107_read_rate(phydev);
+}
+
 static int aqr107_read_status(struct phy_device *phydev)
 {
 	int val, ret;
@@ -460,7 +505,7 @@ static void aqr107_chip_info(struct phy_
 	build_id = FIELD_GET(VEND1_GLOBAL_RSVD_STAT1_FW_BUILD_ID, val);
 	prov_id = FIELD_GET(VEND1_GLOBAL_RSVD_STAT1_PROV_ID, val);
 
-	phydev_dbg(phydev, "FW %u.%u, Build %u, Provisioning %u\n",
+	phydev_info(phydev, "FW %u.%u, Build %u, Provisioning %u\n",
 		   fw_major, fw_minor, build_id, prov_id);
 }
 
@@ -632,6 +677,24 @@ static struct phy_driver aqr_driver[] =
 	.link_change_notify = aqr107_link_change_notify,
 },
 {
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR113C),
+	.name		= "Aquantia AQR113C",
+	.probe		= aqr107_probe,
+	.config_init	= aqr107_config_init,
+	.config_aneg    = aqr_config_aneg,
+	.config_intr	= aqr_config_intr,
+	.ack_interrupt	= aqr_ack_interrupt,
+	.read_status	= aqr113c_read_status,
+	.get_tunable    = aqr107_get_tunable,
+	.set_tunable    = aqr107_set_tunable,
+	.suspend	= aqr107_suspend,
+	.resume		= aqr107_resume,
+	.get_sset_count	= aqr107_get_sset_count,
+	.get_strings	= aqr107_get_strings,
+	.get_stats	= aqr107_get_stats,
+	.link_change_notify = aqr107_link_change_notify,
+},
+{
 	PHY_ID_MATCH_MODEL(PHY_ID_AQCS109),
 	.name		= "Aquantia AQCS109",
 	.probe		= aqr107_probe,
@@ -657,6 +720,24 @@ static struct phy_driver aqr_driver[] =
 	.ack_interrupt	= aqr_ack_interrupt,
 	.read_status	= aqr_read_status,
 },
+{
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR813),
+	.name		= "Aquantia AQR813",
+	.probe		= aqr107_probe,
+	.config_init	= aqr107_config_init,
+	.config_aneg    = aqr_config_aneg,
+	.config_intr	= aqr_config_intr,
+	.ack_interrupt	= aqr_ack_interrupt,
+	.read_status	= aqr113c_read_status,
+	.get_tunable    = aqr107_get_tunable,
+	.set_tunable    = aqr107_set_tunable,
+	.suspend	= aqr107_suspend,
+	.resume		= aqr107_resume,
+	.get_sset_count	= aqr107_get_sset_count,
+	.get_strings	= aqr107_get_strings,
+	.get_stats	= aqr107_get_stats,
+	.link_change_notify = aqr107_link_change_notify,
+},
 };
 
 module_phy_driver(aqr_driver);
@@ -667,8 +748,10 @@ static struct mdio_device_id __maybe_unu
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR105) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR106) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR107) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR113C) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQCS109) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR405) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR813) },
 	{ }
 };
 
