#
# Copyright © 2017 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
cisco-mx100-hw)
	ucidef_set_led_usbport "usb" "USB" "mx100:green:usb" "1-1-port2"
	ucidef_set_led_default "diag" "DIAG" "mx100:green:ha" "1"
	;;
pc-engines-apu1|pc-engines-apu2|pc-engines-apu3)
	ucidef_set_led_netdev "wan" "WAN" "apu:green:3" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "apu:green:2" "br-lan"
	ucidef_set_led_default "diag" "DIAG" "apu:green:1" "1"
	;;
traverse-technologies-geos)
	ucidef_set_led_netdev "lan" "LAN" "geos:1" "br-lan" "tx rx"
	ucidef_set_led_netdev "wlan" "WiFi" "geos:2" "phy0tpt"
	ucidef_set_led_default "diag" "DIAG" "geos:3" "1"
	;;
esac
board_config_flush

exit 0
