// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9331.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &eth0;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "blue:system";
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};
	};

	reg_usb_vbus: reg_usb_vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				reg = <0x0 0x20000>;
				label = "u-boot";
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				reg = <0x20000 0x3d0000>;
				label = "firmware";
			};

			art: partition@3f0000 {
				reg = <0x3f0000 0x10000>;
				label = "art";
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";

	gmac-config {
		device = <&gmac>;

		switch-phy-addr-swap = <0>;
		switch-phy-swap = <0>;
	};
};

&eth1 {
	status = "okay";

	compatible = "syscon", "simple-mfd";
};

&usb {
	dr_mode = "host";
	vbus-supply = <&reg_usb_vbus>;
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";
};

&uboot {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_uboot_1fc00: macaddr@1fc00 {
		reg = <0x1fc00 0x6>;
	};
};
