--- b/arch/arm/boot/dts/qcom-ipq8064.dtsi
+++ a/arch/arm/boot/dts/qcom-ipq8064.dtsi
@@ -1392,6 +1392,12 @@
 			status = "disabled";
 		};
 
+		nss-gmac-common {
+			compatible = "qcom,nss-gmac-common";
+			reg = <0x03000000 0x0000FFFF 0x1bb00000 0x0000FFFF 0x00900000 0x00004000>;
+			reg-names = "nss_reg_base", "qsgmii_reg_base", "clk_ctl_base";
+		};
+
 		gmac0: ethernet@37000000 {
 			device_type = "network";
 			compatible = "qcom,ipq806x-gmac";
@@ -1492,7 +1498,132 @@
 			regulator-always-on;
 		};
 
-		sdcc1bam:dma@12402000 {
+		nss0: nss@40000000 {
+			compatible = "qcom,nss";
+			qcom,low-frequency = <733000000>; /* orig value 110000000 */
+			qcom,mid-frequency = <733000000>; /* orig value 550000000 */
+			qcom,max-frequency = <733000000>;
+
+			interrupts = <GIC_SPI 213 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 232 IRQ_TYPE_LEVEL_HIGH>;
+			reg = <0x36000000 0x1000 0x39000000 0x10000>;
+			reg-names = "nphys", "vphys";
+			clocks = <&gcc NSS_CORE_CLK>, <&gcc NSSTCM_CLK_SRC>,
+				 <&gcc NSSTCM_CLK>, <&rpmcc RPM_NSS_FABRIC_0_CLK>,
+				 <&rpmcc RPM_NSS_FABRIC_1_CLK>;
+			clock-names = "nss-core-clk", "nss-tcm-src",
+				      "nss-tcm-clk", "nss-fab0-clk",
+				      "nss-fab1-clk";
+			resets = <&gcc UBI32_CORE1_CLKRST_CLAMP_RESET>,
+				 <&gcc UBI32_CORE1_CLAMP_RESET>,
+				 <&gcc UBI32_CORE1_AHB_RESET>,
+				 <&gcc UBI32_CORE1_AXI_RESET>;
+			reset-names = "clkrst-clamp", "clamp", "ahb", "axi";
+
+			qcom,id = <0>;
+			qcom,num-irq = <2>;
+			qcom,num-queue = <2>;
+			qcom,load-addr = <0x40000000>;
+			qcom,turbo-frequency;
+
+			qcom,bridge-enabled;
+			qcom,gre-enabled;
+			qcom,gre-redir-enabled;
+			qcom,gre_tunnel_enabled;
+			qcom,ipv4-enabled;
+			qcom,ipv4-reasm-enabled;
+			qcom,ipv6-enabled;
+			qcom,ipv6-reasm-enabled;
+			qcom,l2tpv2-enabled;
+			qcom,map-t-enabled;
+			qcom,pppoe-enabled;
+			qcom,pptp-enabled;
+			qcom,portid-enabled;
+			qcom,shaping-enabled;
+			qcom,tun6rd-enabled;
+			qcom,tunipip6-enabled;
+			qcom,vlan-enabled;
+			qcom,wlan-dataplane-offload-enabled;
+			qcom,wlanredirect-enabled;
+			qcom,pxvlan-enabled;
+			qcom,vxlan-enabled;
+			qcom,match-enabled;
+			qcom,mirror-enabled;
+			qcom,rmnet-enabled;
+			qcom,clmap-enabled;
+		};
+
+		nss1: nss@40800000 {
+			compatible = "qcom,nss";
+			qcom,low-frequency = <733000000>; /* orig value 110000000 */
+			qcom,mid-frequency = <733000000>; /* orig value 550000000 */
+			qcom,max-frequency = <733000000>;
+
+			interrupts = <GIC_SPI 214 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 233 IRQ_TYPE_LEVEL_HIGH>;
+			reg = <0x36400000 0x1000 0x39010000 0x10000>;
+			reg-names = "nphys", "vphys";
+			resets = <&gcc UBI32_CORE2_CLKRST_CLAMP_RESET>,
+				 <&gcc UBI32_CORE2_CLAMP_RESET>,
+				 <&gcc UBI32_CORE2_AHB_RESET>,
+				 <&gcc UBI32_CORE2_AXI_RESET>;
+			reset-names = "clkrst-clamp", "clamp", "ahb", "axi";
+
+			qcom,id = <1>;
+			qcom,num-irq = <2>;
+			qcom,load-addr = <0x40800000>;
+			qcom,num-queue = <2>;
+			qcom,turbo-frequency;
+
+			qcom,capwap-enabled;
+			qcom,crypto-enabled;
+			qcom,dtls-enabled;
+			qcom,ipsec-enabled;
+		};
+
+		crypto1: crypto@38000000 {
+			compatible = "qcom,nss-crypto";
+			reg = <0x38000000 0x20000>, <0x38004000 0x22000>;
+			reg-names = "crypto_pbase", "bam_base";
+			clocks = <&gcc CE5_CORE_CLK>, <&gcc CE5_A_CLK>, <&gcc CE5_H_CLK>;
+			clock-names = "ce5_core", "ce5_aclk", "ce5_hclk";
+			resets = <&gcc CRYPTO_ENG1_RESET>, <&gcc CRYPTO_AHB_RESET>;
+			reset-names = "rst_eng", "rst_ahb";
+			qcom,id = <0>;
+			qcom,ee = <0>;
+		};
+
+		crypto2: crypto@38400000 {
+			compatible = "qcom,nss-crypto";
+			reg = <0x38400000 0x20000>, <0x38404000 0x22000>;
+			reg-names = "crypto_pbase", "bam_base";
+			resets = <&gcc CRYPTO_ENG2_RESET>;
+			reset-names = "rst_eng";
+			qcom,id = <1>;
+			qcom,ee = <0>;
+		};
+
+		crypto3: crypto@38800000 {
+			compatible = "qcom,nss-crypto";
+			reg = <0x38800000 0x20000>, <0x38804000 0x22000>;
+			reg-names = "crypto_pbase", "bam_base";
+			resets = <&gcc CRYPTO_ENG3_RESET>;
+			reset-names = "rst_eng";
+			qcom,id = <2>;
+			qcom,ee = <0>;
+		};
+
+		crypto4: crypto@38c00000 {
+			compatible = "qcom,nss-crypto";
+			reg = <0x38c00000 0x20000>, <0x38c04000 0x22000>;
+			reg-names = "crypto_pbase", "bam_base";
+			resets = <&gcc CRYPTO_ENG4_RESET>;
+			reset-names = "rst_eng";
+			qcom,id = <3>;
+			qcom,ee = <0>;
+		};
+
+		sdcc1bam: dma@12402000 {
 			compatible = "qcom,bam-v1.3.0";
 			reg = <0x12402000 0x8000>;
 			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
@@ -1558,6 +1689,20 @@
 				dma-names = "tx", "rx";
 			};
 		};
+
+		nss-common {
+			compatible = "qcom,nss-common";
+			reg = <0x03000000 0x00001000>;
+			reg-names = "nss_fpb_base";
+			clocks = <&gcc NSS_CORE_CLK>, <&gcc NSSTCM_CLK>,
+				<&rpmcc RPM_NSS_FABRIC_0_CLK>, <&rpmcc RPM_NSS_FABRIC_1_CLK>;
+			clock-names = "nss_core_clk", "nss_tcm_clk",
+				"nss-fab0-clk", "nss-fab1-clk";
+			nss_core-supply = <&smb208_s1b>;
+			nss_core_vdd_nominal = <1100000>;
+			nss_core_vdd_high = <1150000>;
+			nss_core_threshold_freq = <733000000>;
+		};
 	};
 
 	sfpb_mutex: sfpb-mutex {
