// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "avm,fritz736x", "lantiq,xway", "lantiq,vr9";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;

		led-dsl = &led_info_green;
		led-wifi = &led_wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		dect {
			label = "dect";
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_PHONE>;
		};

		wifi {
			label = "wifi";
			gpios = <&gpio 29 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RFKILL>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 32 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
		};

		led_info_green: info_green {
			label = "green:info";
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
		};

		led_wifi: wifi {
			label = "green:wlan";
			gpios = <&gpio 36 GPIO_ACTIVE_LOW>;
		};

		info_red {
			label = "red:info";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
		};

		dect {
			label = "green:dect";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};
	};
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		phy-rst {
			lantiq,pins = "io37", "io44";
			lantiq,pull = <0>;
			lantiq,open-drain;
			lantiq,output = <1>;
		};
	};

};

&gswip {
	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
};

&gswip_mdio {
	phy0: ethernet-phy@0 {
		reg = <0x00>;
		reset-gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
	};

	phy1: ethernet-phy@1 {
		reg = <0x01>;
		reset-gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
	};

	phy11: ethernet-phy@11 {
		reg = <0x11>;
	};

	phy13: ethernet-phy@13 {
		reg = <0x13>;
	};
};

&gswip_ports {
	port@0 {
		reg = <0>;
		label = "lan3";
		phy-mode = "rmii";
		phy-handle = <&phy0>;
	};

	port@1 {
		reg = <1>;
		label = "lan4";
		phy-mode = "rmii";
		phy-handle = <&phy1>;
	};

	port@2 {
		reg = <2>;
		label = "lan2";
		phy-mode = "internal";
		phy-handle = <&phy11>;
	};

	port@4 {
		reg = <4>;
		label = "lan1";
		phy-mode = "internal";
		phy-handle = <&phy13>;
	};
};

&pcie0 {
	status = "okay";

	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <1>;
		#address-cells = <2>;
		device_type = "pci";

		wifi@168c,002e {
			compatible = "pci168c,002e";
			reg = <0 0 0 0 0>;
			qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:01:00.0.bin */
		};
	};
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb1 {
	status = "okay";
};
