// SPDX-License-Identifier: GPL-2.0
#include "qcom-ipq8064-v2.0.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	compatible = "asrock,g10", "qcom,ipq8064";
	model = "ASRock G10";

	aliases {
		ethernet0 = &gmac1;
		ethernet1 = &gmac0;

		led-boot = &led_status_blue;
		led-failsafe = &led_status_amber;
		led-running = &led_status_blue;
		led-upgrade = &led_status_amber;
	};

	chosen {
		bootargs-override = "console=ttyMSM0,115200n8";
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		/*
		 * this is a bit misleading. Because there are about seven
		 * multicolor LEDs connected all wired together in parallel.
		 */

		status_yellow {
			label = "yellow:status";
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		led_status_amber: status_amber {
			label = "amber:status";
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		led_status_blue: status_blue {
			label = "blue:status";
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		/*
		 * LED is declared in vendors boardfile but it's not
		 * working and the manual doesn't mention anything
		 * about the LED being white.

		status_white {
			label = "white:status";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
		};
		*/
	};

	i2c-gpio {
		#address-cells = <1>;
		#size-cells = <0>;

		compatible = "i2c-gpio";
		gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>, /* sda */
			<&qcom_pinmux 54 GPIO_ACTIVE_HIGH>; /* scl */
		i2c-gpio,delay-us = <5>;
		i2c-gpio,scl-output-only;

		mcu@50 {
			reg = <0x50>;
			compatible = "sonix,sn8f25e21";
		};
	};

	keys {
		compatible = "gpio-keys";

		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		ir-remote {
			label = "ir-remote";
			gpios = <&qcom_pinmux 15 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps5g {
			label = "wps5g";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps2g {
			label = "wps2g";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};
};

&adm_dma {
	status = "okay";
};

&gmac1 {
	status = "okay";
	compatible = "qcom,nss-gmac";
	reg = <0x37200000 0x200000>;
	interrupts = <GIC_SPI 223 IRQ_TYPE_LEVEL_HIGH>;
	phy-mode = "rgmii";
	qcom,id = <1>;
	qcom,pcs-chanid = <0>;
	qcom,phy-mdio-addr = <4>;
	qcom,poll-required = <0>;
	qcom,rgmii-delay = <1>;
	qcom,phy_mii_type = <0>;
	qcom,emulation = <0>;
	qcom,forced-speed = <1000>;
	qcom,forced-duplex = <1>;
	qcom,socver = <0>;
	qcom,irq = <255>;
	mdiobus = <&mdio0>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";
	compatible = "qcom,nss-gmac";
	reg = <0x37400000 0x200000>;
	interrupts = <GIC_SPI 226 IRQ_TYPE_LEVEL_HIGH>;
	phy-mode = "sgmii";
	qcom,id = <2>;
	qcom,pcs-chanid = <1>;
	qcom,phy-mdio-addr = <0>;
	qcom,poll-required = <0>;	/* no polling */
	qcom,rgmii-delay = <0>;
	qcom,phy_mii_type = <1>;
	qcom,emulation = <0>;
	qcom,forced-speed = <1000>;
	qcom,forced-duplex = <1>;
	qcom,socver = <0>;
	qcom,irq = <258>;
	mdiobus = <&mdio0>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gsbi4_serial {
	pinctrl-0 = <&uart0_pins>;
	pinctrl-names = "default";
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	ethernet-phy@0 {
		reg = <0>;
		qca,ar8327-initvals = <
			0x00004 0x7600000   /* PAD0_MODE */
			0x00008 0x1000000   /* PAD5_MODE */
			0x0000c 0x80        /* PAD6_MODE */
			0x000e4 0x6a545     /* MAC_POWER_SEL */
			0x000e0 0xc74164de  /* SGMII_CTRL */
			0x0007c 0x4e        /* PORT0_STATUS */
			0x00094 0x4e        /* PORT6_STATUS */
			>;
	};
	
	ethernet-phy@4 {
		reg = <4>;
	};
};

&nand_controller {
	status = "okay";

	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";

	nand@0 {
		reg = <0>;
		compatible = "qcom,nandcs";

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;
		nand-ecc-step-size = <512>;

		partitions {
			compatible = "qcom,smem-part";
		};
	};
};

&pcie0 {
	status = "okay";
};

&pcie1 {
	status = "okay";
};

&qcom_pinmux {
	led_pins: led_pins {
		mux {
			pins = "gpio7", "gpio8", "gpio9", "gpio26";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	button_pins: button_pins {
		mux {
			pins = "gpio15", "gpio16", "gpio64", "gpio65";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	uart0_pins: uart0_pins {
		mux {
			pins = "gpio10", "gpio11";
			function = "gsbi4";
			drive-strength = <10>;
			bias-disable;
		};
	};
};

&rpm {
	pinctrl-0 = <&i2c4_pins>;
	pinctrl-names = "default";
};

&usb3_0 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&tcsr {
	qcom,usb-ctrl-select = <TCSR_USB_SELECT_USB3_DUAL>;
};

/delete-node/ &pcie2_pins;
/delete-node/ &pcie2;
