From caaa71fac36ec8c19145dbf8262a9b77ab09f1a1 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Wed, 4 Mar 2020 22:38:32 +0100
Subject: net: mdio: add ipq8064 mdio driver

Currently ipq806x soc use generic bitbang driver to
comunicate with the gmac ethernet interface.
Add a dedicated driver created by chunkeey to fix this.

Co-developed-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/Kconfig        |   8 ++
 drivers/net/phy/Makefile       |   1 +
 drivers/net/phy/mdio-ipq8064.c | 166 +++++++++++++++++++++++++++++++++++++++++
 3 files changed, 175 insertions(+)
 create mode 100644 drivers/net/phy/mdio-ipq8064.c

--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -156,6 +156,14 @@ config MDIO_I2C
 
 	  This is library mode.
 
+config MDIO_IPQ8064
+	tristate "Qualcomm IPQ8064 MDIO interface support"
+	depends on HAS_IOMEM && OF_MDIO
+	depends on MFD_SYSCON
+	help
+	  This driver supports the MDIO interface found in the network
+	  interface units of the IPQ8064 SoC
+
 config MDIO_MOXART
 	tristate "MOXA ART MDIO interface support"
 	depends on ARCH_MOXART || COMPILE_TEST
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -50,6 +50,7 @@ obj-$(CONFIG_MDIO_CAVIUM)	+= mdio-cavium
 obj-$(CONFIG_MDIO_GPIO)		+= mdio-gpio.o
 obj-$(CONFIG_MDIO_HISI_FEMAC)	+= mdio-hisi-femac.o
 obj-$(CONFIG_MDIO_I2C)		+= mdio-i2c.o
+obj-$(CONFIG_MDIO_IPQ8064)	+= mdio-ipq8064.o
 obj-$(CONFIG_MDIO_MOXART)	+= mdio-moxart.o
 obj-$(CONFIG_MDIO_MSCC_MIIM)	+= mdio-mscc-miim.o
 obj-$(CONFIG_MDIO_OCTEON)	+= mdio-octeon.o
--- /dev/null
+++ b/drivers/net/phy/mdio-ipq8064.c
@@ -0,0 +1,166 @@
+// SPDX-License-Identifier: GPL-2.0
+/* Qualcomm IPQ8064 MDIO interface driver
+ *
+ * Copyright (C) 2019 Christian Lamparter <chunkeey@gmail.com>
+ * Copyright (C) 2020 Ansuel Smith <ansuelsmth@gmail.com>
+ */
+
+#include <linux/delay.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/regmap.h>
+#include <linux/of_mdio.h>
+#include <linux/phy.h>
+#include <linux/platform_device.h>
+#include <linux/mfd/syscon.h>
+
+/* MII address register definitions */
+#define MII_ADDR_REG_ADDR                       0x10
+#define MII_BUSY                                BIT(0)
+#define MII_WRITE                               BIT(1)
+#define MII_CLKRANGE_60_100M                    (0 << 2)
+#define MII_CLKRANGE_100_150M                   (1 << 2)
+#define MII_CLKRANGE_20_35M                     (2 << 2)
+#define MII_CLKRANGE_35_60M                     (3 << 2)
+#define MII_CLKRANGE_150_250M                   (4 << 2)
+#define MII_CLKRANGE_250_300M                   (5 << 2)
+#define MII_CLKRANGE_MASK			GENMASK(4, 2)
+#define MII_REG_SHIFT				6
+#define MII_REG_MASK				GENMASK(10, 6)
+#define MII_ADDR_SHIFT				11
+#define MII_ADDR_MASK				GENMASK(15, 11)
+
+#define MII_DATA_REG_ADDR                       0x14
+
+#define MII_MDIO_DELAY_USEC                     (1000)
+#define MII_MDIO_RETRY_MSEC                     (10)
+
+struct ipq8064_mdio {
+	struct regmap *base; /* NSS_GMAC0_BASE */
+};
+
+static int
+ipq8064_mdio_wait_busy(struct ipq8064_mdio *priv)
+{
+	u32 busy;
+
+	return regmap_read_poll_timeout(priv->base, MII_ADDR_REG_ADDR, busy,
+					!(busy & MII_BUSY), MII_MDIO_DELAY_USEC,
+					MII_MDIO_RETRY_MSEC * USEC_PER_MSEC);
+}
+
+static int
+ipq8064_mdio_read(struct mii_bus *bus, int phy_addr, int reg_offset)
+{
+	u32 miiaddr = MII_BUSY | MII_CLKRANGE_250_300M;
+	struct ipq8064_mdio *priv = bus->priv;
+	u32 ret_val;
+	int err;
+
+	/* Reject clause 45 */
+	if (reg_offset & MII_ADDR_C45)
+		return -EOPNOTSUPP;
+
+	miiaddr |= ((phy_addr << MII_ADDR_SHIFT) & MII_ADDR_MASK) |
+		   ((reg_offset << MII_REG_SHIFT) & MII_REG_MASK);
+
+	regmap_write(priv->base, MII_ADDR_REG_ADDR, miiaddr);
+	usleep_range(8, 10);
+
+	err = ipq8064_mdio_wait_busy(priv);
+	if (err)
+		return err;
+
+	regmap_read(priv->base, MII_DATA_REG_ADDR, &ret_val);
+	return (int)ret_val;
+}
+
+static int
+ipq8064_mdio_write(struct mii_bus *bus, int phy_addr, int reg_offset, u16 data)
+{
+	u32 miiaddr = MII_WRITE | MII_BUSY | MII_CLKRANGE_250_300M;
+	struct ipq8064_mdio *priv = bus->priv;
+
+	/* Reject clause 45 */
+	if (reg_offset & MII_ADDR_C45)
+		return -EOPNOTSUPP;
+
+	regmap_write(priv->base, MII_DATA_REG_ADDR, data);
+
+	miiaddr |= ((phy_addr << MII_ADDR_SHIFT) & MII_ADDR_MASK) |
+		   ((reg_offset << MII_REG_SHIFT) & MII_REG_MASK);
+
+	regmap_write(priv->base, MII_ADDR_REG_ADDR, miiaddr);
+	usleep_range(8, 10);
+
+	return ipq8064_mdio_wait_busy(priv);
+}
+
+static int
+ipq8064_mdio_probe(struct platform_device *pdev)
+{
+	struct device_node *np = pdev->dev.of_node;
+	struct ipq8064_mdio *priv;
+	struct mii_bus *bus;
+	int ret;
+
+	bus = devm_mdiobus_alloc_size(&pdev->dev, sizeof(*priv));
+	if (!bus)
+		return -ENOMEM;
+
+	bus->name = "ipq8064_mdio_bus";
+	bus->read = ipq8064_mdio_read;
+	bus->write = ipq8064_mdio_write;
+	snprintf(bus->id, MII_BUS_ID_SIZE, "%s-mii", dev_name(&pdev->dev));
+	bus->parent = &pdev->dev;
+
+	priv = bus->priv;
+	priv->base = device_node_to_regmap(np);
+	if (IS_ERR(priv->base)) {
+		if (priv->base == ERR_PTR(-EPROBE_DEFER))
+			return -EPROBE_DEFER;
+
+		dev_err(&pdev->dev, "error getting device regmap, error=%pe\n",
+			priv->base);
+		return PTR_ERR(priv->base);
+	}
+
+	ret = of_mdiobus_register(bus, np);
+	if (ret)
+		return ret;
+
+	platform_set_drvdata(pdev, bus);
+	return 0;
+}
+
+static int
+ipq8064_mdio_remove(struct platform_device *pdev)
+{
+	struct mii_bus *bus = platform_get_drvdata(pdev);
+
+	mdiobus_unregister(bus);
+
+	return 0;
+}
+
+static const struct of_device_id ipq8064_mdio_dt_ids[] = {
+	{ .compatible = "qcom,ipq8064-mdio" },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, ipq8064_mdio_dt_ids);
+
+static struct platform_driver ipq8064_mdio_driver = {
+	.probe = ipq8064_mdio_probe,
+	.remove = ipq8064_mdio_remove,
+	.driver = {
+		.name = "ipq8064-mdio",
+		.of_match_table = ipq8064_mdio_dt_ids,
+	},
+};
+
+module_platform_driver(ipq8064_mdio_driver);
+
+MODULE_DESCRIPTION("Qualcomm IPQ8064 MDIO interface driver");
+MODULE_AUTHOR("Christian Lamparter <chunkeey@gmail.com>");
+MODULE_AUTHOR("Ansuel Smith <ansuelsmth@gmail.com>");
+MODULE_LICENSE("GPL");
