#include "amazonse.dtsi"

/ {
	compatible = "allnet,all0333cj", "lantiq,xway", "lantiq,ase";
	model = "Allnet ALL0333CJ DSL Modem";

	chosen {
		bootargs = "console=ttyLTQ0,115200";

		aliases {
			led-boot = &power;
			led-failsafe = &power;
			led-running = &power;
			led-upgrade = &power;

			led-dsl = &dsl;
			led-internet = &online_green;
		};
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x1000000>;
	};

	leds {
		compatible = "gpio-leds";

		/* power led: red=off, green=on */
		power: power {
			label = "green:power";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		lan: lan {
			label = "green:lan";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		dsl: dsl {
			label = "green:dsl";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		online_green: online {
			label = "green:online";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};
		online_red {
			label = "red:online";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		keys_in {
			lantiq,pins = "io0",/* "io25", */"io29";
			lantiq,pull = <2>;
			lantiq,open-drain = <1>;
		};
	};
};

&gsw {
	phy-mode = "mii";
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x400000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x10000>;
				read-only;
			};

			partition@10000 {
				label = "firmware";
				reg = <0x10000 0x3ef200>;
			};

			partition@3ff200 {
				label = "u-boot-env";
				reg = <0x3ff200 0xc00>;
				read-only;
			};

			partition@3ffe00 {
				label = "dummy_bits";
				reg = <0x3ffe00 0x200>;
				read-only;
			};
		};
	};
};
