// SPDX-License-Identifier: BSD-3-Clause
/*
 *  Copyright(c) 2017 Kristian Evensen <kristian.evensen@gmail.com>.
 *  Copyright(c) 2017 Piotr Dymacz <pepe2k@gmail.com>.
 *  All rights reserved.
 */

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "unielec,u7621-06", "mediatek,mt7621-soc";

	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	gpio-export {
		compatible = "gpio-export";
		#size-cells = <0>;

		modem_reset {
			gpio-export,name = "modem_reset";
			gpio-export,output = <1>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status: status {
			label = "green:status";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
		};

		led4 {
			label = "green:led4";
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
		};

		led5 {
			label = "green:led5";
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
		};
	};
};

&sdhci {
	status = "okay";
};

&pcie {
	status = "okay";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan1";
		};

		port@1 {
			status = "okay";
			label = "lan2";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};

		port@3 {
			status = "okay";
			label = "lan4";
		};

		wan: port@4 {
			status = "okay";
			label = "wan";
		};
	};
};

&state_default {
	gpio {
		groups = "jtag", "uart2", "wdt";
		function = "gpio";
	};
};
