From a58855e02a8a0a0de898efcfb0e4790076a0d640 Mon Sep 17 00:00:00 2001
From: Marc Kleine-Budde <mkl@pengutronix.de>
Date: Sat, 2 Jan 2021 21:38:58 +0100
Subject: [PATCH] overlays: Add overlay for Seeed Studio CAN BUS FD HAT
 v1 (based on mcp2517fd)

This patch adds the overlay for the Seeed Studio CAN BUS FD HAT v1 with two CAN
FD Channels (based on mcp2517fd).

https://www.seeedstudio.com/2-Channel-CAN-BUS-FD-Shield-for-Raspberry-Pi-p-4072.html

The overlay was generated by:
ovmerge -c spi1-1cs-overlay.dts,cs0_pin=18,cs0_spidev=false \
           mcp251xfd-overlay.dts,spi0-0,interrupt=25 \
           mcp251xfd-overlay.dts,spi1-0,interrupt=24

Signed-off-by: Marc Kleine-Budde <mkl@pengutronix.de>
---
 arch/arm/boot/dts/overlays/Makefile           |   1 +
 arch/arm/boot/dts/overlays/README             |   8 +
 .../overlays/seeed-can-fd-hat-v1-overlay.dts  | 138 ++++++++++++++++++
 3 files changed, 147 insertions(+)
 create mode 100644 arch/arm/boot/dts/overlays/seeed-can-fd-hat-v1-overlay.dts

--- a/arch/arm/boot/dts/overlays/Makefile
+++ b/arch/arm/boot/dts/overlays/Makefile
@@ -161,6 +161,7 @@ dtbo-$(CONFIG_ARCH_BCM2835) += \
 	sc16is752-spi1.dtbo \
 	sdhost.dtbo \
 	sdio.dtbo \
+	seeed-can-fd-hat-v1.dtbo \
 	seeed-can-fd-hat-v2.dtbo \
 	sh1106-spi.dtbo \
 	smi.dtbo \
--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -2504,6 +2504,14 @@ Info:   This overlay is now deprecated.
 Load:   <Deprecated>
 
 
+Name:   seeed-can-fd-hat-v1
+Info:   Overlay for Seeed Studio CAN BUS FD HAT with two CAN FD channels
+        (based on the mcp2517fd).
+        https://www.seeedstudio.com/2-Channel-CAN-BUS-FD-Shield-for-Raspberry-Pi-p-4072.html
+Load:   dtoverlay=seeed-can-fd-hat-v1
+Params: <None>
+
+
 Name:   seeed-can-fd-hat-v2
 Info:   Overlay for Seeed Studio CAN BUS FD HAT with two CAN FD channels
         (based on the mcp2518fd) and an RTC.
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/seeed-can-fd-hat-v1-overlay.dts
@@ -0,0 +1,138 @@
+// redo: ovmerge -c spi1-1cs-overlay.dts,cs0_pin=18,cs0_spidev=false mcp251xfd-overlay.dts,spi0-0,interrupt=25 mcp251xfd-overlay.dts,spi1-0,interrupt=24
+
+// Device tree overlay for https://www.seeedstudio.com/2-Channel-CAN-BUS-FD-Shield-for-Raspberry-Pi-p-4072.html
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/interrupt-controller/irq.h>
+#include <dt-bindings/pinctrl/bcm2835.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi1_pins: spi1_pins {
+				brcm,pins = <19 20 21>;
+				brcm,function = <3>;
+			};
+			spi1_cs_pins: spi1_cs_pins {
+				brcm,pins = <18>;
+				brcm,function = <1>;
+			};
+		};
+	};
+	fragment@1 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins &spi1_cs_pins>;
+			cs-gpios = <&gpio 18 1>;
+			status = "okay";
+			spidev@0 {
+				compatible = "spidev";
+				reg = <0>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "disabled";
+			};
+		};
+	};
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@3 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+	fragment@4 {
+		target = <&gpio>;
+		__overlay__ {
+			mcp251xfd_pins: mcp251xfd_spi0_0_pins {
+				brcm,pins = <25>;
+				brcm,function = <BCM2835_FSEL_GPIO_IN>;
+			};
+		};
+	};
+	fragment@5 {
+		target-path = "/clocks";
+		__overlay__ {
+			clk_mcp251xfd_osc: mcp251xfd-spi0-0-osc {
+				#clock-cells = <0>;
+				compatible = "fixed-clock";
+				clock-frequency = <40000000>;
+			};
+		};
+	};
+	fragment@6 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			mcp251xfd@0 {
+				compatible = "microchip,mcp251xfd";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&mcp251xfd_pins>;
+				spi-max-frequency = <20000000>;
+				interrupt-parent = <&gpio>;
+				interrupts = <25 IRQ_TYPE_LEVEL_LOW>;
+				clocks = <&clk_mcp251xfd_osc>;
+			};
+		};
+	};
+	fragment@7 {
+		target-path = "spi1/spidev@0";
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+	fragment@8 {
+		target = <&gpio>;
+		__overlay__ {
+			mcp251xfd_pins_1: mcp251xfd_spi1_0_pins {
+				brcm,pins = <24>;
+				brcm,function = <BCM2835_FSEL_GPIO_IN>;
+			};
+		};
+	};
+	fragment@9 {
+		target-path = "/clocks";
+		__overlay__ {
+			clk_mcp251xfd_osc_1: mcp251xfd-spi1-0-osc {
+				#clock-cells = <0>;
+				compatible = "fixed-clock";
+				clock-frequency = <40000000>;
+			};
+		};
+	};
+	fragment@10 {
+		target = <&spi1>;
+		__overlay__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			mcp251xfd@0 {
+				compatible = "microchip,mcp251xfd";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&mcp251xfd_pins_1>;
+				spi-max-frequency = <20000000>;
+				interrupt-parent = <&gpio>;
+				interrupts = <24 IRQ_TYPE_LEVEL_LOW>;
+				clocks = <&clk_mcp251xfd_osc_1>;
+			};
+		};
+	};
+};
