From 85252792bc07b398582e8dacf6ec6d09a5075195 Mon Sep 17 00:00:00 2001
From: Alex Marginean <alexandru.marginean@nxp.com>
Date: Tue, 7 Jan 2020 15:15:29 +0200
Subject: [PATCH] arm64: dts: fsl-ls1028a-rdb: fix QSGMII PHY node names

Use ethernet-phy@ADDR, previously the numbers were wrong.

Signed-off-by: Alex Marginean <alexandru.marginean@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1028a-rdb.dts | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1028a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1028a-rdb.dts
@@ -215,19 +215,19 @@
 };
 
 &enetc_mdio_pf3 {
-	qsgmii_phy1: ethernet-phy@4 {
+	qsgmii_phy1: ethernet-phy@10 {
 		reg = <0x10>;
 	};
 
-	qsgmii_phy2: ethernet-phy@5 {
+	qsgmii_phy2: ethernet-phy@11 {
 		reg = <0x11>;
 	};
 
-	qsgmii_phy3: ethernet-phy@6 {
+	qsgmii_phy3: ethernet-phy@12 {
 		reg = <0x12>;
 	};
 
-	qsgmii_phy4: ethernet-phy@7 {
+	qsgmii_phy4: ethernet-phy@13 {
 		reg = <0x13>;
 	};
 };
