From 709ef2034f5ba06da35f89856ad7baf2b7a41287 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Mon, 28 Jan 2013 20:06:28 +0100
Subject: [PATCH 10/11] MIPS: BCM63XX: register EHCI controller if board
 enables it

BCM63XX-based board can control the registration of the EHCI controller
by setting their has_ehci0 flag to 1. Handle this in the generic
code dealing with board registration and call the actual helper to register
the EHCI controller.

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |    4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -27,6 +27,7 @@
 #include <bcm63xx_dev_hsspi.h>
 #include <bcm63xx_dev_pcmcia.h>
 #include <bcm63xx_dev_spi.h>
+#include <bcm63xx_dev_usb_ehci.h>
 #include <bcm63xx_dev_usb_ohci.h>
 #include <bcm63xx_dev_usb_usbd.h>
 #include <board_bcm963xx.h>
@@ -893,6 +894,9 @@ int __init board_register_devices(void)
 	if (board.has_usbd)
 		bcm63xx_usbd_register(&board.usbd);
 
+	if (board.has_ehci0)
+		bcm63xx_ehci_register();
+
 	if (board.has_ohci0)
 		bcm63xx_ohci_register();
 
