From cf908990d4a8ccdb73ee4484aa8cadad379ca314 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Sun, 30 Nov 2014 14:54:27 +0100
Subject: [PATCH 2/5] irqchip: add support for bcm6345-style external
 interrupt controller

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 .../interrupt-controller/brcm,bcm6345-ext-intc.txt |   29 ++
 drivers/irqchip/Kconfig                            |    4 +
 drivers/irqchip/Makefile                           |    1 +
 drivers/irqchip/irq-bcm6345-ext.c                  |  287 ++++++++++++++++++++
 include/linux/irqchip/irq-bcm6345-ext.h            |   14 +
 5 files changed, 335 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/interrupt-controller/brcm,bcm6345-ext-intc.txt
 create mode 100644 drivers/irqchip/irq-bcm6345-ext.c
 create mode 100644 include/linux/irqchip/irq-bcm6345-ext.h

--- /dev/null
+++ b/Documentation/devicetree/bindings/interrupt-controller/brcm,bcm6345-ext-intc.txt
@@ -0,0 +1,29 @@
+Broadcom BCM6345-style external interrupt controller
+
+Required properties:
+
+- compatible: Should be "brcm,bcm6345-ext-intc" or "brcm,bcm6318-ext-intc".
+- reg: Specifies the base physical addresses and size of the registers.
+- interrupt-controller: identifies the node as an interrupt controller.
+- #interrupt-cells: Specifies the number of cells needed to encode an interrupt
+  source, Should be 2.
+- interrupt-parent: Specifies the phandle to the parent interrupt controller
+  this one is cascaded from.
+- interrupts: Specifies the interrupt line(s) in the interrupt-parent controller
+  node, valid values depend on the type of parent interrupt controller.
+
+Optional properties:
+
+- brcm,field-width: Size of each field (mask, clear, sense, ...) in bits in the
+  register. Defaults to 4.
+
+Example:
+
+ext_intc: interrupt-controller@10000018 {
+	compatible = "brcm,bcm6345-ext-intc";
+	interrupt-parent = <&periph_intc>;
+	#interrupt-cells = <2>;
+	reg = <0x10000018 0x4>;
+	interrupt-controller;
+	interrupts = <24>, <25>, <26>, <27>;
+};
--- a/drivers/irqchip/Kconfig
+++ b/drivers/irqchip/Kconfig
@@ -145,6 +145,10 @@ config DAVINCI_CP_INTC
 	select GENERIC_IRQ_CHIP
 	select IRQ_DOMAIN
 
+config BCM6345_EXT_IRQ
+	bool
+	select IRQ_DOMAIN
+
 config BCM6345_PERIPH_IRQ
 	bool
 	select IRQ_DOMAIN
--- a/drivers/irqchip/Makefile
+++ b/drivers/irqchip/Makefile
@@ -17,6 +17,7 @@ obj-$(CONFIG_ARCH_MMP)			+= irq-mmp.o
 obj-$(CONFIG_IRQ_MXS)			+= irq-mxs.o
 obj-$(CONFIG_ARCH_TEGRA)		+= irq-tegra.o
 obj-$(CONFIG_ARCH_S3C24XX)		+= irq-s3c24xx.o
+obj-$(CONFIG_BCM6345_EXT_IRQ)		+= irq-bcm6345-ext.o
 obj-$(CONFIG_BCM6345_PERIPH_IRQ)	+= irq-bcm6345-periph.o
 obj-$(CONFIG_DW_APB_ICTL)		+= irq-dw-apb-ictl.o
 obj-$(CONFIG_CLPS711X_IRQCHIP)		+= irq-clps711x.o
--- /dev/null
+++ b/drivers/irqchip/irq-bcm6345-ext.c
@@ -0,0 +1,301 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 2014 Jonas Gorski <jogo@openwrt.org>
+ */
+
+#include <linux/ioport.h>
+#include <linux/irq.h>
+#include <linux/irqchip.h>
+#include <linux/irqchip/chained_irq.h>
+#include <linux/irqchip/irq-bcm6345-ext.h>
+#include <linux/kernel.h>
+#include <linux/of.h>
+#include <linux/of_irq.h>
+#include <linux/of_address.h>
+#include <linux/slab.h>
+#include <linux/spinlock.h>
+
+#ifdef CONFIG_BCM63XX
+#include <asm/mach-bcm63xx/bcm63xx_irq.h>
+
+#define VIRQ_BASE		IRQ_EXTERNAL_BASE
+#else
+#define VIRQ_BASE		0
+#endif
+
+#define MAX_IRQS		4
+
+#define EXTIRQ_CFG_SENSE	0
+#define EXTIRQ_CFG_STAT		1
+#define EXTIRQ_CFG_CLEAR	2
+#define EXTIRQ_CFG_MASK		3
+#define EXTIRQ_CFG_BOTHEDGE	4
+#define EXTIRQ_CFG_LEVELSENSE	5
+
+struct intc_data {
+	struct irq_chip chip;
+	struct irq_domain *domain;
+	raw_spinlock_t lock;
+
+	int parent_irq[MAX_IRQS];
+	void __iomem *reg;
+	int shift;
+	unsigned int toggle_clear_on_ack:1;
+};
+
+static void bcm6345_ext_intc_irq_handle(struct irq_desc *desc)
+{
+	struct intc_data *data = irq_desc_get_handler_data(desc);
+	struct irq_chip *chip = irq_desc_get_chip(desc);
+	unsigned int irq = irq_desc_get_irq(desc);
+	unsigned int idx;
+
+	chained_irq_enter(chip, desc);
+
+	for (idx = 0; idx < MAX_IRQS; idx++) {
+		if (data->parent_irq[idx] != irq)
+			continue;
+
+		generic_handle_irq(irq_find_mapping(data->domain, idx));
+	}
+
+	chained_irq_exit(chip, desc);
+}
+
+static void bcm6345_ext_intc_irq_ack(struct irq_data *data)
+{
+	struct intc_data *priv = data->domain->host_data;
+	irq_hw_number_t hwirq = irqd_to_hwirq(data);
+	u32 reg;
+
+	raw_spin_lock(&priv->lock);
+	reg = __raw_readl(priv->reg);
+	__raw_writel(reg | (1 << (hwirq + EXTIRQ_CFG_CLEAR * priv->shift)),
+		     priv->reg);
+	if (priv->toggle_clear_on_ack)
+		__raw_writel(reg, priv->reg);
+	raw_spin_unlock(&priv->lock);
+}
+
+static void bcm6345_ext_intc_irq_mask(struct irq_data *data)
+{
+	struct intc_data *priv = data->domain->host_data;
+	irq_hw_number_t hwirq = irqd_to_hwirq(data);
+	u32 reg;
+
+	raw_spin_lock(&priv->lock);
+	reg = __raw_readl(priv->reg);
+	reg &= ~(1 << (hwirq + EXTIRQ_CFG_MASK * priv->shift));
+	__raw_writel(reg, priv->reg);
+	raw_spin_unlock(&priv->lock);
+}
+
+static void bcm6345_ext_intc_irq_unmask(struct irq_data *data)
+{
+	struct intc_data *priv = data->domain->host_data;
+	irq_hw_number_t hwirq = irqd_to_hwirq(data);
+	u32 reg;
+
+	raw_spin_lock(&priv->lock);
+	reg = __raw_readl(priv->reg);
+	reg |= 1 << (hwirq + EXTIRQ_CFG_MASK * priv->shift);
+	__raw_writel(reg, priv->reg);
+	raw_spin_unlock(&priv->lock);
+}
+
+static int bcm6345_ext_intc_set_type(struct irq_data *data,
+				     unsigned int flow_type)
+{
+	struct intc_data *priv = data->domain->host_data;
+	irq_hw_number_t hwirq = irqd_to_hwirq(data);
+	bool levelsense = 0, sense = 0, bothedge = 0;
+	u32 reg;
+
+	flow_type &= IRQ_TYPE_SENSE_MASK;
+
+	if (flow_type == IRQ_TYPE_NONE)
+		flow_type = IRQ_TYPE_LEVEL_LOW;
+
+	switch (flow_type) {
+	case IRQ_TYPE_EDGE_BOTH:
+		bothedge = 1;
+		break;
+
+	case IRQ_TYPE_EDGE_RISING:
+		sense = 1;
+		break;
+
+	case IRQ_TYPE_EDGE_FALLING:
+		break;
+
+	case IRQ_TYPE_LEVEL_HIGH:
+		levelsense = 1;
+		sense = 1;
+		break;
+
+	case IRQ_TYPE_LEVEL_LOW:
+		levelsense = 1;
+		break;
+
+	default:
+		pr_err("bogus flow type combination given!\n");
+		return -EINVAL;
+	}
+
+	raw_spin_lock(&priv->lock);
+	reg = __raw_readl(priv->reg);
+
+	if (levelsense)
+		reg |= 1 << (hwirq + EXTIRQ_CFG_LEVELSENSE * priv->shift);
+	else
+		reg &= ~(1 << (hwirq + EXTIRQ_CFG_LEVELSENSE * priv->shift));
+	if (sense)
+		reg |= 1 << (hwirq + EXTIRQ_CFG_SENSE * priv->shift);
+	else
+		reg &= ~(1 << (hwirq + EXTIRQ_CFG_SENSE * priv->shift));
+	if (bothedge)
+		reg |= 1 << (hwirq + EXTIRQ_CFG_BOTHEDGE * priv->shift);
+	else
+		reg &= ~(1 << (hwirq + EXTIRQ_CFG_BOTHEDGE * priv->shift));
+
+	__raw_writel(reg, priv->reg);
+	raw_spin_unlock(&priv->lock);
+
+	irqd_set_trigger_type(data, flow_type);
+	if (flow_type & (IRQ_TYPE_LEVEL_LOW | IRQ_TYPE_LEVEL_HIGH))
+		irq_set_handler_locked(data, handle_level_irq);
+	else
+		irq_set_handler_locked(data, handle_edge_irq);
+
+	return 0;
+}
+
+static int bcm6345_ext_intc_map(struct irq_domain *d, unsigned int irq,
+				irq_hw_number_t hw)
+{
+	struct intc_data *priv = d->host_data;
+
+	irq_set_chip_and_handler(irq, &priv->chip, handle_level_irq);
+
+	return 0;
+}
+
+static const struct irq_domain_ops bcm6345_ext_domain_ops = {
+	.xlate = irq_domain_xlate_twocell,
+	.map = bcm6345_ext_intc_map,
+};
+
+static int __init __bcm6345_ext_intc_init(struct device_node *node,
+					  int num_irqs, int *irqs,
+					  void __iomem *reg, int shift,
+					  bool toggle_clear_on_ack)
+{
+	struct intc_data *data;
+	unsigned int i;
+	int start = VIRQ_BASE;
+
+	data = kzalloc(sizeof(*data), GFP_KERNEL);
+	if (!data)
+		return -ENOMEM;
+
+	raw_spin_lock_init(&data->lock);
+
+	for (i = 0; i < num_irqs; i++) {
+		data->parent_irq[i] = irqs[i];
+
+		irq_set_handler_data(irqs[i], data);
+		irq_set_chained_handler(irqs[i], bcm6345_ext_intc_irq_handle);
+	}
+
+	data->reg = reg;
+	data->shift = shift;
+	data->toggle_clear_on_ack = toggle_clear_on_ack;
+
+	data->chip.name = "bcm6345-ext-intc";
+	data->chip.irq_ack = bcm6345_ext_intc_irq_ack;
+	data->chip.irq_mask = bcm6345_ext_intc_irq_mask;
+	data->chip.irq_unmask = bcm6345_ext_intc_irq_unmask;
+	data->chip.irq_set_type = bcm6345_ext_intc_set_type;
+
+	/*
+	 * If we have less than 4 irqs, this is the second controller on
+	 * bcm63xx. So increase the VIRQ start to not overlap with the first
+	 * one, but only do so if we actually use a non-zero start.
+	 *
+	 * This can be removed when bcm63xx has no legacy users anymore.
+	 */
+	if (start && num_irqs < 4)
+		start += 4;
+
+	data->domain = irq_domain_add_simple(node, num_irqs, start,
+					     &bcm6345_ext_domain_ops, data);
+	if (!data->domain) {
+		kfree(data);
+		return -ENOMEM;
+	}
+
+	return 0;
+}
+
+void __init bcm6345_ext_intc_init(int num_irqs, int *irqs, void __iomem *reg,
+				  int shift)
+{
+	__bcm6345_ext_intc_init(NULL, num_irqs, irqs, reg, shift, false);
+}
+
+#ifdef CONFIG_OF
+static int __init bcm6345_ext_intc_of_init(struct device_node *node,
+					   struct device_node *parent)
+{
+	int num_irqs, ret = -EINVAL;
+	unsigned i;
+	void __iomem *base;
+	int irqs[MAX_IRQS] = { 0 };
+	u32 shift;
+	bool toggle_clear_on_ack = false;
+
+	num_irqs = of_irq_count(node);
+
+	if (!num_irqs || num_irqs > MAX_IRQS)
+		return -EINVAL;
+
+	if (of_property_read_u32(node, "brcm,field-width", &shift))
+		shift = 4;
+
+	/* on BCM6318 setting CLEAR seems to continuously mask interrupts */
+	if (of_device_is_compatible(node, "brcm,bcm6318-ext-intc"))
+		toggle_clear_on_ack = true;
+
+	for (i = 0; i < num_irqs; i++) {
+		irqs[i] = irq_of_parse_and_map(node, i);
+		if (!irqs[i]) {
+			ret = -ENOMEM;
+			goto out_unmap;
+		}
+	}
+
+	base = of_iomap(node, 0);
+	if (!base)
+		goto out_unmap;
+
+	ret = __bcm6345_ext_intc_init(node, num_irqs, irqs, base, shift,
+				      toggle_clear_on_ack);
+	if (!ret)
+		return 0;
+out_unmap:
+	iounmap(base);
+
+	for (i = 0; i < num_irqs; i++)
+		irq_dispose_mapping(irqs[i]);
+
+	return ret;
+}
+
+IRQCHIP_DECLARE(bcm6318_ext_intc, "brcm,bcm6318-ext-intc",
+		bcm6345_ext_intc_of_init);
+IRQCHIP_DECLARE(bcm6345_ext_intc, "brcm,bcm6345-ext-intc",
+		bcm6345_ext_intc_of_init);
+#endif
--- /dev/null
+++ b/include/linux/irqchip/irq-bcm6345-ext.h
@@ -0,0 +1,14 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 2014 Jonas Gorski <jogo@openwrt.org>
+ */
+
+#ifndef __INCLUDE_LINUX_IRQCHIP_IRQ_BCM6345_EXT_H
+#define __INCLUDE_LINUX_IRQCHIP_IRQ_BCM6345_EXT_H
+
+void bcm6345_ext_intc_init(int n_irqs, int *irqs, void __iomem *reg, int shift);
+
+#endif /* __INCLUDE_LINUX_IRQCHIP_IRQ_BCM6345_EXT_H */
