// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "rtl8382_d-link_dgs-1210.dtsi"

/ {
	compatible = "d-link,dgs-1210-16", "realtek,rtl838x-soc";
	model = "D-Link DGS-1210-16";
};

&ethernet0 {
	mdio: mdio-bus {
		compatible = "realtek,rtl838x-mdio";
		regmap = <&ethernet0>;
		#address-cells = <1>;
		#size-cells = <0>;

		EXTERNAL_PHY(0)
		EXTERNAL_PHY(1)
		EXTERNAL_PHY(2)
		EXTERNAL_PHY(3)
		EXTERNAL_PHY(4)
		EXTERNAL_PHY(5)
		EXTERNAL_PHY(6)
		EXTERNAL_PHY(7)

		INTERNAL_PHY(8)
		INTERNAL_PHY(9)
		INTERNAL_PHY(10)
		INTERNAL_PHY(11)
		INTERNAL_PHY(12)
		INTERNAL_PHY(13)
		INTERNAL_PHY(14)
		INTERNAL_PHY(15)

		EXTERNAL_SFP_PHY(24)
		EXTERNAL_SFP_PHY(25)
		EXTERNAL_SFP_PHY(26)
		EXTERNAL_SFP_PHY(27)
	};
};

&switch0 {
	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		SWITCH_PORT(0, 1, qsgmii)
		SWITCH_PORT(1, 2, qsgmii)
		SWITCH_PORT(2, 3, qsgmii)
		SWITCH_PORT(3, 4, qsgmii)
		SWITCH_PORT(4, 5, qsgmii)
		SWITCH_PORT(5, 6, qsgmii)
		SWITCH_PORT(6, 7, qsgmii)
		SWITCH_PORT(7, 8, qsgmii)

		SWITCH_PORT(8, 9, internal)
		SWITCH_PORT(9, 10, internal)
		SWITCH_PORT(10, 11, internal)
		SWITCH_PORT(11, 12, internal)
		SWITCH_PORT(12, 13, internal)
		SWITCH_PORT(13, 14, internal)
		SWITCH_PORT(14, 15, internal)
		SWITCH_PORT(15, 16, internal)

		SWITCH_PORT(24, 17, qsgmii)
		SWITCH_PORT(25, 18, qsgmii)
		SWITCH_PORT(26, 19, qsgmii)
		SWITCH_PORT(27, 20, qsgmii)

		port@28 {
			ethernet = <&ethernet0>;
			reg = <28>;
			phy-mode = "internal";
			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};
	};
};
