From 038ee7126dcfe172eefa1ee4c271af51fc9e633c Mon Sep 17 00:00:00 2001
From: Naushir Patuck <naush@raspberrypi.com>
Date: Wed, 2 Dec 2020 16:48:41 +0000
Subject: [PATCH] media: bcm2835-unicam: Clear clock state when
 stopping streaming

Commit 65e08c465020d4c5b51afb452efc2246d80fd66f failed to clear the
clock state when the device stopped streaming. Fix this, as it might
again cause the same problems when doing an unprepare.

Signed-off-by: Naushir Patuck <naush@raspberrypi.com>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -1769,6 +1769,7 @@ static void unicam_stop_streaming(struct
 
 			clk_disable_unprepare(dev->vpu_clock);
 			clk_disable_unprepare(dev->clock);
+			dev->clocks_enabled = false;
 		}
 		unicam_runtime_put(dev);
 
