// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "ASUS RT-AC58U";
	compatible = "asus,rt-ac58u";

	memory {
		device_type = "memory";
		reg = <0x80000000 0x8000000>;
	};

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	chosen {
		bootargs-append = " ubi.mtd=UBI_DEV";
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
		};

		ess-psgmii@98000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		usb3@8af8800 {
			status = "okay";

			dwc3@8a00000 {
				#address-cells = <1>;
				#size-cells = <0>;

				usb3_port1: port@1 {
					reg = <1>;
					#trigger-source-cells = <0>;
				};

				usb3_port2: port@2 {
					reg = <2>;
					#trigger-source-cells = <0>;
				};
			};
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};

		ess-switch@c000000 {
			status = "okay";
		};

		edma@c080000 {
			status = "okay";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 4 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: status {
			label = "blue:status";
			gpios = <&tlmm 3 GPIO_ACTIVE_HIGH>;
		};

		wan {
			label = "blue:wan";
			gpios = <&tlmm 1 GPIO_ACTIVE_HIGH>;
		};

		wlan2G {
			label = "blue:wlan2G";
			gpios = <&tlmm 58 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5G {
			label = "blue:wlan5G";
			gpios = <&tlmm 5 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};

		usb {
			label = "blue:usb";
			gpios = <&tlmm 0 GPIO_ACTIVE_HIGH>;
			trigger-sources = <&usb3_port1>, <&usb3_port2>;
			linux,default-trigger = "usbport";
		};

		lan {
			label = "blue:lan";
			gpios = <&tlmm 2 GPIO_ACTIVE_HIGH>;
		};
	};
};

&cryptobam {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		mux {
			function = "blsp_spi0";
			pins = "gpio55", "gpio56", "gpio57";
			drive-strength = <12>;
			bias-disable;
		};

		mux_cs {
			function = "gpio";
			pins = "gpio54", "gpio59";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp1_spi1 { /* BLSP1 QUP1 */
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>,
		   <&tlmm 59 GPIO_ACTIVE_HIGH>;

	flash@0 {
		/*
		 * U-boot looks for "n25q128a11" node,
		 * if we don't have it, it will spit out the following warning:
		 * "ipq: fdt fixup unable to find compatible node".
		 */
		compatible = "jedec,spi-nor";
		reg = <0>;
		linux,modalias = "m25p80", "mx25l1606e", "n25q128a11";
		spi-max-frequency = <30000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x00000000 0x00040000>;
				read-only;
			};
			partition@40000 {
				label = "MIBIB";
				reg = <0x00040000 0x00020000>;
				read-only;
			};
			partition@60000 {
				label = "QSEE";
				reg = <0x00060000 0x00060000>;
				read-only;
			};
			partition@c0000 {
				label = "CDT";
				reg = <0x000c0000 0x00010000>;
				read-only;
			};
			partition@d0000 {
				label = "DDRPARAMS";
				reg = <0x000d0000 0x00010000>;
				read-only;
			};
			partition@e0000 {
				label = "APPSBLENV"; /* uboot env*/
				reg = <0x000e0000 0x00010000>;
				read-only;
			};
			partition@f0000 {
				label = "APPSBL"; /* uboot */
				reg = <0x000f0000 0x00080000>;
				read-only;
			};
			partition@170000 {
				label = "ART";
				reg = <0x00170000 0x00010000>;
				read-only;
			};
			/* 0x00180000 - 0x00200000 unused */
		};
	};

	spi-nand@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <30000000>;

		/*
		 * U-boot looks for "spinand,mt29f" node,
		 * if we don't have it, it will spit out the following warning:
		 * "ipq: fdt fixup unable to find compatible node".
		 */

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				/*
				 * TODO: change to label = "ubi" once we drop 4.14.
				 *       also drop the bootargs-append and all the
				 *	 userspace CI_UBIPART="UBI_DEV" remains.
				 */
				label = "UBI_DEV";
				reg = <0x00000000 0x08000000>;
			};
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&usb3_ss_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "RT-AC58U";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "RT-AC58U";
};
