#include "rt3050.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "unbranded,wr512-3gn", "ralink,rt3052-soc";

	aliases {
		led-boot = &led_wps;
		led-failsafe = &led_wps;
		led-running = &led_wps;
		led-upgrade = &led_wps;
	};

	leds {
		compatible = "gpio-leds";

		3g {
			label = "green:3g";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		gateway {
			label = "green:gateway";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		ap {
			label = "green:ap";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		led_wps: wps {
			label = "green:wps";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};

		station {
			label = "green:station";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset_wps {
			label = "reset_wps";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		mode {
			label = "mode";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};
	};
};

&state_default {
	gpio {
		groups = "spi", "i2c", "jtag", "rgmii", "mdio", "uartf";
		function = "gpio";
	};
};

&esw {
	mediatek,portmap = <0x2f>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;
};

&otg {
	status = "okay";
};
