#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power;
		led-running = &power;
		led-upgrade = &power;

		led-dsl = &dsl;
		led-internet = &online;
		led-usb = &led_usb;
		led-wifi = &wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	ath5k_eep {
		compatible = "ath5k,eeprom";
		ath,eep-flash = <&boardconfig 0x400>;
		ath,mac-offset = <0x16>;
		ath,mac-increment = <1>;
		ath,eep-swap;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		rfkill {
			label = "rfkill";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		power: power {
			label = "power";
			gpios = <&gpio 3 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};
		dsl: dsl {
			label = "dsl";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		online: online {
			label = "online";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "wifi";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		wps {
			label = "wps";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};
		dsl2 {
			label = "dsl2";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		led_usb: usb {
			label = "usb";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
		voice {
			label = "voice";
			gpios = <&gpiomm 0 GPIO_ACTIVE_LOW>;
		};
		fxs1 {
			label = "fxs1";
			gpios = <&gpiomm 1 GPIO_ACTIVE_LOW>;
		};
		fxs2 {
			label = "fxs2";
			gpios = <&gpiomm 2 GPIO_ACTIVE_LOW>;
		};
		fxo {
			label = "fxo";
			gpios = <&gpiomm 3 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 14 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		ebu {
			lantiq,groups = "ebu cs1";
			lantiq,function = "ebu";
		};
	};
};

&gsw {
	phy-mode = "mii";
	nvmem-cells = <&macaddr_boardconfig_16>;
	nvmem-cell-names = "mac-address";
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x2000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x10000>; /* 64 KB */
				read-only;
			};

			partition@10000 {
				label = "u-boot-env";
				reg = <0x10000 0x10000>; /* 64 KB */
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0x3d0000>;
			};

			boardconfig: partition@3f0000 {
				label = "boardconfig";
				reg = <0x3f0000 0x10000>;
				read-only;
			};
		};
	};

	gpiomm: gpio@1 {
		compatible = "lantiq,gpio-mm";
		reg = <1 0x0 0x10 >;
		#address-cells = <1>;
		#size-cells = <1>;
		#gpio-cells = <2>;
		gpio-controller;
		lantiq,shadow = <0x0>;
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_gnt2_pins>,
		    <&pci_req1_pins>, <&pci_req2_pins>;
	pinctrl-names = "default";

	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
	req-mask = <0xf>;
};

&usb_phy {
	status = "okay";
};

&usb {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&vmmc {
	status = "okay";
	gpios = <&gpio 31 GPIO_ACTIVE_HIGH>;
};

&boardconfig {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_boardconfig_16: macaddr@16 {
		reg = <0x16 0x6>;
	};
};
