From: Felix Fietkau <nbd@nbd.name>
Date: Sun, 26 Jul 2020 14:03:21 +0200
Subject: [PATCH] net: add support for threaded NAPI polling

For some drivers (especially 802.11 drivers), doing a lot of work in the NAPI
poll function does not perform well. Since NAPI poll is bound to the CPU it
was scheduled from, we can easily end up with a few very busy CPUs spending
most of their time in softirq/ksoftirqd and some idle ones.

Introduce threaded NAPI for such drivers based on a workqueue. The API is the
same except for using netif_threaded_napi_add instead of netif_napi_add.

In my tests with mt76 on MT7621 using threaded NAPI + a thread for tx scheduling
improves LAN->WLAN bridging throughput by 10-50%. Throughput without threaded
NAPI is wildly inconsistent, depending on the CPU that runs the tx scheduling
thread.

With threaded NAPI it seems stable and consistent (and higher than the best
results I got without it).

Based on a patch by Hillf Danton

Cc: Hillf Danton <hdanton@sina.com>
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/include/linux/netdevice.h
+++ b/include/linux/netdevice.h
@@ -340,6 +340,7 @@ struct napi_struct {
 	struct list_head	dev_list;
 	struct hlist_node	napi_hash_node;
 	unsigned int		napi_id;
+	struct work_struct	work;
 };
 
 enum {
@@ -350,6 +351,7 @@ enum {
 	NAPI_STATE_HASHED,	/* In NAPI hash (busy polling possible) */
 	NAPI_STATE_NO_BUSY_POLL,/* Do not add in napi_hash, no busy polling */
 	NAPI_STATE_IN_BUSY_POLL,/* sk_busy_loop() owns this NAPI */
+	NAPI_STATE_THREADED,	/* Use threaded NAPI */
 };
 
 enum {
@@ -360,6 +362,7 @@ enum {
 	NAPIF_STATE_HASHED	 = BIT(NAPI_STATE_HASHED),
 	NAPIF_STATE_NO_BUSY_POLL = BIT(NAPI_STATE_NO_BUSY_POLL),
 	NAPIF_STATE_IN_BUSY_POLL = BIT(NAPI_STATE_IN_BUSY_POLL),
+	NAPIF_STATE_THREADED	 = BIT(NAPI_STATE_THREADED),
 };
 
 enum gro_result {
@@ -2101,6 +2104,7 @@ struct net_device {
 	struct lock_class_key	addr_list_lock_key;
 	bool			proto_down;
 	unsigned		wol_enabled:1;
+	unsigned		threaded:1;
 };
 #define to_net_dev(d) container_of(d, struct net_device, dev)
 
@@ -2281,6 +2285,26 @@ void netif_napi_add(struct net_device *d
 		    int (*poll)(struct napi_struct *, int), int weight);
 
 /**
+ *	netif_threaded_napi_add - initialize a NAPI context
+ *	@dev:  network device
+ *	@napi: NAPI context
+ *	@poll: polling function
+ *	@weight: default weight
+ *
+ * This variant of netif_napi_add() should be used from drivers using NAPI
+ * with CPU intensive poll functions.
+ * This will schedule polling from a high priority workqueue
+ */
+static inline void netif_threaded_napi_add(struct net_device *dev,
+					   struct napi_struct *napi,
+					   int (*poll)(struct napi_struct *, int),
+					   int weight)
+{
+	set_bit(NAPI_STATE_THREADED, &napi->state);
+	netif_napi_add(dev, napi, poll, weight);
+}
+
+/**
  *	netif_tx_napi_add - initialize a NAPI context
  *	@dev:  network device
  *	@napi: NAPI context
--- a/net/core/dev.c
+++ b/net/core/dev.c
@@ -156,6 +156,7 @@ static DEFINE_SPINLOCK(offload_lock);
 struct list_head ptype_base[PTYPE_HASH_SIZE] __read_mostly;
 struct list_head ptype_all __read_mostly;	/* Taps */
 static struct list_head offload_base __read_mostly;
+static struct workqueue_struct *napi_workq __read_mostly;
 
 static int netif_rx_internal(struct sk_buff *skb);
 static int call_netdevice_notifiers_info(unsigned long val,
@@ -5931,6 +5932,11 @@ void __napi_schedule(struct napi_struct
 {
 	unsigned long flags;
 
+	if (test_bit(NAPI_STATE_THREADED, &n->state)) {
+		queue_work(napi_workq, &n->work);
+		return;
+	}
+
 	local_irq_save(flags);
 	____napi_schedule(this_cpu_ptr(&softnet_data), n);
 	local_irq_restore(flags);
@@ -5982,6 +5988,10 @@ EXPORT_SYMBOL(napi_schedule_prep);
  */
 void __napi_schedule_irqoff(struct napi_struct *n)
 {
+	if (test_bit(NAPI_STATE_THREADED, &n->state)) {
+		queue_work(napi_workq, &n->work);
+		return;
+	}
 	if (!IS_ENABLED(CONFIG_PREEMPT_RT))
 		____napi_schedule(this_cpu_ptr(&softnet_data), n);
 	else
@@ -6246,9 +6256,89 @@ static void init_gro_hash(struct napi_st
 	napi->gro_bitmask = 0;
 }
 
+static int __napi_poll(struct napi_struct *n, bool *repoll)
+{
+	int work, weight;
+
+	weight = n->weight;
+
+	/* This NAPI_STATE_SCHED test is for avoiding a race
+	 * with netpoll's poll_napi().  Only the entity which
+	 * obtains the lock and sees NAPI_STATE_SCHED set will
+	 * actually make the ->poll() call.  Therefore we avoid
+	 * accidentally calling ->poll() when NAPI is not scheduled.
+	 */
+	work = 0;
+	if (test_bit(NAPI_STATE_SCHED, &n->state)) {
+		work = n->poll(n, weight);
+		trace_napi_poll(n, work, weight);
+	}
+
+	WARN_ON_ONCE(work > weight);
+
+	if (likely(work < weight))
+		return work;
+
+	/* Drivers must not modify the NAPI state if they
+	 * consume the entire weight.  In such cases this code
+	 * still "owns" the NAPI instance and therefore can
+	 * move the instance around on the list at-will.
+	 */
+	if (unlikely(napi_disable_pending(n))) {
+		napi_complete(n);
+		return work;
+	}
+
+	if (n->gro_bitmask) {
+		/* flush too old packets
+		 * If HZ < 1000, flush all packets.
+		 */
+		napi_gro_flush(n, HZ >= 1000);
+	}
+
+	gro_normal_list(n);
+
+	*repoll = true;
+
+	return work;
+}
+
+static void napi_workfn(struct work_struct *work)
+{
+	struct napi_struct *n = container_of(work, struct napi_struct, work);
+	void *have;
+
+	for (;;) {
+		bool repoll = false;
+
+		local_bh_disable();
+
+		have = netpoll_poll_lock(n);
+		__napi_poll(n, &repoll);
+		netpoll_poll_unlock(have);
+
+		local_bh_enable();
+
+		if (!repoll)
+			return;
+
+		if (!need_resched())
+			continue;
+
+		/*
+		 * have to pay for the latency of task switch even if
+		 * napi is scheduled
+		 */
+		queue_work(napi_workq, work);
+		return;
+	}
+}
+
 void netif_napi_add(struct net_device *dev, struct napi_struct *napi,
 		    int (*poll)(struct napi_struct *, int), int weight)
 {
+	if (dev->threaded)
+		set_bit(NAPI_STATE_THREADED, &napi->state);
 	INIT_LIST_HEAD(&napi->poll_list);
 	hrtimer_init(&napi->timer, CLOCK_MONOTONIC, HRTIMER_MODE_REL_PINNED);
 	napi->timer.function = napi_watchdog;
@@ -6265,6 +6355,7 @@ void netif_napi_add(struct net_device *d
 #ifdef CONFIG_NETPOLL
 	napi->poll_owner = -1;
 #endif
+	INIT_WORK(&napi->work, napi_workfn);
 	set_bit(NAPI_STATE_SCHED, &napi->state);
 	set_bit(NAPI_STATE_NPSVC, &napi->state);
 	list_add_rcu(&napi->dev_list, &dev->napi_list);
@@ -6305,6 +6396,7 @@ static void flush_gro_hash(struct napi_s
 void netif_napi_del(struct napi_struct *napi)
 {
 	might_sleep();
+	cancel_work_sync(&napi->work);
 	if (napi_hash_del(napi))
 		synchronize_net();
 	list_del_init(&napi->dev_list);
@@ -6317,50 +6409,18 @@ EXPORT_SYMBOL(netif_napi_del);
 
 static int napi_poll(struct napi_struct *n, struct list_head *repoll)
 {
+	bool do_repoll = false;
 	void *have;
-	int work, weight;
+	int work;
 
 	list_del_init(&n->poll_list);
 
 	have = netpoll_poll_lock(n);
 
-	weight = n->weight;
-
-	/* This NAPI_STATE_SCHED test is for avoiding a race
-	 * with netpoll's poll_napi().  Only the entity which
-	 * obtains the lock and sees NAPI_STATE_SCHED set will
-	 * actually make the ->poll() call.  Therefore we avoid
-	 * accidentally calling ->poll() when NAPI is not scheduled.
-	 */
-	work = 0;
-	if (test_bit(NAPI_STATE_SCHED, &n->state)) {
-		work = n->poll(n, weight);
-		trace_napi_poll(n, work, weight);
-	}
-
-	WARN_ON_ONCE(work > weight);
+	work = __napi_poll(n, &do_repoll);
 
-	if (likely(work < weight))
-		goto out_unlock;
-
-	/* Drivers must not modify the NAPI state if they
-	 * consume the entire weight.  In such cases this code
-	 * still "owns" the NAPI instance and therefore can
-	 * move the instance around on the list at-will.
-	 */
-	if (unlikely(napi_disable_pending(n))) {
-		napi_complete(n);
+	if (!do_repoll)
 		goto out_unlock;
-	}
-
-	if (n->gro_bitmask) {
-		/* flush too old packets
-		 * If HZ < 1000, flush all packets.
-		 */
-		napi_gro_flush(n, HZ >= 1000);
-	}
-
-	gro_normal_list(n);
 
 	/* Some drivers may have called napi_schedule
 	 * prior to exhausting their budget.
@@ -10340,6 +10400,10 @@ static int __init net_dev_init(void)
 		sd->backlog.weight = weight_p;
 	}
 
+	napi_workq = alloc_workqueue("napi_workq", WQ_UNBOUND | WQ_HIGHPRI,
+				     WQ_UNBOUND_MAX_ACTIVE | WQ_SYSFS);
+	BUG_ON(!napi_workq);
+
 	dev_boot_phase = 0;
 
 	/* The loopback device is special if any other network devices
--- a/net/core/net-sysfs.c
+++ b/net/core/net-sysfs.c
@@ -442,6 +442,52 @@ static ssize_t proto_down_store(struct d
 }
 NETDEVICE_SHOW_RW(proto_down, fmt_dec);
 
+static int change_napi_threaded(struct net_device *dev, unsigned long val)
+{
+	struct napi_struct *napi;
+
+	if (list_empty(&dev->napi_list))
+		return -EOPNOTSUPP;
+
+	list_for_each_entry(napi, &dev->napi_list, dev_list) {
+		if (val)
+			set_bit(NAPI_STATE_THREADED, &napi->state);
+		else
+			clear_bit(NAPI_STATE_THREADED, &napi->state);
+	}
+
+	return 0;
+}
+
+static ssize_t napi_threaded_store(struct device *dev,
+				struct device_attribute *attr,
+				const char *buf, size_t len)
+{
+	return netdev_store(dev, attr, buf, len, change_napi_threaded);
+}
+
+static ssize_t napi_threaded_show(struct device *dev,
+				  struct device_attribute *attr,
+				  char *buf)
+{
+	struct net_device *netdev = to_net_dev(dev);
+	struct napi_struct *napi;
+	bool enabled = false;
+
+	if (!rtnl_trylock())
+		return restart_syscall();
+
+	list_for_each_entry(napi, &netdev->napi_list, dev_list) {
+		if (test_bit(NAPI_STATE_THREADED, &napi->state))
+			enabled = true;
+	}
+
+	rtnl_unlock();
+
+	return sprintf(buf, fmt_dec, enabled);
+}
+static DEVICE_ATTR_RW(napi_threaded);
+
 static ssize_t phys_port_id_show(struct device *dev,
 				 struct device_attribute *attr, char *buf)
 {
@@ -532,6 +578,7 @@ static struct attribute *net_class_attrs
 	&dev_attr_flags.attr,
 	&dev_attr_tx_queue_len.attr,
 	&dev_attr_gro_flush_timeout.attr,
+	&dev_attr_napi_threaded.attr,
 	&dev_attr_phys_port_id.attr,
 	&dev_attr_phys_port_name.attr,
 	&dev_attr_phys_switch_id.attr,
