--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -2650,6 +2650,9 @@ static int mv88e6xxx_setup_port(struct m
 	if (dsa_is_cpu_port(ds, port))
 		reg = 0;
 
+	/* Disable ATU member violation interrupt */
+	reg |= MV88E6XXX_PORT_ASSOC_VECTOR_IGNORE_WRONG;
+
 	err = mv88e6xxx_port_write(chip, port, MV88E6XXX_PORT_ASSOC_VECTOR,
 				   reg);
 	if (err)
