
. /lib/functions/uci-defaults.sh

board_config_update

if [ -e "/sys/bus/mdio_bus/drivers/IC+ IP175C/0:00" -o \
     -e "/sys/bus/mdio_bus/drivers/IC+ IP17xx/0:00" ] && \
   [ -x /sbin/swconfig ];
then
	ucidef_add_switch "eth0" \
		"0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "5@eth0"

elif [ -e "/sys/bus/mdio_bus/drivers/Infineon ADM6996/0:00" -o \
       -e "/sys/bus/mdio_bus/drivers/Marvell 88E6060/0:10" ];
then
	ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"

elif [ -d /sys/class/net/eth1 ]; then
	ucidef_set_interfaces_lan_wan "eth0" "eth1"

else
	ucidef_set_interface_lan "eth0"
fi

board_config_flush

exit 0
