From 632ddf978565378e7efb9ea77c0ba239ea66bfdc Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Fri, 13 Nov 2020 11:09:19 +0100
Subject: [PATCH] ARM: dts: BCM5301X: Disable USB 3 PHY on devices without USB
 3
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

It seems pointless to have it enabled.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm4708-luxul-xap-1510.dts       | 4 ----
 arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts       | 4 ----
 arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts | 4 ----
 arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts      | 4 ----
 arch/arm/boot/dts/bcm47081-luxul-xwr-1200.dts      | 4 ----
 arch/arm/boot/dts/bcm47081-tplink-archer-c5-v2.dts | 4 ----
 6 files changed, 24 deletions(-)

--- a/arch/arm/boot/dts/bcm4708-luxul-xap-1510.dts
+++ b/arch/arm/boot/dts/bcm4708-luxul-xap-1510.dts
@@ -57,10 +57,6 @@
 	status = "okay";
 };
 
-&usb3_phy {
-	status = "okay";
-};
-
 &srab {
 	status = "okay";
 
--- a/arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts
+++ b/arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts
@@ -64,10 +64,6 @@
 	status = "okay";
 };
 
-&usb3_phy {
-	status = "okay";
-};
-
 &srab {
 	status = "okay";
 
--- a/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
@@ -117,7 +117,3 @@
 		};
 	};
 };
-
-&usb3_phy {
-	status = "okay";
-};
--- a/arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts
+++ b/arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts
@@ -57,10 +57,6 @@
 	status = "okay";
 };
 
-&usb3_phy {
-	status = "okay";
-};
-
 &srab {
 	status = "okay";
 
--- a/arch/arm/boot/dts/bcm47081-luxul-xwr-1200.dts
+++ b/arch/arm/boot/dts/bcm47081-luxul-xwr-1200.dts
@@ -105,10 +105,6 @@
 	status = "okay";
 };
 
-&usb3_phy {
-	status = "okay";
-};
-
 &srab {
 	status = "okay";
 
--- a/arch/arm/boot/dts/bcm47081-tplink-archer-c5-v2.dts
+++ b/arch/arm/boot/dts/bcm47081-tplink-archer-c5-v2.dts
@@ -126,7 +126,3 @@
 &usb2 {
 	vcc-gpio = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
 };
-
-&usb3_phy {
-	status = "okay";
-};
