From 9b3303413379af8bed307cd465fe7aa1bc3569ea Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Wed, 24 Mar 2021 09:19:18 +0100
Subject: [PATCH 17/22] dt-bindings: add BCM63268 pincontroller binding
 documentation
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add binding documentation for the pincontrol core found in the BCM63268
family SoCs.

Co-developed-by: Jonas Gorski <jonas.gorski@gmail.com>
Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Reviewed-by: Rob Herring <robh@kernel.org>
Link: https://lore.kernel.org/r/20210324081923.20379-18-noltari@gmail.com
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 .../pinctrl/brcm,bcm63268-pinctrl.yaml        | 164 ++++++++++++++++++
 1 file changed, 164 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/pinctrl/brcm,bcm63268-pinctrl.yaml

--- /dev/null
+++ b/Documentation/devicetree/bindings/pinctrl/brcm,bcm63268-pinctrl.yaml
@@ -0,0 +1,164 @@
+# SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/pinctrl/brcm,bcm63268-pinctrl.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Broadcom BCM63268 pin controller
+
+maintainers:
+  - Álvaro Fernández Rojas <noltari@gmail.com>
+  - Jonas Gorski <jonas.gorski@gmail.com>
+
+description:
+  Bindings for Broadcom's BCM63268 memory-mapped pin controller.
+
+properties:
+  compatible:
+    const: brcm,bcm63268-pinctrl
+
+  reg:
+    maxItems: 3
+
+patternProperties:
+  '-pins$':
+    type: object
+    $ref: pinmux-node.yaml#
+
+    properties:
+      function:
+        enum: [ serial_led_clk, serial_led_data, hsspi_cs4, hsspi_cs5,
+                hsspi_cs6, hsspi_cs7, adsl_spi_miso, adsl_spi_mosi,
+                vreq_clk, pcie_clkreq_b, robosw_led_clk, robosw_led_data,
+                nand, gpio35_alt, dectpd, vdsl_phy_override_0,
+                vdsl_phy_override_1, vdsl_phy_override_2,
+                vdsl_phy_override_3, dsl_gpio8, dsl_gpio9 ]
+
+      pins:
+        enum: [ gpio0, gpio1, gpio16, gpio17, gpio8, gpio9, gpio18, gpio19,
+                gpio22, gpio23, gpio30, gpio31, nand_grp, gpio35
+                dectpd_grp, vdsl_phy_override_0_grp,
+                vdsl_phy_override_1_grp, vdsl_phy_override_2_grp,
+                vdsl_phy_override_3_grp, dsl_gpio8, dsl_gpio9 ]
+
+required:
+  - compatible
+  - reg
+
+additionalProperties: false
+
+examples:
+  - |
+    pinctrl@10 {
+      compatible = "brcm,bcm63268-pinctrl";
+      reg = <0x10 0x4>, <0x18 0x8>, <0x38 0x4>;
+
+      pinctrl_serial_led: serial_led-pins {
+        pinctrl_serial_led_clk: serial_led_clk-pins {
+          function = "serial_led_clk";
+          pins = "gpio0";
+        };
+
+        pinctrl_serial_led_data: serial_led_data-pins {
+          function = "serial_led_data";
+          pins = "gpio1";
+        };
+      };
+
+      pinctrl_hsspi_cs4: hsspi_cs4-pins {
+        function = "hsspi_cs4";
+        pins = "gpio16";
+      };
+
+      pinctrl_hsspi_cs5: hsspi_cs5-pins {
+        function = "hsspi_cs5";
+        pins = "gpio17";
+      };
+
+      pinctrl_hsspi_cs6: hsspi_cs6-pins {
+        function = "hsspi_cs6";
+        pins = "gpio8";
+      };
+
+      pinctrl_hsspi_cs7: hsspi_cs7-pins {
+        function = "hsspi_cs7";
+        pins = "gpio9";
+      };
+
+      pinctrl_adsl_spi: adsl_spi-pins {
+        pinctrl_adsl_spi_miso: adsl_spi_miso-pins {
+          function = "adsl_spi_miso";
+          pins = "gpio18";
+        };
+
+        pinctrl_adsl_spi_mosi: adsl_spi_mosi-pins {
+          function = "adsl_spi_mosi";
+          pins = "gpio19";
+        };
+      };
+
+      pinctrl_vreq_clk: vreq_clk-pins {
+        function = "vreq_clk";
+        pins = "gpio22";
+      };
+
+      pinctrl_pcie_clkreq_b: pcie_clkreq_b-pins {
+        function = "pcie_clkreq_b";
+        pins = "gpio23";
+      };
+
+      pinctrl_robosw_led_clk: robosw_led_clk-pins {
+        function = "robosw_led_clk";
+        pins = "gpio30";
+      };
+
+      pinctrl_robosw_led_data: robosw_led_data-pins {
+        function = "robosw_led_data";
+        pins = "gpio31";
+      };
+
+      pinctrl_nand: nand-pins {
+        function = "nand";
+        group = "nand_grp";
+      };
+
+      pinctrl_gpio35_alt: gpio35_alt-pins {
+        function = "gpio35_alt";
+        pin = "gpio35";
+      };
+
+      pinctrl_dectpd: dectpd-pins {
+        function = "dectpd";
+        group = "dectpd_grp";
+      };
+
+      pinctrl_vdsl_phy_override_0: vdsl_phy_override_0-pins {
+        function = "vdsl_phy_override_0";
+        group = "vdsl_phy_override_0_grp";
+      };
+
+      pinctrl_vdsl_phy_override_1: vdsl_phy_override_1-pins {
+        function = "vdsl_phy_override_1";
+        group = "vdsl_phy_override_1_grp";
+      };
+
+      pinctrl_vdsl_phy_override_2: vdsl_phy_override_2-pins {
+        function = "vdsl_phy_override_2";
+        group = "vdsl_phy_override_2_grp";
+      };
+
+      pinctrl_vdsl_phy_override_3: vdsl_phy_override_3-pins {
+        function = "vdsl_phy_override_3";
+        group = "vdsl_phy_override_3_grp";
+      };
+
+      pinctrl_dsl_gpio8: dsl_gpio8-pins {
+        function = "dsl_gpio8";
+        group = "dsl_gpio8";
+      };
+
+      pinctrl_dsl_gpio9: dsl_gpio9-pins {
+        function = "dsl_gpio9";
+        group = "dsl_gpio9";
+      };
+    };
