--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -49,6 +49,17 @@ config BSC9132_QDS
 	  and dual StarCore SC3850 DSP cores.
 	  Manufacturer : Freescale Semiconductor, Inc
 
+config HIVEAP_330
+    bool "Aerohive HiveAP-330"
+    select DEFAULT_UIMAGE
+    select ARCH_REQUIRE_GPIOLIB
+    select GPIO_MPC8XXX
+    help
+      This option enables support for the Aerohive HiveAP-330 board.
+
+      This board is a Concurrent Dual-Band wireless access point with a
+      Freescale P1020 SoC.
+
 config MPC8540_ADS
 	bool "Freescale MPC8540 ADS"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -10,6 +10,7 @@ obj-y += common.o
 obj-$(CONFIG_BSC9131_RDB) += bsc913x_rdb.o
 obj-$(CONFIG_BSC9132_QDS) += bsc913x_qds.o
 obj-$(CONFIG_C293_PCIE)   += c293pcie.o
+obj-$(CONFIG_HIVEAP_330) += hiveap-330.o
 obj-$(CONFIG_MPC8540_ADS) += mpc85xx_ads.o
 obj-$(CONFIG_MPC8560_ADS) += mpc85xx_ads.o
 obj-$(CONFIG_MPC85xx_CDS) += mpc85xx_cds.o
