From fdba7c7bc334f72bd8641bbd63f3596ba68650c1 Mon Sep 17 00:00:00 2001
From: Biwen Li <biwen.li@nxp.com>
Date: Thu, 8 Aug 2019 12:13:02 +0800
Subject: [PATCH] arm64: dts: fix endianness of rcpm

Add little-endian property of rcpm for ls1028a,ls1088a,ls208xa

Signed-off-by: Biwen Li <biwen.li@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1028a.dtsi | 1 +
 arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi | 1 +
 arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi | 1 +
 3 files changed, 3 insertions(+)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1028a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1028a.dtsi
@@ -836,6 +836,7 @@
 			compatible = "fsl,ls1028a-rcpm", "fsl,qoriq-rcpm-2.1+";
 			reg = <0x0 0x1e34040 0x0 0x1c>;
 			#fsl,rcpm-wakeup-cells = <7>;
+			little-endian;
 		};
 
 		ftm_alarm0: timer@2800000 {
--- a/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
@@ -792,6 +792,7 @@
 			compatible = "fsl,ls1088a-rcpm", "fsl,qoriq-rcpm-2.1+";
 			reg = <0x0 0x1e34040 0x0 0x18>;
 			#fsl,rcpm-wakeup-cells = <6>;
+			little-endian;
 		};
 
 		ftm_alarm0: timer@2800000 {
--- a/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
@@ -761,6 +761,7 @@
 			compatible = "fsl,ls208xa-rcpm", "fsl,qoriq-rcpm-2.1+";
 			reg = <0x0 0x1e34040 0x0 0x18>;
 			#fsl,rcpm-wakeup-cells = <6>;
+			little-endian;
 		};
 
 		ftm_alarm0: timer@2800000 {
