From patchwork Thu Feb  6 17:19:41 2020
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Daniel Golle <daniel@makrotopia.org>
X-Patchwork-Id: 1234465
Date: Thu, 6 Feb 2020 19:19:41 +0200
From: Daniel Golle <daniel@makrotopia.org>
To: linux-mtd@lists.infradead.org
Subject: [PATCH v2] mtd: spi-nor: Add support for xt25f128b chip
Message-ID: <20200206171941.GA2398@makrotopia.org>
MIME-Version: 1.0
Content-Disposition: inline
List-Subscribe: <http://lists.infradead.org/mailman/listinfo/linux-mtd>,
 <mailto:linux-mtd-request@lists.infradead.org?subject=subscribe>
Cc: Eitan Cohen <eitan@neot-semadar.com>, Piotr Dymacz <pepe2k@gmail.com>,
 Tudor Ambarus <tudor.ambarus@microchip.com>
Sender: "linux-mtd" <linux-mtd-bounces@lists.infradead.org>
Errors-To: linux-mtd-bounces+incoming=patchwork.ozlabs.org@lists.infradead.org

Add XT25F128B made by XTX Technology (Shenzhen) Limited.
This chip supports dual and quad read and uniform 4K-byte erase.
Verified on Teltonika RUT955 which comes with XT25F128B in recent
versions of the device.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/mtd/spi-nor/spi-nor.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -2506,6 +2506,9 @@ static const struct flash_info spi_nor_i
 	/* XMC (Wuhan Xinxin Semiconductor Manufacturing Corp.) */
 	{ "XM25QH64A", INFO(0x207017, 0, 64 * 1024, 128, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ "XM25QH128A", INFO(0x207018, 0, 64 * 1024, 256, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+
+	/* XTX Technology (Shenzhen) Limited */
+	{ "xt25f128b", INFO(0x0B4018, 0, 64 * 1024, 256, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ },
 };
 
