// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "TP-Link RE350K v1";
	compatible = "tplink,re350k-v1", "qca,qca9558";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		mdio-gpio0 = &mdio2;
	};

	keys {
		compatible = "gpio-keys";

		app-config {
			label = "app-config";
			linux,code = <BTN_0>;
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		led {
			label = "led";
			linux,code = <BTN_1>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g_green {
			label = "green:wlan2g";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan2g_red {
			label = "red:wlan2g";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
		};

		wlan5g_green {
			label = "green:wlan5g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g_red {
			label = "red:wlan5g";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};
	};

	mdio2: mdio {
		compatible = "virtual,mdio-gpio";

		#address-cells = <1>;
		#size-cells = <0>;

		gpios = <&gpio 23 GPIO_ACTIVE_HIGH>,
			<&gpio 18 GPIO_ACTIVE_HIGH>;

		phy4: ethernet-phy@4 {
			reg = <4>;

			phy-mode = "rgmii-rxid";
			eee-broken-100tx;
			eee-broken-1000t;
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy4>;
	pll-data = <0x9e000000 0x80000101 0x80001313>;

	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";

	gmac-config {
		device = <&gmac>;

		rxdv-delay = <2>;
		rxd-delay = <2>;
		txen-delay = <0>;
		txd-delay = <0>;
		rgmii-enabled = <1>;
	};
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0xd70000>;
			};

			partition@d90000 {
				label = "partition-table";
				reg = <0xd90000 0x010000>;
				read-only;
			};

			info: partition@da0000 {
				label = "info";
				reg = <0xda0000 0x020000>;
				read-only;
			};

			partition@dc0000 {
				label = "config";
				reg = <0xdc0000 0x230000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&info {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_info_8: macaddr@8 {
		reg = <0x8 0x6>;
	};
};
