// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "OCEDO Raccoon";
	compatible = "ocedo,raccoon", "qca,ar9344";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	leds {
		compatible = "gpio-leds";

		power {
			label = "green:power";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "yellow:wlan24";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led_system: system {
			label = "blue:sys";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan5g {
			label = "red:wlan5";
			gpios = <&ath9k 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0x740000>;
			};

			partition@790000 {
				label = "vendor";
				reg = <0x790000 0x740000>;
				read-only;
			};

			partition@ed0000 {
				label = "data";
				reg = <0xed0000 0x110000>;
				read-only;
			};

			partition@fe0000 {
				label = "id";
				reg = <0xfe0000 0x010000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,0030";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&macaddr_art_c>;
		nvmem-cell-names = "mac-address";
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";
};

&mdio0 {
	status = "okay";

	phy-mask = <0>;

	phy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x06000000 0x00000101 0x00001313>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii-id";
	phy-handle = <&phy0>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};

	macaddr_art_6: macaddr@6 {
		reg = <0x6 0x6>;
	};

	macaddr_art_c: macaddr@c {
		reg = <0xc 0x6>;
	};
};
