// SPDX-License-Identifier: GPL-2.0-only

#include "ar9132.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "tplink,tl-wr1043nd-v1", "qca,ar9132";
	model = "TP-Link TL-WR1043ND v1";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &eth0;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <40000000>;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		qss {
			label = "qss";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		usb {
			label = "green:usb";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port>;
			linux,default-trigger = "usbport";
		};

		led_system: system {
			label = "green:system";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "heartbeat";
		};

		qss {
			label = "green:qss";
			gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	rtl8366rb {
		compatible = "realtek,rtl8366rb";
		gpio-sda = <&gpio 18 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio 19 GPIO_ACTIVE_HIGH>;

		resets = <&rst 8>;
		reset-names = "switch";
	};
};

&pll {
	clocks = <&extosc>;
};

&usb {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&usb_phy {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x7D0000>;
			};

			art: partition@7F0000 {
				label = "art";
				reg = <0x7F0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";

	phy-mode = "rgmii";
	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";
};

&uboot {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_uboot_1fc00: macaddr@1fc00 {
		reg = <0x1fc00 0x6>;
	};
};
