From 01cb60004018afba6e2b60149e4adbbf9e87d90b Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 10 Nov 2020 11:21:56 +0000
Subject: [PATCH] drm/panel/raspberrypi-ts: Insert delay before polling
 for startup state

In switching to the hardware I2C controller there is an issue
where we seem to not get back the correct state from the Pi
touchscreen.
Insert a delay before polling to avoid this condition.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/panel/panel-raspberrypi-touchscreen.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/gpu/drm/panel/panel-raspberrypi-touchscreen.c
+++ b/drivers/gpu/drm/panel/panel-raspberrypi-touchscreen.c
@@ -299,6 +299,7 @@ static int rpi_touchscreen_enable(struct
 	int i;
 
 	rpi_touchscreen_i2c_write(ts, REG_POWERON, 1);
+	usleep_range(20000, 25000);
 	/* Wait for nPWRDWN to go low to indicate poweron is done. */
 	for (i = 0; i < 100; i++) {
 		if (rpi_touchscreen_i2c_read(ts, REG_PORTB) & 1)
