#include "bcm6368.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Actiontec R1000H";
	compatible = "actiontec,r1000h", "brcm,bcm6368";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&pinctrl 34 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&pinctrl 35 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		inet_green {
			label = "green:inet";
			gpios = <&pinctrl 5 0>;
		};

		usb_green {
			label = "green:usb";
			gpios = <&pinctrl 21 1>;
		};

		led_power_green: power_green {
			label = "green:power";
			gpios = <&pinctrl 22 0>;
			default-state = "on";
		};

		wps_green {
			label = "green:wps";
			gpios = <&pinctrl 23 1>;
		};

		power_red {
			label = "red:power";
			gpios = <&pinctrl 24 0>;
		};

		wps_red {
			label = "red:wps";
			gpios = <&pinctrl 30 1>;
		};

		inet_red {
			label = "red:inet";
			gpios = <&pinctrl 31 0>;
		};
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		CFE@0 {
			reg = <0x000000 0x020000>;
			read-only;
		};

		linux@20000 {
			reg = <0x020000 0x1fc0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		nvram@1fe0000 {
			reg = <0x1fe0000 0x20000>;
		};
	};
};

&uart0 {
	status = "okay";
};

&uart1 {
	status = "okay";
};
