From 81589b5e28022d0a4738981f9e5ffb9fadcfaa5b Mon Sep 17 00:00:00 2001
From: notro <notro@tronnes.org>
Date: Wed, 9 Jul 2014 14:46:08 +0200
Subject: [PATCH] BCM2708: Add core Device Tree support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add the bare minimum needed to boot BCM2708 from a Device Tree.

Signed-off-by: Noralf Tronnes <notro@tronnes.org>

BCM2708: DT: change 'axi' nodename to 'soc'

Change DT node named 'axi' to 'soc' so it matches ARCH_BCM2835.
The VC4 bootloader fills in certain properties in the 'axi' subtree,
but since this is part of an upstreaming effort, the name is changed.

Signed-off-by: Noralf Tronnes notro@tronnes.org

BCM2708_DT: Correct length of the peripheral space

Use dts-dirs feature for overlays.

The kernel makefiles have a dts-dirs target that is for vendor subdirectories.

Using this fixes the install_dtbs target, which previously did not install the overlays.

BCM270X_DT: configure I2S DMA channels

Signed-off-by: Matthias Reichl <hias@horus.com>

BCM270X_DT: switch to bcm2835-i2s

I2S soundcard drivers with proper devicetree support (i.e. not linking
to the cpu_dai/platform via name but to cpu/platform via of_node)
will work out of the box without any modifications.

When the kernel is compiled without devicetree support the platform
code will instantiate the bcm2708-i2s driver and I2S soundcard drivers
will link to it via name, as before.

Signed-off-by: Matthias Reichl <hias@horus.com>

SDIO-overlay: add poll_once-boolean parameter

Add paramter to toggle sdio-device-polling
done every second or once at boot-time.

Signed-off-by: Patrick Boettcher <patrick.boettcher@posteo.de>

BCM270X_DT: Make mmc overlay compatible with current firmware

The original DT overlay logic followed a merge-then-patch procedure,
i.e. parameters are applied to the loaded overlay before the overlay
is merged into the base DTB. This sequence has been changed to
patch-then-merge, in order to support parameterised node names, and
to protect against bad overlays. As a result, overrides (parameters)
must only target labels in the overlay, but the overlay can obviously target nodes in the base DTB.

mmc-overlay.dts (that switches back to the original mmc sdcard
driver) is the only overlay violating that rule, and this patch
fixes it.

bcm270x_dt: Use the sdhost MMC controller by default

The "mmc" overlay reverts to using the other controller.

squash: Add cprman to dt

BCM270X_DT: Use clk_core for I2C interfaces

BCM270X_DT: Use bcm283x.dtsi, bcm2835.dtsi and bcm2836.dtsi

The mainline Device Tree files are quite close to downstream now.
Let's use bcm283x.dtsi, bcm2835.dtsi and bcm2836.dtsi as base files
for our dts files.

Mainline dts files are based on these files:

          bcm2835-rpi.dtsi
  bcm2835.dtsi    bcm2836.dtsi
          bcm283x.dtsi

Current downstream are based on these:

  bcm2708.dtsi    bcm2709.dtsi    bcm2710.dtsi
             bcm2708_common.dtsi

This patch introduces this dependency:

  bcm2708.dtsi    bcm2709.dtsi
          bcm2708-rpi.dtsi
          bcm270x.dtsi
  bcm2835.dtsi    bcm2836.dtsi
          bcm283x.dtsi

And:
          bcm2710.dtsi
          bcm2708-rpi.dtsi
          bcm270x.dtsi
          bcm283x.dtsi

bcm270x.dtsi contains the downstream bcm283x.dtsi diff.
bcm2708-rpi.dtsi is the downstream version of bcm2835-rpi.dtsi.

Other changes:
- The led node has moved from /soc/leds to /leds. This is not a problem
  since the label is used to reference it.
- The clk_osc reg property changes from 6 to 3.
- The gpu nodes has their interrupt property set in the base file.
- the clocks label does not point to the /clocks node anymore, but
  points to the cprman node. This is not a problem since the overlays
  that use the clock node refer to it directly: target-path = "/clocks";
- some nodes now have 2 labels since mainline and downstream differs in
  this respect: cprman/clocks, spi0/spi, gpu/vc4.
- some nodes doesn't have an explicit status = "okay" since they're not
  disabled in the base file: watchdog and random.
- gpiomem doesn't need an explicit status = "okay".
- bcm2708-rpi-cm.dts got the hpd-gpios property from bcm2708_common.dtsi,
  it's now set directly in that file.
- bcm2709-rpi-2-b.dts has the timer node moved from /soc/timer to /timer.
- Removed clock-frequency property on the bcm{2709,2710}.dtsi timer nodes.

Signed-off-by: Noralf Trønnes <noralf@tronnes.org>

BCM270X_DT: Use raspberrypi-power to turn on USB power

Use the raspberrypi-power driver to turn on USB power.

Signed-off-by: Noralf Trønnes <noralf@tronnes.org>

BCM270X_DT: Add a .dtbo target, use for overlays

Change the filenames and extensions to keep the pre-DDT style of
overlay (<name>-overlay.dtb) distinct from new ones that use a
different style of local fixups (<name>.dtbo), and to match other
platforms.

The RPi firmware uses the DDTK trailer atom to choose which type of
overlay to use for each kernel.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>

BCM270X_DT: Don't generate "linux,phandle" props

The EPAPR standard says to use "phandle" properties to store phandles,
rather than the deprecated "linux,phandle" version. By default, dtc
generates both, but adding "-H epapr" causes it to only generate
"phandle"s, saving some space and clutter.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>

BCM270X_DT: Add overlay for enc28j60 on SPI2

Works on SPI2 for compute module

BCM270X_DT: Add midi-uart0 overlay

MIDI requires 31.25kbaud, a baudrate unsupported by Linux. The
midi-uart0 overlay configures uart0 (ttyAMA0) to use a fake clock
so that requesting 38.4kbaud actually gets 31.25kbaud.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>

BCM270X_DT: Add i2c-sensor overlay

The i2c-sensor overlay is a container for various pressure and
temperature sensors, currently bmp085 and bmp280. The standalone
bmp085_i2c-sensor overlay is now deprecated.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>

BCM270X_DT: overlays/*-overlay.dtb -> overlays/*.dtbo (#1752)

We now create overlays as .dtbo files.

build: support for .dtbo files for dtb overlays

Kernel 4.4.6+ on RaspberryPi support .dtbo files for overlays, instead of .dtb.
Patch the kernel, which has faulty rules to generate .dtbo the way yocto does

Signed-off-by: Herve Jourdain <herve.jourdain@neuf.fr>
Signed-off-by: Khem Raj <raj.khem@gmail.com>

BCM270X: Drop position requirement for CMA in VC4 overlay.

No longer necessary since 2aefcd576195a739a7a256099571c9c4a401005f,
and will probably let peeople that want to choose a larger CMA
allocation (particularly on pi0/1).

Signed-off-by: Eric Anholt <eric@anholt.net>

BCM270X_DT: RPi Device Tree tidy

Use the upstream sdhost node, add thermal-zones, and factor out some
common elements.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>

kbuild: Silence unhelpful DTC warnings

Signed-off-by: Phil Elwell <phil@raspberrypi.org>

BCM270X_DT: DT build rules no longer arch-specific

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 .gitignore                                    |    1 +
 arch/arm/boot/dts/Makefile                    |   27 +-
 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts      |  124 +
 arch/arm/boot/dts/bcm2708-rpi-b-rev1.dts      |  127 +
 arch/arm/boot/dts/bcm2708-rpi-b.dts           |  114 +
 arch/arm/boot/dts/bcm2708-rpi-bt.dtsi         |   26 +
 arch/arm/boot/dts/bcm2708-rpi-cm.dts          |   97 +
 arch/arm/boot/dts/bcm2708-rpi-cm.dtsi         |   18 +
 arch/arm/boot/dts/bcm2708-rpi-zero-w.dts      |  163 +
 arch/arm/boot/dts/bcm2708-rpi-zero.dts        |  117 +
 arch/arm/boot/dts/bcm2708-rpi.dtsi            |   36 +
 arch/arm/boot/dts/bcm2708.dtsi                |   12 +
 arch/arm/boot/dts/bcm2709-rpi-2-b.dts         |  124 +
 arch/arm/boot/dts/bcm2709-rpi.dtsi            |    5 +
 arch/arm/boot/dts/bcm2709.dtsi                |   22 +
 arch/arm/boot/dts/bcm270x-rpi.dtsi            |  154 +
 arch/arm/boot/dts/bcm270x.dtsi                |  197 ++
 arch/arm/boot/dts/bcm2710-rpi-2-b.dts         |  124 +
 arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts    |  196 ++
 arch/arm/boot/dts/bcm2710-rpi-3-b.dts         |  198 ++
 arch/arm/boot/dts/bcm2710-rpi-cm3.dts         |  133 +
 arch/arm/boot/dts/bcm2710.dtsi                |   29 +
 arch/arm/boot/dts/bcm2711-rpi-4-b.dts         |  306 +-
 arch/arm/boot/dts/bcm2711-rpi-cm4.dts         |  609 ++++
 arch/arm/boot/dts/bcm2711-rpi.dtsi            |  201 ++
 arch/arm/boot/dts/bcm2711.dtsi                |   34 +-
 arch/arm/boot/dts/bcm271x-rpi-bt.dtsi         |   26 +
 arch/arm/boot/dts/bcm2835-common.dtsi         |    4 +-
 arch/arm/boot/dts/bcm2835-rpi-a-plus.dts      |    5 +
 arch/arm/boot/dts/bcm2835-rpi-a.dts           |    7 +
 arch/arm/boot/dts/bcm2835-rpi-b-plus.dts      |    5 +
 arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts      |    7 +
 arch/arm/boot/dts/bcm2835-rpi-b.dts           |    7 +
 arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts     |    5 +
 arch/arm/boot/dts/bcm2835-rpi-zero-w.dts      |    5 +
 arch/arm/boot/dts/bcm2835-rpi-zero.dts        |    5 +
 arch/arm/boot/dts/bcm2835-rpi.dtsi            |   15 +-
 arch/arm/boot/dts/bcm2835.dtsi                |    2 +-
 arch/arm/boot/dts/bcm2836-rpi-2-b.dts         |    5 +
 arch/arm/boot/dts/bcm2837-rpi-3-a-plus.dts    |    5 +
 arch/arm/boot/dts/bcm2837-rpi-3-b-plus.dts    |    5 +
 arch/arm/boot/dts/bcm2837-rpi-3-b.dts         |    5 +
 arch/arm/boot/dts/bcm2837-rpi-cm3-io3.dts     |    5 +
 arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi |    4 +
 arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi |    4 +
 arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi |    4 +
 .../boot/dts/bcm283x-rpi-i2c0mux_0_28.dtsi    |    4 +
 .../boot/dts/bcm283x-rpi-i2c0mux_0_44.dtsi    |    4 +
 .../boot/dts/bcm283x-rpi-usb-peripheral.dtsi  |    7 -
 arch/arm/boot/dts/bcm283x.dtsi                |   26 +-
 arch/arm/boot/dts/overlays/Makefile           |  216 ++
 arch/arm/boot/dts/overlays/README             | 3040 +++++++++++++++++
 .../arm/boot/dts/overlays/act-led-overlay.dts |   27 +
 .../boot/dts/overlays/adafruit18-overlay.dts  |   55 +
 .../dts/overlays/adau1977-adc-overlay.dts     |   40 +
 .../dts/overlays/adau7002-simple-overlay.dts  |   52 +
 .../arm/boot/dts/overlays/ads1015-overlay.dts |   98 +
 .../arm/boot/dts/overlays/ads1115-overlay.dts |  103 +
 .../arm/boot/dts/overlays/ads7846-overlay.dts |   89 +
 .../boot/dts/overlays/adv7282m-overlay.dts    |   65 +
 .../boot/dts/overlays/adv728x-m-overlay.dts   |   37 +
 .../overlays/akkordion-iqdacplus-overlay.dts  |   49 +
 .../allo-boss-dac-pcm512x-audio-overlay.dts   |   59 +
 .../dts/overlays/allo-digione-overlay.dts     |   44 +
 .../allo-katana-dac-audio-overlay.dts         |   57 +
 .../allo-piano-dac-pcm512x-audio-overlay.dts  |   54 +
 ...o-piano-dac-plus-pcm512x-audio-overlay.dts |   55 +
 arch/arm/boot/dts/overlays/anyspi-overlay.dts |  205 ++
 .../boot/dts/overlays/apds9960-overlay.dts    |   57 +
 .../boot/dts/overlays/applepi-dac-overlay.dts |   57 +
 .../boot/dts/overlays/at86rf233-overlay.dts   |   57 +
 .../overlays/audioinjector-addons-overlay.dts |   60 +
 ...dioinjector-isolated-soundcard-overlay.dts |   55 +
 .../overlays/audioinjector-ultra-overlay.dts  |   71 +
 .../audioinjector-wm8731-audio-overlay.dts    |   39 +
 .../dts/overlays/audiosense-pi-overlay.dts    |   82 +
 .../boot/dts/overlays/audremap-overlay.dts    |   35 +
 .../boot/dts/overlays/balena-fin-overlay.dts  |  125 +
 arch/arm/boot/dts/overlays/cma-overlay.dts    |   36 +
 arch/arm/boot/dts/overlays/dht11-overlay.dts  |   41 +
 .../dts/overlays/dionaudio-loco-overlay.dts   |   39 +
 .../overlays/dionaudio-loco-v2-overlay.dts    |   49 +
 .../boot/dts/overlays/disable-bt-overlay.dts  |   64 +
 .../dts/overlays/disable-wifi-overlay.dts     |   20 +
 arch/arm/boot/dts/overlays/dpi18-overlay.dts  |   39 +
 arch/arm/boot/dts/overlays/dpi24-overlay.dts  |   39 +
 arch/arm/boot/dts/overlays/draws-overlay.dts  |  208 ++
 .../arm/boot/dts/overlays/dwc-otg-overlay.dts |   14 +
 arch/arm/boot/dts/overlays/dwc2-overlay.dts   |   26 +
 .../boot/dts/overlays/enc28j60-overlay.dts    |   53 +
 .../dts/overlays/enc28j60-spi2-overlay.dts    |   47 +
 .../arm/boot/dts/overlays/exc3000-overlay.dts |   48 +
 .../boot/dts/overlays/fe-pi-audio-overlay.dts |   70 +
 .../boot/dts/overlays/fsm-demo-overlay.dts    |  104 +
 .../boot/dts/overlays/ghost-amp-overlay.dts   |  119 +
 arch/arm/boot/dts/overlays/goodix-overlay.dts |   46 +
 .../googlevoicehat-soundcard-overlay.dts      |   49 +
 .../boot/dts/overlays/gpio-fan-overlay.dts    |   79 +
 .../arm/boot/dts/overlays/gpio-ir-overlay.dts |   49 +
 .../boot/dts/overlays/gpio-ir-tx-overlay.dts  |   36 +
 .../boot/dts/overlays/gpio-key-overlay.dts    |   48 +
 .../overlays/gpio-no-bank0-irq-overlay.dts    |   14 +
 .../boot/dts/overlays/gpio-no-irq-overlay.dts |   14 +
 .../dts/overlays/gpio-poweroff-overlay.dts    |   37 +
 .../dts/overlays/gpio-shutdown-overlay.dts    |   84 +
 .../boot/dts/overlays/hd44780-lcd-overlay.dts |   46 +
 .../hdmi-backlight-hwhack-gpio-overlay.dts    |   47 +
 .../dts/overlays/hifiberry-amp-overlay.dts    |   39 +
 .../dts/overlays/hifiberry-dac-overlay.dts    |   34 +
 .../overlays/hifiberry-dacplus-overlay.dts    |   65 +
 .../overlays/hifiberry-dacplusadc-overlay.dts |   72 +
 .../hifiberry-dacplusadcpro-overlay.dts       |   65 +
 .../overlays/hifiberry-dacplusdsp-overlay.dts |   34 +
 .../overlays/hifiberry-dacplushd-overlay.dts  |  106 +
 .../dts/overlays/hifiberry-digi-overlay.dts   |   41 +
 .../overlays/hifiberry-digi-pro-overlay.dts   |   43 +
 .../boot/dts/overlays/highperi-overlay.dts    |   63 +
 arch/arm/boot/dts/overlays/hy28a-overlay.dts  |   93 +
 .../boot/dts/overlays/hy28b-2017-overlay.dts  |  152 +
 arch/arm/boot/dts/overlays/hy28b-overlay.dts  |  148 +
 .../boot/dts/overlays/i-sabre-q2m-overlay.dts |   39 +
 .../boot/dts/overlays/i2c-bcm2708-overlay.dts |   13 +
 .../boot/dts/overlays/i2c-gpio-overlay.dts    |   47 +
 .../arm/boot/dts/overlays/i2c-mux-overlay.dts |  139 +
 .../dts/overlays/i2c-pwm-pca9685a-overlay.dts |   26 +
 .../dts/overlays/i2c-rtc-gpio-overlay.dts     |  266 ++
 .../arm/boot/dts/overlays/i2c-rtc-overlay.dts |  278 ++
 .../boot/dts/overlays/i2c-sensor-overlay.dts  |  271 ++
 arch/arm/boot/dts/overlays/i2c0-overlay.dts   |   74 +
 arch/arm/boot/dts/overlays/i2c1-overlay.dts   |   44 +
 arch/arm/boot/dts/overlays/i2c3-overlay.dts   |   36 +
 arch/arm/boot/dts/overlays/i2c4-overlay.dts   |   36 +
 arch/arm/boot/dts/overlays/i2c5-overlay.dts   |   36 +
 arch/arm/boot/dts/overlays/i2c6-overlay.dts   |   36 +
 .../dts/overlays/i2s-gpio28-31-overlay.dts    |   18 +
 .../boot/dts/overlays/ilitek251x-overlay.dts  |   45 +
 arch/arm/boot/dts/overlays/imx219-overlay.dts |  119 +
 arch/arm/boot/dts/overlays/imx290-overlay.dts |   32 +
 .../boot/dts/overlays/imx290_327-overlay.dtsi |  145 +
 arch/arm/boot/dts/overlays/imx477-overlay.dts |  119 +
 .../dts/overlays/iqaudio-codec-overlay.dts    |   42 +
 .../boot/dts/overlays/iqaudio-dac-overlay.dts |   46 +
 .../dts/overlays/iqaudio-dacplus-overlay.dts  |   49 +
 .../iqaudio-digi-wm8804-audio-overlay.dts     |   47 +
 .../arm/boot/dts/overlays/irs1125-overlay.dts |   85 +
 .../dts/overlays/jedec-spi-nor-overlay.dts    |  309 ++
 .../dts/overlays/justboom-both-overlay.dts    |   65 +
 .../dts/overlays/justboom-dac-overlay.dts     |   46 +
 .../dts/overlays/justboom-digi-overlay.dts    |   41 +
 .../arm/boot/dts/overlays/ltc294x-overlay.dts |   86 +
 .../boot/dts/overlays/max98357a-overlay.dts   |   84 +
 .../boot/dts/overlays/maxtherm-overlay.dts    |  166 +
 .../boot/dts/overlays/mbed-dac-overlay.dts    |   64 +
 .../boot/dts/overlays/mcp23017-overlay.dts    |   69 +
 .../boot/dts/overlays/mcp23s17-overlay.dts    |  732 ++++
 .../dts/overlays/mcp2515-can0-overlay.dts     |   73 +
 .../dts/overlays/mcp2515-can1-overlay.dts     |   73 +
 .../arm/boot/dts/overlays/mcp3008-overlay.dts |  205 ++
 .../arm/boot/dts/overlays/mcp3202-overlay.dts |  205 ++
 .../arm/boot/dts/overlays/mcp342x-overlay.dts |  164 +
 .../dts/overlays/media-center-overlay.dts     |  134 +
 .../boot/dts/overlays/merus-amp-overlay.dts   |   60 +
 .../boot/dts/overlays/midi-uart0-overlay.dts  |   36 +
 .../boot/dts/overlays/midi-uart1-overlay.dts  |   43 +
 .../boot/dts/overlays/miniuart-bt-overlay.dts |   93 +
 arch/arm/boot/dts/overlays/mmc-overlay.dts    |   46 +
 .../arm/boot/dts/overlays/mpu6050-overlay.dts |   28 +
 .../arm/boot/dts/overlays/mz61581-overlay.dts |  117 +
 arch/arm/boot/dts/overlays/ov5647-overlay.dts |   92 +
 arch/arm/boot/dts/overlays/ov7251-overlay.dts |  111 +
 arch/arm/boot/dts/overlays/ov9281-overlay.dts |  111 +
 arch/arm/boot/dts/overlays/overlay_map.dts    |  141 +
 .../arm/boot/dts/overlays/papirus-overlay.dts |   89 +
 .../arm/boot/dts/overlays/pca953x-overlay.dts |  240 ++
 arch/arm/boot/dts/overlays/pibell-overlay.dts |   81 +
 .../dts/overlays/pifacedigital-overlay.dts    |  144 +
 arch/arm/boot/dts/overlays/piglow-overlay.dts |   97 +
 .../boot/dts/overlays/piscreen-overlay.dts    |  102 +
 .../boot/dts/overlays/piscreen2r-overlay.dts  |  106 +
 .../arm/boot/dts/overlays/pisound-overlay.dts |  120 +
 .../arm/boot/dts/overlays/pitft22-overlay.dts |   69 +
 .../overlays/pitft28-capacitive-overlay.dts   |   91 +
 .../overlays/pitft28-resistive-overlay.dts    |  119 +
 .../overlays/pitft35-resistive-overlay.dts    |  119 +
 .../boot/dts/overlays/pps-gpio-overlay.dts    |   38 +
 .../boot/dts/overlays/pwm-2chan-overlay.dts   |   49 +
 .../boot/dts/overlays/pwm-ir-tx-overlay.dts   |   40 +
 arch/arm/boot/dts/overlays/pwm-overlay.dts    |   45 +
 .../arm/boot/dts/overlays/qca7000-overlay.dts |   55 +
 .../dts/overlays/rotary-encoder-overlay.dts   |   59 +
 .../dts/overlays/rpi-backlight-overlay.dts    |   21 +
 .../overlays/rpi-cirrus-wm5102-overlay.dts    |  172 +
 .../arm/boot/dts/overlays/rpi-dac-overlay.dts |   34 +
 .../boot/dts/overlays/rpi-display-overlay.dts |   91 +
 .../boot/dts/overlays/rpi-ft5406-overlay.dts  |   25 +
 .../arm/boot/dts/overlays/rpi-poe-overlay.dts |   95 +
 .../boot/dts/overlays/rpi-proto-overlay.dts   |   39 +
 .../boot/dts/overlays/rpi-sense-overlay.dts   |   47 +
 arch/arm/boot/dts/overlays/rpi-tv-overlay.dts |   34 +
 .../boot/dts/overlays/rpivid-v4l2-overlay.dts |   61 +
 .../rra-digidac1-wm8741-audio-overlay.dts     |   49 +
 .../boot/dts/overlays/sainsmart18-overlay.dts |   52 +
 .../dts/overlays/sc16is750-i2c-overlay.dts    |   43 +
 .../dts/overlays/sc16is752-i2c-overlay.dts    |   43 +
 .../dts/overlays/sc16is752-spi0-overlay.dts   |   49 +
 .../dts/overlays/sc16is752-spi1-overlay.dts   |   67 +
 arch/arm/boot/dts/overlays/sdhost-overlay.dts |   38 +
 arch/arm/boot/dts/overlays/sdio-overlay.dts   |   77 +
 .../arm/boot/dts/overlays/sdtweak-overlay.dts |   25 +
 .../boot/dts/overlays/sh1106-spi-overlay.dts  |   84 +
 .../arm/boot/dts/overlays/smi-dev-overlay.dts |   20 +
 .../boot/dts/overlays/smi-nand-overlay.dts    |   66 +
 arch/arm/boot/dts/overlays/smi-overlay.dts    |   37 +
 .../dts/overlays/spi-gpio35-39-overlay.dts    |   31 +
 .../dts/overlays/spi-gpio40-45-overlay.dts    |   36 +
 .../arm/boot/dts/overlays/spi-rtc-overlay.dts |   33 +
 .../boot/dts/overlays/spi0-1cs-overlay.dts    |   42 +
 .../boot/dts/overlays/spi0-2cs-overlay.dts    |   37 +
 .../boot/dts/overlays/spi1-1cs-overlay.dts    |   57 +
 .../boot/dts/overlays/spi1-2cs-overlay.dts    |   69 +
 .../boot/dts/overlays/spi1-3cs-overlay.dts    |   81 +
 .../boot/dts/overlays/spi2-1cs-overlay.dts    |   57 +
 .../boot/dts/overlays/spi2-2cs-overlay.dts    |   69 +
 .../boot/dts/overlays/spi2-3cs-overlay.dts    |   81 +
 .../boot/dts/overlays/spi3-1cs-overlay.dts    |   44 +
 .../boot/dts/overlays/spi3-2cs-overlay.dts    |   56 +
 .../boot/dts/overlays/spi4-1cs-overlay.dts    |   44 +
 .../boot/dts/overlays/spi4-2cs-overlay.dts    |   56 +
 .../boot/dts/overlays/spi5-1cs-overlay.dts    |   44 +
 .../boot/dts/overlays/spi5-2cs-overlay.dts    |   56 +
 .../boot/dts/overlays/spi6-1cs-overlay.dts    |   44 +
 .../boot/dts/overlays/spi6-2cs-overlay.dts    |   56 +
 .../arm/boot/dts/overlays/ssd1306-overlay.dts |   36 +
 .../boot/dts/overlays/ssd1306-spi-overlay.dts |   84 +
 .../boot/dts/overlays/ssd1351-spi-overlay.dts |   83 +
 .../dts/overlays/superaudioboard-overlay.dts  |   73 +
 arch/arm/boot/dts/overlays/sx150x-overlay.dts | 1706 +++++++++
 .../dts/overlays/tc358743-audio-overlay.dts   |   52 +
 .../boot/dts/overlays/tc358743-overlay.dts    |  107 +
 .../boot/dts/overlays/tinylcd35-overlay.dts   |  222 ++
 .../boot/dts/overlays/tpm-slb9670-overlay.dts |   44 +
 arch/arm/boot/dts/overlays/uart0-overlay.dts  |   32 +
 arch/arm/boot/dts/overlays/uart1-overlay.dts  |   38 +
 arch/arm/boot/dts/overlays/uart2-overlay.dts  |   27 +
 arch/arm/boot/dts/overlays/uart3-overlay.dts  |   27 +
 arch/arm/boot/dts/overlays/uart4-overlay.dts  |   27 +
 arch/arm/boot/dts/overlays/uart5-overlay.dts  |   27 +
 arch/arm/boot/dts/overlays/udrc-overlay.dts   |  128 +
 .../boot/dts/overlays/upstream-overlay.dts    |  113 +
 .../dts/overlays/upstream-pi4-overlay.dts     |  161 +
 .../dts/overlays/vc4-fkms-v3d-overlay.dts     |   40 +
 .../overlays/vc4-kms-kippah-7inch-overlay.dts |   43 +
 .../boot/dts/overlays/vc4-kms-v3d-overlay.dts |  122 +
 .../dts/overlays/vc4-kms-v3d-pi4-overlay.dts  |  186 +
 arch/arm/boot/dts/overlays/vga666-overlay.dts |   30 +
 .../arm/boot/dts/overlays/w1-gpio-overlay.dts |   40 +
 .../dts/overlays/w1-gpio-pullup-overlay.dts   |   42 +
 arch/arm/boot/dts/overlays/w5500-overlay.dts  |   63 +
 .../arm/boot/dts/overlays/wittypi-overlay.dts |   44 +
 arch/arm64/boot/dts/Makefile                  |    2 +
 arch/arm64/boot/dts/broadcom/Makefile         |   16 +-
 .../boot/dts/broadcom/bcm2710-rpi-2-b.dts     |    3 +
 .../dts/broadcom/bcm2710-rpi-3-b-plus.dts     |    3 +
 .../boot/dts/broadcom/bcm2710-rpi-3-b.dts     |    3 +
 .../boot/dts/broadcom/bcm2710-rpi-cm3.dts     |    3 +
 .../boot/dts/broadcom/bcm2711-rpi-4-b.dts     |    5 +-
 .../dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi  |    1 +
 .../dts/broadcom/bcm283x-rpi-lan7515.dtsi     |    1 +
 arch/arm64/boot/dts/overlays                  |    1 +
 scripts/Makefile.dtbinst                      |    6 +-
 scripts/Makefile.lib                          |   13 +
 271 files changed, 23898 insertions(+), 31 deletions(-)
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-b-rev1.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-bt.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-cm.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-zero-w.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi-zero.dts
 create mode 100644 arch/arm/boot/dts/bcm2708-rpi.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2708.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2709-rpi-2-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2709-rpi.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2709.dtsi
 create mode 100644 arch/arm/boot/dts/bcm270x-rpi.dtsi
 create mode 100644 arch/arm/boot/dts/bcm270x.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2710-rpi-2-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
 create mode 100644 arch/arm/boot/dts/bcm2710-rpi-3-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2710-rpi-cm3.dts
 create mode 100644 arch/arm/boot/dts/bcm2710.dtsi
 create mode 100644 arch/arm/boot/dts/bcm2711-rpi-cm4.dts
 create mode 100644 arch/arm/boot/dts/bcm2711-rpi.dtsi
 create mode 100644 arch/arm/boot/dts/bcm271x-rpi-bt.dtsi
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_28.dtsi
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_44.dtsi
 delete mode 100644 arch/arm/boot/dts/bcm283x-rpi-usb-peripheral.dtsi
 create mode 100644 arch/arm/boot/dts/overlays/Makefile
 create mode 100644 arch/arm/boot/dts/overlays/README
 create mode 100644 arch/arm/boot/dts/overlays/act-led-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/adafruit18-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/adau1977-adc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/adau7002-simple-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ads1015-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ads1115-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ads7846-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/adv7282m-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/adv728x-m-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/akkordion-iqdacplus-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/allo-boss-dac-pcm512x-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/allo-digione-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/allo-katana-dac-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/allo-piano-dac-pcm512x-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/allo-piano-dac-plus-pcm512x-audio-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/anyspi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/apds9960-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/applepi-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/at86rf233-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/audioinjector-addons-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/audioinjector-isolated-soundcard-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/audioinjector-ultra-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/audioinjector-wm8731-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/audiosense-pi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/audremap-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/balena-fin-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/cma-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dht11-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dionaudio-loco-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dionaudio-loco-v2-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/disable-bt-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/disable-wifi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dpi18-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dpi24-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/draws-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dwc-otg-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/dwc2-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/enc28j60-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/enc28j60-spi2-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/exc3000-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/fsm-demo-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ghost-amp-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/goodix-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/googlevoicehat-soundcard-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-fan-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-ir-tx-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-key-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/gpio-no-bank0-irq-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-no-irq-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-poweroff-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/gpio-shutdown-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hd44780-lcd-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hdmi-backlight-hwhack-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-amp-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dacplus-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dacplusadc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dacplusadcpro-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dacplusdsp-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-dacplushd-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-digi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hifiberry-digi-pro-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/highperi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hy28a-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hy28b-2017-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/hy28b-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i-sabre-q2m-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-bcm2708-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-mux-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-rtc-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c-sensor-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c0-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c1-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c3-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c4-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c5-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2c6-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/i2s-gpio28-31-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ilitek251x-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/imx219-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/imx290-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/imx290_327-overlay.dtsi
 create mode 100644 arch/arm/boot/dts/overlays/imx477-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/iqaudio-codec-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/iqaudio-dacplus-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/iqaudio-digi-wm8804-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/irs1125-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/jedec-spi-nor-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/justboom-both-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/justboom-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/justboom-digi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ltc294x-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/max98357a-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/maxtherm-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mbed-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mcp23017-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mcp23s17-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/mcp2515-can0-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mcp2515-can1-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/mcp3008-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/mcp3202-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mcp342x-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/media-center-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/merus-amp-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/midi-uart0-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/midi-uart1-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/miniuart-bt-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mmc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mpu6050-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/mz61581-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ov5647-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ov7251-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ov9281-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/overlay_map.dts
 create mode 100644 arch/arm/boot/dts/overlays/papirus-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pca953x-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pibell-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pifacedigital-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/piglow-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/piscreen-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/piscreen2r-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pisound-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pitft22-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pitft28-capacitive-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pitft28-resistive-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pitft35-resistive-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pps-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pwm-ir-tx-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/pwm-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/qca7000-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rotary-encoder-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-backlight-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-cirrus-wm5102-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-dac-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-display-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-poe-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-proto-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpi-tv-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rpivid-v4l2-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/rra-digidac1-wm8741-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sainsmart18-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sc16is752-i2c-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sc16is752-spi0-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sc16is752-spi1-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sdhost-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sdio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sdtweak-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sh1106-spi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/smi-dev-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/smi-nand-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/smi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi-gpio35-39-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi-gpio40-45-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi-rtc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi0-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi0-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi1-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi1-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi1-3cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi2-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi2-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi2-3cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi3-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi3-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi4-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi4-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi5-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi5-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi6-1cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/spi6-2cs-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ssd1306-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ssd1306-spi-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/ssd1351-spi-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/superaudioboard-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/sx150x-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/tc358743-audio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/tc358743-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/tinylcd35-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/tpm-slb9670-overlay.dts
 create mode 100755 arch/arm/boot/dts/overlays/uart0-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/uart1-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/uart2-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/uart3-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/uart4-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/uart5-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/udrc-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/upstream-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/upstream-pi4-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/vc4-fkms-v3d-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/vc4-kms-kippah-7inch-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/vga666-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/w1-gpio-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/w1-gpio-pullup-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/w5500-overlay.dts
 create mode 100644 arch/arm/boot/dts/overlays/wittypi-overlay.dts
 create mode 100644 arch/arm64/boot/dts/broadcom/bcm2710-rpi-2-b.dts
 create mode 100644 arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b-plus.dts
 create mode 100644 arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b.dts
 create mode 100644 arch/arm64/boot/dts/broadcom/bcm2710-rpi-cm3.dts
 create mode 120000 arch/arm64/boot/dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi
 create mode 120000 arch/arm64/boot/dts/broadcom/bcm283x-rpi-lan7515.dtsi
 create mode 120000 arch/arm64/boot/dts/overlays

diff --git a/.gitignore b/.gitignore
index 67d2f3503128..8b0b16eeca88 100644
--- a/.gitignore
+++ b/.gitignore
@@ -18,6 +18,7 @@
 *.c.[012]*.*
 *.dt.yaml
 *.dtb
+*.dtbo
 *.dtb.S
 *.dwo
 *.elf
diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index ce66ffd5a1bb..87241fe26e10 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -1,4 +1,20 @@
 # SPDX-License-Identifier: GPL-2.0
+
+dtb-$(CONFIG_ARCH_BCM2835) += \
+	bcm2708-rpi-b.dtb \
+	bcm2708-rpi-b-rev1.dtb \
+	bcm2708-rpi-b-plus.dtb \
+	bcm2708-rpi-cm.dtb \
+	bcm2708-rpi-zero.dtb \
+	bcm2708-rpi-zero-w.dtb \
+	bcm2709-rpi-2-b.dtb \
+	bcm2710-rpi-2-b.dtb \
+	bcm2710-rpi-3-b.dtb \
+	bcm2711-rpi-4-b.dtb \
+	bcm2710-rpi-3-b-plus.dtb \
+	bcm2710-rpi-cm3.dtb \
+	bcm2711-rpi-cm4.dtb
+
 dtb-$(CONFIG_ARCH_ALPINE) += \
 	alpine-db.dtb
 dtb-$(CONFIG_MACH_ARTPEC6) += \
@@ -92,7 +108,6 @@ dtb-$(CONFIG_ARCH_BCM2835) += \
 	bcm2837-rpi-3-b.dtb \
 	bcm2837-rpi-3-b-plus.dtb \
 	bcm2837-rpi-cm3-io3.dtb \
-	bcm2711-rpi-4-b.dtb \
 	bcm2835-rpi-zero.dtb \
 	bcm2835-rpi-zero-w.dtb
 dtb-$(CONFIG_ARCH_BCM_5301X) += \
@@ -1408,3 +1423,13 @@ dtb-$(CONFIG_ARCH_ASPEED) += \
 	aspeed-bmc-opp-zaius.dtb \
 	aspeed-bmc-portwell-neptune.dtb \
 	aspeed-bmc-quanta-q71l.dtb
+
+targets += dtbs dtbs_install
+targets += $(dtb-y)
+
+subdir-y	:= overlays
+
+# Enable fixups to support overlays on BCM2835 platforms
+ifeq ($(CONFIG_ARCH_BCM2835),y)
+	DTC_FLAGS ?= -@
+endif
diff --git a/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts b/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
new file mode 100644
index 000000000000..98581eec4bdc
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
@@ -0,0 +1,124 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+#include "bcm2708-rpi.dtsi"
+#include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+
+/ {
+	compatible = "raspberrypi,model-b-plus", "brcm,bcm2835";
+	model = "Raspberry Pi Model B+";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 45>;
+		brcm,function = <4>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&gpio 35 0>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-b-rev1.dts b/arch/arm/boot/dts/bcm2708-rpi-b-rev1.dts
new file mode 100644
index 000000000000..7b554b465b27
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-b-rev1.dts
@@ -0,0 +1,127 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+#include "bcm2708-rpi.dtsi"
+#include "bcm283x-rpi-smsc9512.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+
+/ {
+	compatible = "raspberrypi,model-b", "brcm,bcm2835";
+	model = "Raspberry Pi Model B";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <28 29 30 31>;
+		brcm,function = <6>; /* alt2 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 45>;
+		brcm,function = <4>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+/delete-node/ &i2c0mux;
+
+i2c0: &i2c0if {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+i2c_csi_dsi: &i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+/ {
+	aliases {
+		i2c0 = &i2c0;
+	};
+
+	__overrides__ {
+		i2c0 = <&i2c0>, "status";
+	};
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 16 1>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_HIGH>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-b.dts b/arch/arm/boot/dts/bcm2708-rpi-b.dts
new file mode 100644
index 000000000000..305f1dbde60f
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-b.dts
@@ -0,0 +1,114 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+#include "bcm2708-rpi.dtsi"
+#include "bcm283x-rpi-smsc9512.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+
+/ {
+	compatible = "raspberrypi,model-b", "brcm,bcm2835";
+	model = "Raspberry Pi Model B";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <28 29 30 31>;
+		brcm,function = <6>; /* alt2 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 45>;
+		brcm,function = <4>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 16 1>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_HIGH>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-bt.dtsi b/arch/arm/boot/dts/bcm2708-rpi-bt.dtsi
new file mode 100644
index 000000000000..a18f80af97d3
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-bt.dtsi
@@ -0,0 +1,26 @@
+// SPDX-License-Identifier: GPL-2.0
+
+&uart0 {
+	bt: bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		max-speed = <3000000>;
+		shutdown-gpios = <&gpio 45 GPIO_ACTIVE_HIGH>;
+		status = "disabled";
+	};
+};
+
+&uart1 {
+	minibt: bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		max-speed = <460800>;
+		shutdown-gpios = <&gpio 45 GPIO_ACTIVE_HIGH>;
+		status = "disabled";
+	};
+};
+
+/ {
+	__overrides__ {
+		krnbt = <&bt>,"status";
+		krnbt_baudrate = <&bt>,"max-speed:0";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-cm.dts b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
new file mode 100644
index 000000000000..93062c4ffad2
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
@@ -0,0 +1,97 @@
+/dts-v1/;
+
+#include "bcm2708-rpi-cm.dtsi"
+#include "bcm283x-rpi-csi0-2lane.dtsi"
+#include "bcm283x-rpi-csi1-4lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+
+/ {
+	compatible = "raspberrypi,compute-module", "brcm,bcm2835";
+	model = "Raspberry Pi Compute Module";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins;
+		brcm,function;
+	};
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_HIGH>;
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-cm.dtsi b/arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
new file mode 100644
index 000000000000..dce160f420fd
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dtsi
@@ -0,0 +1,18 @@
+#include "bcm2708.dtsi"
+#include "bcm2708-rpi.dtsi"
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-zero-w.dts b/arch/arm/boot/dts/bcm2708-rpi-zero-w.dts
new file mode 100644
index 000000000000..f1bbed9fbf73
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-zero-w.dts
@@ -0,0 +1,163 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+#include "bcm2708-rpi.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+#include "bcm2708-rpi-bt.dtsi"
+
+/ {
+	compatible = "raspberrypi,model-zero-w", "brcm,bcm2835";
+	model = "Raspberry Pi Zero W";
+
+	chosen {
+		bootargs = "coherent_pool=1M 8250.nr_uarts=1 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+	};
+
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart0;
+		mmc1 = &mmcnr;
+	};
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins = <34 35 36 37 38 39>;
+		brcm,function = <7>; /* ALT3 = SD1 */
+		brcm,pull = <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins = <43>;
+		brcm,function = <4>; /* alt0:GPCLK2 */
+		brcm,pull = <0>; /* none */
+	};
+
+	uart0_pins: uart0_pins {
+		brcm,pins = <30 31 32 33>;
+		brcm,function = <7>; /* alt3=UART0 */
+		brcm,pull = <2 0 0 2>; /* up none none up */
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins;
+		brcm,function;
+		brcm,pull;
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <>;
+		brcm,function = <>;
+	};
+};
+
+&mmcnr {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins &bt_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "actpwr";
+		gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi-zero.dts b/arch/arm/boot/dts/bcm2708-rpi-zero.dts
new file mode 100644
index 000000000000..e7578788b839
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi-zero.dts
@@ -0,0 +1,117 @@
+/dts-v1/;
+
+#include "bcm2708.dtsi"
+#include "bcm2708-rpi.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+
+/ {
+	compatible = "raspberrypi,model-zero", "brcm,bcm2835";
+	model = "Raspberry Pi Zero";
+
+	chosen {
+		bootargs = "coherent_pool=1M snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+	};
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <>;
+		brcm,function = <>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "actpwr";
+		gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2708-rpi.dtsi b/arch/arm/boot/dts/bcm2708-rpi.dtsi
new file mode 100644
index 000000000000..e2458b15d64a
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708-rpi.dtsi
@@ -0,0 +1,36 @@
+/* Downstream modifications common to bcm2835, bcm2836, bcm2837 */
+
+#include "bcm2835-rpi.dtsi"
+#include "bcm270x-rpi.dtsi"
+
+/ {
+	memory@0 {
+		device_type = "memory";
+		reg = <0x0 0x0>;
+	};
+
+	aliases {
+		i2c2 = &i2c2;
+	};
+
+	__overrides__ {
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		sd_poll_once = <&sdhost>,"non-removable?";
+	};
+};
+
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_gpio48>;
+	status = "okay";
+};
+
+&hdmi {
+	power-domains = <&power RPI_POWER_DOMAIN_HDMI>;
+	status = "disabled";
+};
+
+&i2c2 {
+	status = "disabled";
+};
diff --git a/arch/arm/boot/dts/bcm2708.dtsi b/arch/arm/boot/dts/bcm2708.dtsi
new file mode 100644
index 000000000000..36ec4989403f
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2708.dtsi
@@ -0,0 +1,12 @@
+#include "bcm2835.dtsi"
+#include "bcm270x.dtsi"
+
+/ {
+	__overrides__ {
+		arm_freq;
+	};
+};
+
+&vc4 {
+	status = "disabled";
+};
diff --git a/arch/arm/boot/dts/bcm2709-rpi-2-b.dts b/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
new file mode 100644
index 000000000000..6b2e3c291d72
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
@@ -0,0 +1,124 @@
+/dts-v1/;
+
+#include "bcm2709.dtsi"
+#include "bcm2709-rpi.dtsi"
+#include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+
+/ {
+	compatible = "raspberrypi,2-model-b", "brcm,bcm2836";
+	model = "Raspberry Pi 2 Model B";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 45>;
+		brcm,function = <4>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&gpio 35 0>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2709-rpi.dtsi b/arch/arm/boot/dts/bcm2709-rpi.dtsi
new file mode 100644
index 000000000000..babfa41cd9f7
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2709-rpi.dtsi
@@ -0,0 +1,5 @@
+#include "bcm2708-rpi.dtsi"
+
+&vchiq {
+	compatible = "brcm,bcm2836-vchiq", "brcm,bcm2835-vchiq";
+};
diff --git a/arch/arm/boot/dts/bcm2709.dtsi b/arch/arm/boot/dts/bcm2709.dtsi
new file mode 100644
index 000000000000..68eafc1b281a
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2709.dtsi
@@ -0,0 +1,22 @@
+#include "bcm2836.dtsi"
+#include "bcm270x.dtsi"
+
+/ {
+	soc {
+		ranges = <0x7e000000 0x3f000000 0x01000000>,
+		         <0x40000000 0x40000000 0x00040000>;
+
+		/delete-node/ timer@7e003000;
+	};
+
+	__overrides__ {
+		arm_freq = <&v7_cpu0>, "clock-frequency:0",
+			   <&v7_cpu1>, "clock-frequency:0",
+			   <&v7_cpu2>, "clock-frequency:0",
+			   <&v7_cpu3>, "clock-frequency:0";
+	};
+};
+
+&vc4 {
+	status = "disabled";
+};
diff --git a/arch/arm/boot/dts/bcm270x-rpi.dtsi b/arch/arm/boot/dts/bcm270x-rpi.dtsi
new file mode 100644
index 000000000000..68a7e1c09db1
--- /dev/null
+++ b/arch/arm/boot/dts/bcm270x-rpi.dtsi
@@ -0,0 +1,154 @@
+/* Downstream modifications to bcm2835-rpi.dtsi */
+
+/ {
+	aliases {
+		audio = &audio;
+		aux = &aux;
+		sound = &sound;
+		soc = &soc;
+		dma = &dma;
+		intc = &intc;
+		watchdog = &watchdog;
+		random = &random;
+		mailbox = &mailbox;
+		gpio = &gpio;
+		uart0 = &uart0;
+		uart1 = &uart1;
+		sdhost = &sdhost;
+		mmc = &mmc;
+		mmc1 = &mmc;
+		mmc0 = &sdhost;
+		i2s = &i2s;
+		i2c0 = &i2c0;
+		i2c1 = &i2c1;
+		i2c10 = &i2c_csi_dsi;
+		spi0 = &spi0;
+		spi1 = &spi1;
+		spi2 = &spi2;
+		usb = &usb;
+		leds = &leds;
+		fb = &fb;
+		thermal = &thermal;
+		axiperf = &axiperf;
+	};
+
+	/* Define these notional regulators for use by overlays */
+	vdd_3v3_reg: fixedregulator_3v3 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-max-microvolt = <3300000>;
+		regulator-min-microvolt = <3300000>;
+		regulator-name = "3v3";
+	};
+
+	vdd_5v0_reg: fixedregulator_5v0 {
+		compatible = "regulator-fixed";
+		regulator-always-on;
+		regulator-max-microvolt = <5000000>;
+		regulator-min-microvolt = <5000000>;
+		regulator-name = "5v0";
+	};
+
+	leds: leds {
+		compatible = "gpio-leds";
+	};
+
+	soc {
+		gpiomem {
+			compatible = "brcm,bcm2835-gpiomem";
+			reg = <0x7e200000 0x1000>;
+		};
+
+		fb: fb {
+			compatible = "brcm,bcm2708-fb";
+			firmware = <&firmware>;
+			status = "okay";
+		};
+
+		vcsm: vcsm {
+			compatible = "raspberrypi,bcm2835-vcsm";
+			firmware = <&firmware>;
+			status = "okay";
+		};
+
+		/* External sound card */
+		sound: sound {
+			status = "disabled";
+		};
+	};
+
+	__overrides__ {
+		cache_line_size;
+
+		uart0 = <&uart0>,"status";
+		uart1 = <&uart1>,"status";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0if>,"status",<&i2c0mux>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c0_baudrate = <&i2c0if>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+		sd_overclock = <&sdhost>,"brcm,overclock-50:0";
+		sd_force_pio = <&sdhost>,"brcm,force-pio?";
+		sd_pio_limit = <&sdhost>,"brcm,pio-limit:0";
+		sd_debug     = <&sdhost>,"brcm,debug";
+		sdio_overclock = <&mmc>,"brcm,overclock-50:0",
+				 <&mmcnr>,"brcm,overclock-50:0";
+		axiperf      = <&axiperf>,"status";
+	};
+};
+
+&uart0 {
+	skip-init;
+};
+
+&uart1 {
+	skip-init;
+};
+
+&txp {
+	status = "disabled";
+};
+
+&i2c0if {
+	status = "disabled";
+};
+
+&i2c0mux {
+	status = "disabled";
+};
+
+&i2c1 {
+	status = "disabled";
+};
+
+&clocks {
+	firmware = <&firmware>;
+};
+
+&sdhci {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emmc_gpio48>;
+	bus-width = <4>;
+};
+
+&cpu_thermal {
+	/delete-node/ trips;
+};
+
+&vec {
+	status = "disabled";
+};
+
+&vchiq {
+	/* Onboard audio */
+	audio: bcm2835_audio {
+		compatible = "brcm,bcm2835-audio";
+		brcm,pwm-channels = <8>;
+		status = "disabled";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm270x.dtsi b/arch/arm/boot/dts/bcm270x.dtsi
new file mode 100644
index 000000000000..446d4ff64842
--- /dev/null
+++ b/arch/arm/boot/dts/bcm270x.dtsi
@@ -0,0 +1,197 @@
+/* Downstream bcm283x.dtsi diff */
+#include <dt-bindings/power/raspberrypi-power.h>
+
+/ {
+	chosen {
+		bootargs = "coherent_pool=1M snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+		/delete-property/ stdout-path;
+	};
+
+	soc: soc {
+
+		watchdog: watchdog@7e100000 {
+			/* Add label */
+		};
+
+		random: rng@7e104000 {
+			/* Add label */
+		};
+
+		spi0: spi@7e204000 {
+			/* Add label */
+		};
+
+#ifndef BCM2711
+		pixelvalve0: pixelvalve@7e206000 {
+			/* Add label */
+			status = "disabled";
+		};
+
+		pixelvalve1: pixelvalve@7e207000 {
+			/* Add label */
+			status = "disabled";
+		};
+#endif
+
+		/delete-node/ sdhci@7e300000;
+
+		sdhci: mmc: mmc@7e300000 {
+			compatible = "brcm,bcm2835-mmc", "brcm,bcm2835-sdhci";
+			reg = <0x7e300000 0x100>;
+			interrupts = <2 30>;
+			clocks = <&clocks BCM2835_CLOCK_EMMC>;
+			dmas = <&dma 11>;
+			dma-names = "rx-tx";
+			brcm,overclock-50 = <0>;
+			status = "disabled";
+		};
+
+		/* A clone of mmc but with non-removable set */
+		mmcnr: mmcnr@7e300000 {
+			compatible = "brcm,bcm2835-mmc", "brcm,bcm2835-sdhci";
+			reg = <0x7e300000 0x100>;
+			interrupts = <2 30>;
+			clocks = <&clocks BCM2835_CLOCK_EMMC>;
+			dmas = <&dma 11>;
+			dma-names = "rx-tx";
+			brcm,overclock-50 = <0>;
+			non-removable;
+			status = "disabled";
+		};
+
+		hvs: hvs@7e400000 {
+			/* Add label */
+			status = "disabled";
+		};
+
+		firmwarekms: firmwarekms@7e600000 {
+			compatible = "raspberrypi,rpi-firmware-kms";
+			/* SMI interrupt reg */
+			reg = <0x7e600000 0x100>;
+			interrupts = <2 16>;
+			brcm,firmware = <&firmware>;
+			status = "disabled";
+		};
+
+		smi: smi@7e600000 {
+			compatible = "brcm,bcm2835-smi";
+			reg = <0x7e600000 0x100>;
+			interrupts = <2 16>;
+			clocks = <&clocks BCM2835_CLOCK_SMI>;
+			assigned-clocks = <&clocks BCM2835_CLOCK_SMI>;
+			assigned-clock-rates = <125000000>;
+			dmas = <&dma 4>;
+			dma-names = "rx-tx";
+			status = "disabled";
+		};
+
+		csi0: csi@7e800000 {
+			compatible = "brcm,bcm2835-unicam";
+			reg = <0x7e800000 0x800>,
+			      <0x7e802000 0x4>;
+			interrupts = <2 6>;
+			clocks = <&clocks BCM2835_CLOCK_CAM0>,
+				 <&firmware_clocks 4>;
+			clock-names = "lp", "vpu";
+			power-domains = <&power RPI_POWER_DOMAIN_UNICAM0>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			#clock-cells = <1>;
+			status = "disabled";
+		};
+
+		csi1: csi@7e801000 {
+			compatible = "brcm,bcm2835-unicam";
+			reg = <0x7e801000 0x800>,
+			      <0x7e802004 0x4>;
+			interrupts = <2 7>;
+			clocks = <&clocks BCM2835_CLOCK_CAM1>,
+				 <&firmware_clocks 4>;
+			clock-names = "lp", "vpu";
+			power-domains = <&power RPI_POWER_DOMAIN_UNICAM1>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			#clock-cells = <1>;
+			status = "disabled";
+		};
+
+#ifndef BCM2711
+		pixelvalve2: pixelvalve@7e807000 {
+			/* Add label */
+			status = "disabled";
+		};
+#endif
+
+		hdmi@7e902000 { /* hdmi */
+			status = "disabled";
+		};
+
+		usb@7e980000 { /* usb */
+			compatible = "brcm,bcm2708-usb";
+			reg = <0x7e980000 0x10000>,
+			      <0x7e006000 0x1000>;
+			interrupt-names = "usb",
+					  "soft";
+			interrupts = <1 9>,
+				     <2 0>;
+		};
+
+#ifndef BCM2711
+		v3d@7ec00000 { /* vd3 */
+			compatible = "brcm,vc4-v3d";
+			power-domains = <&power RPI_POWER_DOMAIN_V3D>;
+			status = "disabled";
+		};
+#endif
+
+		axiperf: axiperf {
+			compatible = "brcm,bcm2835-axiperf";
+			reg = <0x7e009800 0x100>,
+			      <0x7ee08000 0x100>;
+			firmware = <&firmware>;
+			status = "disabled";
+		};
+	};
+
+	__overrides__ {
+		cam0-pwdn-ctrl;
+		cam0-pwdn;
+		cam0-led-ctrl;
+		cam0-led;
+	};
+};
+
+&gpio {
+	interrupts = <2 17>, <2 18>;
+
+	dpi_18bit_gpio0: dpi_18bit_gpio0 {
+		brcm,pins = <0 1 2 3 4 5 6 7 8 9 10 11
+			     12 13 14 15 16 17 18 19
+			     20 21>;
+		brcm,function = <BCM2835_FSEL_ALT2>;
+	};
+};
+
+&uart0 {
+	/* Enable CTS bug workaround */
+	cts-event-workaround;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	dmas = <&dma 2>, <&dma 3>;
+	dma-names = "tx", "rx";
+};
+
+&sdhost {
+	dmas = <&dma (13|(1<<29))>;
+	dma-names = "rx-tx";
+	bus-width = <4>;
+	brcm,overclock-50 = <0>;
+	brcm,pio-limit = <1>;
+};
+
+&spi0 {
+	dmas = <&dma 6>, <&dma 7>;
+	dma-names = "tx", "rx";
+};
diff --git a/arch/arm/boot/dts/bcm2710-rpi-2-b.dts b/arch/arm/boot/dts/bcm2710-rpi-2-b.dts
new file mode 100644
index 000000000000..49cfda63606e
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710-rpi-2-b.dts
@@ -0,0 +1,124 @@
+/dts-v1/;
+
+#include "bcm2710.dtsi"
+#include "bcm2709-rpi.dtsi"
+#include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+
+/ {
+	compatible = "raspberrypi,2-model-b-rev2", "brcm,bcm2837";
+	model = "Raspberry Pi 2 Model B rev 1.2";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 45>;
+		brcm,function = <4>;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&gpio 35 0>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts b/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
new file mode 100644
index 000000000000..4e4e47100831
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
@@ -0,0 +1,196 @@
+/dts-v1/;
+
+#include "bcm2710.dtsi"
+#include "bcm2709-rpi.dtsi"
+#include "bcm283x-rpi-lan7515.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_44.dtsi"
+#include "bcm271x-rpi-bt.dtsi"
+
+/ {
+	compatible = "raspberrypi,3-model-b-plus", "brcm,bcm2837";
+	model = "Raspberry Pi 3 Model B+";
+
+	chosen {
+		bootargs = "coherent_pool=1M 8250.nr_uarts=1 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+	};
+
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart0;
+		mmc1 = &mmcnr;
+	};
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins =     <34 35 36 37 38 39>;
+		brcm,function = <7>; // alt3 = SD1
+		brcm,pull =     <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins = <43>;
+		brcm,function = <4>; /* alt0:GPCLK2 */
+		brcm,pull = <0>;
+	};
+
+	uart0_pins: uart0_pins {
+		brcm,pins = <32 33>;
+		brcm,function = <7>; /* alt3=UART0 */
+		brcm,pull = <0 2>;
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins;
+		brcm,function;
+		brcm,pull;
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 41>;
+		brcm,function = <4>;
+	};
+};
+
+&mmcnr {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&firmware {
+	expgpio: expgpio {
+		compatible = "raspberrypi,firmware-gpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		status = "okay";
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins &bt_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 29 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "default-on";
+		gpios = <&expgpio 2 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+&eth_phy {
+	microchip,eee-enabled;
+	microchip,tx-lpi-timer = <600>; /* non-aggressive*/
+	microchip,downshift-after = <2>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+
+		eee = <&eth_phy>,"microchip,eee-enabled?";
+		tx_lpi_timer = <&eth_phy>,"microchip,tx-lpi-timer:0";
+		eth_led0 = <&eth_phy>,"microchip,led-modes:0";
+		eth_led1 = <&eth_phy>,"microchip,led-modes:4";
+		eth_downshift_after = <&eth_phy>,"microchip,downshift-after:0";
+		eth_max_speed = <&eth_phy>,"max-speed:0";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
new file mode 100644
index 000000000000..8989c00b03e5
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -0,0 +1,198 @@
+/dts-v1/;
+
+#include "bcm2710.dtsi"
+#include "bcm2709-rpi.dtsi"
+#include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_44.dtsi"
+#include "bcm271x-rpi-bt.dtsi"
+
+/ {
+	compatible = "raspberrypi,3-model-b", "brcm,bcm2837";
+	model = "Raspberry Pi 3 Model B";
+
+	chosen {
+		bootargs = "coherent_pool=1M 8250.nr_uarts=1 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+	};
+
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart0;
+		mmc1 = &mmcnr;
+	};
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins =     <34 35 36 37 38 39>;
+		brcm,function = <7>; // alt3 = SD1
+		brcm,pull =     <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins = <43>;
+		brcm,function = <4>; /* alt0:GPCLK2 */
+		brcm,pull = <0>;
+	};
+
+	uart0_pins: uart0_pins {
+		brcm,pins = <32 33>;
+		brcm,function = <7>; /* alt3=UART0 */
+		brcm,pull = <0 2>;
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins;
+		brcm,function;
+		brcm,pull;
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins = <40 41>;
+		brcm,function = <4>;
+	};
+};
+
+&mmcnr {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&soc {
+	virtgpio: virtgpio {
+		compatible = "brcm,bcm2835-virtgpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		firmware = <&firmware>;
+		status = "okay";
+	};
+
+};
+
+&firmware {
+	expgpio: expgpio {
+		compatible = "raspberrypi,firmware-gpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		status = "okay";
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins &bt_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "okay";
+};
+
+&bt {
+	max-speed = <921600>;
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&virtgpio 0 0>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "input";
+		gpios = <&expgpio 7 0>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&expgpio 4 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2710-rpi-cm3.dts b/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
new file mode 100644
index 000000000000..f972979281f5
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
@@ -0,0 +1,133 @@
+/dts-v1/;
+
+#include "bcm2710.dtsi"
+#include "bcm2709-rpi.dtsi"
+#include "bcm283x-rpi-csi0-2lane.dtsi"
+#include "bcm283x-rpi-csi1-4lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_28.dtsi"
+/ {
+	compatible = "raspberrypi,3-compute-module", "brcm,bcm2837";
+	model = "Raspberry Pi Compute Module 3";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	audio_pins: audio_pins {
+		brcm,pins;
+		brcm,function;
+	};
+};
+
+&soc {
+	virtgpio: virtgpio {
+		compatible = "brcm,bcm2835-virtgpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		firmware = <&firmware>;
+		status = "okay";
+	};
+
+};
+
+&firmware {
+	expgpio: expgpio {
+		compatible = "raspberrypi,firmware-gpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		status = "okay";
+	};
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&virtgpio 0 0>;
+	};
+};
+
+&hdmi {
+	hpd-gpios = <&expgpio 0 GPIO_ACTIVE_LOW>;
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2710.dtsi b/arch/arm/boot/dts/bcm2710.dtsi
new file mode 100644
index 000000000000..4e47480dd933
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710.dtsi
@@ -0,0 +1,29 @@
+#include "bcm2837.dtsi"
+#include "bcm270x.dtsi"
+
+/ {
+	compatible = "brcm,bcm2837", "brcm,bcm2836";
+
+	arm-pmu {
+#ifdef RPI364
+		compatible = "arm,armv8-pmuv3", "arm,cortex-a7-pmu";
+#else
+		compatible = "arm,cortex-a7-pmu";
+#endif
+	};
+
+	soc {
+		/delete-node/ timer@7e003000;
+	};
+
+	__overrides__ {
+		arm_freq = <&cpu0>, "clock-frequency:0",
+		       <&cpu1>, "clock-frequency:0",
+		       <&cpu2>, "clock-frequency:0",
+		       <&cpu3>, "clock-frequency:0";
+	};
+};
+
+&vc4 {
+	status = "disabled";
+};
diff --git a/arch/arm/boot/dts/bcm2711-rpi-4-b.dts b/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
index 5395e8c2484e..3e67c2b634be 100644
--- a/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
+++ b/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
@@ -2,7 +2,6 @@
 /dts-v1/;
 #include "bcm2711.dtsi"
 #include "bcm2835-rpi.dtsi"
-#include "bcm283x-rpi-usb-peripheral.dtsi"
 
 #include <dt-bindings/reset/raspberrypi,firmware-reset.h>
 
@@ -95,7 +94,7 @@ expgpio: gpio {
 				  "VDD_SD_IO_SEL",
 				  "CAM_GPIO",
 				  "SD_PWR_ON",
-				  "";
+				  "SD_OC_N";
 		status = "okay";
 	};
 
@@ -301,3 +300,306 @@ &vc4 {
 &vec {
 	status = "disabled";
 };
+
+// =============================================
+// Downstream rpi- changes
+
+#define BCM2711
+
+#include "bcm270x.dtsi"
+#include "bcm271x-rpi-bt.dtsi"
+
+/ {
+	soc {
+		/delete-node/ pixelvalve@7e807000;
+		/delete-node/ hdmi@7e902000;
+	};
+};
+
+#include "bcm2711-rpi.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_44.dtsi"
+
+/ {
+	chosen {
+		bootargs = "coherent_pool=1M 8250.nr_uarts=1 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+	};
+
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart0;
+		mmc0 = &emmc2;
+		mmc1 = &mmcnr;
+		mmc2 = &sdhost;
+		/delete-property/ i2c2;
+		i2c3 = &i2c3;
+		i2c4 = &i2c4;
+		i2c5 = &i2c5;
+		i2c6 = &i2c6;
+		/delete-property/ intc;
+	};
+
+	/delete-node/ wifi-pwrseq;
+};
+
+&mmcnr {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pins &bt_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-0 = <&uart1_pins>;
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi3_pins: spi3_pins {
+		brcm,pins = <1 2 3>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi3_cs_pins: spi3_cs_pins {
+		brcm,pins = <0 24>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi4_pins: spi4_pins {
+		brcm,pins = <5 6 7>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi4_cs_pins: spi4_cs_pins {
+		brcm,pins = <4 25>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi5_pins: spi5_pins {
+		brcm,pins = <13 14 15>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi5_cs_pins: spi5_cs_pins {
+		brcm,pins = <12 26>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi6_pins: spi6_pins {
+		brcm,pins = <19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi6_cs_pins: spi6_cs_pins {
+		brcm,pins = <18 27>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c3_pins: i2c3 {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c4_pins: i2c4 {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c5_pins: i2c5 {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c6_pins: i2c6 {
+		brcm,pins = <22 23>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins =     <34 35 36 37 38 39>;
+		brcm,function = <BCM2835_FSEL_ALT3>; // alt3 = SD1
+		brcm,pull =     <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins = "-"; // non-empty to keep btuart happy, //4 = 0
+				 // to fool pinctrl
+		brcm,function = <0>;
+		brcm,pull = <2>;
+	};
+
+	uart0_pins: uart0_pins {
+		brcm,pins = <32 33>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+		brcm,pull = <0 2>;
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins;
+		brcm,function;
+		brcm,pull;
+	};
+
+	uart2_pins: uart2_pins {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart3_pins: uart3_pins {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart4_pins: uart4_pins {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart5_pins: uart5_pins {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+/ {
+	__overrides__ {
+		/delete-property/ i2c2_baudrate;
+		/delete-property/ i2c2_iknowwhatimdoing;
+	};
+};
+
+// =============================================
+// Board specific stuff here
+
+&sdhost {
+	status = "disabled";
+};
+
+&phy1 {
+	led-modes = <0x00 0x08>; /* link/activity link */
+};
+
+&gpio {
+	audio_pins: audio_pins {
+		brcm,pins = <40 41>;
+		brcm,function = <4>;
+	};
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 42 GPIO_ACTIVE_HIGH>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "default-on";
+		gpios = <&expgpio 2 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&pwm1 {
+	status = "disabled";
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+
+		eth_led0 = <&phy1>,"led-modes:0";
+		eth_led1 = <&phy1>,"led-modes:4";
+
+		sd_poll_once = <&emmc2>, "non-removable?";
+		spi_dma4 = <&spi0>, "dmas:0=", <&dma40>,
+			   <&spi0>, "dmas:8=", <&dma40>;
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2711-rpi-cm4.dts b/arch/arm/boot/dts/bcm2711-rpi-cm4.dts
new file mode 100644
index 000000000000..0ca3a0126220
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2711-rpi-cm4.dts
@@ -0,0 +1,609 @@
+// SPDX-License-Identifier: GPL-2.0
+/dts-v1/;
+#include "bcm2711.dtsi"
+#include "bcm2835-rpi.dtsi"
+
+/ {
+	compatible = "raspberrypi,4-compute-module", "brcm,bcm2711";
+	model = "Raspberry Pi Compute Module 4";
+
+	chosen {
+		/* 8250 auxiliary UART instead of pl011 */
+		stdout-path = "serial1:115200n8";
+	};
+
+	/* Will be filled by the bootloader */
+	memory@0 {
+		device_type = "memory";
+		reg = <0 0 0>;
+	};
+
+	aliases {
+		emmc2bus = &emmc2bus;
+		ethernet0 = &genet;
+		pcie0 = &pcie0;
+	};
+
+	leds {
+		act {
+			gpios = <&gpio 42 GPIO_ACTIVE_HIGH>;
+		};
+
+		pwr {
+			label = "PWR";
+			gpios = <&expgpio 2 GPIO_ACTIVE_LOW>;
+			default-state = "keep";
+			linux,default-trigger = "default-on";
+		};
+	};
+
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&expgpio 1 GPIO_ACTIVE_LOW>;
+	};
+
+	sd_io_1v8_reg: sd_io_1v8_reg {
+		compatible = "regulator-gpio";
+		regulator-name = "vdd-sd-io";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+		regulator-settling-time-us = <5000>;
+		gpios = <&expgpio 4 GPIO_ACTIVE_HIGH>;
+		states = <1800000 0x1
+			  3300000 0x0>;
+		status = "okay";
+	};
+
+	sd_vcc_reg: sd_vcc_reg {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc-sd";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&expgpio 6 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+&ddc0 {
+	status = "okay";
+};
+
+&ddc1 {
+	status = "okay";
+};
+
+&firmware {
+	expgpio: gpio {
+		compatible = "raspberrypi,firmware-gpio";
+		gpio-controller;
+		#gpio-cells = <2>;
+		gpio-line-names = "BT_ON",
+				  "WL_ON",
+				  "PWR_LED_OFF",
+				  "ANT1",
+				  "VDD_SD_IO_SEL",
+				  "CAM_GPIO",
+				  "SD_PWR_ON",
+				  "ANT2";
+		status = "okay";
+
+		ant1: ant1 {
+			gpio-hog;
+			gpios = <3 GPIO_ACTIVE_HIGH>;
+			output-high;
+		};
+
+		ant2: ant2 {
+			gpio-hog;
+			gpios = <7 GPIO_ACTIVE_HIGH>;
+			output-low;
+		};
+	};
+};
+
+&gpio {
+	/*
+	 * Parts taken from rpi_SCH_4b_4p0_reduced.pdf and
+	 * the official GPU firmware DT blob.
+	 *
+	 * Legend:
+	 * "FOO" = GPIO line named "FOO" on the schematic
+	 * "FOO_N" = GPIO line named "FOO" on schematic, active low
+	 */
+	gpio-line-names = "ID_SDA",
+			  "ID_SCL",
+			  "SDA1",
+			  "SCL1",
+			  "GPIO_GCLK",
+			  "GPIO5",
+			  "GPIO6",
+			  "SPI_CE1_N",
+			  "SPI_CE0_N",
+			  "SPI_MISO",
+			  "SPI_MOSI",
+			  "SPI_SCLK",
+			  "GPIO12",
+			  "GPIO13",
+			  /* Serial port */
+			  "TXD1",
+			  "RXD1",
+			  "GPIO16",
+			  "GPIO17",
+			  "GPIO18",
+			  "GPIO19",
+			  "GPIO20",
+			  "GPIO21",
+			  "GPIO22",
+			  "GPIO23",
+			  "GPIO24",
+			  "GPIO25",
+			  "GPIO26",
+			  "GPIO27",
+			  "RGMII_MDIO",
+			  "RGMIO_MDC",
+			  /* Used by BT module */
+			  "CTS0",
+			  "RTS0",
+			  "TXD0",
+			  "RXD0",
+			  /* Used by Wifi */
+			  "SD1_CLK",
+			  "SD1_CMD",
+			  "SD1_DATA0",
+			  "SD1_DATA1",
+			  "SD1_DATA2",
+			  "SD1_DATA3",
+			  /* Shared with SPI flash */
+			  "PWM0_MISO",
+			  "PWM1_MOSI",
+			  "STATUS_LED_G_CLK",
+			  "SPIFLASH_CE_N",
+			  "SDA0",
+			  "SCL0",
+			  "RGMII_RXCLK",
+			  "RGMII_RXCTL",
+			  "RGMII_RXD0",
+			  "RGMII_RXD1",
+			  "RGMII_RXD2",
+			  "RGMII_RXD3",
+			  "RGMII_TXCLK",
+			  "RGMII_TXCTL",
+			  "RGMII_TXD0",
+			  "RGMII_TXD1",
+			  "RGMII_TXD2",
+			  "RGMII_TXD3";
+};
+
+&hdmi0 {
+	clocks = <&firmware_clocks 13>, <&firmware_clocks 14>, <&dvp 0>, <&clk_27MHz>;
+	clock-names = "hdmi", "bvb", "audio", "cec";
+	status = "okay";
+};
+
+&hdmi1 {
+	clocks = <&firmware_clocks 13>, <&firmware_clocks 14>, <&dvp 1>, <&clk_27MHz>;
+	clock-names = "hdmi", "bvb", "audio", "cec";
+	status = "okay";
+};
+
+&hvs {
+	clocks = <&firmware_clocks 4>;
+};
+
+&pixelvalve0 {
+	status = "okay";
+};
+
+&pixelvalve1 {
+	status = "okay";
+};
+
+&pixelvalve2 {
+	status = "okay";
+};
+
+&pixelvalve4 {
+	status = "okay";
+};
+
+&vc4 {
+	status = "okay";
+};
+
+&vec {
+	status = "disabled";
+};
+
+&pwm1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm1_0_gpio40 &pwm1_1_gpio41>;
+	status = "okay";
+};
+
+/* SDHCI is used to control the SDIO for wireless */
+&sdhci {
+	#address-cells = <1>;
+	#size-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&emmc_gpio34>;
+	bus-width = <4>;
+	non-removable;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	status = "okay";
+
+	brcmf: wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+	};
+};
+
+/* EMMC2 is used to drive the EMMC card */
+&emmc2 {
+	bus-width = <8>;
+	vqmmc-supply = <&sd_io_1v8_reg>;
+	vmmc-supply = <&sd_vcc_reg>;
+	broken-cd;
+	status = "okay";
+};
+
+&genet {
+	phy-handle = <&phy1>;
+	phy-mode = "rgmii-rxid";
+	status = "okay";
+};
+
+&genet_mdio {
+	phy1: ethernet-phy@1 {
+		/* No PHY interrupt */
+		reg = <0x1>;
+	};
+};
+
+/* uart0 communicates with the BT module */
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_ctsrts_gpio30 &uart0_gpio32>;
+	uart-has-rtscts;
+	status = "okay";
+
+	bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		max-speed = <2000000>;
+		shutdown-gpios = <&expgpio 0 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+/* uart1 is mapped to the pin header */
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_gpio14>;
+	status = "okay";
+};
+
+&vchiq {
+	interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+// =============================================
+// Downstream rpi- changes
+
+#define BCM2711
+
+#include "bcm270x.dtsi"
+#include "bcm271x-rpi-bt.dtsi"
+
+/ {
+	soc {
+		/delete-node/ pixelvalve@7e807000;
+		/delete-node/ hdmi@7e902000;
+	};
+};
+
+#include "bcm2711-rpi.dtsi"
+#include "bcm283x-rpi-csi0-2lane.dtsi"
+#include "bcm283x-rpi-csi1-4lane.dtsi"
+#include "bcm283x-rpi-i2c0mux_0_44.dtsi"
+
+/ {
+	chosen {
+		bootargs = "coherent_pool=1M 8250.nr_uarts=1 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1 snd_bcm2835.enable_headphones=1";
+	};
+
+	aliases {
+		serial0 = &uart1;
+		serial1 = &uart0;
+		mmc0 = &emmc2;
+		mmc1 = &mmcnr;
+		mmc2 = &sdhost;
+		/delete-property/ i2c2;
+		i2c3 = &i2c3;
+		i2c4 = &i2c4;
+		i2c5 = &i2c5;
+		i2c6 = &i2c6;
+		/delete-property/ intc;
+	};
+
+	/delete-node/ wifi-pwrseq;
+};
+
+&mmcnr {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-0 = <&uart0_pins &bt_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-0 = <&uart1_pins>;
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev0: spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+
+	spidev1: spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <125000000>;
+	};
+};
+
+&gpio {
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi3_pins: spi3_pins {
+		brcm,pins = <1 2 3>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi3_cs_pins: spi3_cs_pins {
+		brcm,pins = <0 24>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi4_pins: spi4_pins {
+		brcm,pins = <5 6 7>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi4_cs_pins: spi4_cs_pins {
+		brcm,pins = <4 25>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi5_pins: spi5_pins {
+		brcm,pins = <13 14 15>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi5_cs_pins: spi5_cs_pins {
+		brcm,pins = <12 26>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	spi6_pins: spi6_pins {
+		brcm,pins = <19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+	};
+
+	spi6_cs_pins: spi6_cs_pins {
+		brcm,pins = <18 27>;
+		brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c3_pins: i2c3 {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c4_pins: i2c4 {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c5_pins: i2c5 {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2c6_pins: i2c6 {
+		brcm,pins = <22 23>;
+		brcm,function = <BCM2835_FSEL_ALT5>;
+		brcm,pull = <BCM2835_PUD_UP>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins =     <34 35 36 37 38 39>;
+		brcm,function = <BCM2835_FSEL_ALT3>; // alt3 = SD1
+		brcm,pull =     <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins = "-"; // non-empty to keep btuart happy, //4 = 0
+				 // to fool pinctrl
+		brcm,function = <0>;
+		brcm,pull = <2>;
+	};
+
+	uart0_pins: uart0_pins {
+		brcm,pins = <32 33>;
+		brcm,function = <BCM2835_FSEL_ALT3>;
+		brcm,pull = <0 2>;
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins;
+		brcm,function;
+		brcm,pull;
+	};
+
+	uart2_pins: uart2_pins {
+		brcm,pins = <0 1>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart3_pins: uart3_pins {
+		brcm,pins = <4 5>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart4_pins: uart4_pins {
+		brcm,pins = <8 9>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+
+	uart5_pins: uart5_pins {
+		brcm,pins = <12 13>;
+		brcm,function = <BCM2835_FSEL_ALT4>;
+		brcm,pull = <0 2>;
+	};
+};
+
+&i2c0if {
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+/ {
+	__overrides__ {
+		/delete-property/ i2c2_baudrate;
+		/delete-property/ i2c2_iknowwhatimdoing;
+	};
+};
+
+// =============================================
+// Board specific stuff here
+
+&pcie0 {
+       brcm,enable-l1ss;
+};
+
+&sdhost {
+	status = "disabled";
+};
+
+&phy1 {
+	led-modes = <0x00 0x08>; /* link/activity link */
+};
+
+&gpio {
+	audio_pins: audio_pins {
+		brcm,pins = <40 41>;
+		brcm,function = <4>;
+	};
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 42 GPIO_ACTIVE_HIGH>;
+	};
+
+	pwr_led: pwr {
+		label = "led1";
+		linux,default-trigger = "default-on";
+		gpios = <&expgpio 2 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&pwm1 {
+	status = "disabled";
+};
+
+&audio {
+	pinctrl-names = "default";
+	pinctrl-0 = <&audio_pins>;
+};
+
+/ {
+	__overrides__ {
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		pwr_led_gpio = <&pwr_led>,"gpios:4";
+		pwr_led_activelow = <&pwr_led>,"gpios:8";
+		pwr_led_trigger = <&pwr_led>,"linux,default-trigger";
+
+		eth_led0 = <&phy1>,"led-modes:0";
+		eth_led1 = <&phy1>,"led-modes:4";
+
+		ant1 =  <&ant1>,"output-high?=on",
+			<&ant1>, "output-low?=off",
+			<&ant2>, "output-high?=off",
+			<&ant2>, "output-low?=on";
+		ant2 =  <&ant1>,"output-high?=off",
+			<&ant1>, "output-low?=on",
+			<&ant2>, "output-high?=on",
+			<&ant2>, "output-low?=off";
+		noant = <&ant1>,"output-high?=off",
+			<&ant1>, "output-low?=on",
+			<&ant2>, "output-high?=off",
+			<&ant2>, "output-low?=on";
+
+		sd_poll_once = <&emmc2>, "non-removable?";
+		spi_dma4 = <&spi0>, "dmas:0=", <&dma40>,
+			   <&spi0>, "dmas:8=", <&dma40>;
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2711-rpi.dtsi b/arch/arm/boot/dts/bcm2711-rpi.dtsi
new file mode 100644
index 000000000000..4f903a787d65
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2711-rpi.dtsi
@@ -0,0 +1,201 @@
+// SPDX-License-Identifier: GPL-2.0
+#include "bcm270x-rpi.dtsi"
+
+/ {
+	__overrides__ {
+		arm_freq;
+	};
+
+	v3dbus: v3dbus {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <2>;
+		ranges = <0x7c500000  0x0 0xfc500000  0x0 0x03300000>,
+			 <0x40000000  0x0 0xff800000  0x0 0x00800000>;
+		dma-ranges = <0x00000000  0x0 0x00000000  0x4 0x00000000>;
+
+		v3d: v3d@7ec04000 {
+			compatible = "brcm,2711-v3d";
+			reg =
+			    <0x7ec00000  0x0 0x4000>,
+			    <0x7ec04000  0x0 0x4000>;
+			reg-names = "hub", "core0";
+
+			power-domains = <&pm BCM2835_POWER_DOMAIN_GRAFX_V3D>;
+			resets = <&pm BCM2835_RESET_V3D>;
+			clocks = <&firmware_clocks 5>;
+			clocks-names = "v3d";
+			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+		};
+	};
+
+	scb: scb {
+	     /* Add a label */
+	};
+};
+
+&cma {
+	/* Limit cma to the lower 768MB to allow room for HIGHMEM on 32-bit */
+	alloc-ranges = <0x0 0x00000000 0x30000000>;
+};
+
+&scb {
+	ranges = <0x0 0x7c000000  0x0 0xfc000000  0x0 0x03800000>,
+		 <0x0 0x40000000  0x0 0xff800000  0x0 0x00800000>,
+		 <0x6 0x00000000  0x6 0x00000000  0x0 0x40000000>,
+		 <0x0 0x00000000  0x0 0x00000000  0x0 0xfc000000>;
+	dma-ranges = <0x0 0x00000000  0x0 0x00000000  0x4 0x00000000>;
+
+	dma40: dma@7e007b00 {
+		compatible = "brcm,bcm2711-dma";
+		reg = <0x0 0x7e007b00  0x0 0x400>;
+		interrupts =
+			<GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>, /* dma4 11 */
+			<GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>, /* dma4 12 */
+			<GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>, /* dma4 13 */
+			<GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>; /* dma4 14 */
+		interrupt-names = "dma11",
+			"dma12",
+			"dma13",
+			"dma14";
+		#dma-cells = <1>;
+		brcm,dma-channel-mask = <0x7800>;
+	};
+
+	xhci: xhci@7e9c0000 {
+		compatible = "generic-xhci";
+		status = "disabled";
+		reg = <0x0 0x7e9c0000  0x0 0x100000>;
+		interrupts = <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>;
+		power-domains = <&power RPI_POWER_DOMAIN_USB>;
+	};
+
+	hevc-decoder@7eb00000 {
+		compatible = "raspberrypi,rpivid-hevc-decoder";
+		reg = <0x0 0x7eb00000  0x0 0x10000>;
+		status = "okay";
+	};
+
+	rpivid-local-intc@7eb10000 {
+		compatible = "raspberrypi,rpivid-local-intc";
+		reg = <0x0 0x7eb10000  0x0 0x1000>;
+		status = "okay";
+		interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
+	h264-decoder@7eb20000 {
+		compatible = "raspberrypi,rpivid-h264-decoder";
+		reg = <0x0 0x7eb20000  0x0 0x10000>;
+		status = "okay";
+	};
+
+	vp9-decoder@7eb30000 {
+		compatible = "raspberrypi,rpivid-vp9-decoder";
+		reg = <0x0 0x7eb30000  0x0 0x10000>;
+		status = "okay";
+	};
+};
+
+&dma40 {
+	/* The VPU firmware uses DMA channel 11 for VCHIQ */
+	brcm,dma-channel-mask = <0x7000>;
+};
+
+&vchiq {
+	compatible = "brcm,bcm2711-vchiq";
+};
+
+&firmwarekms {
+	compatible = "raspberrypi,rpi-firmware-kms-2711";
+	interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&smi {
+	interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&mmc {
+	interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&mmcnr {
+	interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&csi0 {
+	interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&csi1 {
+	interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&random {
+	compatible = "brcm,bcm2711-rng200";
+	status = "okay";
+};
+
+&usb {
+	/* Enable the FIQ support */
+	reg = <0x7e980000 0x10000>,
+	      <0x7e00b200 0x200>;
+	interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
+	status = "disabled";
+};
+
+&gpio {
+	interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
+		     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
+};
+
+&emmc2 {
+	mmc-ddr-3_3v;
+};
+
+&vc4 {
+	status = "disabled";
+};
+
+&pixelvalve0 {
+	status = "disabled";
+};
+
+&pixelvalve1 {
+	status = "disabled";
+};
+
+&pixelvalve2 {
+	status = "disabled";
+};
+
+&pixelvalve3 {
+	status = "disabled";
+};
+
+&pixelvalve4 {
+	status = "disabled";
+};
+
+&hdmi0 {
+	dmas = <&dma (10|(1<<27))>;
+	status = "disabled";
+};
+
+&ddc0 {
+	status = "disabled";
+};
+
+&hdmi1 {
+	dmas = <&dma (17|(1<<27))>;
+	status = "disabled";
+};
+
+&ddc1 {
+	status = "disabled";
+};
+
+&dvp {
+	status = "disabled";
+};
diff --git a/arch/arm/boot/dts/bcm2711.dtsi b/arch/arm/boot/dts/bcm2711.dtsi
index 3d040f6e2a20..6e0339266027 100644
--- a/arch/arm/boot/dts/bcm2711.dtsi
+++ b/arch/arm/boot/dts/bcm2711.dtsi
@@ -318,7 +318,8 @@ hdmi0: hdmi@7ef00700 {
 			      <0x7ef01f00 0x400>,
 			      <0x7ef00200 0x80>,
 			      <0x7ef04300 0x100>,
-			      <0x7ef20000 0x100>;
+			      <0x7ef20000 0x100>,
+			      <0x7ef00100 0x30>;
 			reg-names = "hdmi",
 				    "dvp",
 				    "phy",
@@ -327,12 +328,18 @@ hdmi0: hdmi@7ef00700 {
 				    "metadata",
 				    "csc",
 				    "cec",
-				    "hd";
+				    "hd",
+				    "intr2";
+			clocks = <&firmware_clocks 13>,
+				 <&firmware_clocks 14>,
+				 <&dvp 0>,
+				 <&clk_27MHz>;
 			clock-names = "hdmi", "bvb", "audio", "cec";
 			resets = <&dvp 0>;
 			ddc = <&ddc0>;
 			dmas = <&dma 10>;
 			dma-names = "audio-rx";
+			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
 			status = "disabled";
 		};
 
@@ -354,7 +361,8 @@ hdmi1: hdmi@7ef05700 {
 			      <0x7ef06f00 0x400>,
 			      <0x7ef00280 0x80>,
 			      <0x7ef09300 0x100>,
-			      <0x7ef20000 0x100>;
+			      <0x7ef20000 0x100>,
+			      <0x7ef00100 0x30>;
 			reg-names = "hdmi",
 				    "dvp",
 				    "phy",
@@ -363,12 +371,18 @@ hdmi1: hdmi@7ef05700 {
 				    "metadata",
 				    "csc",
 				    "cec",
-				    "hd";
+				    "hd",
+				    "intr2";
 			ddc = <&ddc1>;
 			clock-names = "hdmi", "bvb", "audio", "cec";
+			clocks = <&firmware_clocks 13>,
+				 <&firmware_clocks 14>,
+				 <&dvp 0>,
+				 <&clk_27MHz>;
 			resets = <&dvp 1>;
 			dmas = <&dma 17>;
 			dma-names = "audio-rx";
+			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
 			status = "disabled";
 		};
 
@@ -468,14 +482,14 @@ cpu3: cpu@3 {
 	scb {
 		compatible = "simple-bus";
 		#address-cells = <2>;
-		#size-cells = <1>;
+		#size-cells = <2>;
 
-		ranges = <0x0 0x7c000000  0x0 0xfc000000  0x03800000>,
-			 <0x6 0x00000000  0x6 0x00000000  0x40000000>;
+		ranges = <0x0 0x7c000000  0x0 0xfc000000  0x0 0x03800000>,
+			 <0x6 0x00000000  0x6 0x00000000  0x0 0x40000000>;
 
 		pcie0: pcie@7d500000 {
 			compatible = "brcm,bcm2711-pcie";
-			reg = <0x0 0x7d500000 0x9310>;
+			reg = <0x0 0x7d500000  0x0 0x9310>;
 			device_type = "pci";
 			#address-cells = <3>;
 			#interrupt-cells = <1>;
@@ -503,7 +517,7 @@ pcie0: pcie@7d500000 {
 
 		genet: ethernet@7d580000 {
 			compatible = "brcm,bcm2711-genet-v5";
-			reg = <0x0 0x7d580000 0x10000>;
+			reg = <0x0 0x7d580000  0x0 0x10000>;
 			#address-cells = <0x1>;
 			#size-cells = <0x1>;
 			interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
@@ -1010,7 +1024,7 @@ &cma {
 	alloc-ranges = <0x0 0x00000000 0x40000000>;
 };
 
-&i2c0 {
+&i2c0if {
 	compatible = "brcm,bcm2711-i2c", "brcm,bcm2835-i2c";
 	interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
 };
diff --git a/arch/arm/boot/dts/bcm271x-rpi-bt.dtsi b/arch/arm/boot/dts/bcm271x-rpi-bt.dtsi
new file mode 100644
index 000000000000..6b9b79f74cf3
--- /dev/null
+++ b/arch/arm/boot/dts/bcm271x-rpi-bt.dtsi
@@ -0,0 +1,26 @@
+// SPDX-License-Identifier: GPL-2.0
+
+&uart0 {
+	bt: bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		max-speed = <3000000>;
+		shutdown-gpios = <&expgpio 0 GPIO_ACTIVE_HIGH>;
+		status = "disabled";
+	};
+};
+
+&uart1 {
+	minibt: bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		max-speed = <460800>;
+		shutdown-gpios = <&expgpio 0 GPIO_ACTIVE_HIGH>;
+		status = "disabled";
+	};
+};
+
+/ {
+	__overrides__ {
+		krnbt = <&bt>,"status";
+		krnbt_baudrate = <&bt>,"max-speed:0";
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2835-common.dtsi b/arch/arm/boot/dts/bcm2835-common.dtsi
index 4119271c979d..bd77ba3a3562 100644
--- a/arch/arm/boot/dts/bcm2835-common.dtsi
+++ b/arch/arm/boot/dts/bcm2835-common.dtsi
@@ -116,12 +116,14 @@ hdmi: hdmi@7e902000 {
 			compatible = "brcm,bcm2835-hdmi";
 			reg = <0x7e902000 0x600>,
 			      <0x7e808000 0x100>;
+			reg-names = "hdmi",
+				    "hd";
 			interrupts = <2 8>, <2 9>;
 			ddc = <&i2c2>;
 			clocks = <&clocks BCM2835_PLLH_PIX>,
 				 <&clocks BCM2835_CLOCK_HSM>;
 			clock-names = "pixel", "hdmi";
-			dmas = <&dma 17>;
+			dmas = <&dma (17|(1<<27))>;
 			dma-names = "audio-rx";
 			status = "disabled";
 		};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts b/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
index 40b9405f1a8e..d2384d8e8555 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
@@ -126,3 +126,8 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 28&29 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-a.dts b/arch/arm/boot/dts/bcm2835-rpi-a.dts
index 11edb581dbaf..4ceca674b752 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-a.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-a.dts
@@ -121,3 +121,10 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* i2c0 on camera/display connector is gpio 0&1. Not exposed on header.
+ * To avoid having to remap everything, map both ports to gpios 0&1
+ */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio0>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts b/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
index 1b435c64bd9c..8f2d10d82fa1 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
@@ -128,3 +128,8 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 28&29 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts b/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
index a23c25c00eea..547c88a3ae9f 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
@@ -121,3 +121,10 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* i2c0 on camera/display connector is gpio 0&1. Not exposed on header.
+ * To avoid having to remap everything, map both ports to gpios 0&1
+ */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio0>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-b.dts b/arch/arm/boot/dts/bcm2835-rpi-b.dts
index 1b63d6b19750..073fc99ef8a2 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b.dts
@@ -116,3 +116,10 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* camera/display connector use BSC1 on GPIOS 2&3.
+ * To avoid having to remap everything, map both ports to gpios 0&1
+ */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio0>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts b/arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts
index a75c882e6575..95564c93a645 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-cm1-io1.dts
@@ -95,3 +95,8 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* WHAT TO DO HERE? */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-zero-w.dts b/arch/arm/boot/dts/bcm2835-rpi-zero-w.dts
index 33b2b77aa47d..3ea5c7e6be54 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-zero-w.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-zero-w.dts
@@ -149,3 +149,8 @@ &uart1 {
 	pinctrl-0 = <&uart1_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 28&29 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi-zero.dts b/arch/arm/boot/dts/bcm2835-rpi-zero.dts
index 6f9b3a908f28..a0eabab12c99 100644
--- a/arch/arm/boot/dts/bcm2835-rpi-zero.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-zero.dts
@@ -117,3 +117,8 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 28&29 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm2835-rpi.dtsi b/arch/arm/boot/dts/bcm2835-rpi.dtsi
index 87ddcad76083..1b16cb9ccb88 100644
--- a/arch/arm/boot/dts/bcm2835-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2835-rpi.dtsi
@@ -19,6 +19,11 @@ firmware: firmware {
 
 			mboxes = <&mailbox>;
 			dma-ranges;
+
+			firmware_clocks: clocks {
+				compatible = "raspberrypi,firmware-clocks";
+				#clock-cells = <1>;
+			};
 		};
 
 		power: power {
@@ -49,13 +54,17 @@ alt0: alt0 {
 	};
 };
 
-&i2c0 {
-	pinctrl-names = "default";
-	pinctrl-0 = <&i2c0_gpio0>;
+&i2c0if {
 	status = "okay";
 	clock-frequency = <100000>;
 };
 
+&i2c0mux {
+	pinctrl-0 = <&i2c0_gpio0>;
+	/* pinctrl-1 varies based on platform */
+	status = "okay";
+};
+
 &i2c1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c1_gpio2>;
diff --git a/arch/arm/boot/dts/bcm2835.dtsi b/arch/arm/boot/dts/bcm2835.dtsi
index 0549686134ea..2ea891228ea0 100644
--- a/arch/arm/boot/dts/bcm2835.dtsi
+++ b/arch/arm/boot/dts/bcm2835.dtsi
@@ -19,7 +19,7 @@ cpu@0 {
 
 	soc {
 		ranges = <0x7e000000 0x20000000 0x02000000>;
-		dma-ranges = <0x40000000 0x00000000 0x20000000>;
+		dma-ranges = <0x80000000 0x00000000 0x20000000>;
 	};
 
 	arm-pmu {
diff --git a/arch/arm/boot/dts/bcm2836-rpi-2-b.dts b/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
index d8af8eeac7b6..bf22b74359d8 100644
--- a/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
+++ b/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
@@ -128,3 +128,8 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 28&29 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm2837-rpi-3-a-plus.dts b/arch/arm/boot/dts/bcm2837-rpi-3-a-plus.dts
index 77099a7871b0..9529c0475673 100644
--- a/arch/arm/boot/dts/bcm2837-rpi-3-a-plus.dts
+++ b/arch/arm/boot/dts/bcm2837-rpi-3-a-plus.dts
@@ -178,3 +178,8 @@ &uart1 {
 	pinctrl-0 = <&uart1_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 44&45 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio44>;
+};
diff --git a/arch/arm/boot/dts/bcm2837-rpi-3-b-plus.dts b/arch/arm/boot/dts/bcm2837-rpi-3-b-plus.dts
index 61010266ca9a..40cb269aed0f 100644
--- a/arch/arm/boot/dts/bcm2837-rpi-3-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2837-rpi-3-b-plus.dts
@@ -181,3 +181,8 @@ &uart1 {
 	pinctrl-0 = <&uart1_gpio14>;
 	status = "okay";
 };
+
+/* i2c on camera/display connector is gpio 44&45 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio44>;
+};
diff --git a/arch/arm/boot/dts/bcm2837-rpi-3-b.dts b/arch/arm/boot/dts/bcm2837-rpi-3-b.dts
index dd4a48604097..8f16b6b3fe08 100644
--- a/arch/arm/boot/dts/bcm2837-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2837-rpi-3-b.dts
@@ -174,3 +174,8 @@ &sdhost {
 	status = "okay";
 	bus-width = <4>;
 };
+
+/* i2c on camera/display connector is gpio 44&45 */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio44>;
+};
diff --git a/arch/arm/boot/dts/bcm2837-rpi-cm3-io3.dts b/arch/arm/boot/dts/bcm2837-rpi-cm3-io3.dts
index 588d9411ceb6..dde209ade51b 100644
--- a/arch/arm/boot/dts/bcm2837-rpi-cm3-io3.dts
+++ b/arch/arm/boot/dts/bcm2837-rpi-cm3-io3.dts
@@ -94,3 +94,8 @@ &uart0 {
 	pinctrl-0 = <&uart0_gpio14>;
 	status = "okay";
 };
+
+/* WHAT TO DO HERE? */
+&i2c0mux {
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi b/arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi
new file mode 100644
index 000000000000..6e4ce8622b47
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi
@@ -0,0 +1,4 @@
+// SPDX-License-Identifier: GPL-2.0-only
+&csi0 {
+	brcm,num-data-lanes = <2>;
+};
diff --git a/arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi b/arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi
new file mode 100644
index 000000000000..6938f4daacdc
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi
@@ -0,0 +1,4 @@
+// SPDX-License-Identifier: GPL-2.0-only
+&csi1 {
+	brcm,num-data-lanes = <2>;
+};
diff --git a/arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi b/arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi
new file mode 100644
index 000000000000..b37037437bee
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi
@@ -0,0 +1,4 @@
+// SPDX-License-Identifier: GPL-2.0-only
+&csi1 {
+	brcm,num-data-lanes = <4>;
+};
diff --git a/arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_28.dtsi b/arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_28.dtsi
new file mode 100644
index 000000000000..38f0074bce3f
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_28.dtsi
@@ -0,0 +1,4 @@
+&i2c0mux {
+	pinctrl-0 = <&i2c0_gpio0>;
+	pinctrl-1 = <&i2c0_gpio28>;
+};
diff --git a/arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_44.dtsi b/arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_44.dtsi
new file mode 100644
index 000000000000..119946d878db
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-i2c0mux_0_44.dtsi
@@ -0,0 +1,4 @@
+&i2c0mux {
+	pinctrl-0 = <&i2c0_gpio0>;
+	pinctrl-1 = <&i2c0_gpio44>;
+};
diff --git a/arch/arm/boot/dts/bcm283x-rpi-usb-peripheral.dtsi b/arch/arm/boot/dts/bcm283x-rpi-usb-peripheral.dtsi
deleted file mode 100644
index 0ff0e9e25327..000000000000
--- a/arch/arm/boot/dts/bcm283x-rpi-usb-peripheral.dtsi
+++ /dev/null
@@ -1,7 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-&usb {
-	dr_mode = "peripheral";
-	g-rx-fifo-size = <256>;
-	g-np-tx-fifo-size = <32>;
-	g-tx-fifo-size = <256 256 512 512 512 768 768>;
-};
diff --git a/arch/arm/boot/dts/bcm283x.dtsi b/arch/arm/boot/dts/bcm283x.dtsi
index 0f3be55201a5..6d305b8b5ebe 100644
--- a/arch/arm/boot/dts/bcm283x.dtsi
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -334,7 +334,7 @@ spi: spi@7e204000 {
 			status = "disabled";
 		};
 
-		i2c0: i2c@7e205000 {
+		i2c0if: i2c@7e205000 {
 			compatible = "brcm,bcm2835-i2c";
 			reg = <0x7e205000 0x200>;
 			interrupts = <2 21>;
@@ -344,6 +344,30 @@ i2c0: i2c@7e205000 {
 			status = "disabled";
 		};
 
+		i2c0mux: i2c0mux {
+			compatible = "i2c-mux-pinctrl";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			i2c-parent = <&i2c0if>;
+
+			pinctrl-names = "i2c0", "i2c_csi_dsi";
+
+			status = "disabled";
+
+			i2c0: i2c@0 {
+				reg = <0>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+
+			i2c_csi_dsi: i2c@1 {
+				reg = <1>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
 		dpi: dpi@7e208000 {
 			compatible = "brcm,bcm2835-dpi";
 			reg = <0x7e208000 0x8c>;
diff --git a/arch/arm/boot/dts/overlays/Makefile b/arch/arm/boot/dts/overlays/Makefile
new file mode 100644
index 000000000000..b30568e29526
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/Makefile
@@ -0,0 +1,216 @@
+# Overlays for the Raspberry Pi platform
+
+dtb-$(CONFIG_ARCH_BCM2835) += overlay_map.dtb
+
+dtbo-$(CONFIG_ARCH_BCM2835) += \
+	act-led.dtbo \
+	adafruit18.dtbo \
+	adau1977-adc.dtbo \
+	adau7002-simple.dtbo \
+	ads1015.dtbo \
+	ads1115.dtbo \
+	ads7846.dtbo \
+	adv7282m.dtbo \
+	adv728x-m.dtbo \
+	akkordion-iqdacplus.dtbo \
+	allo-boss-dac-pcm512x-audio.dtbo \
+	allo-digione.dtbo \
+	allo-katana-dac-audio.dtbo \
+	allo-piano-dac-pcm512x-audio.dtbo \
+	allo-piano-dac-plus-pcm512x-audio.dtbo \
+	anyspi.dtbo \
+	apds9960.dtbo \
+	applepi-dac.dtbo \
+	at86rf233.dtbo \
+	audioinjector-addons.dtbo \
+	audioinjector-isolated-soundcard.dtbo \
+	audioinjector-ultra.dtbo \
+	audioinjector-wm8731-audio.dtbo \
+	audiosense-pi.dtbo \
+	audremap.dtbo \
+	balena-fin.dtbo \
+	cma.dtbo \
+	dht11.dtbo \
+	dionaudio-loco.dtbo \
+	dionaudio-loco-v2.dtbo \
+	disable-bt.dtbo \
+	disable-wifi.dtbo \
+	dpi18.dtbo \
+	dpi24.dtbo \
+	draws.dtbo \
+	dwc-otg.dtbo \
+	dwc2.dtbo \
+	enc28j60.dtbo \
+	enc28j60-spi2.dtbo \
+	exc3000.dtbo \
+	fe-pi-audio.dtbo \
+	fsm-demo.dtbo \
+	ghost-amp.dtbo \
+	goodix.dtbo \
+	googlevoicehat-soundcard.dtbo \
+	gpio-fan.dtbo \
+	gpio-ir.dtbo \
+	gpio-ir-tx.dtbo \
+	gpio-key.dtbo \
+	gpio-no-bank0-irq.dtbo \
+	gpio-no-irq.dtbo \
+	gpio-poweroff.dtbo \
+	gpio-shutdown.dtbo \
+	hd44780-lcd.dtbo \
+	hdmi-backlight-hwhack-gpio.dtbo \
+	hifiberry-amp.dtbo \
+	hifiberry-dac.dtbo \
+	hifiberry-dacplus.dtbo \
+	hifiberry-dacplusadc.dtbo \
+	hifiberry-dacplusadcpro.dtbo \
+	hifiberry-dacplusdsp.dtbo \
+	hifiberry-dacplushd.dtbo \
+	hifiberry-digi.dtbo \
+	hifiberry-digi-pro.dtbo \
+	highperi.dtbo \
+	hy28a.dtbo \
+	hy28b.dtbo \
+	hy28b-2017.dtbo \
+	i-sabre-q2m.dtbo \
+	i2c-bcm2708.dtbo \
+	i2c-gpio.dtbo \
+	i2c-mux.dtbo \
+	i2c-pwm-pca9685a.dtbo \
+	i2c-rtc.dtbo \
+	i2c-rtc-gpio.dtbo \
+	i2c-sensor.dtbo \
+	i2c0.dtbo \
+	i2c1.dtbo \
+	i2c3.dtbo \
+	i2c4.dtbo \
+	i2c5.dtbo \
+	i2c6.dtbo \
+	i2s-gpio28-31.dtbo \
+	ilitek251x.dtbo \
+	imx219.dtbo \
+	imx290.dtbo \
+	imx477.dtbo \
+	iqaudio-codec.dtbo \
+	iqaudio-dac.dtbo \
+	iqaudio-dacplus.dtbo \
+	iqaudio-digi-wm8804-audio.dtbo \
+	irs1125.dtbo \
+	jedec-spi-nor.dtbo \
+	justboom-both.dtbo \
+	justboom-dac.dtbo \
+	justboom-digi.dtbo \
+	ltc294x.dtbo \
+	max98357a.dtbo \
+	maxtherm.dtbo \
+	mbed-dac.dtbo \
+	mcp23017.dtbo \
+	mcp23s17.dtbo \
+	mcp2515-can0.dtbo \
+	mcp2515-can1.dtbo \
+	mcp3008.dtbo \
+	mcp3202.dtbo \
+	mcp342x.dtbo \
+	media-center.dtbo \
+	merus-amp.dtbo \
+	midi-uart0.dtbo \
+	midi-uart1.dtbo \
+	miniuart-bt.dtbo \
+	mmc.dtbo \
+	mpu6050.dtbo \
+	mz61581.dtbo \
+	ov5647.dtbo \
+	ov7251.dtbo \
+	ov9281.dtbo \
+	papirus.dtbo \
+	pca953x.dtbo \
+	pibell.dtbo \
+	pifacedigital.dtbo \
+	piglow.dtbo \
+	piscreen.dtbo \
+	piscreen2r.dtbo \
+	pisound.dtbo \
+	pitft22.dtbo \
+	pitft28-capacitive.dtbo \
+	pitft28-resistive.dtbo \
+	pitft35-resistive.dtbo \
+	pps-gpio.dtbo \
+	pwm.dtbo \
+	pwm-2chan.dtbo \
+	pwm-ir-tx.dtbo \
+	qca7000.dtbo \
+	rotary-encoder.dtbo \
+	rpi-backlight.dtbo \
+	rpi-cirrus-wm5102.dtbo \
+	rpi-dac.dtbo \
+	rpi-display.dtbo \
+	rpi-ft5406.dtbo \
+	rpi-poe.dtbo \
+	rpi-proto.dtbo \
+	rpi-sense.dtbo \
+	rpi-tv.dtbo \
+	rpivid-v4l2.dtbo \
+	rra-digidac1-wm8741-audio.dtbo \
+	sainsmart18.dtbo \
+	sc16is750-i2c.dtbo \
+	sc16is752-i2c.dtbo \
+	sc16is752-spi0.dtbo \
+	sc16is752-spi1.dtbo \
+	sdhost.dtbo \
+	sdio.dtbo \
+	sdtweak.dtbo \
+	sh1106-spi.dtbo \
+	smi.dtbo \
+	smi-dev.dtbo \
+	smi-nand.dtbo \
+	spi-gpio35-39.dtbo \
+	spi-gpio40-45.dtbo \
+	spi-rtc.dtbo \
+	spi0-1cs.dtbo \
+	spi0-2cs.dtbo \
+	spi1-1cs.dtbo \
+	spi1-2cs.dtbo \
+	spi1-3cs.dtbo \
+	spi2-1cs.dtbo \
+	spi2-2cs.dtbo \
+	spi2-3cs.dtbo \
+	spi3-1cs.dtbo \
+	spi3-2cs.dtbo \
+	spi4-1cs.dtbo \
+	spi4-2cs.dtbo \
+	spi5-1cs.dtbo \
+	spi5-2cs.dtbo \
+	spi6-1cs.dtbo \
+	spi6-2cs.dtbo \
+	ssd1306.dtbo \
+	ssd1306-spi.dtbo \
+	ssd1351-spi.dtbo \
+	superaudioboard.dtbo \
+	sx150x.dtbo \
+	tc358743.dtbo \
+	tc358743-audio.dtbo \
+	tinylcd35.dtbo \
+	tpm-slb9670.dtbo \
+	uart0.dtbo \
+	uart1.dtbo \
+	uart2.dtbo \
+	uart3.dtbo \
+	uart4.dtbo \
+	uart5.dtbo \
+	udrc.dtbo \
+	upstream.dtbo \
+	upstream-pi4.dtbo \
+	vc4-fkms-v3d.dtbo \
+	vc4-kms-kippah-7inch.dtbo \
+	vc4-kms-v3d.dtbo \
+	vc4-kms-v3d-pi4.dtbo \
+	vga666.dtbo \
+	w1-gpio.dtbo \
+	w1-gpio-pullup.dtbo \
+	w5500.dtbo \
+	wittypi.dtbo
+
+targets += dtbs dtbs_install
+targets += $(dtbo-y)
+
+always-y	:= $(dtbo-y)
+clean-files	:= *.dtbo
diff --git a/arch/arm/boot/dts/overlays/README b/arch/arm/boot/dts/overlays/README
new file mode 100644
index 000000000000..eff90baed406
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/README
@@ -0,0 +1,3040 @@
+Introduction
+============
+
+This directory contains Device Tree overlays. Device Tree makes it possible
+to support many hardware configurations with a single kernel and without the
+need to explicitly load or blacklist kernel modules. Note that this isn't a
+"pure" Device Tree configuration (c.f. MACH_BCM2835) - some on-board devices
+are still configured by the board support code, but the intention is to
+eventually reach that goal.
+
+On Raspberry Pi, Device Tree usage is controlled from /boot/config.txt. By
+default, the Raspberry Pi kernel boots with device tree enabled. You can
+completely disable DT usage (for now) by adding:
+
+    device_tree=
+
+to your config.txt, which should cause your Pi to revert to the old way of
+doing things after a reboot.
+
+In /boot you will find a .dtb for each base platform. This describes the
+hardware that is part of the Raspberry Pi board. The loader (start.elf and its
+siblings) selects the .dtb file appropriate for the platform by name, and reads
+it into memory. At this point, all of the optional interfaces (i2c, i2s, spi)
+are disabled, but they can be enabled using Device Tree parameters:
+
+    dtparam=i2c=on,i2s=on,spi=on
+
+However, this shouldn't be necessary in many use cases because loading an
+overlay that requires one of those interfaces will cause it to be enabled
+automatically, and it is advisable to only enable interfaces if they are
+needed.
+
+Configuring additional, optional hardware is done using Device Tree overlays
+(see below).
+
+GPIO numbering uses the hardware pin numbering scheme (aka BCM scheme) and
+not the physical pin numbers.
+
+raspi-config
+============
+
+The Advanced Options section of the raspi-config utility can enable and disable
+Device Tree use, as well as toggling the I2C and SPI interfaces. Note that it
+is possible to both enable an interface and blacklist the driver, if for some
+reason you should want to defer the loading.
+
+Modules
+=======
+
+As well as describing the hardware, Device Tree also gives enough information
+to allow suitable driver modules to be located and loaded, with the corollary
+that unneeded modules are not loaded. As a result it should be possible to
+remove lines from /etc/modules, and /etc/modprobe.d/raspi-blacklist.conf can
+have its contents deleted (or commented out).
+
+Using Overlays
+==============
+
+Overlays are loaded using the "dtoverlay" config.txt setting. As an example,
+consider I2C Real Time Clock drivers. In the pre-DT world these would be loaded
+by writing a magic string comprising a device identifier and an I2C address to
+a special file in /sys/class/i2c-adapter, having first loaded the driver for
+the I2C interface and the RTC device - something like this:
+
+    modprobe i2c-bcm2835
+    modprobe rtc-ds1307
+    echo ds1307 0x68 > /sys/class/i2c-adapter/i2c-1/new_device
+
+With DT enabled, this becomes a line in config.txt:
+
+    dtoverlay=i2c-rtc,ds1307
+
+This causes the file /boot/overlays/i2c-rtc.dtbo to be loaded and a "node"
+describing the DS1307 I2C device to be added to the Device Tree for the Pi. By
+default it usees address 0x68, but this can be modified with an additional DT
+parameter:
+
+    dtoverlay=i2c-rtc,ds1307,addr=0x68
+
+Parameters usually have default values, although certain parameters are
+mandatory. See the list of overlays below for a description of the parameters
+and their defaults.
+
+The Overlay and Parameter Reference
+===================================
+
+N.B. When editing this file, please preserve the indentation levels to make it
+simple to parse programmatically. NO HARD TABS.
+
+
+Name:   <The base DTB>
+Info:   Configures the base Raspberry Pi hardware
+Load:   <loaded automatically>
+Params:
+        ant1                    Select antenna 1 (default). CM4 only.
+
+        ant2                    Select antenna 2. CM4 only.
+
+        noant                   Disable both antennas. CM4 only.
+
+        audio                   Set to "on" to enable the onboard ALSA audio
+                                interface (default "off")
+
+        axiperf                 Set to "on" to enable the AXI bus performance
+                                monitors.
+                                See /sys/kernel/debug/raspberrypi_axi_monitor
+                                for the results.
+
+        eee                     Enable Energy Efficient Ethernet support for
+                                compatible devices (default "on"). See also
+                                "tx_lpi_timer". Pi3B+ only.
+
+        eth_downshift_after     Set the number of auto-negotiation failures
+                                after which the 1000Mbps modes are disabled.
+                                Legal values are 2, 3, 4, 5 and 0, where
+                                0 means never downshift (default 2). Pi3B+ only.
+
+        eth_led0                Set mode of LED0 - amber on Pi3B+ (default "1"),
+                                green on Pi4 (default "0").
+                                The legal values are:
+
+                                Pi3B+
+
+                                0=link/activity          1=link1000/activity
+                                2=link100/activity       3=link10/activity
+                                4=link100/1000/activity  5=link10/1000/activity
+                                6=link10/100/activity    14=off    15=on
+
+                                Pi4
+
+                                0=Speed/Activity         1=Speed
+                                2=Flash activity         3=FDX
+                                4=Off                    5=On
+                                6=Alt                    7=Speed/Flash
+                                8=Link                   9=Activity
+
+        eth_led1                Set mode of LED1 - green on Pi3B+ (default "6"),
+                                amber on Pi4 (default "8"). See eth_led0 for
+                                legal values.
+
+        eth_max_speed           Set the maximum speed a link is allowed
+                                to negotiate. Legal values are 10, 100 and
+                                1000 (default 1000). Pi3B+ only.
+
+        i2c_arm                 Set to "on" to enable the ARM's i2c interface
+                                (default "off")
+
+        i2c_vc                  Set to "on" to enable the i2c interface
+                                usually reserved for the VideoCore processor
+                                (default "off")
+
+        i2c                     An alias for i2c_arm
+
+        i2c_arm_baudrate        Set the baudrate of the ARM's i2c interface
+                                (default "100000")
+
+        i2c_vc_baudrate         Set the baudrate of the VideoCore i2c interface
+                                (default "100000")
+
+        i2c_baudrate            An alias for i2c_arm_baudrate
+
+        i2s                     Set to "on" to enable the i2s interface
+                                (default "off")
+
+        krnbt                   Set to "on" to enable autoprobing of Bluetooth
+                                driver without need of hciattach/btattach
+                                (default "off")
+
+        krnbt_baudrate          Set the baudrate of the PL011 UART when used
+                                with krnbt=on
+
+        spi                     Set to "on" to enable the spi interfaces
+                                (default "off")
+
+        spi_dma4                Use to enable 40-bit DMA on spi interfaces
+                                (the assigned value doesn't matter)
+                                (2711 only)
+
+        random                  Set to "on" to enable the hardware random
+                                number generator (default "on")
+
+        sd_overclock            Clock (in MHz) to use when the MMC framework
+                                requests 50MHz
+
+        sd_poll_once            Looks for a card once after booting. Useful
+                                for network booting scenarios to avoid the
+                                overhead of continuous polling. N.B. Using
+                                this option restricts the system to using a
+                                single card per boot (or none at all).
+                                (default off)
+
+        sd_force_pio            Disable DMA support for SD driver (default off)
+
+        sd_pio_limit            Number of blocks above which to use DMA for
+                                SD card (default 1)
+
+        sd_debug                Enable debug output from SD driver (default off)
+
+        sdio_overclock          Clock (in MHz) to use when the MMC framework
+                                requests 50MHz for the SDIO/WiFi interface.
+
+        tx_lpi_timer            Set the delay in microseconds between going idle
+                                and entering the low power state (default 600).
+                                Requires EEE to be enabled - see "eee".
+
+        uart0                   Set to "off" to disable uart0 (default "on")
+
+        uart1                   Set to "on" or "off" to enable or disable uart1
+                                (default varies)
+
+        watchdog                Set to "on" to enable the hardware watchdog
+                                (default "off")
+
+        act_led_trigger         Choose which activity the LED tracks.
+                                Use "heartbeat" for a nice load indicator.
+                                (default "mmc")
+
+        act_led_activelow       Set to "on" to invert the sense of the LED
+                                (default "off")
+                                N.B. For Pi 3B, 3B+, 3A+ and 4B, use the act-led
+                                overlay.
+
+        act_led_gpio            Set which GPIO to use for the activity LED
+                                (in case you want to connect it to an external
+                                device)
+                                (default "16" on a non-Plus board, "47" on a
+                                Plus or Pi 2)
+                                N.B. For Pi 3B, 3B+, 3A+ and 4B, use the act-led
+                                overlay.
+
+        pwr_led_trigger
+        pwr_led_activelow
+        pwr_led_gpio
+                                As for act_led_*, but using the PWR LED.
+                                Not available on Model A/B boards.
+
+        N.B. It is recommended to only enable those interfaces that are needed.
+        Leaving all interfaces enabled can lead to unwanted behaviour (i2c_vc
+        interfering with Pi Camera, I2S and SPI hogging GPIO pins, etc.)
+        Note also that i2c, i2c_arm and i2c_vc are aliases for the physical
+        interfaces i2c0 and i2c1. Use of the numeric variants is still possible
+        but deprecated because the ARM/VC assignments differ between board
+        revisions. The same board-specific mapping applies to i2c_baudrate,
+        and the other i2c baudrate parameters.
+
+
+Name:   act-led
+Info:   Pi 3B, 3B+, 3A+ and 4B use a GPIO expander to drive the LEDs which can
+        only be accessed from the VPU. There is a special driver for this with a
+        separate DT node, which has the unfortunate consequence of breaking the
+        act_led_gpio and act_led_activelow dtparams.
+        This overlay changes the GPIO controller back to the standard one and
+        restores the dtparams.
+Load:   dtoverlay=act-led,<param>=<val>
+Params: activelow               Set to "on" to invert the sense of the LED
+                                (default "off")
+
+        gpio                    Set which GPIO to use for the activity LED
+                                (in case you want to connect it to an external
+                                device)
+                                REQUIRED
+
+
+Name:   adafruit18
+Info:   Overlay for the SPI-connected Adafruit 1.8" display (based on the
+        ST7735R chip). It includes support for the "green tab" version.
+Load:   dtoverlay=adafruit18,<param>=<val>
+Params: green                   Use the adafruit18_green variant.
+        rotate                  Display rotation {0,90,180,270}
+        speed                   SPI bus speed in Hz (default 4000000)
+        fps                     Display frame rate in Hz
+        bgr                     Enable BGR mode (default off)
+        debug                   Debug output level {0-7}
+        dc_pin                  GPIO pin for D/C (default 24)
+        reset_pin               GPIO pin for RESET (default 25)
+        led_pin                 GPIO used to control backlight (default 18)
+
+
+Name:   adau1977-adc
+Info:   Overlay for activation of ADAU1977 ADC codec over I2C for control
+        and I2S for data.
+Load:   dtoverlay=adau1977-adc
+Params: <None>
+
+
+Name:   adau7002-simple
+Info:   Overlay for the activation of ADAU7002 stereo PDM to I2S converter.
+Load:   dtoverlay=adau7002-simple,<param>=<val>
+Params: card-name               Override the default, "adau7002", card name.
+
+
+Name:   ads1015
+Info:   Overlay for activation of Texas Instruments ADS1015 ADC over I2C
+Load:   dtoverlay=ads1015,<param>=<val>
+Params: addr                    I2C bus address of device. Set based on how the
+                                addr pin is wired. (default=0x48 assumes addr
+                                is pulled to GND)
+        cha_enable              Enable virtual channel a. (default=true)
+        cha_cfg                 Set the configuration for virtual channel a.
+                                (default=4 configures this channel for the
+                                voltage at A0 with respect to GND)
+        cha_datarate            Set the datarate (samples/sec) for this channel.
+                                (default=4 sets 1600 sps)
+        cha_gain                Set the gain of the Programmable Gain
+                                Amplifier for this channel. (default=2 sets the
+                                full scale of the channel to 2.048 Volts)
+
+        Channel (ch) parameters can be set for each enabled channel.
+        A maximum of 4 channels can be enabled (letters a thru d).
+        For more information refer to the device datasheet at:
+        http://www.ti.com/lit/ds/symlink/ads1015.pdf
+
+
+Name:   ads1115
+Info:   Texas Instruments ADS1115 ADC
+Load:   dtoverlay=ads1115,<param>[=<val>]
+Params: addr                    I2C bus address of device. Set based on how the
+                                addr pin is wired. (default=0x48 assumes addr
+                                is pulled to GND)
+        cha_enable              Enable virtual channel a.
+        cha_cfg                 Set the configuration for virtual channel a.
+                                (default=4 configures this channel for the
+                                voltage at A0 with respect to GND)
+        cha_datarate            Set the datarate (samples/sec) for this channel.
+                                (default=7 sets 860 sps)
+        cha_gain                Set the gain of the Programmable Gain
+                                Amplifier for this channel. (Default 1 sets the
+                                full scale of the channel to 4.096 Volts)
+
+        Channel parameters can be set for each enabled channel.
+        A maximum of 4 channels can be enabled (letters a thru d).
+        For more information refer to the device datasheet at:
+        http://www.ti.com/lit/ds/symlink/ads1115.pdf
+
+
+Name:   ads7846
+Info:   ADS7846 Touch controller
+Load:   dtoverlay=ads7846,<param>=<val>
+Params: cs                      SPI bus Chip Select (default 1)
+        speed                   SPI bus speed (default 2MHz, max 3.25MHz)
+        penirq                  GPIO used for PENIRQ. REQUIRED
+        penirq_pull             Set GPIO pull (default 0=none, 2=pullup)
+        swapxy                  Swap x and y axis
+        xmin                    Minimum value on the X axis (default 0)
+        ymin                    Minimum value on the Y axis (default 0)
+        xmax                    Maximum value on the X axis (default 4095)
+        ymax                    Maximum value on the Y axis (default 4095)
+        pmin                    Minimum reported pressure value (default 0)
+        pmax                    Maximum reported pressure value (default 65535)
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+                                (default 400)
+
+        penirq is required and usually xohms (60-100) has to be set as well.
+        Apart from that, pmax (255) and swapxy are also common.
+        The rest of the calibration can be done with xinput-calibrator.
+        See: github.com/notro/fbtft/wiki/FBTFT-on-Raspian
+        Device Tree binding document:
+        www.kernel.org/doc/Documentation/devicetree/bindings/input/ads7846.txt
+
+
+Name:   adv7282m
+Info:   Analog Devices ADV7282M analogue video to CSI2 bridge.
+        Uses Unicam1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=adv7282m,<param>=<val>
+Params: addr                    Overrides the I2C address (default 0x21)
+
+
+Name:   adv728x-m
+Info:   Analog Devices ADV728[0|1|2]-M analogue video to CSI2 bridges.
+        This is a wrapper for adv7282m, and defaults to ADV7282M.
+Load:   dtoverlay=adv728x-m,<param>=<val>
+Params: addr                    Overrides the I2C address (default 0x21)
+        adv7280m                Select ADV7280-M.
+        adv7281m                Select ADV7281-M.
+        adv7281ma               Select ADV7281-MA.
+
+
+Name:   akkordion-iqdacplus
+Info:   Configures the Digital Dreamtime Akkordion Music Player (based on the
+        OEM IQAudIO DAC+ or DAC Zero module).
+Load:   dtoverlay=akkordion-iqdacplus,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                dtoverlay=akkordion-iqdacplus,24db_digital_gain
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
+Name:   allo-boss-dac-pcm512x-audio
+Info:   Configures the Allo Boss DAC audio cards.
+Load:   dtoverlay=allo-boss-dac-pcm512x-audio,<param>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=allo-boss-dac-pcm512x-audio,
+                                24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+        slave                   Force Boss DAC into slave mode, using Pi a
+                                master for bit clock and frame clock. Enable
+                                with "dtoverlay=allo-boss-dac-pcm512x-audio,
+                                slave"
+
+
+Name:   allo-digione
+Info:   Configures the Allo Digione audio card
+Load:   dtoverlay=allo-digione
+Params: <None>
+
+
+Name:   allo-katana-dac-audio
+Info:   Configures the Allo Katana DAC audio card
+Load:   dtoverlay=allo-katana-dac-audio
+Params: <None>
+
+
+Name:   allo-piano-dac-pcm512x-audio
+Info:   Configures the Allo Piano DAC (2.0/2.1) audio cards.
+        (NB. This initial support is for 2.0 channel audio ONLY! ie. stereo.
+        The subwoofer outputs on the Piano 2.1 are not currently supported!)
+Load:   dtoverlay=allo-piano-dac-pcm512x-audio,<param>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control.
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
+Name:   allo-piano-dac-plus-pcm512x-audio
+Info:   Configures the Allo Piano DAC (2.1) audio cards.
+Load:   dtoverlay=allo-piano-dac-plus-pcm512x-audio,<param>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control.
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+        glb_mclk                This option is only with Kali board. If enabled,
+                                MCLK for Kali is used and PLL is disabled for
+                                better voice quality. (default Off)
+
+
+Name:   anyspi
+Info:   Universal device tree overlay for SPI devices
+
+        Just specify the SPI address and device name ("compatible" property).
+        This overlay lacks any device-specific parameter support!
+
+        For devices on spi1 or spi2, the interfaces should be enabled
+        with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+
+        Examples:
+        1. SPI NOR flash on spi0.1, maximum SPI clock frequency 45MHz:
+            dtoverlay=anyspi:spi0-1,dev="jedec,spi-nor",speed=45000000
+        2. MCP3204 ADC on spi1.2, maximum SPI clock frequency 500kHz:
+            dtoverlay=anyspi:spi1-2,dev="microchip,mcp3204"
+Load:   dtoverlay=anyspi,<param>=<val>
+Params: spi<n>-<m>              Configure device at spi<n>, cs<m>
+                                (boolean, required)
+        dev                     Set device name to search compatible module
+                                (string, required)
+        speed                   Set SPI clock frequency in Hz
+                                (integer, optional, default 500000)
+
+
+Name:   apds9960
+Info:   Configures the AVAGO APDS9960 digital proximity, ambient light, RGB and
+        gesture sensor
+Load:   dtoverlay=apds9960,<param>=<val>
+Params: gpiopin                 GPIO used for INT (default 4)
+        noints                  Disable the interrupt GPIO line.
+
+
+Name:   applepi-dac
+Info:   Configures the Orchard Audio ApplePi-DAC audio card
+Load:   dtoverlay=applepi-dac
+Params: <None>
+
+
+Name:   at86rf233
+Info:   Configures the Atmel AT86RF233 802.15.4 low-power WPAN transceiver,
+        connected to spi0.0
+Load:   dtoverlay=at86rf233,<param>=<val>
+Params: interrupt               GPIO used for INT (default 23)
+        reset                   GPIO used for Reset (default 24)
+        sleep                   GPIO used for Sleep (default 25)
+        speed                   SPI bus speed in Hz (default 3000000)
+        trim                    Fine tuning of the internal capacitance
+                                arrays (0=+0pF, 15=+4.5pF, default 15)
+
+
+Name:   audioinjector-addons
+Info:   Configures the audioinjector.net audio add on soundcards
+Load:   dtoverlay=audioinjector-addons,<param>=<val>
+Params: non-stop-clocks         Keeps the clocks running even when the stream
+                                is paused or stopped (default off)
+
+
+Name:   audioinjector-isolated-soundcard
+Info:   Configures the audioinjector.net isolated soundcard
+Load:   dtoverlay=audioinjector-isolated-soundcard
+Params: <None>
+
+
+Name:   audioinjector-ultra
+Info:   Configures the audioinjector.net ultra soundcard
+Load:   dtoverlay=audioinjector-ultra
+Params: <None>
+
+
+Name:   audioinjector-wm8731-audio
+Info:   Configures the audioinjector.net audio add on soundcard
+Load:   dtoverlay=audioinjector-wm8731-audio
+Params: <None>
+
+
+Name:   audiosense-pi
+Info:   Configures the audiosense-pi add on soundcard
+        For more information refer to
+        https://gitlab.com/kakar0t/audiosense-pi
+Load:   dtoverlay=audiosense-pi
+Params: <None>
+
+
+Name:   audremap
+Info:   Switches PWM sound output to GPIOs on the 40-pin header
+Load:   dtoverlay=audremap,<param>=<val>
+Params: swap_lr                 Reverse the channel allocation, which will also
+                                swap the audio jack outputs (default off)
+        enable_jack             Don't switch off the audio jack output
+                                (default off)
+        pins_12_13              Select GPIOs 12 & 13 (default)
+        pins_18_19              Select GPIOs 18 & 19
+
+
+Name:   balena-fin
+Info:   Overlay that enables WiFi, Bluetooth and the GPIO expander on the
+        balenaFin carrier board for the Raspberry Pi Compute Module 3/3+ Lite.
+Load:   dtoverlay=balena-fin
+Params: <None>
+
+
+Name:   bmp085_i2c-sensor
+Info:   This overlay is now deprecated - see i2c-sensor
+Load:   <Deprecated>
+
+
+Name:   cma
+Info:   Set custom CMA sizes, only use if you know what you are doing, might
+        clash with other overlays like vc4-fkms-v3d and vc4-kms-v3d.
+Load:   dtoverlay=cma,<param>=<val>
+Params: cma-512                 CMA is 512MB (needs 1GB)
+        cma-448                 CMA is 448MB (needs 1GB)
+        cma-384                 CMA is 384MB (needs 1GB)
+        cma-320                 CMA is 320MB (needs 1GB)
+        cma-256                 CMA is 256MB (needs 1GB)
+        cma-192                 CMA is 192MB (needs 1GB)
+        cma-128                 CMA is 128MB
+        cma-96                  CMA is 96MB
+        cma-64                  CMA is 64MB
+        cma-size                CMA size in bytes, 4MB aligned
+        cma-default             Use upstream's default value
+
+
+Name:   dht11
+Info:   Overlay for the DHT11/DHT21/DHT22 humidity/temperature sensors
+        Also sometimes found with the part number(s) AM230x.
+Load:   dtoverlay=dht11,<param>=<val>
+Params: gpiopin                 GPIO connected to the sensor's DATA output.
+                                (default 4)
+
+
+Name:   dionaudio-loco
+Info:   Configures the Dion Audio LOCO DAC-AMP
+Load:   dtoverlay=dionaudio-loco
+Params: <None>
+
+
+Name:   dionaudio-loco-v2
+Info:   Configures the Dion Audio LOCO-V2 DAC-AMP
+Load:   dtoverlay=dionaudio-loco-v2,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=hifiberry-dacplus,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24dB_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
+Name:   disable-bt
+Info:   Disable onboard Bluetooth on Pi 3B, 3B+, 3A+, 4B and Zero W, restoring
+        UART0/ttyAMA0 over GPIOs 14 & 15.
+        N.B. To disable the systemd service that initialises the modem so it
+        doesn't use the UART, use 'sudo systemctl disable hciuart'.
+Load:   dtoverlay=disable-bt
+Params: <None>
+
+
+Name:   disable-wifi
+Info:   Disable onboard WiFi on Pi 3B, 3B+, 3A+, 4B and Zero W.
+Load:   dtoverlay=disable-wifi
+Params: <None>
+
+
+Name:   dpi18
+Info:   Overlay for a generic 18-bit DPI display
+        This uses GPIOs 0-21 (so no I2C, uart etc.), and activates the output
+        2-3 seconds after the kernel has started.
+Load:   dtoverlay=dpi18
+Params: <None>
+
+
+Name:   dpi24
+Info:   Overlay for a generic 24-bit DPI display
+        This uses GPIOs 0-27 (so no I2C, uart etc.), and activates the output
+        2-3 seconds after the kernel has started.
+Load:   dtoverlay=dpi24
+Params: <None>
+
+
+Name:   draws
+Info:   Configures the NW Digital Radio DRAWS Hat
+
+        The board includes an ADC to measure various board values and also
+        provides two analog user inputs on the expansion header.  The ADC
+        can be configured for various sample rates and gain values to adjust
+        the input range.  Tables describing the two parameters follow.
+
+        ADC Gain Values:
+            0 = +/- 6.144V
+            1 = +/- 4.096V
+            2 = +/- 2.048V
+            3 = +/- 1.024V
+            4 = +/- 0.512V
+            5 = +/- 0.256V
+            6 = +/- 0.256V
+            7 = +/- 0.256V
+
+        ADC Datarate Values:
+            0 = 128sps
+            1 = 250sps
+            2 = 490sps
+            3 = 920sps
+            4 = 1600sps (default)
+            5 = 2400sps
+            6 = 3300sps
+            7 = 3300sps
+Load:   dtoverlay=draws,<param>=<val>
+Params: draws_adc_ch4_gain      Sets the full scale resolution of the ADCs
+                                input voltage sensor (default 1)
+
+        draws_adc_ch4_datarate  Sets the datarate of the ADCs input voltage
+                                sensor
+
+        draws_adc_ch5_gain      Sets the full scale resolution of the ADCs
+                                5V rail voltage sensor (default 1)
+
+        draws_adc_ch5_datarate  Sets the datarate of the ADCs 4V rail voltage
+                                sensor
+
+        draws_adc_ch6_gain      Sets the full scale resolution of the ADCs
+                                AIN2 input (default 2)
+
+        draws_adc_ch6_datarate  Sets the datarate of the ADCs AIN2 input
+
+        draws_adc_ch7_gain      Sets the full scale resolution of the ADCs
+                                AIN3 input (default 2)
+
+        draws_adc_ch7_datarate  Sets the datarate of the ADCs AIN3 input
+
+        alsaname                Name of the ALSA audio device (default "draws")
+
+
+Name:   dwc-otg
+Info:   Selects the dwc_otg USB controller driver which has fiq support. This
+        is the default on all except the Pi Zero which defaults to dwc2.
+Load:   dtoverlay=dwc-otg
+Params: <None>
+
+
+Name:   dwc2
+Info:   Selects the dwc2 USB controller driver
+Load:   dtoverlay=dwc2,<param>=<val>
+Params: dr_mode                 Dual role mode: "host", "peripheral" or "otg"
+
+        g-rx-fifo-size          Size of rx fifo size in gadget mode
+
+        g-np-tx-fifo-size       Size of non-periodic tx fifo size in gadget
+                                mode
+
+
+[ The ds1307-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+Name:   enc28j60
+Info:   Overlay for the Microchip ENC28J60 Ethernet Controller on SPI0
+Load:   dtoverlay=enc28j60,<param>=<val>
+Params: int_pin                 GPIO used for INT (default 25)
+
+        speed                   SPI bus speed (default 12000000)
+
+
+Name:   enc28j60-spi2
+Info:   Overlay for the Microchip ENC28J60 Ethernet Controller on SPI2
+Load:   dtoverlay=enc28j60-spi2,<param>=<val>
+Params: int_pin                 GPIO used for INT (default 39)
+
+        speed                   SPI bus speed (default 12000000)
+
+
+Name:   exc3000
+Info:   Enables I2C connected EETI EXC3000 multiple touch controller using
+        GPIO 4 (pin 7 on GPIO header) for interrupt.
+Load:   dtoverlay=exc3000,<param>=<val>
+Params: interrupt               GPIO used for interrupt (default 4)
+        sizex                   Touchscreen size x (default 4096)
+        sizey                   Touchscreen size y (default 4096)
+        invx                    Touchscreen inverted x axis
+        invy                    Touchscreen inverted y axis
+        swapxy                  Touchscreen swapped x y axis
+
+
+Name:   fe-pi-audio
+Info:   Configures the Fe-Pi Audio Sound Card
+Load:   dtoverlay=fe-pi-audio
+Params: <None>
+
+
+Name:   fsm-demo
+Info:   A demonstration of the gpio-fsm driver. The GPIOs are chosen to work
+        nicely with a "traffic-light" display of red, amber and green LEDs on
+        GPIOs 7, 8 and 25 respectively.
+Load:   dtoverlay=fsm-demo,<param>=<val>
+Params: fsm_debug               Enable debug logging (default off)
+
+
+Name:   ghost-amp
+Info:   An overlay for the Ghost amplifier.
+Load:   dtoverlay=ghost-amp,<param>=<val>
+Params: fsm_debug               Enable debug logging of the GPIO FSM (default
+                                off)
+
+
+Name:   goodix
+Info:   Enables I2C connected Goodix gt9271 multiple touch controller using
+        GPIOs 4 and 17 (pins 7 and 11 on GPIO header) for interrupt and reset.
+Load:   dtoverlay=goodix,<param>=<val>
+Params: interrupt               GPIO used for interrupt (default 4)
+        reset                   GPIO used for reset (default 17)
+
+
+Name:   googlevoicehat-soundcard
+Info:   Configures the Google voiceHAT soundcard
+Load:   dtoverlay=googlevoicehat-soundcard
+Params: <None>
+
+
+Name:   gpio-fan
+Info:   Configure a GPIO pin to control a cooling fan.
+Load:   dtoverlay=gpio-fan,<param>=<val>
+Params: gpiopin                 GPIO used to control the fan (default 12)
+        temp                    Temperature at which the fan switches on, in
+                                millicelcius (default 55000)
+
+
+Name:   gpio-ir
+Info:   Use GPIO pin as rc-core style infrared receiver input. The rc-core-
+        based gpio_ir_recv driver maps received keys directly to a
+        /dev/input/event* device, all decoding is done by the kernel - LIRC is
+        not required! The key mapping and other decoding parameters can be
+        configured by "ir-keytable" tool.
+Load:   dtoverlay=gpio-ir,<param>=<val>
+Params: gpio_pin                Input pin number. Default is 18.
+
+        gpio_pull               Desired pull-up/down state (off, down, up)
+                                Default is "up".
+
+        invert                  "1" = invert the input (active-low signalling).
+                                "0" = non-inverted input (active-high
+                                signalling). Default is "1".
+
+        rc-map-name             Default rc keymap (can also be changed by
+                                ir-keytable), defaults to "rc-rc6-mce"
+
+
+Name:   gpio-ir-tx
+Info:   Use GPIO pin as bit-banged infrared transmitter output.
+        This is an alternative to "pwm-ir-tx". gpio-ir-tx doesn't require
+        a PWM so it can be used together with onboard analog audio.
+Load:   dtoverlay=gpio-ir-tx,<param>=<val>
+Params: gpio_pin                Output GPIO (default 18)
+
+        invert                  "1" = invert the output (make it active-low).
+                                Default is "0" (active-high).
+
+
+Name:   gpio-key
+Info:   This is a generic overlay for activating GPIO keypresses using
+        the gpio-keys library and this dtoverlay. Multiple keys can be
+        set up using multiple calls to the overlay for configuring
+        additional buttons or joysticks. You can see available keycodes
+        at https://github.com/torvalds/linux/blob/v4.12/include/uapi/
+        linux/input-event-codes.h#L64
+Load:   dtoverlay=gpio-key,<param>=<val>
+Params: gpio                    GPIO pin to trigger on (default 3)
+        active_low              When this is 1 (active low), a falling
+                                edge generates a key down event and a
+                                rising edge generates a key up event.
+                                When this is 0 (active high), this is
+                                reversed. The default is 1 (active low)
+        gpio_pull               Desired pull-up/down state (off, down, up)
+                                Default is "up". Note that the default pin
+                                (GPIO3) has an external pullup
+        label                   Set a label for the key
+        keycode                 Set the key code for the button
+
+
+Name:   gpio-no-bank0-irq
+Info:   Use this overlay to disable GPIO interrupts for GPIOs in bank 0 (0-27),
+        which can be useful for UIO drivers.
+        N.B. Using this overlay will trigger a kernel WARN during booting, but
+        this can safely be ignored - the system should work as expected.
+Load:   dtoverlay=gpio-no-bank0-irq
+Params: <None>
+
+
+Name:   gpio-no-irq
+Info:   Use this overlay to disable all GPIO interrupts, which can be useful
+        for user-space GPIO edge detection systems.
+Load:   dtoverlay=gpio-no-irq
+Params: <None>
+
+
+Name:   gpio-poweroff
+Info:   Drives a GPIO high or low on poweroff (including halt). Enabling this
+        overlay will prevent the ability to boot by driving GPIO3 low.
+Load:   dtoverlay=gpio-poweroff,<param>=<val>
+Params: gpiopin                 GPIO for signalling (default 26)
+
+        active_low              Set if the power control device requires a
+                                high->low transition to trigger a power-down.
+                                Note that this will require the support of a
+                                custom dt-blob.bin to prevent a power-down
+                                during the boot process, and that a reboot
+                                will also cause the pin to go low.
+        input                   Set if the gpio pin should be configured as
+                                an input.
+        export                  Set to export the configured pin to sysfs
+        timeout_ms              Specify (in ms) how long the kernel waits for
+                                power-down before issuing a WARN (default 3000).
+
+
+Name:   gpio-shutdown
+Info:   Initiates a shutdown when GPIO pin changes. The given GPIO pin
+        is configured as an input key that generates KEY_POWER events.
+
+        This event is handled by systemd-logind by initiating a
+        shutdown. Systemd versions older than 225 need an udev rule
+        enable listening to the input device:
+
+                ACTION!="REMOVE", SUBSYSTEM=="input", KERNEL=="event*", \
+                        SUBSYSTEMS=="platform", DRIVERS=="gpio-keys", \
+                        ATTRS{keys}=="116", TAG+="power-switch"
+
+        Alternatively this event can be handled also on systems without
+        systemd, just by traditional SysV init daemon. KEY_POWER event
+        (keycode 116) needs to be mapped to KeyboardSignal on console
+        and then kb::kbrequest inittab action which is triggered by
+        KeyboardSignal from console can be configured to issue system
+        shutdown. Steps for this configuration are:
+
+            Add following lines to the /etc/console-setup/remap.inc file:
+
+                # Key Power as special keypress
+                keycode 116 = KeyboardSignal
+
+            Then add following lines to /etc/inittab file:
+
+                # Action on special keypress (Key Power)
+                kb::kbrequest:/sbin/shutdown -t1 -a -h -P now
+
+            And finally reload configuration by calling following commands:
+
+                # dpkg-reconfigure console-setup
+                # service console-setup reload
+                # init q
+
+        This overlay only handles shutdown. After shutdown, the system
+        can be powered up again by driving GPIO3 low. The default
+        configuration uses GPIO3 with a pullup, so if you connect a
+        button between GPIO3 and GND (pin 5 and 6 on the 40-pin header),
+        you get a shutdown and power-up button. Please note that
+        Raspberry Pi 1 Model B rev 1 uses GPIO1 instead of GPIO3.
+Load:   dtoverlay=gpio-shutdown,<param>=<val>
+Params: gpio_pin                GPIO pin to trigger on (default 3)
+                                For Raspberry Pi 1 Model B rev 1 set this
+                                explicitly to value 1, e.g.:
+
+                                    dtoverlay=gpio-shutdown,gpio_pin=1
+
+        active_low              When this is 1 (active low), a falling
+                                edge generates a key down event and a
+                                rising edge generates a key up event.
+                                When this is 0 (active high), this is
+                                reversed. The default is 1 (active low).
+
+        gpio_pull               Desired pull-up/down state (off, down, up)
+                                Default is "up".
+
+                                Note that the default pin (GPIO3) has an
+                                external pullup. Same applies for GPIO1
+                                on Raspberry Pi 1 Model B rev 1.
+
+        debounce                Specify the debounce interval in milliseconds
+                                (default 100)
+
+
+Name:   hd44780-lcd
+Info:   Configures an HD44780 compatible LCD display. Uses 4 gpio pins for
+        data, 2 gpio pins for enable and register select and 1 optional pin
+        for enabling/disabling the backlight display.
+Load:   dtoverlay=hd44780-lcd,<param>=<val>
+Params: pin_d4                  GPIO pin for data pin D4 (default 6)
+
+        pin_d5                  GPIO pin for data pin D5 (default 13)
+
+        pin_d6                  GPIO pin for data pin D6 (default 19)
+
+        pin_d7                  GPIO pin for data pin D7 (default 26)
+
+        pin_en                  GPIO pin for "Enable" (default 21)
+
+        pin_rs                  GPIO pin for "Register Select" (default 20)
+
+        pin_bl                  Optional pin for enabling/disabling the
+                                display backlight. (default disabled)
+
+        display_height          Height of the display in characters
+
+        display_width           Width of the display in characters
+
+
+Name:   hdmi-backlight-hwhack-gpio
+Info:   Devicetree overlay for GPIO based backlight on/off capability.
+        Use this if you have one of those HDMI displays whose backlight cannot
+        be controlled via DPMS over HDMI and plan to do a little soldering to
+        use an RPi gpio pin for on/off switching. See:
+        https://www.waveshare.com/wiki/7inch_HDMI_LCD_(C)#Backlight_Control
+Load:   dtoverlay=hdmi-backlight-hwhack-gpio,<param>=<val>
+Params: gpio_pin                GPIO pin used (default 17)
+        active_low              Set this to 1 if the display backlight is
+                                switched on when the wire goes low.
+                                Leave the default (value 0) if the backlight
+                                expects a high to switch it on.
+
+
+Name:   hifiberry-amp
+Info:   Configures the HifiBerry Amp and Amp+ audio cards
+Load:   dtoverlay=hifiberry-amp
+Params: <None>
+
+
+Name:   hifiberry-dac
+Info:   Configures the HifiBerry DAC audio card
+Load:   dtoverlay=hifiberry-dac
+Params: <None>
+
+
+Name:   hifiberry-dacplus
+Info:   Configures the HifiBerry DAC+ audio card
+Load:   dtoverlay=hifiberry-dacplus,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=hifiberry-dacplus,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24dB_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+        slave                   Force DAC+ Pro into slave mode, using Pi as
+                                master for bit clock and frame clock.
+        leds_off                If set to 'true' the onboard indicator LEDs
+                                are switched off at all times.
+
+
+Name:   hifiberry-dacplusadc
+Info:   Configures the HifiBerry DAC+ADC audio card
+Load:   dtoverlay=hifiberry-dacplusadc,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=hifiberry-dacplus,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24dB_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+        slave                   Force DAC+ Pro into slave mode, using Pi as
+                                master for bit clock and frame clock.
+        leds_off                If set to 'true' the onboard indicator LEDs
+                                are switched off at all times.
+
+
+Name:   hifiberry-dacplusadcpro
+Info:   Configures the HifiBerry DAC+ADC PRO audio card
+Load:   dtoverlay=hifiberry-dacplusadcpro,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=hifiberry-dacplusadcpro,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24dB_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+        slave                   Force DAC+ADC Pro into slave mode, using Pi as
+                                master for bit clock and frame clock.
+        leds_off                If set to 'true' the onboard indicator LEDs
+                                are switched off at all times.
+
+
+Name:   hifiberry-dacplusdsp
+Info:   Configures the HifiBerry DAC+DSP audio card
+Load:   dtoverlay=hifiberry-dacplusdsp
+Params: <None>
+
+
+Name:   hifiberry-dacplushd
+Info:   Configures the HifiBerry DAC+ HD audio card
+Load:   dtoverlay=hifiberry-dacplushd
+Params: <None>
+
+
+Name:   hifiberry-digi
+Info:   Configures the HifiBerry Digi and Digi+ audio card
+Load:   dtoverlay=hifiberry-digi
+Params: <None>
+
+
+Name:   hifiberry-digi-pro
+Info:   Configures the HifiBerry Digi+ Pro audio card
+Load:   dtoverlay=hifiberry-digi-pro
+Params: <None>
+
+
+Name:   highperi
+Info:   Enables "High Peripheral" mode
+Load:   dtoverlay=highperi
+Params: <None>
+
+
+Name:   hy28a
+Info:   HY28A - 2.8" TFT LCD Display Module by HAOYU Electronics
+        Default values match Texy's display shield
+Load:   dtoverlay=hy28a,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+
+        resetgpio               GPIO used to reset controller
+
+        ledgpio                 GPIO used to control backlight
+
+
+Name:   hy28b
+Info:   HY28B - 2.8" TFT LCD Display Module by HAOYU Electronics
+        Default values match Texy's display shield
+Load:   dtoverlay=hy28b,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+
+        resetgpio               GPIO used to reset controller
+
+        ledgpio                 GPIO used to control backlight
+
+
+Name:   hy28b-2017
+Info:   HY28B 2017 version - 2.8" TFT LCD Display Module by HAOYU Electronics
+        Default values match Texy's display shield
+Load:   dtoverlay=hy28b-2017,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+
+        resetgpio               GPIO used to reset controller
+
+        ledgpio                 GPIO used to control backlight
+
+
+Name:   i-sabre-q2m
+Info:   Configures the Audiophonics I-SABRE Q2M DAC
+Load:   dtoverlay=i-sabre-q2m
+Params: <None>
+
+
+Name:   i2c-bcm2708
+Info:   Fall back to the i2c_bcm2708 driver for the i2c_arm bus.
+Load:   dtoverlay=i2c-bcm2708
+Params: <None>
+
+
+Name:   i2c-gpio
+Info:   Adds support for software i2c controller on gpio pins
+Load:   dtoverlay=i2c-gpio,<param>=<val>
+Params: i2c_gpio_sda            GPIO used for I2C data (default "23")
+
+        i2c_gpio_scl            GPIO used for I2C clock (default "24")
+
+        i2c_gpio_delay_us       Clock delay in microseconds
+                                (default "2" = ~100kHz)
+
+        bus                     Set to a unique, non-zero value if wanting
+                                multiple i2c-gpio busses. If set, will be used
+                                as the preferred bus number (/dev/i2c-<n>). If
+                                not set, the default value is 0, but the bus
+                                number will be dynamically assigned - probably
+                                3.
+
+
+Name:   i2c-mux
+Info:   Adds support for a number of I2C bus multiplexers on i2c_arm
+Load:   dtoverlay=i2c-mux,<param>=<val>
+Params: pca9542                 Select the NXP PCA9542 device
+
+        pca9545                 Select the NXP PCA9545 device
+
+        pca9548                 Select the NXP PCA9548 device
+
+        addr                    Change I2C address of the device (default 0x70)
+
+
+[ The i2c-mux-pca9548a overlay has been deleted. See i2c-mux. ]
+
+
+Name:   i2c-pwm-pca9685a
+Info:   Adds support for an NXP PCA9685A I2C PWM controller on i2c_arm
+Load:   dtoverlay=i2c-pwm-pca9685a,<param>=<val>
+Params: addr                    I2C address of PCA9685A (default 0x40)
+
+
+Name:   i2c-rtc
+Info:   Adds support for a number of I2C Real Time Clock devices
+Load:   dtoverlay=i2c-rtc,<param>=<val>
+Params: abx80x                  Select one of the ABx80x family:
+                                  AB0801, AB0803, AB0804, AB0805,
+                                  AB1801, AB1803, AB1804, AB1805
+
+        ds1307                  Select the DS1307 device
+
+        ds1339                  Select the DS1339 device
+
+        ds3231                  Select the DS3231 device
+
+        m41t62                  Select the M41T62 device
+
+        mcp7940x                Select the MCP7940x device
+
+        mcp7941x                Select the MCP7941x device
+
+        pcf2127                 Select the PCF2127 device
+
+        pcf2129                 Select the PCF2129 device
+
+        pcf8523                 Select the PCF8523 device
+
+        pcf85363                Select the PCF85363 device
+
+        pcf8563                 Select the PCF8563 device
+
+        rv1805                  Select the Micro Crystal RV1805 device
+
+        rv3028                  Select the Micro Crystal RV3028 device
+
+        sd3078                  Select the ZXW Shenzhen whwave SD3078 device
+
+        addr                    Sets the address for the RTC. Note that the
+                                device must be configured to use the specified
+                                address.
+
+        trickle-diode-type      Diode type for trickle charge - "standard" or
+                                "schottky" (ABx80x and RV1805 only)
+
+        trickle-resistor-ohms   Resistor value for trickle charge (DS1339,
+                                ABx80x, RV1805, RV3028)
+
+        wakeup-source           Specify that the RTC can be used as a wakeup
+                                source
+
+        backup-switchover-mode  Backup power supply switch mode. Must be 0 for
+                                off or 1 for Vdd < VBackup (RV3028 only)
+
+
+Name:   i2c-rtc-gpio
+Info:   Adds support for a number of I2C Real Time Clock devices
+        using the software i2c controller
+Load:   dtoverlay=i2c-rtc-gpio,<param>=<val>
+Params: abx80x                  Select one of the ABx80x family:
+                                  AB0801, AB0803, AB0804, AB0805,
+                                  AB1801, AB1803, AB1804, AB1805
+
+        ds1307                  Select the DS1307 device
+
+        ds1339                  Select the DS1339 device
+
+        ds3231                  Select the DS3231 device
+
+        m41t62                  Select the M41T62 device
+
+        mcp7940x                Select the MCP7940x device
+
+        mcp7941x                Select the MCP7941x device
+
+        pcf2127                 Select the PCF2127 device
+
+        pcf2129                 Select the PCF2129 device
+
+        pcf8523                 Select the PCF8523 device
+
+        pcf8563                 Select the PCF8563 device
+
+        rv1805                  Select the Micro Crystal RV1805 device
+
+        rv3028                  Select the Micro Crystal RV3028 device
+
+        addr                    Sets the address for the RTC. Note that the
+                                device must be configured to use the specified
+                                address.
+
+        trickle-diode-type      Diode type for trickle charge - "standard" or
+                                "schottky" (ABx80x and RV1805 only)
+
+        trickle-resistor-ohms   Resistor value for trickle charge (DS1339,
+                                ABx80x, RV1805, RV3028)
+
+        wakeup-source           Specify that the RTC can be used as a wakeup
+                                source
+
+        backup-switchover-mode  Backup power supply switch mode. Must be 0 for
+                                off or 1 for Vdd < VBackup (RV3028 only)
+
+        i2c_gpio_sda            GPIO used for I2C data (default "23")
+
+        i2c_gpio_scl            GPIO used for I2C clock (default "24")
+
+        i2c_gpio_delay_us       Clock delay in microseconds
+                                (default "2" = ~100kHz)
+
+
+Name:   i2c-sensor
+Info:   Adds support for a number of I2C barometric pressure and temperature
+        sensors on i2c_arm
+Load:   dtoverlay=i2c-sensor,<param>=<val>
+Params: addr                    Set the address for the BME280, BME680, BMP280,
+                                DS1621, HDC100X, LM75, SHT3x or TMP102
+
+        bme280                  Select the Bosch Sensortronic BME280
+                                Valid addresses 0x76-0x77, default 0x76
+
+        bme680                  Select the Bosch Sensortronic BME680
+                                Valid addresses 0x76-0x77, default 0x76
+
+        bmp085                  Select the Bosch Sensortronic BMP085
+
+        bmp180                  Select the Bosch Sensortronic BMP180
+
+        bmp280                  Select the Bosch Sensortronic BMP280
+                                Valid addresses 0x76-0x77, default 0x76
+
+        ds1621                  Select the Dallas Semiconductors DS1621 temp
+                                sensor. Valid addresses 0x48-0x4f, default 0x48
+
+        hdc100x                 Select the Texas Instruments HDC100x temp sensor
+                                Valid addresses 0x40-0x43, default 0x40
+
+        htu21                   Select the HTU21 temperature and humidity sensor
+
+        lm75                    Select the Maxim LM75 temperature sensor
+                                Valid addresses 0x48-0x4f, default 0x4f
+
+        lm75addr                Deprecated - use addr parameter instead
+
+        max17040                Select the Maxim Integrated MAX17040 battery
+                                monitor
+
+        sht3x                   Select the Sensiron SHT3x temperature and
+                                humidity sensor. Valid addresses 0x44-0x45,
+                                default 0x44
+
+        si7020                  Select the Silicon Labs Si7013/20/21 humidity/
+                                temperature sensor
+
+        sps30                   Select the Sensirion SPS30 particulate matter
+                                sensor. Fixed address 0x69.
+
+        tmp102                  Select the Texas Instruments TMP102 temp sensor
+                                Valid addresses 0x48-0x4b, default 0x48
+
+        tsl4531                 Select the AMS TSL4531 digital ambient light
+                                sensor
+
+        veml6070                Select the Vishay VEML6070 ultraviolet light
+                                sensor
+
+
+Name:   i2c0
+Info:   Change i2c0 pin usage. Not all pin combinations are usable on all
+        platforms - platforms other then Compute Modules can only use this
+        to disable transaction combining.
+        Do NOT use in conjunction with dtparam=i2c_vc=on. From the 5.4 kernel
+        onwards the base DT includes the use of i2c_mux_pinctrl to expose two
+        muxings of BSC0 - GPIOs 0&1, and whichever combination is used for the
+        camera and display connectors. This overlay disables that mux and
+        configures /dev/i2c0 to point at whichever set of pins is requested.
+        dtparam=i2c_vc=on will try and enable the mux, so combining the two
+        will cause conflicts.
+Load:   dtoverlay=i2c0,<param>=<val>
+Params: pins_0_1                Use pins 0 and 1 (default)
+        pins_28_29              Use pins 28 and 29
+        pins_44_45              Use pins 44 and 45
+        pins_46_47              Use pins 46 and 47
+        combine                 Allow transactions to be combined (default
+                                "yes")
+
+
+Name:   i2c0-bcm2708
+Info:   Deprecated, legacy version of i2c0.
+Load:   <Deprecated>
+
+
+Name:   i2c1
+Info:   Change i2c1 pin usage. Not all pin combinations are usable on all
+        platforms - platforms other then Compute Modules can only use this
+        to disable transaction combining.
+Load:   dtoverlay=i2c1,<param>=<val>
+Params: pins_2_3                Use pins 2 and 3 (default)
+        pins_44_45              Use pins 44 and 45
+        combine                 Allow transactions to be combined (default
+                                "yes")
+
+
+Name:   i2c1-bcm2708
+Info:   Deprecated, legacy version of i2c1.
+Load:   <Deprecated>
+
+
+Name:   i2c3
+Info:   Enable the i2c3 bus. BCM2711 only.
+Load:   dtoverlay=i2c3,<param>
+Params: pins_2_3                Use GPIOs 2 and 3
+        pins_4_5                Use GPIOs 4 and 5 (default)
+        baudrate                Set the baudrate for the interface (default
+                                "100000")
+
+
+Name:   i2c4
+Info:   Enable the i2c4 bus. BCM2711 only.
+Load:   dtoverlay=i2c4,<param>
+Params: pins_6_7                Use GPIOs 6 and 7
+        pins_8_9                Use GPIOs 8 and 9 (default)
+        baudrate                Set the baudrate for the interface (default
+                                "100000")
+
+
+Name:   i2c5
+Info:   Enable the i2c5 bus. BCM2711 only.
+Load:   dtoverlay=i2c5,<param>
+Params: pins_10_11              Use GPIOs 10 and 11
+        pins_12_13              Use GPIOs 12 and 13 (default)
+        baudrate                Set the baudrate for the interface (default
+                                "100000")
+
+
+Name:   i2c6
+Info:   Enable the i2c6 bus. BCM2711 only.
+Load:   dtoverlay=i2c6,<param>
+Params: pins_0_1                Use GPIOs 0 and 1
+        pins_22_23              Use GPIOs 22 and 23 (default)
+        baudrate                Set the baudrate for the interface (default
+                                "100000")
+
+
+Name:   i2s-gpio28-31
+Info:   move I2S function block to GPIO 28 to 31
+Load:   dtoverlay=i2s-gpio28-31
+Params: <None>
+
+
+Name:   ilitek251x
+Info:   Enables I2C connected Ilitek 251x multiple touch controller using
+        GPIO 4 (pin 7 on GPIO header) for interrupt.
+Load:   dtoverlay=ilitek251x,<param>=<val>
+Params: interrupt               GPIO used for interrupt (default 4)
+        sizex                   Touchscreen size x, horizontal resolution of
+                                touchscreen (in pixels)
+        sizey                   Touchscreen size y, vertical resolution of
+                                touchscreen (in pixels)
+
+
+Name:   imx219
+Info:   Sony IMX219 camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=imx219,<param>=<val>
+Params: rotation                Mounting rotation of the camera sensor (0 or
+                                180, default 180)
+
+
+Name:   imx290
+Info:   Sony IMX290 camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants. NB This currently uses 4 CSI2 data lanes and therefore will
+        only work on a CM.
+Load:   dtoverlay=imx290,<param>
+Params: 4lane                   Enable 4 CSI2 lanes. This requires a Compute
+                                Module (1, 3, or 4).
+        clock-frequency         Sets the clock frequency to match that used on
+                                the board.
+                                Modules from Vision Components use 37.125MHz
+                                (the default), whilst those from Innomaker use
+                                74.25MHz.
+        mono                    Denote that the module is a mono sensor.
+
+
+Name:   imx477
+Info:   Sony IMX477 camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=imx477,<param>=<val>
+Params: rotation                Mounting rotation of the camera sensor (0 or
+                                180, default 180)
+
+
+Name:   iqaudio-codec
+Info:   Configures the IQaudio Codec audio card
+Load:   dtoverlay=iqaudio-codec
+Params: <None>
+
+
+Name:   iqaudio-dac
+Info:   Configures the IQaudio DAC audio card
+Load:   dtoverlay=iqaudio-dac,<param>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=iqaudio-dac,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
+Name:   iqaudio-dacplus
+Info:   Configures the IQaudio DAC+ audio card
+Load:   dtoverlay=iqaudio-dacplus,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=iqaudio-dacplus,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24db_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+        auto_mute_amp           If specified, unmute/mute the IQaudIO amp when
+                                starting/stopping audio playback.
+        unmute_amp              If specified, unmute the IQaudIO amp once when
+                                the DAC driver module loads.
+
+
+Name:   iqaudio-digi-wm8804-audio
+Info:   Configures the IQAudIO Digi WM8804 audio card
+Load:   dtoverlay=iqaudio-digi-wm8804-audio,<param>=<val>
+Params: card_name               Override the default, "IQAudIODigi", card name.
+        dai_name                Override the default, "IQAudIO Digi", dai name.
+        dai_stream_name         Override the default, "IQAudIO Digi HiFi",
+                                dai stream name.
+
+
+Name:   irs1125
+Info:   Infineon irs1125 TOF camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=irs1125
+Params: <None>
+
+
+Name:   jedec-spi-nor
+Info:   Adds support for JEDEC-compliant SPI NOR flash devices.  (Note: The
+        "jedec,spi-nor" kernel driver was formerly known as "m25p80".)
+Load:   dtoverlay=jedec-spi-nor,<param>=<val>
+Params: flash-spi<n>-<m>        Enables flash device on SPI<n>, CS#<m>.
+        flash-fastr-spi<n>-<m>  Enables flash device with fast read capability
+                                on SPI<n>, CS#<m>.
+
+
+Name:   justboom-both
+Info:   Simultaneous usage of an justboom-dac and justboom-digi based
+        card
+Load:   dtoverlay=justboom-both,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=justboom-dac,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24dB_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
+Name:   justboom-dac
+Info:   Configures the JustBoom DAC HAT, Amp HAT, DAC Zero and Amp Zero audio
+        cards
+Load:   dtoverlay=justboom-dac,<param>=<val>
+Params: 24db_digital_gain       Allow gain to be applied via the PCM512x codec
+                                Digital volume control. Enable with
+                                "dtoverlay=justboom-dac,24db_digital_gain"
+                                (The default behaviour is that the Digital
+                                volume control is limited to a maximum of
+                                0dB. ie. it can attenuate but not provide
+                                gain. For most users, this will be desired
+                                as it will prevent clipping. By appending
+                                the 24dB_digital_gain parameter, the Digital
+                                volume control will allow up to 24dB of
+                                gain. If this parameter is enabled, it is the
+                                responsibility of the user to ensure that
+                                the Digital volume control is set to a value
+                                that does not result in clipping/distortion!)
+
+
+Name:   justboom-digi
+Info:   Configures the JustBoom Digi HAT and Digi Zero audio cards
+Load:   dtoverlay=justboom-digi
+Params: <None>
+
+
+Name:   lirc-rpi
+Info:   This overlay has been deprecated and removed - see gpio-ir
+Load:   <Deprecated>
+
+
+Name:   ltc294x
+Info:   Adds support for the ltc294x family of battery gauges
+Load:   dtoverlay=ltc294x,<param>=<val>
+Params: ltc2941                 Select the ltc2941 device
+
+        ltc2942                 Select the ltc2942 device
+
+        ltc2943                 Select the ltc2943 device
+
+        ltc2944                 Select the ltc2944 device
+
+        resistor-sense          The sense resistor value in milli-ohms.
+                                Can be a 32-bit negative value when the battery
+                                has been connected to the wrong end of the
+                                resistor.
+
+        prescaler-exponent      Range and accuracy of the gauge. The value is
+                                programmed into the chip only if it differs
+                                from the current setting.
+                                For LTC2941 only:
+                                - Default value is 128
+                                - the exponent is in the range 0-7 (default 7)
+                                See the datasheet for more information.
+
+
+Name:   max98357a
+Info:   Configures the Maxim MAX98357A I2S DAC
+Load:   dtoverlay=max98357a,<param>=<val>
+Params: no-sdmode               Driver does not manage the state of the DAC's
+                                SD_MODE pin (i.e. chip is always on).
+        sdmode-pin              integer, GPIO pin connected to the SD_MODE input
+                                of the DAC (default GPIO4 if parameter omitted).
+
+
+Name:   maxtherm
+Info:   Configure a MAX6675 or MAX31855 thermocouple as an IIO device.
+
+        For devices on spi1 or spi2, the interfaces should be enabled
+        with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+        The overlay expects to disable the relevant spidev node, so also using
+        e.g. cs0_spidev=off is unnecessary.
+
+        Note:   with the 5.7 kernel (and later) there will also be
+                overlays for MAX31855E, MAX31855J, MAX31855K,
+                MAX31885N, MAX31855R, MAX31855S and MAX31855T.
+
+        Example:
+        MAX31855 on /dev/spidev0.0
+            dtoverlay=maxtherm,spi0-0,max31855
+
+Load:   dtoverlay=maxtherm,<param>=<val>
+Params: spi<n>-<m>              Configure device at spi<n>, cs<m>
+                                (boolean, required)
+        max6675                 Enable support for the MAX6675 (default)
+        max31855                Enable support for the MAX31855
+        max31855e               Enable support for the MAX31855E
+        max31855j               Enable support for the MAX31855J
+        max31855k               Enable support for the MAX31855K
+        max31855n               Enable support for the MAX31855N
+        max31855r               Enable support for the MAX31855R
+        max31855s               Enable support for the MAX31855S
+        max31855t               Enable support for the MAX31855T
+
+
+Name:   mbed-dac
+Info:   Configures the mbed AudioCODEC (TLV320AIC23B)
+Load:   dtoverlay=mbed-dac
+Params: <None>
+
+
+Name:   mcp23017
+Info:   Configures the MCP23017 I2C GPIO expander
+Load:   dtoverlay=mcp23017,<param>=<val>
+Params: gpiopin                 Gpio pin connected to the INTA output of the
+                                MCP23017 (default: 4)
+
+        addr                    I2C address of the MCP23017 (default: 0x20)
+
+        mcp23008                Configure an MCP23008 instead.
+        noints                  Disable the interrupt GPIO line.
+
+
+Name:   mcp23s17
+Info:   Configures the MCP23S08/17 SPI GPIO expanders.
+        If devices are present on SPI1 or SPI2, those interfaces must be enabled
+        with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+        If interrupts are enabled for a device on a given CS# on a SPI bus, that
+        device must be the only one present on that SPI bus/CS#.
+Load:   dtoverlay=mcp23s17,<param>=<val>
+Params: s08-spi<n>-<m>-present  4-bit integer, bitmap indicating MCP23S08
+                                devices present on SPI<n>, CS#<m>
+
+        s17-spi<n>-<m>-present  8-bit integer, bitmap indicating MCP23S17
+                                devices present on SPI<n>, CS#<m>
+
+        s08-spi<n>-<m>-int-gpio integer, enables interrupts on a single
+                                MCP23S08 device on SPI<n>, CS#<m>, specifies
+                                the GPIO pin to which INT output of MCP23S08
+                                is connected.
+
+        s17-spi<n>-<m>-int-gpio integer, enables mirrored interrupts on a
+                                single MCP23S17 device on SPI<n>, CS#<m>,
+                                specifies the GPIO pin to which either INTA
+                                or INTB output of MCP23S17 is connected.
+
+
+Name:   mcp2515-can0
+Info:   Configures the MCP2515 CAN controller on spi0.0
+Load:   dtoverlay=mcp2515-can0,<param>=<val>
+Params: oscillator              Clock frequency for the CAN controller (Hz)
+
+        spimaxfrequency         Maximum SPI frequence (Hz)
+
+        interrupt               GPIO for interrupt signal
+
+
+Name:   mcp2515-can1
+Info:   Configures the MCP2515 CAN controller on spi0.1
+Load:   dtoverlay=mcp2515-can1,<param>=<val>
+Params: oscillator              Clock frequency for the CAN controller (Hz)
+
+        spimaxfrequency         Maximum SPI frequence (Hz)
+
+        interrupt               GPIO for interrupt signal
+
+
+Name:   mcp3008
+Info:   Configures MCP3008 A/D converters
+        For devices on spi1 or spi2, the interfaces should be enabled
+        with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+Load:   dtoverlay=mcp3008,<param>[=<val>]
+Params: spi<n>-<m>-present      boolean, configure device at spi<n>, cs<m>
+        spi<n>-<m>-speed        integer, set the spi bus speed for this device
+
+
+Name:   mcp3202
+Info:   Configures MCP3202 A/D converters
+        For devices on spi1 or spi2, the interfaces should be enabled
+        with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+Load:   dtoverlay=mcp3202,<param>[=<val>]
+Params: spi<n>-<m>-present      boolean, configure device at spi<n>, cs<m>
+        spi<n>-<m>-speed        integer, set the spi bus speed for this device
+
+
+Name:   mcp342x
+Info:   Overlay for activation of Microchip MCP3421-3428 ADCs over I2C
+Load:   dtoverlay=mcp342x,<param>=<val>
+Params: addr                    I2C bus address of device, for devices with
+                                addresses that are configurable, e.g. by
+                                hardware links (default=0x68)
+        mcp3421                 The device is an MCP3421
+        mcp3422                 The device is an MCP3422
+        mcp3423                 The device is an MCP3423
+        mcp3424                 The device is an MCP3424
+        mcp3425                 The device is an MCP3425
+        mcp3426                 The device is an MCP3426
+        mcp3427                 The device is an MCP3427
+        mcp3428                 The device is an MCP3428
+
+
+Name:   media-center
+Info:   Media Center HAT - 2.83" Touch Display + extras by Pi Supply
+Load:   dtoverlay=media-center,<param>=<val>
+Params: speed                   Display SPI bus speed
+        rotate                  Display rotation {0,90,180,270}
+        fps                     Delay between frame updates
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+        swapxy                  Swap x and y axis
+        backlight               Change backlight GPIO pin {e.g. 12, 18}
+        gpio_out_pin            GPIO for output (default "17")
+        gpio_in_pin             GPIO for input (default "18")
+        gpio_in_pull            Pull up/down/off on the input pin
+                                (default "down")
+        sense                   Override the IR receive auto-detection logic:
+                                 "0" = force active-high
+                                 "1" = force active-low
+                                 "-1" = use auto-detection
+                                (default "-1")
+        softcarrier             Turn the software carrier "on" or "off"
+                                (default "on")
+        invert                  "on" = invert the output pin (default "off")
+        debug                   "on" = enable additional debug messages
+                                (default "off")
+
+
+Name:   merus-amp
+Info:   Configures the merus-amp audio card
+Load:   dtoverlay=merus-amp
+Params: <None>
+
+
+Name:   midi-uart0
+Info:   Configures UART0 (ttyAMA0) so that a requested 38.4kbaud actually gets
+        31.25kbaud, the frequency required for MIDI
+Load:   dtoverlay=midi-uart0
+Params: <None>
+
+
+Name:   midi-uart1
+Info:   Configures UART1 (ttyS0) so that a requested 38.4kbaud actually gets
+        31.25kbaud, the frequency required for MIDI
+Load:   dtoverlay=midi-uart1
+Params: <None>
+
+
+Name:   miniuart-bt
+Info:   Switch the onboard Bluetooth function on Pi 3B, 3B+, 3A+, 4B and Zero W
+        to use the mini-UART (ttyS0) and restore UART0/ttyAMA0 over GPIOs 14 &
+        15. Note that this may reduce the maximum usable baudrate.
+        N.B. It is also necessary to edit /lib/systemd/system/hciuart.service
+        and replace ttyAMA0 with ttyS0, unless using Raspbian or another
+        distribution with udev rules that create /dev/serial0 and /dev/serial1,
+        in which case use /dev/serial1 instead because it will always be
+        correct. Furthermore, you must also set core_freq and core_freq_min to
+        the same value in config.txt or the miniuart will not work.
+Load:   dtoverlay=miniuart-bt,<param>=<val>
+Params: krnbt                   Set to "on" to enable autoprobing of Bluetooth
+                                driver without need of hciattach/btattach
+
+
+Name:   mmc
+Info:   Selects the bcm2835-mmc SD/MMC driver, optionally with overclock
+Load:   dtoverlay=mmc,<param>=<val>
+Params: overclock_50            Clock (in MHz) to use when the MMC framework
+                                requests 50MHz
+
+
+Name:   mpu6050
+Info:   Overlay for i2c connected mpu6050 imu
+Load:   dtoverlay=mpu6050,<param>=<val>
+Params: interrupt               GPIO pin for interrupt (default 4)
+
+
+Name:   mz61581
+Info:   MZ61581 display by Tontec
+Load:   dtoverlay=mz61581,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        txbuflen                Transmit buffer length (default 32768)
+
+        debug                   Debug output level {0-7}
+
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+
+
+Name:   ov5647
+Info:   Omnivision OV5647 camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=ov5647,<param>=<val>
+Params: rotation                Mounting rotation of the camera sensor (0 or
+                                180, default 0)
+
+
+Name:   ov7251
+Info:   Omnivision OV7251 camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=ov7251
+Params: <None>
+
+
+Name:   ov9281
+Info:   Omnivision OV9281 camera module.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=ov9281
+Params: <None>
+
+
+Name:   papirus
+Info:   PaPiRus ePaper Screen by Pi Supply (both HAT and pHAT)
+Load:   dtoverlay=papirus,<param>=<val>
+Params: panel                   Display panel (required):
+                                1.44": e1144cs021
+                                2.0":  e2200cs021
+                                2.7":  e2271cs021
+
+        speed                   Display SPI bus speed
+
+
+Name:   pca953x
+Info:   TI PCA953x family of I2C GPIO expanders. Default is for NXP PCA9534.
+Load:   dtoverlay=pca953x,<param>=<val>
+Params: addr                    I2C address of expander. Default 0x20.
+        pca6416                 Select the NXP PCA6416 (16 bit)
+        pca9505                 Select the NXP PCA9505 (40 bit)
+        pca9535                 Select the NXP PCA9535 (16 bit)
+        pca9536                 Select the NXP PCA9536 or TI PCA9536 (4 bit)
+        pca9537                 Select the NXP PCA9537 (4 bit)
+        pca9538                 Select the NXP PCA9538 (8 bit)
+        pca9539                 Select the NXP PCA9539 (16 bit)
+        pca9554                 Select the NXP PCA9554 (8 bit)
+        pca9555                 Select the NXP PCA9555 (16 bit)
+        pca9556                 Select the NXP PCA9556 (8 bit)
+        pca9557                 Select the NXP PCA9557 (8 bit)
+        pca9574                 Select the NXP PCA9574 (8 bit)
+        pca9575                 Select the NXP PCA9575 (16 bit)
+        pca9698                 Select the NXP PCA9698 (40 bit)
+        pca16416                Select the NXP PCA16416 (16 bit)
+        pca16524                Select the NXP PCA16524 (24 bit)
+        pca19555a               Select the NXP PCA19555A (16 bit)
+        max7310                 Select the Maxim MAX7310 (8 bit)
+        max7312                 Select the Maxim MAX7312 (16 bit)
+        max7313                 Select the Maxim MAX7313 (16 bit)
+        max7315                 Select the Maxim MAX7315 (8 bit)
+        pca6107                 Select the TI PCA6107 (8 bit)
+        tca6408                 Select the TI TCA6408 (8 bit)
+        tca6416                 Select the TI TCA6416 (16 bit)
+        tca6424                 Select the TI TCA6424 (24 bit)
+        tca9539                 Select the TI TCA9539 (16 bit)
+        tca9554                 Select the TI TCA9554 (8 bit)
+        cat9554                 Select the Onnn CAT9554 (8 bit)
+        pca9654                 Select the Onnn PCA9654 (8 bit)
+        xra1202                 Select the Exar XRA1202 (8 bit)
+
+
+[ The pcf2127-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+[ The pcf8523-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+[ The pcf8563-rtc overlay has been deleted. See i2c-rtc. ]
+
+
+Name:   pi3-act-led
+Info:   This overlay has been renamed act-led, keeping pi3-act-led as an alias
+        for backwards compatibility.
+Load:   <Deprecated>
+
+
+Name:   pi3-disable-bt
+Info:   This overlay has been renamed disable-bt, keeping pi3-disable-bt as an
+        alias for backwards compatibility.
+Load:   <Deprecated>
+
+
+Name:   pi3-disable-wifi
+Info:   This overlay has been renamed disable-wifi, keeping pi3-disable-wifi as
+        an alias for backwards compatibility.
+Load:   <Deprecated>
+
+
+Name:   pi3-miniuart-bt
+Info:   This overlay has been renamed miniuart-bt, keeping pi3-miniuart-bt as
+        an alias for backwards compatibility.
+Load:   <Deprecated>
+
+
+Name:   pibell
+Info:   Configures the pibell audio card.
+Load:   dtoverlay=pibell,<param>=<val>
+Params: alsaname                Set the name as it appears in ALSA (default
+                                "PiBell")
+
+
+Name:   pifacedigital
+Info:   Configures the PiFace Digital mcp23s17 GPIO port expander.
+Load:   dtoverlay=pifacedigital,<param>=<val>
+Params: spi-present-mask        8-bit integer, bitmap indicating MCP23S17 SPI0
+                                CS0 address. PiFace Digital supports addresses
+                                0-3, which can be configured with JP1 and JP2.
+
+
+Name:   piglow
+Info:   Configures the PiGlow by pimoroni.com
+Load:   dtoverlay=piglow
+Params: <None>
+
+
+Name:   piscreen
+Info:   PiScreen display by OzzMaker.com
+Load:   dtoverlay=piscreen,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+
+
+Name:   piscreen2r
+Info:   PiScreen 2 with resistive TP display by OzzMaker.com
+Load:   dtoverlay=piscreen2r,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+
+
+Name:   pisound
+Info:   Configures the Blokas Labs pisound card
+Load:   dtoverlay=pisound
+Params: <None>
+
+
+Name:   pitft22
+Info:   Adafruit PiTFT 2.2" screen
+Load:   dtoverlay=pitft22,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+
+Name:   pitft28-capacitive
+Info:   Adafruit PiTFT 2.8" capacitive touch screen
+Load:   dtoverlay=pitft28-capacitive,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        touch-sizex             Touchscreen size x (default 240)
+
+        touch-sizey             Touchscreen size y (default 320)
+
+        touch-invx              Touchscreen inverted x axis
+
+        touch-invy              Touchscreen inverted y axis
+
+        touch-swapxy            Touchscreen swapped x y axis
+
+
+Name:   pitft28-resistive
+Info:   Adafruit PiTFT 2.8" resistive touch screen
+Load:   dtoverlay=pitft28-resistive,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+
+Name:   pitft35-resistive
+Info:   Adafruit PiTFT 3.5" resistive touch screen
+Load:   dtoverlay=pitft35-resistive,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+
+Name:   pps-gpio
+Info:   Configures the pps-gpio (pulse-per-second time signal via GPIO).
+Load:   dtoverlay=pps-gpio,<param>=<val>
+Params: gpiopin                 Input GPIO (default "18")
+        assert_falling_edge     When present, assert is indicated by a falling
+                                edge, rather than by a rising edge (default
+                                off)
+        capture_clear           Generate clear events on the trailing edge
+                                (default off)
+
+
+Name:   pwm
+Info:   Configures a single PWM channel
+        Legal pin,function combinations for each channel:
+          PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+          PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+        N.B.:
+          1) Pin 18 is the only one available on all platforms, and
+             it is the one used by the I2S audio interface.
+             Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+          2) The onboard analogue audio output uses both PWM channels.
+          3) So be careful mixing audio and PWM.
+          4) Currently the clock must have been enabled and configured
+             by other means.
+Load:   dtoverlay=pwm,<param>=<val>
+Params: pin                     Output pin (default 18) - see table
+        func                    Pin function (default 2 = Alt5) - see above
+        clock                   PWM clock frequency (informational)
+
+
+Name:   pwm-2chan
+Info:   Configures both PWM channels
+        Legal pin,function combinations for each channel:
+          PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+          PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+        N.B.:
+          1) Pin 18 is the only one available on all platforms, and
+             it is the one used by the I2S audio interface.
+             Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+          2) The onboard analogue audio output uses both PWM channels.
+          3) So be careful mixing audio and PWM.
+          4) Currently the clock must have been enabled and configured
+             by other means.
+Load:   dtoverlay=pwm-2chan,<param>=<val>
+Params: pin                     Output pin (default 18) - see table
+        pin2                    Output pin for other channel (default 19)
+        func                    Pin function (default 2 = Alt5) - see above
+        func2                   Function for pin2 (default 2 = Alt5)
+        clock                   PWM clock frequency (informational)
+
+
+Name:   pwm-ir-tx
+Info:   Use GPIO pin as pwm-assisted infrared transmitter output.
+        This is an alternative to "gpio-ir-tx". pwm-ir-tx makes use
+        of PWM0 to reduce the CPU load during transmission compared to
+        gpio-ir-tx which uses bit-banging.
+        Legal pin,function combinations are:
+          12,4(Alt0) 18,2(Alt5) 40,4(Alt0) 52,5(Alt1)
+Load:   dtoverlay=pwm-ir-tx,<param>=<val>
+Params: gpio_pin                Output GPIO (default 18)
+
+        func                    Pin function (default 2 = Alt5)
+
+
+Name:   qca7000
+Info:   I2SE's Evaluation Board for PLC Stamp micro
+Load:   dtoverlay=qca7000,<param>=<val>
+Params: int_pin                 GPIO pin for interrupt signal (default 23)
+
+        speed                   SPI bus speed (default 12 MHz)
+
+
+Name:   rotary-encoder
+Info:   Overlay for GPIO connected rotary encoder.
+Load:   dtoverlay=rotary-encoder,<param>=<val>
+Params: pin_a                   GPIO connected to rotary encoder channel A
+                                (default 4).
+        pin_b                   GPIO connected to rotary encoder channel B
+                                (default 17).
+        relative_axis           register a relative axis rather than an
+                                absolute one. Relative axis will only
+                                generate +1/-1 events on the input device,
+                                hence no steps need to be passed.
+        linux_axis              the input subsystem axis to map to this
+                                rotary encoder. Defaults to 0 (ABS_X / REL_X)
+        rollover                Automatic rollover when the rotary value
+                                becomes greater than the specified steps or
+                                smaller than 0. For absolute axis only.
+        steps-per-period        Number of steps (stable states) per period.
+                                The values have the following meaning:
+                                1: Full-period mode (default)
+                                2: Half-period mode
+                                4: Quarter-period mode
+        steps                   Number of steps in a full turnaround of the
+                                encoder. Only relevant for absolute axis.
+                                Defaults to 24 which is a typical value for
+                                such devices.
+        wakeup                  Boolean, rotary encoder can wake up the
+                                system.
+        encoding                String, the method used to encode steps.
+                                Supported are "gray" (the default and more
+                                common) and "binary".
+
+
+Name:   rpi-backlight
+Info:   Raspberry Pi official display backlight driver
+Load:   dtoverlay=rpi-backlight
+Params: <None>
+
+
+Name:   rpi-cirrus-wm5102
+Info:   Configures the Cirrus Logic Audio Card
+Load:   dtoverlay=rpi-cirrus-wm5102
+Params: <None>
+
+
+Name:   rpi-dac
+Info:   Configures the RPi DAC audio card
+Load:   dtoverlay=rpi-dac
+Params: <None>
+
+
+Name:   rpi-display
+Info:   RPi-Display - 2.8" Touch Display by Watterott
+Load:   dtoverlay=rpi-display,<param>=<val>
+Params: speed                   Display SPI bus speed
+        rotate                  Display rotation {0,90,180,270}
+        fps                     Delay between frame updates
+        debug                   Debug output level {0-7}
+        xohms                   Touchpanel sensitivity (X-plate resistance)
+        swapxy                  Swap x and y axis
+        backlight               Change backlight GPIO pin {e.g. 12, 18}
+
+
+Name:   rpi-ft5406
+Info:   Official Raspberry Pi display touchscreen
+Load:   dtoverlay=rpi-ft5406,<param>=<val>
+Params: touchscreen-size-x      Touchscreen X resolution (default 800)
+        touchscreen-size-y      Touchscreen Y resolution (default 600);
+        touchscreen-inverted-x  Invert touchscreen X coordinates (default 0);
+        touchscreen-inverted-y  Invert touchscreen Y coordinates (default 0);
+        touchscreen-swapped-x-y Swap X and Y cordinates (default 0);
+
+
+Name:   rpi-poe
+Info:   Raspberry Pi PoE HAT fan
+Load:   dtoverlay=rpi-poe,<param>[=<val>]
+Params: poe_fan_temp0           Temperature (in millicelcius) at which the fan
+                                turns on (default 40000)
+        poe_fan_temp0_hyst      Temperature delta (in millicelcius) at which
+                                the fan turns off (default 2000)
+        poe_fan_temp1           Temperature (in millicelcius) at which the fan
+                                speeds up (default 45000)
+        poe_fan_temp1_hyst      Temperature delta (in millicelcius) at which
+                                the fan slows down (default 2000)
+        poe_fan_temp2           Temperature (in millicelcius) at which the fan
+                                speeds up (default 50000)
+        poe_fan_temp2_hyst      Temperature delta (in millicelcius) at which
+                                the fan slows down (default 2000)
+        poe_fan_temp3           Temperature (in millicelcius) at which the fan
+                                speeds up (default 55000)
+        poe_fan_temp3_hyst      Temperature delta (in millicelcius) at which
+                                the fan slows down (default 5000)
+
+
+Name:   rpi-proto
+Info:   Configures the RPi Proto audio card
+Load:   dtoverlay=rpi-proto
+Params: <None>
+
+
+Name:   rpi-sense
+Info:   Raspberry Pi Sense HAT
+Load:   dtoverlay=rpi-sense
+Params: <None>
+
+
+Name:   rpi-tv
+Info:   Raspberry Pi TV HAT
+Load:   dtoverlay=rpi-tv
+Params: <None>
+
+
+Name:   rpivid-v4l2
+Info:   Load the V4L2 stateless video decoder driver for the HEVC block,
+        disabling the memory mapped devices in the process.
+Load:   dtoverlay=rpivid-v4l2
+Params: <None>
+
+
+Name:   rra-digidac1-wm8741-audio
+Info:   Configures the Red Rocks Audio DigiDAC1 soundcard
+Load:   dtoverlay=rra-digidac1-wm8741-audio
+Params: <None>
+
+
+Name:   sainsmart18
+Info:   Overlay for the SPI-connected Sainsmart 1.8" display (based on the
+        ST7735R chip).
+Load:   dtoverlay=sainsmart18,<param>=<val>
+Params: rotate                  Display rotation {0,90,180,270}
+        speed                   SPI bus speed in Hz (default 4000000)
+        fps                     Display frame rate in Hz
+        bgr                     Enable BGR mode (default off)
+        debug                   Debug output level {0-7}
+        dc_pin                  GPIO pin for D/C (default 24)
+        reset_pin               GPIO pin for RESET (default 25)
+
+
+Name:   sc16is750-i2c
+Info:   Overlay for the NXP SC16IS750 UART with I2C Interface
+        Enables the chip on I2C1 at 0x48 (or the "addr" parameter value). To
+        select another address, please refer to table 10 in reference manual.
+Load:   dtoverlay=sc16is750-i2c,<param>=<val>
+Params: int_pin                 GPIO used for IRQ (default 24)
+        addr                    Address (default 0x48)
+        xtal                    On-board crystal frequency (default 14745600)
+
+
+Name:   sc16is752-i2c
+Info:   Overlay for the NXP SC16IS752 dual UART with I2C Interface
+        Enables the chip on I2C1 at 0x48 (or the "addr" parameter value). To
+        select another address, please refer to table 10 in reference manual.
+Load:   dtoverlay=sc16is752-i2c,<param>=<val>
+Params: int_pin                 GPIO used for IRQ (default 24)
+        addr                    Address (default 0x48)
+        xtal                    On-board crystal frequency (default 14745600)
+
+
+Name:   sc16is752-spi0
+Info:   Overlay for the NXP SC16IS752 Dual UART with SPI Interface
+        Enables the chip on SPI0.
+Load:   dtoverlay=sc16is752-spi0,<param>=<val>
+Params: int_pin                 GPIO used for IRQ (default 24)
+        xtal                    On-board crystal frequency (default 14745600)
+
+
+Name:   sc16is752-spi1
+Info:   Overlay for the NXP SC16IS752 Dual UART with SPI Interface
+        Enables the chip on SPI1.
+        N.B.: spi1 is only accessible on devices with a 40pin header, eg:
+              A+, B+, Zero and PI2 B; as well as the Compute Module.
+
+Load:   dtoverlay=sc16is752-spi1,<param>=<val>
+Params: int_pin                 GPIO used for IRQ (default 24)
+        xtal                    On-board crystal frequency (default 14745600)
+
+
+Name:   sdhost
+Info:   Selects the bcm2835-sdhost SD/MMC driver, optionally with overclock.
+        N.B. This overlay is designed for situations where the mmc driver is
+        the default, so it disables the other (mmc) interface - this will kill
+        WiFi on a Pi3. If this isn't what you want, either use the sdtweak
+        overlay or the new sd_* dtparams of the base DTBs.
+Load:   dtoverlay=sdhost,<param>=<val>
+Params: overclock_50            Clock (in MHz) to use when the MMC framework
+                                requests 50MHz
+
+        force_pio               Disable DMA support (default off)
+
+        pio_limit               Number of blocks above which to use DMA
+                                (default 1)
+
+        debug                   Enable debug output (default off)
+
+
+Name:   sdio
+Info:   Selects the bcm2835-sdhost SD/MMC driver, optionally with overclock,
+        and enables SDIO via GPIOs 22-27. An example of use in 1-bit mode is
+        "dtoverlay=sdio,bus_width=1,gpios_22_25"
+Load:   dtoverlay=sdio,<param>=<val>
+Params: sdio_overclock          SDIO Clock (in MHz) to use when the MMC
+                                framework requests 50MHz
+
+        poll_once               Disable SDIO-device polling every second
+                                (default on: polling once at boot-time)
+
+        bus_width               Set the SDIO host bus width (default 4 bits)
+
+        gpios_22_25             Select GPIOs 22-25 for 1-bit mode. Must be used
+                                with bus_width=1. This replaces the sdio-1bit
+                                overlay, which is now deprecated.
+
+        gpios_34_37             Select GPIOs 34-37 for 1-bit mode. Must be used
+                                with bus_width=1.
+
+        gpios_34_39             Select GPIOs 34-39 for 4-bit mode. Must be used
+                                with bus_width=4 (the default).
+
+
+Name:   sdio-1bit
+Info:   This overlay is now deprecated. Use
+        "dtoverlay=sdio,bus_width=1,gpios_22_25" instead.
+Load:   <Deprecated>
+
+
+Name:   sdtweak
+Info:   Tunes the bcm2835-sdhost SD/MMC driver
+        N.B. This functionality is now available via the sd_* dtparams in the
+        base DTB.
+Load:   dtoverlay=sdtweak,<param>=<val>
+Params: overclock_50            Clock (in MHz) to use when the MMC framework
+                                requests 50MHz
+
+        force_pio               Disable DMA support (default off)
+
+        pio_limit               Number of blocks above which to use DMA
+                                (default 1)
+
+        debug                   Enable debug output (default off)
+
+        poll_once               Looks for a card once after booting. Useful
+                                for network booting scenarios to avoid the
+                                overhead of continuous polling. N.B. Using
+                                this option restricts the system to using a
+                                single card per boot (or none at all).
+                                (default off)
+
+        enable                  Set to off to completely disable the interface
+                                (default on)
+
+
+Name:   sh1106-spi
+Info:   Overlay for SH1106 OLED via SPI using fbtft staging driver.
+Load:   dtoverlay=sh1106-spi,<param>=<val>
+Params: speed                   SPI bus speed (default 4000000)
+        rotate                  Display rotation (0, 90, 180 or 270; default 0)
+        fps                     Delay between frame updates (default 25)
+        debug                   Debug output level (0-7; default 0)
+        dc_pin                  GPIO pin for D/C (default 24)
+        reset_pin               GPIO pin for RESET (default 25)
+        height                  Display height (32 or 64; default 64)
+
+
+Name:   smi
+Info:   Enables the Secondary Memory Interface peripheral. Uses GPIOs 2-25!
+Load:   dtoverlay=smi
+Params: <None>
+
+
+Name:   smi-dev
+Info:   Enables the userspace interface for the SMI driver
+Load:   dtoverlay=smi-dev
+Params: <None>
+
+
+Name:   smi-nand
+Info:   Enables access to NAND flash via the SMI interface
+Load:   dtoverlay=smi-nand
+Params: <None>
+
+
+Name:   spi-gpio35-39
+Info:   Move SPI function block to GPIO 35 to 39
+Load:   dtoverlay=spi-gpio35-39
+Params: <None>
+
+
+Name:   spi-gpio40-45
+Info:   Move SPI function block to GPIOs 40 to 45
+Load:   dtoverlay=spi-gpio40-45
+Params: <None>
+
+
+Name:   spi-rtc
+Info:   Adds support for a number of SPI Real Time Clock devices
+Load:   dtoverlay=spi-rtc,<param>=<val>
+Params: pcf2123                 Select the PCF2123 device
+
+
+Name:   spi0-1cs
+Info:   Only use one CS pin for SPI0
+Load:   dtoverlay=spi0-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 8)
+        no_miso                 Don't claim and use the MISO pin (9), freeing
+                                it for other uses.
+
+
+Name:   spi0-2cs
+Info:   Change the CS pins for SPI0
+Load:   dtoverlay=spi0-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 8)
+        cs1_pin                 GPIO pin for CS1 (default 7)
+        no_miso                 Don't claim and use the MISO pin (9), freeing
+                                it for other uses.
+
+
+Name:   spi0-cs
+Info:   This overlay has been renamed spi0-2cs, keeping spi0-cs as an
+        alias for backwards compatibility.
+Load:   <Deprecated>
+
+
+Name:   spi0-hw-cs
+Info:   This overlay has been deprecated and removed because it is no longer
+        necessary and has been seen to prevent spi0 from working.
+Load:   <Deprecated>
+
+
+Name:   spi1-1cs
+Info:   Enables spi1 with a single chip select (CS) line and associated spidev
+        dev node. The gpio pin number for the CS line and spidev device node
+        creation are configurable.
+        N.B.: spi1 is only accessible on devices with a 40pin header, eg:
+              A+, B+, Zero and PI2 B; as well as the Compute Module.
+Load:   dtoverlay=spi1-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 18 - BCM SPI1_CE0).
+        cs0_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev1.0 (default
+                                is 'okay' or enabled).
+
+
+Name:   spi1-2cs
+Info:   Enables spi1 with two chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable.
+        N.B.: spi1 is only accessible on devices with a 40pin header, eg:
+              A+, B+, Zero and PI2 B; as well as the Compute Module.
+Load:   dtoverlay=spi1-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 18 - BCM SPI1_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 17 - BCM SPI1_CE1).
+        cs0_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev1.0 (default
+                                is 'okay' or enabled).
+        cs1_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev1.1 (default
+                                is 'okay' or enabled).
+
+
+Name:   spi1-3cs
+Info:   Enables spi1 with three chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable.
+        N.B.: spi1 is only accessible on devices with a 40pin header, eg:
+              A+, B+, Zero and PI2 B; as well as the Compute Module.
+Load:   dtoverlay=spi1-3cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 18 - BCM SPI1_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 17 - BCM SPI1_CE1).
+        cs2_pin                 GPIO pin for CS2 (default 16 - BCM SPI1_CE2).
+        cs0_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev1.0 (default
+                                is 'okay' or enabled).
+        cs1_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev1.1 (default
+                                is 'okay' or enabled).
+        cs2_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev1.2 (default
+                                is 'okay' or enabled).
+
+
+Name:   spi2-1cs
+Info:   Enables spi2 with a single chip select (CS) line and associated spidev
+        dev node. The gpio pin number for the CS line and spidev device node
+        creation are configurable.
+        N.B.: spi2 is only accessible with the Compute Module.
+Load:   dtoverlay=spi2-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 43 - BCM SPI2_CE0).
+        cs0_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev2.0 (default
+                                is 'okay' or enabled).
+
+
+Name:   spi2-2cs
+Info:   Enables spi2 with two chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable.
+        N.B.: spi2 is only accessible with the Compute Module.
+Load:   dtoverlay=spi2-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 43 - BCM SPI2_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 44 - BCM SPI2_CE1).
+        cs0_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev2.0 (default
+                                is 'okay' or enabled).
+        cs1_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev2.1 (default
+                                is 'okay' or enabled).
+
+
+Name:   spi2-3cs
+Info:   Enables spi2 with three chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable.
+        N.B.: spi2 is only accessible with the Compute Module.
+Load:   dtoverlay=spi2-3cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 43 - BCM SPI2_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 44 - BCM SPI2_CE1).
+        cs2_pin                 GPIO pin for CS2 (default 45 - BCM SPI2_CE2).
+        cs0_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev2.0 (default
+                                is 'okay' or enabled).
+        cs1_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev2.1 (default
+                                is 'okay' or enabled).
+        cs2_spidev              Set to 'disabled' to stop the creation of a
+                                userspace device node /dev/spidev2.2 (default
+                                is 'okay' or enabled).
+
+
+Name:   spi3-1cs
+Info:   Enables spi3 with a single chip select (CS) line and associated spidev
+        dev node. The gpio pin number for the CS line and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi3-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 0 - BCM SPI3_CE0).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev3.0 (default
+                                is 'on' or enabled).
+
+
+Name:   spi3-2cs
+Info:   Enables spi3 with two chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi3-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 0 - BCM SPI3_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 24 - BCM SPI3_CE1).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev3.0 (default
+                                is 'on' or enabled).
+        cs1_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev3.1 (default
+                                is 'on' or enabled).
+
+
+Name:   spi4-1cs
+Info:   Enables spi4 with a single chip select (CS) line and associated spidev
+        dev node. The gpio pin number for the CS line and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi4-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 4 - BCM SPI4_CE0).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev4.0 (default
+                                is 'on' or enabled).
+
+
+Name:   spi4-2cs
+Info:   Enables spi4 with two chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi4-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 4 - BCM SPI4_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 25 - BCM SPI4_CE1).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev4.0 (default
+                                is 'on' or enabled).
+        cs1_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev4.1 (default
+                                is 'on' or enabled).
+
+
+Name:   spi5-1cs
+Info:   Enables spi5 with a single chip select (CS) line and associated spidev
+        dev node. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi5-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 12 - BCM SPI5_CE0).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev5.0 (default
+                                is 'on' or enabled).
+
+
+Name:   spi5-2cs
+Info:   Enables spi5 with two chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi5-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 12 - BCM SPI5_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 26 - BCM SPI5_CE1).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev5.0 (default
+                                is 'on' or enabled).
+        cs1_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev5.1 (default
+                                is 'on' or enabled).
+
+
+Name:   spi6-1cs
+Info:   Enables spi6 with a single chip select (CS) line and associated spidev
+        dev node. The gpio pin number for the CS line and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi6-1cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 18 - BCM SPI6_CE0).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev6.0 (default
+                                is 'on' or enabled).
+
+
+Name:   spi6-2cs
+Info:   Enables spi6 with two chip select (CS) lines and associated spidev
+        dev nodes. The gpio pin numbers for the CS lines and spidev device node
+        creation are configurable. BCM2711 only.
+Load:   dtoverlay=spi6-2cs,<param>=<val>
+Params: cs0_pin                 GPIO pin for CS0 (default 18 - BCM SPI6_CE0).
+        cs1_pin                 GPIO pin for CS1 (default 27 - BCM SPI6_CE1).
+        cs0_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev6.0 (default
+                                is 'on' or enabled).
+        cs1_spidev              Set to 'off' to prevent the creation of a
+                                userspace device node /dev/spidev6.1 (default
+                                is 'on' or enabled).
+
+
+Name:   ssd1306
+Info:   Overlay for activation of SSD1306 over I2C OLED display framebuffer.
+Load:   dtoverlay=ssd1306,<param>=<val>
+Params: address                 Location in display memory of first character.
+                                (default=0)
+        width                   Width of display. (default=128)
+        height                  Height of display. (default=64)
+        offset                  virtual channel a. (default=0)
+        normal                  Has no effect on displays tested. (default=not
+                                set)
+        sequential              Set this if every other scan line is missing.
+                                (default=not set)
+        remapped                Set this if display is garbled. (default=not
+                                set)
+        inverted                Set this if display is inverted and mirrored.
+                                (default=not set)
+
+        Examples:
+        Typical usage for 128x64 display: dtoverlay=ssd1306,inverted
+
+        Typical usage for 128x32 display: dtoverlay=ssd1306,inverted,sequential
+
+        i2c_baudrate=400000 will speed up the display.
+
+        i2c_baudrate=1000000 seems to work even though it's not officially
+        supported by the hardware, and is faster still.
+
+        For more information refer to the device datasheet at:
+        https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf
+
+
+Name:   ssd1306-spi
+Info:   Overlay for SSD1306 OLED via SPI using fbtft staging driver.
+Load:   dtoverlay=ssd1306-spi,<param>=<val>
+Params: speed                   SPI bus speed (default 10000000)
+        rotate                  Display rotation (0, 90, 180 or 270; default 0)
+        fps                     Delay between frame updates (default 25)
+        debug                   Debug output level (0-7; default 0)
+        dc_pin                  GPIO pin for D/C (default 24)
+        reset_pin               GPIO pin for RESET (default 25)
+        height                  Display height (32 or 64; default 64)
+
+
+Name:   ssd1351-spi
+Info:   Overlay for SSD1351 OLED via SPI using fbtft staging driver.
+Load:   dtoverlay=ssd1351-spi,<param>=<val>
+Params: speed                   SPI bus speed (default 4500000)
+        rotate                  Display rotation (0, 90, 180 or 270; default 0)
+        fps                     Delay between frame updates (default 25)
+        debug                   Debug output level (0-7; default 0)
+        dc_pin                  GPIO pin for D/C (default 24)
+        reset_pin               GPIO pin for RESET (default 25)
+
+
+Name:   superaudioboard
+Info:   Configures the SuperAudioBoard sound card
+Load:   dtoverlay=superaudioboard,<param>=<val>
+Params: gpiopin                 GPIO pin for codec reset
+
+
+Name:   sx150x
+Info:   Configures the Semtech SX150X I2C GPIO expanders.
+Load:   dtoverlay=sx150x,<param>=<val>
+Params: sx150<x>-<n>-<m>        Enables SX150X device on I2C#<n> with slave
+                                address <m>. <x> may be 1-9. <n> may be 0 or 1.
+                                Permissible values of <m> (which is denoted in
+                                hex) depend on the device variant. For SX1501,
+                                SX1502, SX1504 and SX1505, <m> may be 20 or 21.
+                                For SX1503 and SX1506, <m> may be 20. For
+                                SX1507 and SX1509, <m> may be 3E, 3F, 70 or 71.
+                                For SX1508, <m> may be 20, 21, 22 or 23.
+
+        sx150<x>-<n>-<m>-int-gpio
+                                Integer, enables interrupts on SX150X device on
+                                I2C#<n> with slave address <m>, specifies
+                                the GPIO pin to which NINT output of SX150X is
+                                connected.
+
+
+Name:   tc358743
+Info:   Toshiba TC358743 HDMI to CSI-2 bridge chip.
+        Uses Unicam 1, which is the standard camera connector on most Pi
+        variants.
+Load:   dtoverlay=tc358743,<param>=<val>
+Params: 4lane                   Use 4 lanes (only applicable to Compute Modules
+                                CAM1 connector).
+
+        link-frequency          Set the link frequency. Only values of 297000000
+                                (574Mbit/s) and 486000000 (972Mbit/s - default)
+                                are supported by the driver.
+
+
+Name:   tc358743-audio
+Info:   Used in combination with the tc358743-fast overlay to route the audio
+        from the TC358743 over I2S to the Pi.
+        Wiring is LRCK/WFS to GPIO 19, BCK/SCK to GPIO 18, and DATA/SD to GPIO
+        20.
+Load:   dtoverlay=tc358743-audio,<param>=<val>
+Params: card-name               Override the default, "tc358743", card name.
+
+
+Name:   tinylcd35
+Info:   3.5" Color TFT Display by www.tinylcd.com
+        Options: Touch, RTC, keypad
+Load:   dtoverlay=tinylcd35,<param>=<val>
+Params: speed                   Display SPI bus speed
+
+        rotate                  Display rotation {0,90,180,270}
+
+        fps                     Delay between frame updates
+
+        debug                   Debug output level {0-7}
+
+        touch                   Enable touch panel
+
+        touchgpio               Touch controller IRQ GPIO
+
+        xohms                   Touchpanel: Resistance of X-plate in ohms
+
+        rtc-pcf                 PCF8563 Real Time Clock
+
+        rtc-ds                  DS1307 Real Time Clock
+
+        keypad                  Enable keypad
+
+        Examples:
+            Display with touchpanel, PCF8563 RTC and keypad:
+                dtoverlay=tinylcd35,touch,rtc-pcf,keypad
+            Old touch display:
+                dtoverlay=tinylcd35,touch,touchgpio=3
+
+
+Name:   tpm-slb9670
+Info:   Enables support for Infineon SLB9670 Trusted Platform Module add-on
+        boards, which can be used as a secure key storage and hwrng,
+        available as "Iridium SLB9670" by Infineon and "LetsTrust TPM" by pi3g.
+Load:   dtoverlay=tpm-slb9670
+Params: <None>
+
+
+Name:   uart0
+Info:   Change the pin usage of uart0
+Load:   dtoverlay=uart0,<param>=<val>
+Params: txd0_pin                GPIO pin for TXD0 (14, 32 or 36 - default 14)
+
+        rxd0_pin                GPIO pin for RXD0 (15, 33 or 37 - default 15)
+
+        pin_func                Alternative pin function - 4(Alt0) for 14&15,
+                                7(Alt3) for 32&33, 6(Alt2) for 36&37
+
+
+Name:   uart1
+Info:   Change the pin usage of uart1
+Load:   dtoverlay=uart1,<param>=<val>
+Params: txd1_pin                GPIO pin for TXD1 (14, 32 or 40 - default 14)
+
+        rxd1_pin                GPIO pin for RXD1 (15, 33 or 41 - default 15)
+
+
+Name:   uart2
+Info:   Enable uart 2 on GPIOs 0-3. BCM2711 only.
+Load:   dtoverlay=uart2,<param>
+Params: ctsrts                  Enable CTS/RTS on GPIOs 2-3 (default off)
+
+
+Name:   uart3
+Info:   Enable uart 3 on GPIOs 4-7. BCM2711 only.
+Load:   dtoverlay=uart3,<param>
+Params: ctsrts                  Enable CTS/RTS on GPIOs 6-7 (default off)
+
+
+Name:   uart4
+Info:   Enable uart 4 on GPIOs 8-11. BCM2711 only.
+Load:   dtoverlay=uart4,<param>
+Params: ctsrts                  Enable CTS/RTS on GPIOs 10-11 (default off)
+
+
+Name:   uart5
+Info:   Enable uart 5 on GPIOs 12-15. BCM2711 only.
+Load:   dtoverlay=uart5,<param>
+Params: ctsrts                  Enable CTS/RTS on GPIOs 14-15 (default off)
+
+
+Name:   udrc
+Info:   Configures the NW Digital Radio UDRC Hat
+Load:   dtoverlay=udrc,<param>=<val>
+Params: alsaname                Name of the ALSA audio device (default "udrc")
+
+
+Name:   upstream
+Info:   Allow usage of downstream .dtb with upstream kernel. Comprises the
+        vc4-kms-v3d and dwc2 overlays.
+Load:   dtoverlay=upstream
+Params: <None>
+
+
+Name:   upstream-aux-interrupt
+Info:   This overlay has been deprecated and removed because it is no longer
+        necessary.
+Load:   <Deprecated>
+
+
+Name:   upstream-pi4
+Info:   Allow usage of downstream .dtb with upstream kernel on Pi 4. Comprises
+        the vc4-kms-v3d-pi4 and dwc2 overlays.
+Load:   dtoverlay=upstream-pi4
+Params: <None>
+
+
+Name:   vc4-fkms-v3d
+Info:   Enable Eric Anholt's DRM VC4 V3D driver on top of the dispmanx
+        display stack.
+Load:   dtoverlay=vc4-fkms-v3d,<param>
+Params: cma-512                 CMA is 512MB (needs 1GB)
+        cma-448                 CMA is 448MB (needs 1GB)
+        cma-384                 CMA is 384MB (needs 1GB)
+        cma-320                 CMA is 320MB (needs 1GB)
+        cma-256                 CMA is 256MB (needs 1GB)
+        cma-192                 CMA is 192MB (needs 1GB)
+        cma-128                 CMA is 128MB
+        cma-96                  CMA is 96MB
+        cma-64                  CMA is 64MB
+        cma-size                CMA size in bytes, 4MB aligned
+        cma-default             Use upstream's default value
+
+
+Name:   vc4-kms-kippah-7inch
+Info:   Enable the Adafruit DPI Kippah with the 7" Ontat panel attached.
+        Requires vc4-kms-v3d to be loaded.
+Load:   dtoverlay=vc4-kms-kippah-7inch
+Params: <None>
+
+
+Name:   vc4-kms-v3d
+Info:   Enable Eric Anholt's DRM VC4 HDMI/HVS/V3D driver.
+Load:   dtoverlay=vc4-kms-v3d,<param>
+Params: cma-512                 CMA is 512MB (needs 1GB)
+        cma-448                 CMA is 448MB (needs 1GB)
+        cma-384                 CMA is 384MB (needs 1GB)
+        cma-320                 CMA is 320MB (needs 1GB)
+        cma-256                 CMA is 256MB (needs 1GB)
+        cma-192                 CMA is 192MB (needs 1GB)
+        cma-128                 CMA is 128MB
+        cma-96                  CMA is 96MB
+        cma-64                  CMA is 64MB
+        cma-size                CMA size in bytes, 4MB aligned
+        cma-default             Use upstream's default value
+        audio                   Enable or disable audio over HDMI (default "on")
+        noaudio                 Disable all HDMI audio (default "off")
+
+
+Name:   vc4-kms-v3d-pi4
+Info:   Enable Eric Anholt's DRM VC4 HDMI/HVS/V3D driver for Pi4.
+Load:   dtoverlay=vc4-kms-v3d-pi4,<param>
+Params: cma-512                 CMA is 512MB
+        cma-448                 CMA is 448MB
+        cma-384                 CMA is 384MB
+        cma-320                 CMA is 320MB
+        cma-256                 CMA is 256MB
+        cma-192                 CMA is 192MB
+        cma-128                 CMA is 128MB
+        cma-96                  CMA is 96MB
+        cma-64                  CMA is 64MB
+        cma-size                CMA size in bytes, 4MB aligned
+        cma-default             Use upstream's default value
+        audio                   Enable or disable audio over HDMI0 (default
+                                "on")
+        audio1                  Enable or disable audio over HDMI1 (default
+                                "on")
+        noaudio                 Disable all HDMI audio (default "off")
+        composite               Enable the composite output (disables all other
+                                outputs)
+
+
+Name:   vga666
+Info:   Overlay for the Fen Logic VGA666 board
+        This uses GPIOs 2-21 (so no I2C), and activates the output 2-3 seconds
+        after the kernel has started.
+Load:   dtoverlay=vga666
+Params: <None>
+
+
+Name:   w1-gpio
+Info:   Configures the w1-gpio Onewire interface module.
+        Use this overlay if you *don't* need a GPIO to drive an external pullup.
+Load:   dtoverlay=w1-gpio,<param>=<val>
+Params: gpiopin                 GPIO for I/O (default "4")
+        pullup                  Now enabled by default (ignored)
+
+
+Name:   w1-gpio-pullup
+Info:   Configures the w1-gpio Onewire interface module.
+        Use this overlay if you *do* need a GPIO to drive an external pullup.
+Load:   dtoverlay=w1-gpio-pullup,<param>=<val>
+Params: gpiopin                 GPIO for I/O (default "4")
+        extpullup               GPIO for external pullup (default "5")
+        pullup                  Now enabled by default (ignored)
+
+
+Name:   w5500
+Info:   Overlay for the Wiznet W5500 Ethernet Controller on SPI0
+Load:   dtoverlay=w5500,<param>=<val>
+Params: int_pin                 GPIO used for INT (default 25)
+
+        speed                   SPI bus speed (default 30000000)
+
+        cs                      SPI bus Chip Select (default 0)
+
+
+Name:   wittypi
+Info:   Configures the wittypi RTC module.
+Load:   dtoverlay=wittypi,<param>=<val>
+Params: led_gpio                GPIO for LED (default "17")
+        led_trigger             Choose which activity the LED tracks (default
+                                "default-on")
+
+
+Troubleshooting
+===============
+
+If you are experiencing problems that you think are DT-related, enable DT
+diagnostic output by adding this to /boot/config.txt:
+
+    dtdebug=on
+
+and rebooting. Then run:
+
+    sudo vcdbg log msg
+
+and look for relevant messages.
+
+Further reading
+===============
+
+This is only meant to be a quick introduction to the subject of Device Tree on
+Raspberry Pi. There is a more complete explanation here:
+
+http://www.raspberrypi.org/documentation/configuration/device-tree.md
diff --git a/arch/arm/boot/dts/overlays/act-led-overlay.dts b/arch/arm/boot/dts/overlays/act-led-overlay.dts
new file mode 100644
index 000000000000..2f4bbb407f89
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/act-led-overlay.dts
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/* Pi3 uses a GPIO expander to drive the LEDs which can only be accessed
+   from the VPU. There is a special driver for this with a separate DT node,
+   which has the unfortunate consequence of breaking the act_led_gpio and
+   act_led_activelow dtparams.
+
+   This overlay changes the GPIO controller back to the standard one and
+   restores the dtparams.
+*/
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&act_led>;
+		frag0: __overlay__ {
+			gpios = <&gpio 0 0>;
+		};
+	};
+
+	__overrides__ {
+		gpio = <&frag0>,"gpios:4";
+		activelow = <&frag0>,"gpios:8";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/adafruit18-overlay.dts b/arch/arm/boot/dts/overlays/adafruit18-overlay.dts
new file mode 100644
index 000000000000..e1ce94a8cd3e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/adafruit18-overlay.dts
@@ -0,0 +1,55 @@
+/*
+ * Device Tree overlay for Adafruit 1.8" TFT LCD with ST7735R chip 160x128
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			af18: adafruit18@0 {
+				compatible = "fbtft,adafruit18";
+				reg = <0>;
+				pinctrl-names = "default";
+				spi-max-frequency = <40000000>;
+				rotate = <90>;
+				buswidth = <8>;
+				fps = <50>;
+				height = <160>;
+				width = <128>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 18 0>;
+				debug = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		green = <&af18>, "compatible=fbtft,adafruit18_green";
+		speed     = <&af18>,"spi-max-frequency:0";
+		rotate    = <&af18>,"rotate:0";
+		fps       = <&af18>,"fps:0";
+		bgr       = <&af18>,"bgr?";
+		debug     = <&af18>,"debug:0";
+		dc_pin    = <&af18>,"dc-gpios:4";
+		reset_pin = <&af18>,"reset-gpios:4";
+		led_pin   = <&af18>,"led-gpios:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/adau1977-adc-overlay.dts b/arch/arm/boot/dts/overlays/adau1977-adc-overlay.dts
new file mode 100644
index 000000000000..298488e19156
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/adau1977-adc-overlay.dts
@@ -0,0 +1,40 @@
+// Definitions for ADAU1977 ADC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+    
+	fragment@0 {
+        	target = <&i2c>;
+        	
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+			
+			adau1977: codec@11 {
+                        	compatible = "adi,adau1977";
+                        	reg = <0x11>;
+                        	reset-gpios = <&gpio 5 0>;
+				AVDD-supply = <&vdd_3v3_reg>;
+                	};
+        	};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "adi,adau1977-adc";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/adau7002-simple-overlay.dts b/arch/arm/boot/dts/overlays/adau7002-simple-overlay.dts
new file mode 100644
index 000000000000..5fed769d2526
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/adau7002-simple-overlay.dts
@@ -0,0 +1,52 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+
+    fragment@0 {
+        target = <&i2s>;
+        __overlay__ {
+            status = "okay";
+        };
+    };
+
+    fragment@1 {
+        target-path = "/";
+        __overlay__ {
+                adau7002_codec: adau7002-codec {
+                #sound-dai-cells = <0>;
+                compatible = "adi,adau7002";
+/*                IOVDD-supply = <&supply>;*/
+                status = "okay";
+            };
+        };
+    };
+
+    fragment@2 {
+        target = <&sound>;
+            sound_overlay: __overlay__ {
+            compatible = "simple-audio-card";
+            simple-audio-card,format = "i2s";
+            simple-audio-card,name = "adau7002";
+            simple-audio-card,bitclock-slave = <&dailink0_slave>;
+            simple-audio-card,frame-slave = <&dailink0_slave>;
+            simple-audio-card,widgets =
+                    "Microphone", "Microphone Jack";
+            simple-audio-card,routing =
+                    "PDM_DAT", "Microphone Jack";
+            status = "okay";
+            simple-audio-card,cpu {
+                sound-dai = <&i2s>;
+            };
+            dailink0_slave: simple-audio-card,codec {
+                sound-dai = <&adau7002_codec>;
+            };
+        };
+    };
+
+
+    __overrides__ {
+        card-name = <&sound_overlay>,"simple-audio-card,name";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/ads1015-overlay.dts b/arch/arm/boot/dts/overlays/ads1015-overlay.dts
new file mode 100644
index 000000000000..deeee1228395
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ads1015-overlay.dts
@@ -0,0 +1,98 @@
+/*
+ * 2016 - Erik Sejr
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+    /* ----------- ADS1015 ------------ */
+    fragment@0 {
+        target = <&i2c_arm>;
+        __overlay__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            status = "okay";
+            ads1015: ads1015 {
+                compatible = "ti,ads1015";
+                status = "okay";
+                #address-cells = <1>;
+                #size-cells = <0>;
+                reg = <0x48>;
+            };
+        };
+    };
+
+    fragment@1 {
+        target = <&ads1015>;
+        __overlay__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            channel_a: channel_a {
+                reg = <4>;
+                ti,gain = <2>;
+                ti,datarate = <4>;
+            };
+        };
+    };
+
+    fragment@2 {
+        target = <&ads1015>;
+        __dormant__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            channel_b: channel_b {
+                reg = <5>;
+                ti,gain = <2>;
+                ti,datarate = <4>;
+            };
+        };
+    };
+
+    fragment@3 {
+        target = <&ads1015>;
+        __dormant__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            channel_c: channel_c {
+                reg = <6>;
+                ti,gain = <2>;
+                ti,datarate = <4>;
+            };
+        };
+    };
+
+    fragment@4 {
+        target = <&ads1015>;
+        __dormant__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            channel_d: channel_d {
+                reg = <7>;
+                ti,gain = <2>;
+                ti,datarate = <4>;
+            };
+        };
+    };
+
+    __overrides__ {
+        addr =            <&ads1015>,"reg:0";
+        cha_enable =      <0>,"=1";
+        cha_cfg =         <&channel_a>,"reg:0";
+        cha_gain =        <&channel_a>,"ti,gain:0";
+        cha_datarate =    <&channel_a>,"ti,datarate:0";
+        chb_enable =      <0>,"=2";
+        chb_cfg =         <&channel_b>,"reg:0";
+        chb_gain =        <&channel_b>,"ti,gain:0";
+        chb_datarate =    <&channel_b>,"ti,datarate:0";
+        chc_enable =      <0>,"=3";
+        chc_cfg =         <&channel_c>,"reg:0";
+        chc_gain =        <&channel_c>,"ti,gain:0";
+        chc_datarate =    <&channel_c>,"ti,datarate:0";
+        chd_enable =      <0>,"=4";
+        chd_cfg =         <&channel_d>,"reg:0";
+        chd_gain =        <&channel_d>,"ti,gain:0";
+        chd_datarate =    <&channel_d>,"ti,datarate:0";
+   };
+
+};
diff --git a/arch/arm/boot/dts/overlays/ads1115-overlay.dts b/arch/arm/boot/dts/overlays/ads1115-overlay.dts
new file mode 100644
index 000000000000..4fc571c2db33
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ads1115-overlay.dts
@@ -0,0 +1,103 @@
+/*
+ * TI ADS1115 multi-channel ADC overlay
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ads1115: ads1115 {
+				compatible = "ti,ads1115";
+				status = "okay";
+				#address-cells = <1>;
+				#size-cells = <0>;
+				reg = <0x48>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&ads1115>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			channel_a: channel_a {
+				reg = <4>;
+				ti,gain = <1>;
+				ti,datarate = <7>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&ads1115>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			channel_b: channel_b {
+				reg = <5>;
+				ti,gain = <1>;
+				ti,datarate = <7>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&ads1115>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			channel_c: channel_c {
+				reg = <6>;
+				ti,gain = <1>;
+				ti,datarate = <7>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&ads1115>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			channel_d: channel_d {
+				reg = <7>;
+				ti,gain = <1>;
+				ti,datarate = <7>;
+			};
+		};
+	};
+
+	__overrides__ {
+		addr =            <&ads1115>,"reg:0";
+		cha_enable =      <0>,"=1";
+		cha_cfg =         <&channel_a>,"reg:0";
+		cha_gain =        <&channel_a>,"ti,gain:0";
+		cha_datarate =    <&channel_a>,"ti,datarate:0";
+		chb_enable =      <0>,"=2";
+		chb_cfg =         <&channel_b>,"reg:0";
+		chb_gain =        <&channel_b>,"ti,gain:0";
+		chb_datarate =    <&channel_b>,"ti,datarate:0";
+		chc_enable =      <0>,"=3";
+		chc_cfg =         <&channel_c>,"reg:0";
+		chc_gain =        <&channel_c>,"ti,gain:0";
+		chc_datarate =    <&channel_c>,"ti,datarate:0";
+		chd_enable =      <0>,"=4";
+		chd_cfg =         <&channel_d>,"reg:0";
+		chd_gain =        <&channel_d>,"ti,gain:0";
+		chd_datarate =    <&channel_d>,"ti,datarate:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ads7846-overlay.dts b/arch/arm/boot/dts/overlays/ads7846-overlay.dts
new file mode 100644
index 000000000000..1c5c9b6bb6ff
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ads7846-overlay.dts
@@ -0,0 +1,89 @@
+/*
+ * Generic Device Tree overlay for the ADS7846 touch controller
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			ads7846_pins: ads7846_pins {
+				brcm,pins = <255>; /* illegal default value */
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			ads7846: ads7846@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&ads7846_pins>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <255 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 255 0>;
+
+				/* driver defaults */
+				ti,x-min = /bits/ 16 <0>;
+				ti,y-min = /bits/ 16 <0>;
+				ti,x-max = /bits/ 16 <0x0FFF>;
+				ti,y-max = /bits/ 16 <0x0FFF>;
+				ti,pressure-min = /bits/ 16 <0>;
+				ti,pressure-max = /bits/ 16 <0xFFFF>;
+				ti,x-plate-ohms = /bits/ 16 <400>;
+			};
+		};
+	};
+	__overrides__ {
+		cs =     <&ads7846>,"reg:0";
+		speed =  <&ads7846>,"spi-max-frequency:0";
+		penirq = <&ads7846_pins>,"brcm,pins:0", /* REQUIRED */
+			 <&ads7846>,"interrupts:0",
+			 <&ads7846>,"pendown-gpio:4";
+		penirq_pull = <&ads7846_pins>,"brcm,pull:0";
+		swapxy = <&ads7846>,"ti,swap-xy?";
+		xmin =   <&ads7846>,"ti,x-min;0";
+		ymin =   <&ads7846>,"ti,y-min;0";
+		xmax =   <&ads7846>,"ti,x-max;0";
+		ymax =   <&ads7846>,"ti,y-max;0";
+		pmin =   <&ads7846>,"ti,pressure-min;0";
+		pmax =   <&ads7846>,"ti,pressure-max;0";
+		xohms =  <&ads7846>,"ti,x-plate-ohms;0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/adv7282m-overlay.dts b/arch/arm/boot/dts/overlays/adv7282m-overlay.dts
new file mode 100644
index 000000000000..5d85dfd0595c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/adv7282m-overlay.dts
@@ -0,0 +1,65 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for Analog Devices ADV7282-M video to CSI2 bridge on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			adv728x: adv728x@21 {
+				compatible = "adi,adv7282-m";
+				reg = <0x21>;
+				status = "okay";
+				clock-frequency = <24000000>;
+				port {
+					adv728x_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1>;
+						link-frequencies =
+							/bits/ 64 <297000000>;
+
+						mclk-frequency = <12000000>;
+					};
+				};
+			};
+		};
+	};
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&adv728x_0>;
+					data-lanes = <1>;
+				};
+			};
+		};
+	};
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		addr =			<&adv728x>,"reg:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/adv728x-m-overlay.dts b/arch/arm/boot/dts/overlays/adv728x-m-overlay.dts
new file mode 100644
index 000000000000..ea392e886984
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/adv728x-m-overlay.dts
@@ -0,0 +1,37 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for Analog Devices ADV728[0|1|2]-M video to CSI2 bridges on VC
+// I2C bus
+
+#include "adv7282m-overlay.dts"
+
+/{
+	compatible = "brcm,bcm2835";
+
+	// Fragment numbers deliberately high to avoid conflicts with the
+	// included adv7282m overlay file.
+
+	fragment@101 {
+		target = <&adv728x>;
+		__dormant__ {
+			compatible = "adi,adv7280-m";
+		};
+	};
+	fragment@102 {
+		target = <&adv728x>;
+		__dormant__ {
+			compatible = "adi,adv7281-m";
+		};
+	};
+	fragment@103 {
+		target = <&adv728x>;
+		__dormant__ {
+			compatible = "adi,adv7281-ma";
+		};
+	};
+
+	__overrides__ {
+		adv7280m = <0>, "+101";
+		adv7281m = <0>, "+102";
+		adv7281ma = <0>, "+103";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/akkordion-iqdacplus-overlay.dts b/arch/arm/boot/dts/overlays/akkordion-iqdacplus-overlay.dts
new file mode 100644
index 000000000000..82f9b3734fb1
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/akkordion-iqdacplus-overlay.dts
@@ -0,0 +1,49 @@
+// Definitions for Digital Dreamtime Akkordion using IQaudIO DAC+ or DACZero
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		frag2: __overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			card_name = "Akkordion";
+			dai_name = "IQaudIO DAC";
+			dai_stream_name = "IQaudIO DAC HiFi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&frag2>,"iqaudio,24db_digital_gain?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/allo-boss-dac-pcm512x-audio-overlay.dts b/arch/arm/boot/dts/overlays/allo-boss-dac-pcm512x-audio-overlay.dts
new file mode 100644
index 000000000000..873cb2fab52b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/allo-boss-dac-pcm512x-audio-overlay.dts
@@ -0,0 +1,59 @@
+/*
+ * Definitions for Allo Boss DAC board
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			boss_osc: boss_osc {
+				compatible = "allo,dac-clk";
+				#clock-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				clocks = <&boss_osc>;
+				reg = <0x4d>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		boss_dac: __overlay__ {
+			compatible = "allo,boss-dac";
+			i2s-controller = <&i2s>;
+			mute-gpios = <&gpio 6 1>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&boss_dac>,"allo,24db_digital_gain?";
+		slave = <&boss_dac>,"allo,slave?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/allo-digione-overlay.dts b/arch/arm/boot/dts/overlays/allo-digione-overlay.dts
new file mode 100644
index 000000000000..ea018ace34d4
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/allo-digione-overlay.dts
@@ -0,0 +1,44 @@
+// Definitions for Allo DigiOne
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+				wlf,reset-gpio = <&gpio 17 0>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "allo,allo-digione";
+			i2s-controller = <&i2s>;
+			status = "okay";
+			clock44-gpio = <&gpio 5 0>;
+			clock48-gpio = <&gpio 6 0>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/allo-katana-dac-audio-overlay.dts b/arch/arm/boot/dts/overlays/allo-katana-dac-audio-overlay.dts
new file mode 100644
index 000000000000..b25fd681f09f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/allo-katana-dac-audio-overlay.dts
@@ -0,0 +1,57 @@
+/*
+ * Definitions for Allo Katana DAC boards
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			#sound-dai-cells = <0>;
+			status = "okay";
+			cpu_port: port {
+				cpu_endpoint: endpoint {
+					remote-endpoint = <&codec_endpoint>;
+					bitclock-master = <&codec_endpoint>;
+					frame-master = <&codec_endpoint>;
+					dai-format = "i2s";
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			allo-katana-codec@30 {
+				#sound-dai-cells = <0>;
+				compatible = "allo,allo-katana-codec";
+				reg = <0x30>;
+				port {
+					codec_endpoint: endpoint {
+					remote-endpoint = <&cpu_endpoint>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		katana_dac: __overlay__ {
+			compatible = "audio-graph-card";
+			label = "Allo Katana";
+			dais = <&cpu_port>;
+			status = "okay";
+		};
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/allo-piano-dac-pcm512x-audio-overlay.dts b/arch/arm/boot/dts/overlays/allo-piano-dac-pcm512x-audio-overlay.dts
new file mode 100644
index 000000000000..bfc66da6295a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/allo-piano-dac-pcm512x-audio-overlay.dts
@@ -0,0 +1,54 @@
+/*
+ * Definitions for Allo Piano DAC (2.0/2.1) boards
+ *
+ * NB. The Piano DAC 2.1 board contains 2x TI PCM5142 DAC's. One DAC is stereo
+ * (left/right) and the other provides a subwoofer output, using DSP on the
+ * chip for digital high/low pass crossover.
+ * The initial support for this hardware, that doesn't require any codec driver
+ * modifications, uses only one DAC chip for stereo (left/right) output, the
+ * chip with 0x4c slave address. The other chip at 0x4d is currently ignored!
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5142@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5142";
+				reg = <0x4c>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		piano_dac: __overlay__ {
+			compatible = "allo,piano-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain =
+			<&piano_dac>,"allo,24db_digital_gain?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/allo-piano-dac-plus-pcm512x-audio-overlay.dts b/arch/arm/boot/dts/overlays/allo-piano-dac-plus-pcm512x-audio-overlay.dts
new file mode 100644
index 000000000000..374c553db062
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/allo-piano-dac-plus-pcm512x-audio-overlay.dts
@@ -0,0 +1,55 @@
+// Definitions for Piano DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			allo_pcm5122_4c: pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				status = "okay";
+			};
+			allo_pcm5122_4d: pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		piano_dac: __overlay__ {
+			compatible = "allo,piano-dac-plus";
+			audio-codec = <&allo_pcm5122_4c &allo_pcm5122_4d>;
+			i2s-controller = <&i2s>;
+			mute1-gpios = <&gpio 6 1>;
+			mute2-gpios = <&gpio 25 1>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain =
+			<&piano_dac>,"allo,24db_digital_gain?";
+		glb_mclk =
+			<&piano_dac>,"allo,glb_mclk?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/anyspi-overlay.dts b/arch/arm/boot/dts/overlays/anyspi-overlay.dts
new file mode 100755
index 000000000000..87523dcca318
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/anyspi-overlay.dts
@@ -0,0 +1,205 @@
+/*
+ * Universal device tree overlay for SPI devices
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target-path = "spi1/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target-path = "spi1/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@4 {
+		target-path = "spi1/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@5 {
+		target-path = "spi2/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@6 {
+		target-path = "spi2/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@7 {
+		target-path = "spi2/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@8 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_00: anyspi@0 {
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_01: anyspi@1 {
+				reg = <1>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@10 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_10: anyspi@0 {
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@11 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_11: anyspi@1 {
+				reg = <1>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@12 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_12: anyspi@2 {
+				reg = <2>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@13 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_20: anyspi@0 {
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@14 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_21: anyspi@1 {
+				reg = <1>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@15 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			anyspi_22: anyspi@2 {
+				reg = <2>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	__overrides__ {
+		spi0-0 = <0>, "+0+8";
+		spi0-1 = <0>, "+1+9";
+		spi1-0 = <0>, "+2+10";
+		spi1-1 = <0>, "+3+11";
+		spi1-2 = <0>, "+4+12";
+		spi2-0 = <0>, "+5+13";
+		spi2-1 = <0>, "+6+14";
+		spi2-2 = <0>, "+7+15";
+		dev = <&anyspi_00>,"compatible",
+		      <&anyspi_01>,"compatible",
+		      <&anyspi_10>,"compatible",
+		      <&anyspi_11>,"compatible",
+		      <&anyspi_12>,"compatible",
+		      <&anyspi_20>,"compatible",
+		      <&anyspi_21>,"compatible",
+		      <&anyspi_22>,"compatible";
+		speed = <&anyspi_00>, "spi-max-frequency:0",
+		        <&anyspi_01>, "spi-max-frequency:0",
+		        <&anyspi_10>, "spi-max-frequency:0",
+		        <&anyspi_11>, "spi-max-frequency:0",
+		        <&anyspi_12>, "spi-max-frequency:0",
+		        <&anyspi_20>, "spi-max-frequency:0",
+		        <&anyspi_21>, "spi-max-frequency:0",
+		        <&anyspi_22>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/apds9960-overlay.dts b/arch/arm/boot/dts/overlays/apds9960-overlay.dts
new file mode 100644
index 000000000000..c216932278ab
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/apds9960-overlay.dts
@@ -0,0 +1,57 @@
+// Definitions for APDS-9960 ambient light and gesture sensor
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			apds9960_pins: apds9960_pins@39 {
+				brcm,pins = <4>;
+				brcm,function = <0>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			apds9960: apds@39 {
+				compatible = "avago,apds9960";
+				reg = <0x39>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c1>;
+		__overlay__ {
+			apds9960_irq: apds@39 {
+				#interrupt-cells=<2>;
+				interrupt-parent = <&gpio>;
+				interrupts = <4 1>;
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin = <&apds9960_pins>,"brcm,pins:0",
+				<&apds9960_irq>,"interrupts:0";
+		noints = <0>,"!1!3";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/applepi-dac-overlay.dts b/arch/arm/boot/dts/overlays/applepi-dac-overlay.dts
new file mode 100644
index 000000000000..4769296ec9d6
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/applepi-dac-overlay.dts
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+
+    fragment@0 {
+        target = <&sound>;
+        __overlay__ {
+            compatible = "simple-audio-card";
+            simple-audio-card,name = "ApplePi-DAC";
+
+            status = "okay";
+
+            playback_link: simple-audio-card,dai-link@1 {
+                format = "i2s";
+
+                p_cpu_dai: cpu {
+                    sound-dai = <&i2s>;
+                    dai-tdm-slot-num = <2>;
+                    dai-tdm-slot-width = <32>;
+                };
+
+                p_codec_dai: codec {
+                    sound-dai = <&codec_out>;
+                };
+            };
+        };
+    };
+
+    fragment@1 {
+        target-path = "/";
+        __overlay__ {
+            codec_out: pcm1794a-codec {
+                #sound-dai-cells = <0>;
+                compatible = "ti,pcm1794a";
+                status = "okay";
+            };
+        };
+    };
+
+    fragment@2 {
+        target = <&i2s>;
+        __overlay__ {
+            #sound-dai-cells = <0>;
+            status = "okay";
+        };
+    };
+};
+
+/*
+   Written by: Leonid Ayzenshtat
+   Company: Orchard Audio (www.orchardaudio.com)
+
+   compile with:
+   dtc -@ -H epapr -O dtb -o ApplePi-DAC.dtbo -W no-unit_address_vs_reg ApplePi-DAC.dts
+*/
diff --git a/arch/arm/boot/dts/overlays/at86rf233-overlay.dts b/arch/arm/boot/dts/overlays/at86rf233-overlay.dts
new file mode 100644
index 000000000000..5a3f4571ee78
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/at86rf233-overlay.dts
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/* Overlay for Atmel AT86RF233 IEEE 802.15.4 WPAN transceiver on spi0.0 */
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			lowpan0: at86rf233@0 {
+				compatible = "atmel,at86rf233";
+				reg = <0>;
+				interrupt-parent = <&gpio>;
+				interrupts = <23 4>; /* active high */
+				reset-gpio = <&gpio 24 1>;
+				sleep-gpio = <&gpio 25 1>;
+				spi-max-frequency = <3000000>;
+				xtal-trim = /bits/ 8 <0xf>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			lowpan0_pins: lowpan0_pins {
+				brcm,pins = <23 24 25>;
+				brcm,function = <0 1 1>; /* in out out */
+			};
+		};
+	};
+
+	__overrides__ {
+		interrupt = <&lowpan0>, "interrupts:0",
+			<&lowpan0_pins>, "brcm,pins:0";
+		reset     = <&lowpan0>, "reset-gpio:4",
+			<&lowpan0_pins>, "brcm,pins:4";
+		sleep     = <&lowpan0>, "sleep-gpio:4",
+			<&lowpan0_pins>, "brcm,pins:8";
+		speed     = <&lowpan0>, "spi-max-frequency:0";
+		trim      = <&lowpan0>, "xtal-trim.0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/audioinjector-addons-overlay.dts b/arch/arm/boot/dts/overlays/audioinjector-addons-overlay.dts
new file mode 100644
index 000000000000..57a66eac8e9b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/audioinjector-addons-overlay.dts
@@ -0,0 +1,60 @@
+// Definitions for audioinjector.net audio add on soundcard
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			cs42448_mclk: codec-mclk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <49152000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			cs42448: cs42448@48 {
+				#sound-dai-cells = <0>;
+				compatible = "cirrus,cs42448";
+				reg = <0x48>;
+				clocks = <&cs42448_mclk>;
+				clock-names = "mclk";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		snd: __overlay__ {
+			compatible = "ai,audioinjector-octo-soundcard";
+			mult-gpios = <&gpio 27 0>, <&gpio 22 0>, <&gpio 23 0>,
+				     <&gpio 24 0>;
+			reset-gpios = <&gpio 5 0>;
+			i2s-controller = <&i2s>;
+			codec = <&cs42448>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		non-stop-clocks = <&snd>, "non-stop-clocks?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/audioinjector-isolated-soundcard-overlay.dts b/arch/arm/boot/dts/overlays/audioinjector-isolated-soundcard-overlay.dts
new file mode 100644
index 000000000000..63e05cf9665d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/audioinjector-isolated-soundcard-overlay.dts
@@ -0,0 +1,55 @@
+// Definitions for audioinjector.net audio isolated soundcard
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			cs4272_mclk: codec-mclk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <24576000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			cs4272: cs4271@10 {
+				#sound-dai-cells = <0>;
+				compatible = "cirrus,cs4271";
+				reg = <0x10>;
+				reset-gpio = <&gpio 5 0>;
+				clocks = <&cs4272_mclk>;
+				clock-names = "mclk";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		snd: __overlay__ {
+			compatible = "ai,audioinjector-isolated-soundcard";
+			mute-gpios = <&gpio 17 0>;
+			i2s-controller = <&i2s>;
+			codec = <&cs4272>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/audioinjector-ultra-overlay.dts b/arch/arm/boot/dts/overlays/audioinjector-ultra-overlay.dts
new file mode 100644
index 000000000000..fb4a4678a17a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/audioinjector-ultra-overlay.dts
@@ -0,0 +1,71 @@
+// Definitions for audioinjector.net audio add on soundcard
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			cs4265: cs4265@4e {
+				#sound-dai-cells = <0>;
+				compatible = "cirrus,cs4265";
+				reg = <0x4e>;
+				reset-gpios = <&gpio 5 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "simple-audio-card";
+			i2s-controller = <&i2s>;
+			status = "okay";
+
+			simple-audio-card,name = "audioinjector-ultra";
+
+			simple-audio-card,widgets =
+				"Line", "OUTPUTS",
+				"Line", "INPUTS";
+
+			simple-audio-card,routing =
+				"OUTPUTS","LINEOUTL",
+				"OUTPUTS","LINEOUTR",
+				"OUTPUTS","SPDIFOUT",
+				"LINEINL","INPUTS",
+				"LINEINR","INPUTS",
+				"MICL","INPUTS",
+				"MICR","INPUTS";
+
+			simple-audio-card,format = "i2s";
+
+			simple-audio-card,bitclock-master = <&sound_master>;
+			simple-audio-card,frame-master = <&sound_master>;
+
+			simple-audio-card,cpu {
+				sound-dai = <&i2s>;
+				dai-tdm-slot-num = <2>;
+				dai-tdm-slot-width = <32>;
+			};
+
+			sound_master: simple-audio-card,codec {
+				sound-dai = <&cs4265>;
+				system-clock-frequency = <12288000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/audioinjector-wm8731-audio-overlay.dts b/arch/arm/boot/dts/overlays/audioinjector-wm8731-audio-overlay.dts
new file mode 100644
index 000000000000..68f4427d86c3
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/audioinjector-wm8731-audio-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for audioinjector.net audio add on soundcard
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8731@1a {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8731";
+				reg = <0x1a>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "ai,audioinjector-pi-soundcard";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/audiosense-pi-overlay.dts b/arch/arm/boot/dts/overlays/audiosense-pi-overlay.dts
new file mode 100644
index 000000000000..81af26374d92
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/audiosense-pi-overlay.dts
@@ -0,0 +1,82 @@
+// Definitions for audiosense add on soundcard
+/dts-v1/;
+/plugin/;
+#include <dt-bindings/pinctrl/bcm2835.h>
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			codec_reg_1v8: codec-reg-1v8 {
+				compatible = "regulator-fixed";
+				regulator-name = "tlv320aic3204_1v8";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+			};
+
+			/* audio external oscillator */
+			codec_osc: codec_osc {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <12000000>;	/* 12 MHz */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			codec_rst: codec-rst {
+				brcm,pins = <26>;
+				brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			codec: tlv320aic32x4@18 {
+				#sound-dai-cells = <0>;
+				compatible = "ti,tlv320aic32x4";
+				reg = <0x18>;
+
+				clocks = <&codec_osc>;
+				clock-names = "mclk";
+
+				iov-supply = <&vdd_3v3_reg>;
+				ldoin-supply = <&vdd_3v3_reg>;
+
+				gpio-controller;
+				#gpio-cells = <2>;
+				reset-gpios = <&gpio 26 GPIO_ACTIVE_HIGH>;
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "as,audiosense-pi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/audremap-overlay.dts b/arch/arm/boot/dts/overlays/audremap-overlay.dts
new file mode 100644
index 000000000000..d624bb3a3fea
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/audremap-overlay.dts
@@ -0,0 +1,35 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+        compatible = "brcm,bcm2835";
+
+        fragment@0 {
+                target = <&audio_pins>;
+                frag0: __overlay__ {
+                };
+        };
+
+	fragment@1 {
+                target = <&audio_pins>;
+                __overlay__ {
+                        brcm,pins = < 12 13 >;
+                        brcm,function = < 4 >; /* alt0 alt0 */
+                };
+        };
+
+	fragment@2 {
+		target = <&audio_pins>;
+		__dormant__ {
+                        brcm,pins = < 18 19 >;
+                        brcm,function = < 2 >; /* alt5 alt5 */
+		};
+	};
+
+	__overrides__ {
+		swap_lr = <&frag0>, "swap_lr?";
+		enable_jack = <&frag0>, "enable_jack?";
+		pins_12_13 = <0>,"+1-2";
+		pins_18_19 = <0>,"-1+2";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/balena-fin-overlay.dts b/arch/arm/boot/dts/overlays/balena-fin-overlay.dts
new file mode 100644
index 000000000000..e7ead7cdf5f5
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/balena-fin-overlay.dts
@@ -0,0 +1,125 @@
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&mmcnr>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&sdio_pins>;
+			bus-width = <4>;
+			brcm,overclock-50 = <35>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			sdio_pins: sdio_pins {
+				brcm,pins = <34 35 36 37 38 39>;
+				brcm,function = <7>; /* ALT3 = SD1 */
+				brcm,pull = <0 2 2 2 2 2>;
+			};
+
+			power_ctrl_pins: power_ctrl_pins {
+				brcm,pins = <40>;
+				brcm,function = <1>; // out
+			};
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			// We should switch to mmc-pwrseq-sd8787 after making it
+			// compatible with sd8887
+			// Currently that module requires two GPIOs to function since it
+			// targets a slightly different chip
+			power_ctrl: power_ctrl {
+				compatible = "gpio-poweroff";
+				gpios = <&gpio 40 1>;
+				force;
+				pinctrl-names = "default";
+				pinctrl-0 = <&power_ctrl_pins>;
+			};
+
+			i2c_soft: i2c@0 {
+				compatible = "i2c-gpio";
+				gpios = <&gpio 43 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN) /* sda */
+				         &gpio 42 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN) /* scl */>;
+				i2c-gpio,delay-us = <5>;
+				i2c-gpio,scl-open-drain;
+				i2c-gpio,sda-open-drain;
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+
+			sd8xxx-wlan {
+				drvdbg = <0x6>;
+				drv_mode = <0x1>;
+				cfg80211_wext = <0xf>;
+				sta_name = "wlan";
+				wfd_name = "p2p";
+				cal_data_cfg = "none";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c_soft>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			gpio_expander: gpio_expander@20 {
+				compatible = "nxp,pca9554";
+				gpio-controller;
+				#gpio-cells = <2>;
+				reg = <0x20>;
+				status = "okay";
+			};
+
+			// rtc clock
+			ds1307: ds1307@68 {
+				compatible = "dallas,ds1307";
+				reg = <0x68>;
+				status = "okay";
+			};
+
+			// RGB LEDs (>= v1.1.0)
+			pca9633: pca9633@62 {
+				compatible = "nxp,pca9633";
+				reg = <0x62>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				red@0 {
+					label = "red";
+					reg = <0>;
+					linux,default-trigger = "none";
+				};
+				green@1 {
+					label = "green";
+					reg = <1>;
+					linux,default-trigger = "none";
+				};
+				blue@2 {
+					label = "blue";
+					reg = <2>;
+					linux,default-trigger = "none";
+				};
+				unused@3 {
+					label = "unused";
+					reg = <3>;
+					linux,default-trigger = "none";
+				};
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/cma-overlay.dts b/arch/arm/boot/dts/overlays/cma-overlay.dts
new file mode 100644
index 000000000000..1d87c599f909
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/cma-overlay.dts
@@ -0,0 +1,36 @@
+/*
+ * cma.dts
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&cma>;
+		frag0: __overlay__ {
+			/*
+			 * The default size when using this overlay is 256 MB
+			 * and should be kept as is for backwards
+			 * compatibility.
+			 */
+			size = <0x10000000>;
+		};
+	};
+
+	__overrides__ {
+		cma-512 = <&frag0>,"size:0=",<0x20000000>;
+		cma-448 = <&frag0>,"size:0=",<0x1c000000>;
+		cma-384 = <&frag0>,"size:0=",<0x18000000>;
+		cma-320 = <&frag0>,"size:0=",<0x14000000>;
+		cma-256 = <&frag0>,"size:0=",<0x10000000>;
+		cma-192 = <&frag0>,"size:0=",<0xC000000>;
+		cma-128 = <&frag0>,"size:0=",<0x8000000>;
+		cma-96  = <&frag0>,"size:0=",<0x6000000>;
+		cma-64  = <&frag0>,"size:0=",<0x4000000>;
+		cma-size = <&frag0>,"size:0"; /* in bytes, 4MB aligned */
+		cma-default = <0>,"-0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/dht11-overlay.dts b/arch/arm/boot/dts/overlays/dht11-overlay.dts
new file mode 100644
index 000000000000..6feeeb402493
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dht11-overlay.dts
@@ -0,0 +1,41 @@
+/*
+ * Overlay for the DHT11/21/22 humidity/temperature sensor modules.
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+
+			dht11: dht11@0 {
+				compatible = "dht11";
+				pinctrl-names = "default";
+				pinctrl-0 = <&dht11_pins>;
+				gpios = <&gpio 4 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			dht11_pins: dht11_pins@0 {
+				brcm,pins = <4>;
+				brcm,function = <0>; // in
+				brcm,pull = <0>; // off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin = <&dht11_pins>,"brcm,pins:0",
+			<&dht11_pins>, "reg:0",
+			<&dht11>,"gpios:4",
+			<&dht11>,"reg:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/dionaudio-loco-overlay.dts b/arch/arm/boot/dts/overlays/dionaudio-loco-overlay.dts
new file mode 100644
index 000000000000..d863e5c167cc
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dionaudio-loco-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for Dion Audio LOCO DAC-AMP
+
+/*
+ * PCM5242 DAC (in hardware mode) and TPA3118 AMP.
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pcm5102a-codec {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5102a";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "dionaudio,loco-pcm5242-tpa3118";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/dionaudio-loco-v2-overlay.dts b/arch/arm/boot/dts/overlays/dionaudio-loco-v2-overlay.dts
new file mode 100644
index 000000000000..dfb8922a654b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dionaudio-loco-v2-overlay.dts
@@ -0,0 +1,49 @@
+/*
+ * Definitions for Dion Audio LOCO-V2 DAC-AMP
+ *  eg. dtoverlay=dionaudio-loco-v2
+ *
+ * PCM5242 DAC (in software mode) and TPA3255 AMP.
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&sound>;
+		frag0: __overlay__ {
+			compatible = "dionaudio,dionaudio-loco-v2";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&frag0>,"dionaudio,24db_digital_gain?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/disable-bt-overlay.dts b/arch/arm/boot/dts/overlays/disable-bt-overlay.dts
new file mode 100644
index 000000000000..d5a66e5d76a9
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/disable-bt-overlay.dts
@@ -0,0 +1,64 @@
+/dts-v1/;
+/plugin/;
+
+/* Disable Bluetooth and restore UART0/ttyAMA0 over GPIOs 14 & 15.
+   To disable the systemd service that initialises the modem so it doesn't use
+   the UART:
+
+       sudo systemctl disable hciuart
+*/
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&uart1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&bt>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&uart0_pins>;
+		__overlay__ {
+			brcm,pins;
+			brcm,function;
+			brcm,pull;
+		};
+	};
+
+	fragment@4 {
+		target = <&bt_pins>;
+		__overlay__ {
+			brcm,pins;
+			brcm,function;
+			brcm,pull;
+		};
+	};
+
+	fragment@5 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial0 = "/soc/serial@7e201000";
+			serial1 = "/soc/serial@7e215040";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/disable-wifi-overlay.dts b/arch/arm/boot/dts/overlays/disable-wifi-overlay.dts
new file mode 100644
index 000000000000..75e046463900
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/disable-wifi-overlay.dts
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&mmc>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&mmcnr>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/dpi18-overlay.dts b/arch/arm/boot/dts/overlays/dpi18-overlay.dts
new file mode 100644
index 000000000000..4abe5be744db
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dpi18-overlay.dts
@@ -0,0 +1,39 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	// There is no DPI driver module, but we need a platform device
+	// node (that doesn't already use pinctrl) to hang the pinctrl
+	// reference on - leds will do
+
+	fragment@0 {
+		target = <&fb>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&dpi18_pins>;
+		};
+	};
+
+	fragment@1 {
+		target = <&vc4>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&dpi18_pins>;
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			dpi18_pins: dpi18_pins {
+				brcm,pins = <0 1 2 3 4 5 6 7 8 9 10 11
+					     12 13 14 15 16 17 18 19 20
+					     21>;
+				brcm,function = <6>; /* alt2 */
+				brcm,pull = <0>; /* no pull */
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/dpi24-overlay.dts b/arch/arm/boot/dts/overlays/dpi24-overlay.dts
new file mode 100644
index 000000000000..44335cc81277
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dpi24-overlay.dts
@@ -0,0 +1,39 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	// There is no DPI driver module, but we need a platform device
+	// node (that doesn't already use pinctrl) to hang the pinctrl
+	// reference on - leds will do
+
+	fragment@0 {
+		target = <&fb>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&dpi24_pins>;
+		};
+	};
+
+	fragment@1 {
+		target = <&vc4>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&dpi24_pins>;
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			dpi24_pins: dpi24_pins {
+				brcm,pins = <0 1 2 3 4 5 6 7 8 9 10 11
+					     12 13 14 15 16 17 18 19 20
+					     21 22 23 24 25 26 27>;
+				brcm,function = <6>; /* alt2 */
+				brcm,pull = <0>; /* no pull */
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/draws-overlay.dts b/arch/arm/boot/dts/overlays/draws-overlay.dts
new file mode 100644
index 000000000000..d18187d7f343
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/draws-overlay.dts
@@ -0,0 +1,208 @@
+#include <dt-bindings/clock/bcm2835.h>
+/*
+ * Device tree overlay for the DRAWS Hardware
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+    fragment@0 {
+        target = <&i2s>;
+        __overlay__ {
+            status = "okay";
+        };
+    };
+
+    fragment@1 {
+        target-path = "/";
+        __overlay__ {
+            regulators {
+                compatible = "simple-bus";
+                #address-cells = <1>;
+                #size-cells = <0>;
+
+                udrc0_ldoin: udrc0_ldoin {
+                    compatible = "regulator-fixed";
+                    regulator-name = "ldoin";
+                    regulator-min-microvolt = <3300000>;
+                    regulator-max-microvolt = <3300000>;
+                    regulator-always-on;
+                };
+
+                sc16is752_clk: sc16is752_draws_clk {
+                    compatible = "fixed-clock";
+                    #clock-cells = <0>;
+                    clock-frequency = <1843200>;
+                };
+            };
+
+            pps: pps {
+                compatible = "pps-gpio";
+                pinctrl-names = "default";
+                pinctrl-0 = <&pps_pins>;
+                gpios = <&gpio 7 0>;
+                status = "okay";
+            };
+
+            iio-hwmon {
+                compatible = "iio-hwmon";
+                status = "okay";
+                io-channels = <&tla2024 4>, <&tla2024 5>, <&tla2024 6>,
+                              <&tla2024 7>;
+            };
+        };
+    };
+
+    fragment@2 {
+        target = <&i2c_arm>;
+        __overlay__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            status = "okay";
+
+            tlv320aic32x4: tlv320aic32x4@18 {
+                compatible = "ti,tlv320aic32x4";
+                reg = <0x18>;
+                #sound-dai-cells = <0>;
+                status = "okay";
+
+                clocks = <&clocks BCM2835_CLOCK_GP0>;
+                clock-names = "mclk";
+                assigned-clocks = <&clocks BCM2835_CLOCK_GP0>;
+                assigned-clock-rates = <25000000>;
+
+                pinctrl-names = "default";
+                pinctrl-0 = <&gpclk0_pin &aic3204_reset>;
+
+                reset-gpios = <&gpio 13 0>;
+
+                iov-supply = <&udrc0_ldoin>;
+                ldoin-supply = <&udrc0_ldoin>;
+            };
+
+            sc16is752: sc16is752@50 {
+                compatible = "nxp,sc16is752";
+                reg = <0x50>;
+                clocks = <&sc16is752_clk>;
+                interrupt-parent = <&gpio>;
+                interrupts = <17 2>; /* IRQ_TYPE_EDGE_FALLING */
+
+                pinctrl-names = "default";
+                pinctrl-0 = <&sc16is752_irq>;
+            };
+
+            tla2024: tla2024@48 {
+                compatible = "ti,ads1015";
+                reg = <0x48>;
+                #address-cells = <1>;
+                #size-cells = <0>;
+                #io-channel-cells = <1>;
+
+                adc_ch4: channel@4 {
+                    reg = <4>;
+                    ti,gain = <1>;
+                    ti,datarate = <4>;
+                };
+
+                adc_ch5: channel@5 {
+                    reg = <5>;
+                    ti,gain = <1>;
+                    ti,datarate = <4>;
+                };
+
+                adc_ch6: channel@6 {
+                    reg = <6>;
+                    ti,gain = <2>;
+                    ti,datarate = <4>;
+                };
+
+                adc_ch7: channel@7 {
+                    reg = <7>;
+                    ti,gain = <2>;
+                    ti,datarate = <4>;
+                };
+            };
+        };
+    };
+
+    fragment@3 {
+        target = <&sound>;
+        snd: __overlay__ {
+            compatible = "simple-audio-card";
+            i2s-controller = <&i2s>;
+            status = "okay";
+
+            simple-audio-card,name = "draws";
+            simple-audio-card,format = "i2s";
+
+            simple-audio-card,bitclock-master = <&dailink0_master>;
+            simple-audio-card,frame-master = <&dailink0_master>;
+
+            simple-audio-card,widgets =
+                "Line", "Line In",
+                "Line", "Line Out";
+
+            simple-audio-card,routing =
+                "IN1_R", "Line In",
+                "IN1_L", "Line In",
+                "CM_L", "Line In",
+                "CM_R", "Line In",
+                "Line Out", "LOR",
+                "Line Out", "LOL";
+
+            dailink0_master: simple-audio-card,cpu {
+                sound-dai = <&i2s>;
+            };
+
+            simple-audio-card,codec {
+                sound-dai = <&tlv320aic32x4>;
+            };
+        };
+    };
+
+    fragment@4 {
+        target = <&gpio>;
+        __overlay__ {
+            gpclk0_pin: gpclk0_pin {
+                brcm,pins = <4>;
+                brcm,function = <4>;
+            };
+
+            aic3204_reset: aic3204_reset {
+                brcm,pins = <13>;
+                brcm,function = <1>;
+                brcm,pull = <1>;
+            };
+
+            aic3204_gpio: aic3204_gpio {
+                brcm,pins = <26>;
+            };
+
+            sc16is752_irq: sc16is752_irq {
+                brcm,pins = <17>;
+                brcm,function = <0>;
+                brcm,pull = <2>;
+            };
+
+            pps_pins: pps_pins {
+                brcm,pins = <7>;
+                brcm,function = <0>;
+                brcm,pull = <0>;
+            };
+        };
+    };
+
+    __overrides__ {
+        draws_adc_ch4_gain = <&adc_ch4>,"ti,gain:0";
+        draws_adc_ch4_datarate = <&adc_ch4>,"ti,datarate:0";
+        draws_adc_ch5_gain = <&adc_ch5>,"ti,gain:0";
+        draws_adc_ch5_datarate = <&adc_ch5>,"ti,datarate:0";
+        draws_adc_ch6_gain = <&adc_ch6>,"ti,gain:0";
+        draws_adc_ch6_datarate = <&adc_ch6>,"ti,datarate:0";
+        draws_adc_ch7_gain = <&adc_ch7>,"ti,gain:0";
+        draws_adc_ch7_datarate = <&adc_ch7>,"ti,datarate:0";
+        alsaname = <&snd>, "simple-audio-card,name";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/dwc-otg-overlay.dts b/arch/arm/boot/dts/overlays/dwc-otg-overlay.dts
new file mode 100644
index 000000000000..78c5e9f85048
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dwc-otg-overlay.dts
@@ -0,0 +1,14 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&usb>;
+		__overlay__ {
+			compatible = "brcm,bcm2708-usb";
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/dwc2-overlay.dts b/arch/arm/boot/dts/overlays/dwc2-overlay.dts
new file mode 100644
index 000000000000..0d83e344ad97
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/dwc2-overlay.dts
@@ -0,0 +1,26 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&usb>;
+		#address-cells = <1>;
+		#size-cells = <1>;
+		dwc2_usb: __overlay__ {
+			compatible = "brcm,bcm2835-usb";
+			dr_mode = "otg";
+			g-np-tx-fifo-size = <32>;
+			g-rx-fifo-size = <558>;
+			g-tx-fifo-size = <512 512 512 512 512 256 256>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		dr_mode = <&dwc2_usb>, "dr_mode";
+		g-np-tx-fifo-size = <&dwc2_usb>,"g-np-tx-fifo-size:0";
+		g-rx-fifo-size = <&dwc2_usb>,"g-rx-fifo-size:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/enc28j60-overlay.dts b/arch/arm/boot/dts/overlays/enc28j60-overlay.dts
new file mode 100644
index 000000000000..7af5c2e607ea
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/enc28j60-overlay.dts
@@ -0,0 +1,53 @@
+// Overlay for the Microchip ENC28J60 Ethernet Controller
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			eth1: enc28j60@0{
+				compatible = "microchip,enc28j60";
+				reg = <0>; /* CE0 */
+				pinctrl-names = "default";
+				pinctrl-0 = <&eth1_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <25 0x2>; /* falling edge */
+				spi-max-frequency = <12000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			eth1_pins: eth1_pins {
+				brcm,pins = <25>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&eth1>, "interrupts:0",
+		          <&eth1_pins>, "brcm,pins:0";
+		speed   = <&eth1>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/enc28j60-spi2-overlay.dts b/arch/arm/boot/dts/overlays/enc28j60-spi2-overlay.dts
new file mode 100644
index 000000000000..17cb5b8fa485
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/enc28j60-spi2-overlay.dts
@@ -0,0 +1,47 @@
+// Overlay for the Microchip ENC28J60 Ethernet Controller - SPI2 Compute Module
+// Interrupt pin: 39
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi2>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			eth1: enc28j60@0{
+				compatible = "microchip,enc28j60";
+				reg = <0>; /* CE0 */
+				pinctrl-names = "default";
+				pinctrl-0 = <&eth1_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <39 0x2>; /* falling edge */
+				spi-max-frequency = <12000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			eth1_pins: eth1_pins {
+				brcm,pins = <39>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&eth1>, "interrupts:0",
+		          <&eth1_pins>, "brcm,pins:0";
+		speed   = <&eth1>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/exc3000-overlay.dts b/arch/arm/boot/dts/overlays/exc3000-overlay.dts
new file mode 100644
index 000000000000..6f087fb20661
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/exc3000-overlay.dts
@@ -0,0 +1,48 @@
+// Device tree overlay for I2C connected EETI EXC3000 multiple touch controller
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			exc3000_pins: exc3000_pins {
+				brcm,pins = <4>; // interrupt
+				brcm,function = <0>; // in
+				brcm,pull = <2>; // pull-up
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			exc3000: exc3000@2a {
+				compatible = "eeti,exc3000";
+				reg = <0x2a>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&exc3000_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <4 8>; // active low level-sensitive
+				touchscreen-size-x = <4096>;
+				touchscreen-size-y = <4096>;
+			};
+		};
+	};
+
+	__overrides__ {
+		interrupt = <&exc3000_pins>,"brcm,pins:0",
+			<&exc3000>,"interrupts:0";
+		sizex = <&exc3000>,"touchscreen-size-x:0";
+		sizey = <&exc3000>,"touchscreen-size-y:0";
+		invx = <&exc3000>,"touchscreen-inverted-x?";
+		invy = <&exc3000>,"touchscreen-inverted-y?";
+		swapxy = <&exc3000>,"touchscreen-swapped-x-y?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts b/arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts
new file mode 100644
index 000000000000..743f14ae5768
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/fe-pi-audio-overlay.dts
@@ -0,0 +1,70 @@
+// Definitions for Fe-Pi Audio
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			sgtl5000_mclk: sgtl5000_mclk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <12288000>;
+				clock-output-names = "sgtl5000-mclk";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&soc>;
+		__overlay__ {
+			reg_1v8: reg_1v8@0 {
+				compatible = "regulator-fixed";
+				regulator-name = "1V8";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sgtl5000@0a {
+				#sound-dai-cells = <0>;
+				compatible = "fsl,sgtl5000";
+				reg = <0x0a>;
+				clocks = <&sgtl5000_mclk>;
+				micbias-resistor-k-ohms = <2>;
+				micbias-voltage-m-volts = <3000>;
+				VDDA-supply = <&vdd_3v3_reg>;
+				VDDIO-supply = <&vdd_3v3_reg>;
+				VDDD-supply = <&reg_1v8>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "fe-pi,fe-pi-audio";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/fsm-demo-overlay.dts b/arch/arm/boot/dts/overlays/fsm-demo-overlay.dts
new file mode 100644
index 000000000000..9e06e388e4d3
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/fsm-demo-overlay.dts
@@ -0,0 +1,104 @@
+// Demo overlay for the gpio-fsm driver
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio-fsm.h>
+
+#define BUTTON1 GF_IP(0)
+#define BUTTON2 GF_SW(0)
+#define RED   GF_OP(0) // GPIO7
+#define AMBER GF_OP(1) // GPIO8
+#define GREEN GF_OP(2) // GPIO25
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			fsm_demo: fsm-demo {
+				compatible = "rpi,gpio-fsm";
+
+				debug = <0>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				num-soft-gpios = <1>;
+				gpio-line-names = "button2";
+				input-gpios  = <&gpio 6 1>;  // BUTTON1 (active-low)
+				output-gpios = <&gpio 7 0>,  // RED
+					       <&gpio 8 0>,  // AMBER
+					       <&gpio 25 0>; // GREEN
+				shutdown-timeout-ms = <2000>;
+
+				start {
+					start_state;
+					set = <RED 1>, <AMBER 0>, <GREEN 0>;
+					start2 = <GF_DELAY 250>;
+				};
+
+				start2 {
+					set = <RED 0>, <AMBER 1>;
+					go = <GF_DELAY 250>;
+				};
+
+				go {
+					set = <RED 0>, <AMBER 0>, <GREEN 1>;
+					ready_wait = <BUTTON1 0>;
+					shutdown1 = <GF_SHUTDOWN 0>;
+				};
+
+				ready_wait {
+					// Clear the soft GPIO
+					set = <BUTTON2 0>;
+					ready = <GF_DELAY 1000>;
+					shutdown1 = <GF_SHUTDOWN 0>;
+				};
+
+				ready {
+					stopping = <BUTTON1 1>, <BUTTON2 1>;
+					shutdown1 = <GF_SHUTDOWN 0>;
+				};
+
+				stopping {
+					set = <GREEN 0>, <AMBER 1>;
+					stopped = <GF_DELAY 1000>;
+				};
+
+				stopped {
+					set = <AMBER 0>, <RED 1>;
+					get_set = <GF_DELAY 3000>;
+					shutdown1 = <GF_SHUTDOWN 0>;
+				};
+
+				get_set {
+					set = <AMBER 1>;
+					go = <GF_DELAY 1000>;
+				};
+
+				shutdown1 {
+					set = <RED 0>, <AMBER 0>, <GREEN 1>;
+					shutdown2 = <GF_SHUTDOWN 250>;
+				};
+
+				shutdown2 {
+					set = <AMBER 1>, <GREEN 0>;
+					shutdown3 = <GF_SHUTDOWN 250>;
+				};
+
+				shutdown3 {
+					set = <RED 1>, <AMBER 0>;
+					shutdown4 = <GF_SHUTDOWN 250>;
+				};
+
+				shutdown4 {
+					shutdown_state;
+					set = <RED 0>;
+				};
+			};
+	       };
+        };
+
+	__overrides__ {
+		fsm_debug = <&fsm_demo>,"debug:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ghost-amp-overlay.dts b/arch/arm/boot/dts/overlays/ghost-amp-overlay.dts
new file mode 100644
index 000000000000..afc9f034b5fc
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ghost-amp-overlay.dts
@@ -0,0 +1,119 @@
+// Overlay for the PCM5122-based Ghost amplifier using gpio-fsm
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio-fsm.h>
+
+#define ENABLE GF_SW(0)
+#define FAULT  GF_IP(0) // GPIO5
+#define RELAY1 GF_OP(0) // GPIO22
+#define RELAY2 GF_OP(1) // GPIO23
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		iqaudio_dac: __overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			i2s-controller = <&i2s>;
+			mute-gpios = <&amp 0 0>;
+			iqaudio-dac,auto-mute-amp;
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path = "/";
+		__overlay__ {
+			amp: ghost-amp {
+				compatible = "rpi,gpio-fsm";
+
+				debug = <0>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				num-soft-gpios = <1>;
+				gpio-line-names = "enable";
+				input-gpios  = <&gpio 5 1>;  // FAULT (active low)
+				output-gpios = <&gpio 22 0>, // RELAY1
+					       <&gpio 23 0>; // RELAY2
+				shutdown-timeout-ms = <1000>;
+
+				amp_off {
+					start_state;
+					shutdown_state;
+
+					set = <RELAY2 0>,
+					      <RELAY1 0>;
+					amp_on_1 = <ENABLE 1>;
+					fault = <FAULT 1>;
+				};
+
+				amp_on_1 {
+					set = <RELAY1 1>;
+					amp_on = <GF_DELAY 1500>;
+					amp_off = <ENABLE 0>;
+					fault = <FAULT 1>;
+				};
+
+				amp_on {
+					set = <RELAY2 1>;
+					amp_off_wait = <ENABLE 0>;
+					fault = <FAULT 1>;
+				};
+
+				amp_off_wait {
+					amp_off_1 = <GF_DELAY (30*60*1000)>,
+						    <GF_SHUTDOWN 0>;
+					amp_on = <ENABLE 1>;
+					fault = <FAULT 1>;
+				};
+
+				amp_off_1 {
+					set = <RELAY2 0>;
+					amp_on = <ENABLE 1>;
+					amp_off = <GF_DELAY 100>;
+					fault = <FAULT 1>;
+				};
+
+				// Keep this a distinct state to prevent
+				// changes and for the diagnostic output
+				fault {
+					set = <RELAY2 0>,
+					      <RELAY1 0>;
+					shutdown_state;
+				};
+			};
+		};
+	};
+
+	__overrides__ {
+		fsm_debug = <&amp>,"debug:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/goodix-overlay.dts b/arch/arm/boot/dts/overlays/goodix-overlay.dts
new file mode 100644
index 000000000000..a11d65f81c5e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/goodix-overlay.dts
@@ -0,0 +1,46 @@
+// Device tree overlay for I2C connected Goodix gt9271 multiple touch controller
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			goodix_pins: goodix_pins {
+				brcm,pins = <4 17>; // interrupt and reset
+				brcm,function = <0 0>; // in
+				brcm,pull = <2 2>; // pull-up
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			gt9271: gt9271@14 {
+				compatible = "goodix,gt9271";
+				reg = <0x14>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&goodix_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <4 2>; // high-to-low edge triggered
+				irq-gpios = <&gpio 4 0>; // Pin7 on GPIO header
+				reset-gpios = <&gpio 17 1>; // Pin11 on GPIO header
+			};
+		};
+	};
+
+	__overrides__ {
+		interrupt = <&goodix_pins>,"brcm,pins:0",
+			<&gt9271>,"interrupts:0",
+			<&gt9271>,"irq-gpios:4";
+		reset = <&goodix_pins>,"brcm,pins:4",
+			<&gt9271>,"reset-gpios:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/googlevoicehat-soundcard-overlay.dts b/arch/arm/boot/dts/overlays/googlevoicehat-soundcard-overlay.dts
new file mode 100644
index 000000000000..e443be1f9a0e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/googlevoicehat-soundcard-overlay.dts
@@ -0,0 +1,49 @@
+// Definitions for Google voiceHAT v1 soundcard overlay
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			googlevoicehat_pins: googlevoicehat_pins {
+				brcm,pins = <16>;
+				brcm,function = <1>; /* out */
+				brcm,pull = <0>; /* up */
+			};
+		};
+	};
+
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			voicehat-codec {
+				#sound-dai-cells = <0>;
+				compatible = "google,voicehat";
+				pinctrl-names = "default";
+				pinctrl-0 = <&googlevoicehat_pins>;
+				sdmode-gpios= <&gpio 16 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "googlevoicehat,googlevoicehat-soundcard";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-fan-overlay.dts b/arch/arm/boot/dts/overlays/gpio-fan-overlay.dts
new file mode 100644
index 000000000000..77a7bbb41e3b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-fan-overlay.dts
@@ -0,0 +1,79 @@
+/*
+ * Overlay for the Raspberry Pi GPIO Fan @ BCM GPIO12.
+ * References: 
+ *	- https://www.raspberrypi.org/forums/viewtopic.php?f=107&p=1367135#p1365084
+ *
+ * Optional parameters:
+ *	- "gpiopin"	- BCM number of the pin driving the fan, default 12 (GPIO12);
+ * 	- "temp"	- CPU temperature at which fan is started in millicelsius, default 55000;
+ *
+ * Requires:
+ *	- kernel configurations: CONFIG_SENSORS_GPIO_FAN=m;
+ *	- kernel rebuild;
+ *	- N-MOSFET connected to gpiopin, 2N7002-[https://en.wikipedia.org/wiki/2N7000];
+ *	- DC Fan connected to N-MOSFET Drain terminal, a 12V fan is working fine and quite silently;
+ *	  [https://www.tme.eu/en/details/ee40101s1-999-a/dc12v-fans/sunon/ee40101s1-1000u-999/]
+ *
+ *                   ┌─────────────────────┐
+ *                   │Fan negative terminal│
+ *                   └┬────────────────────┘
+ *                    │D
+ *             G   │──┘
+ * [GPIO12]──────┤ │<─┐  2N7002
+ *                 │──┤
+ *                    │S
+ *                   ─┴─
+ *                   GND
+ *
+ * Build:
+ * 	- `sudo dtc -W no-unit_address_vs_reg -@ -I dts -O dtb -o /boot/overlays/gpio-fan.dtbo gpio-fan-overlay.dts`
+ * Activate:
+ *	- sudo nano /boot/config.txt add "dtoverlay=gpio-fan" or "dtoverlay=gpio-fan,gpiopin=12,temp=45000"
+ *	 or
+ *	- sudo sh -c 'printf "\n# Enable PI GPIO-Fan Default\ndtoverlay=gpio-fan\n" >> /boot/config.txt'
+ *	- sudo sh -c 'printf "\n# Enable PI GPIO-Fan Custom\ndtoverlay=gpio-fan,gpiopin=12,temp=45000\n" >> /boot/config.txt'
+ *
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			fan0: gpio-fan@0 {
+				compatible = "gpio-fan";
+				gpios = <&gpio 12 0>;
+				gpio-fan,speed-map = <0    0>,
+									 <5000 1>;
+				#cooling-cells = <2>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&cpu_thermal>;
+		polling-delay = <2000>;	/* milliseconds */
+		__overlay__ {
+			trips {
+				cpu_hot: trip-point@0 {
+					temperature = <55000>;	/* (millicelsius) Fan started at 55°C */
+					hysteresis = <10000>;	/* (millicelsius) Fan stopped at 45°C */
+					type = "active";
+				};
+			};
+			cooling-maps {
+				map0 {
+					trip = <&cpu_hot>;
+					cooling-device = <&fan0 1 1>;
+				};
+			};
+		};
+	};
+	__overrides__ {
+		gpiopin = <&fan0>,"gpios:4", <&fan0>,"brcm,pins:0";
+		temp = <&cpu_hot>,"temperature:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts b/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
new file mode 100644
index 000000000000..162b6ce07dc9
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
@@ -0,0 +1,49 @@
+// Definitions for ir-gpio module
+/dts-v1/;
+/plugin/;
+
+/ {
+        compatible = "brcm,bcm2835";
+
+        fragment@0 {
+                target-path = "/";
+                __overlay__ {
+                        gpio_ir: ir-receiver@12 {
+                                compatible = "gpio-ir-receiver";
+                                pinctrl-names = "default";
+                                pinctrl-0 = <&gpio_ir_pins>;
+
+                                // pin number, high or low
+                                gpios = <&gpio 18 1>;
+
+                                // parameter for keymap name
+                                linux,rc-map-name = "rc-rc6-mce";
+
+                                status = "okay";
+                        };
+                };
+        };
+
+        fragment@1 {
+                target = <&gpio>;
+                __overlay__ {
+                        gpio_ir_pins: gpio_ir_pins@12 {
+                                brcm,pins = <18>;                       // pin 18
+                                brcm,function = <0>;                    // in
+                                brcm,pull = <2>;                        // up
+                        };
+                };
+        };
+
+        __overrides__ {
+                // parameters
+                gpio_pin =      <&gpio_ir>,"gpios:4",           // pin number
+                                <&gpio_ir>,"reg:0",
+                                <&gpio_ir_pins>,"brcm,pins:0",
+                                <&gpio_ir_pins>,"reg:0";
+                gpio_pull = <&gpio_ir_pins>,"brcm,pull:0";              // pull-up/down state
+                invert = <&gpio_ir>,"gpios:8";                          // 0 = active high input
+
+                rc-map-name = <&gpio_ir>,"linux,rc-map-name";           // default rc map
+        };
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-ir-tx-overlay.dts b/arch/arm/boot/dts/overlays/gpio-ir-tx-overlay.dts
new file mode 100644
index 000000000000..3625431b7560
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-ir-tx-overlay.dts
@@ -0,0 +1,36 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			gpio_ir_tx_pins: gpio_ir_tx_pins@12 {
+				brcm,pins = <18>;
+				brcm,function = <1>;	// out
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			gpio_ir_tx: gpio-ir-transmitter@12 {
+				compatible = "gpio-ir-tx";
+				pinctrl-names = "default";
+				pinctrl-0 = <&gpio_ir_tx_pins>;
+				gpios = <&gpio 18 0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		gpio_pin = <&gpio_ir_tx>, "gpios:4",           	// pin number
+			   <&gpio_ir_tx>, "reg:0",
+			   <&gpio_ir_tx_pins>, "brcm,pins:0",
+			   <&gpio_ir_tx_pins>, "reg:0";
+		invert = <&gpio_ir_tx>, "gpios:8";		// 1 = active low
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-key-overlay.dts b/arch/arm/boot/dts/overlays/gpio-key-overlay.dts
new file mode 100644
index 000000000000..2e7253d1d0ab
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-key-overlay.dts
@@ -0,0 +1,48 @@
+// Definitions for gpio-key module
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		// Configure the gpio pin controller
+		target = <&gpio>;
+		__overlay__ {
+			pin_state: button_pins@0 {
+				brcm,pins = <3>; // gpio number
+				brcm,function = <0>; // 0 = input, 1 = output
+				brcm,pull = <2>; // 0 = none, 1 = pull down, 2 = pull up
+			};
+		};
+	};
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			button: button@0 {
+				compatible = "gpio-keys";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pin_state>;
+				status = "okay";
+
+				key: key {
+					linux,code = <116>;
+					gpios = <&gpio 3 1>;
+					label = "KEY_POWER";
+				};
+			};
+		};
+	};
+
+	__overrides__ {
+		gpio =       <&key>,"gpios:4",
+		             <&button>,"reg:0",
+		             <&pin_state>,"brcm,pins:0",
+		             <&pin_state>,"reg:0";
+		label =      <&key>,"label";
+		keycode =    <&key>,"linux,code:0";
+		gpio_pull =  <&pin_state>,"brcm,pull:0";
+		active_low = <&key>,"gpios:8";
+	};
+
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-no-bank0-irq-overlay.dts b/arch/arm/boot/dts/overlays/gpio-no-bank0-irq-overlay.dts
new file mode 100755
index 000000000000..96cbe80820b7
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-no-bank0-irq-overlay.dts
@@ -0,0 +1,14 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		// Configure the gpio pin controller
+		target = <&gpio>;
+		__overlay__ {
+			    interrupts = <255 255>, <2 18>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-no-irq-overlay.dts b/arch/arm/boot/dts/overlays/gpio-no-irq-overlay.dts
new file mode 100644
index 000000000000..55f9bff3a8f6
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-no-irq-overlay.dts
@@ -0,0 +1,14 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		// Configure the gpio pin controller
+		target = <&gpio>;
+		__overlay__ {
+			    interrupts;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-poweroff-overlay.dts b/arch/arm/boot/dts/overlays/gpio-poweroff-overlay.dts
new file mode 100644
index 000000000000..416aa2bc797a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-poweroff-overlay.dts
@@ -0,0 +1,37 @@
+// Definitions for gpio-poweroff module
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			power_ctrl: power_ctrl {
+				compatible = "gpio-poweroff";
+				gpios = <&gpio 26 0>;
+				force;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			power_ctrl_pins: power_ctrl_pins {
+				brcm,pins = <26>;
+				brcm,function = <1>; // out
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin =       <&power_ctrl>,"gpios:4",
+				<&power_ctrl_pins>,"brcm,pins:0";
+		active_low =    <&power_ctrl>,"gpios:8";
+		input =         <&power_ctrl>,"input?";
+		export =        <&power_ctrl>,"export?";
+		timeout_ms =    <&power_ctrl>,"timeout-ms:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/gpio-shutdown-overlay.dts b/arch/arm/boot/dts/overlays/gpio-shutdown-overlay.dts
new file mode 100644
index 000000000000..0a27595143ec
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/gpio-shutdown-overlay.dts
@@ -0,0 +1,84 @@
+// Definitions for gpio-poweroff module
+/dts-v1/;
+/plugin/;
+
+// This overlay sets up an input device that generates KEY_POWER events
+// when a given GPIO pin changes. It defaults to using GPIO3, which can
+// also be used to wake up (start) the Rpi again after shutdown.
+// Raspberry Pi 1 Model B rev 1 can be wake up only by GPIO1 pin, so for
+// these boards change default GPIO pin to 1 via gpio_pin parameter. Since
+// wakeup is active-low, this defaults to active-low with a pullup
+// enabled, but all of this can be changed using overlay parameters (but
+// note that GPIO3 has an external pullup on at least some boards).
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		// Configure the gpio pin controller
+		target = <&gpio>;
+		__overlay__ {
+			// Define a pinctrl state, that sets up the gpio
+			// as an input with a pullup enabled. This does
+			// not take effect by itself, only when referenced
+			// by a "pinctrl client", as is done below. See:
+			//   https://www.kernel.org/doc/Documentation/devicetree/bindings/pinctrl/pinctrl-bindings.txt
+			//   https://www.kernel.org/doc/Documentation/devicetree/bindings/pinctrl/brcm,bcm2835-gpio.txt
+			pin_state: shutdown_button_pins {
+				brcm,pins = <3>; // gpio number
+				brcm,function = <0>; // 0 = input, 1 = output
+				brcm,pull = <2>; // 0 = none, 1 = pull down, 2 = pull up
+			};
+		};
+	};
+	fragment@1 {
+		// Add a new device to the /soc devicetree node
+		target-path = "/soc";
+		__overlay__ {
+			shutdown_button {
+				// Let the gpio-keys driver handle this device. See:
+				// https://www.kernel.org/doc/Documentation/devicetree/bindings/input/gpio-keys.txt
+				compatible = "gpio-keys";
+
+				// Declare a single pinctrl state (referencing the one declared above) and name it
+				// default, so it is activated automatically.
+				pinctrl-names = "default";
+				pinctrl-0 = <&pin_state>;
+
+				// Enable this device
+				status = "okay";
+
+				// Define a single key, called "shutdown" that monitors the gpio and sends KEY_POWER
+				// (keycode 116, see
+				// https://github.com/torvalds/linux/blob/v4.12/include/uapi/linux/input-event-codes.h#L190)
+				button: shutdown {
+					label = "shutdown";
+					linux,code = <116>; // KEY_POWER
+					gpios = <&gpio 3 1>;
+					debounce-interval = <100>; // ms
+				};
+			};
+		};
+	};
+
+	// This defines parameters that can be specified when loading
+	// the overlay. Each foo = line specifies one parameter, named
+	// foo. The rest of the specification gives properties where the
+	// parameter value is inserted into (changing the values above
+	// or adding new ones).
+	__overrides__ {
+		// Allow overriding the GPIO number.
+		gpio_pin = <&button>,"gpios:4",
+		           <&pin_state>,"brcm,pins:0";
+
+		// Allow changing the internal pullup/down state. 0 = none, 1 = pulldown, 2 = pullup
+		// Note that GPIO3 and GPIO2 are the I2c pins and have an external pullup (at least
+		// on some boards). Same applies for GPIO1 on Raspberry Pi 1 Model B rev 1.
+		gpio_pull = <&pin_state>,"brcm,pull:0";
+
+		// Allow setting the active_low flag. 0 = active high, 1 = active low
+		active_low = <&button>,"gpios:8";
+		debounce = <&button>,"debounce-interval:0";
+	};
+
+};
diff --git a/arch/arm/boot/dts/overlays/hd44780-lcd-overlay.dts b/arch/arm/boot/dts/overlays/hd44780-lcd-overlay.dts
new file mode 100644
index 000000000000..ee726669ff51
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hd44780-lcd-overlay.dts
@@ -0,0 +1,46 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+
+    fragment@0 {
+        target-path = "/";
+        __overlay__ {
+            lcd_screen: auxdisplay {
+                compatible = "hit,hd44780";
+
+                data-gpios = <&gpio 6 0>,
+                             <&gpio 13 0>,
+                             <&gpio 19 0>,
+                             <&gpio 26 0>;
+                enable-gpios = <&gpio 21 0>;
+                rs-gpios = <&gpio 20 0>;
+
+                display-height-chars = <2>;
+                display-width-chars = <16>;
+            };
+
+        };
+    };
+
+    fragment@1 {
+       target = <&lcd_screen>;
+        __dormant__ {
+            backlight-gpios = <&gpio 12 0>;
+        };
+    };
+
+    __overrides__ {
+        pin_d4 = <&lcd_screen>,"data-gpios:4";
+        pin_d5 = <&lcd_screen>,"data-gpios:16";
+        pin_d6 = <&lcd_screen>,"data-gpios:28";
+        pin_d7 = <&lcd_screen>,"data-gpios:40";
+        pin_en = <&lcd_screen>,"enable-gpios:4";
+        pin_rs = <&lcd_screen>,"rs-gpios:4";
+        pin_bl = <0>,"+1", <&lcd_screen>,"backlight-gpios:4";
+        display_height = <&lcd_screen>,"display-height-chars:0";
+        display_width = <&lcd_screen>,"display-width-chars:0";
+    };
+
+};
diff --git a/arch/arm/boot/dts/overlays/hdmi-backlight-hwhack-gpio-overlay.dts b/arch/arm/boot/dts/overlays/hdmi-backlight-hwhack-gpio-overlay.dts
new file mode 100644
index 000000000000..50b9a2665c80
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hdmi-backlight-hwhack-gpio-overlay.dts
@@ -0,0 +1,47 @@
+/*
+ * Devicetree overlay for GPIO based backlight on/off capability.
+ *
+ * Use this if you have one of those HDMI displays whose backlight cannot be
+ * controlled via DPMS over HDMI and plan to do a little soldering to use an
+ * RPi gpio pin for on/off switching.
+ *
+ * See: https://www.waveshare.com/wiki/7inch_HDMI_LCD_(C)#Backlight_Control
+ *
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			hdmi_backlight_hwhack_gpio_pins: hdmi_backlight_hwhack_gpio_pins {
+				brcm,pins = <17>;
+				brcm,function = <1>; /* out */
+			};
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			hdmi_backlight_hwhack_gpio: hdmi_backlight_hwhack_gpio {
+				compatible = "gpio-backlight";
+
+				pinctrl-names = "default";
+				pinctrl-0 = <&hdmi_backlight_hwhack_gpio_pins>;
+
+				gpios = <&gpio 17 0>;
+				default-on;
+			};
+		};
+	};
+
+	__overrides__ {
+		gpio_pin   = <&hdmi_backlight_hwhack_gpio>,"gpios:4",
+		             <&hdmi_backlight_hwhack_gpio_pins>,"brcm,pins:0";
+		active_low = <&hdmi_backlight_hwhack_gpio>,"gpios:8";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-amp-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-amp-overlay.dts
new file mode 100644
index 000000000000..142518ab348b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-amp-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for HiFiBerry Amp/Amp+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			tas5713@1b {
+				#sound-dai-cells = <0>;
+				compatible = "ti,tas5713";
+				reg = <0x1b>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-amp";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
new file mode 100644
index 000000000000..ea8a6c8f36c0
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dac-overlay.dts
@@ -0,0 +1,34 @@
+// Definitions for HiFiBerry DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pcm5102a-codec {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5102a";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-dacplus-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-dacplus-overlay.dts
new file mode 100644
index 000000000000..ff19015ba656
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dacplus-overlay.dts
@@ -0,0 +1,65 @@
+// Definitions for HiFiBerry DAC+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			dacpro_osc: dacpro_osc {
+				compatible = "hifiberry,dacpro-clk";
+				#clock-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				clocks = <&dacpro_osc>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+			hpamp: hpamp@60 {
+				compatible = "ti,tpa6130a2";
+				reg = <0x60>;
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		hifiberry_dacplus: __overlay__ {
+			compatible = "hifiberry,hifiberry-dacplus";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain =
+			<&hifiberry_dacplus>,"hifiberry,24db_digital_gain?";
+		slave = <&hifiberry_dacplus>,"hifiberry-dacplus,slave?";
+		leds_off = <&hifiberry_dacplus>,"hifiberry-dacplus,leds_off?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-dacplusadc-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-dacplusadc-overlay.dts
new file mode 100644
index 000000000000..540563dec10f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dacplusadc-overlay.dts
@@ -0,0 +1,72 @@
+// Definitions for HiFiBerry DAC+ADC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			dacpro_osc: dacpro_osc {
+				compatible = "hifiberry,dacpro-clk";
+				#clock-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm_codec: pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				clocks = <&dacpro_osc>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target-path = "/";
+		__overlay__ {
+			dmic {
+				#sound-dai-cells = <0>;
+				compatible = "dmic-codec";
+				num-channels = <2>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&sound>;
+		hifiberry_dacplusadc: __overlay__ {
+			compatible = "hifiberry,hifiberry-dacplusadc";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain =
+			<&hifiberry_dacplusadc>,"hifiberry,24db_digital_gain?";
+		slave = <&hifiberry_dacplusadc>,"hifiberry-dacplusadc,slave?";
+		leds_off = <&hifiberry_dacplusadc>,"hifiberry-dacplusadc,leds_off?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-dacplusadcpro-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-dacplusadcpro-overlay.dts
new file mode 100644
index 000000000000..cafa2ccd7ff7
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dacplusadcpro-overlay.dts
@@ -0,0 +1,65 @@
+// Definitions for HiFiBerry DAC+ADC PRO
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			dacpro_osc: dacpro_osc {
+				compatible = "hifiberry,dacpro-clk";
+				#clock-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			hb_dac: pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				clocks = <&dacpro_osc>;
+				status = "okay";
+			};
+			hb_adc: pcm186x@4a {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm1863";
+				reg = <0x4a>;
+				clocks = <&dacpro_osc>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		hifiberry_dacplusadcpro: __overlay__ {
+			compatible = "hifiberry,hifiberry-dacplusadcpro";
+			audio-codec = <&hb_dac &hb_adc>;
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain =
+			<&hifiberry_dacplusadcpro>,"hifiberry-dacplusadcpro,24db_digital_gain?";
+		slave = <&hifiberry_dacplusadcpro>,"hifiberry-dacplusadcpro,slave?";
+		leds_off = <&hifiberry_dacplusadcpro>,"hifiberry-dacplusadcpro,leds_off?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-dacplusdsp-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-dacplusdsp-overlay.dts
new file mode 100644
index 000000000000..63432e8b983f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dacplusdsp-overlay.dts
@@ -0,0 +1,34 @@
+// Definitions for hifiberry DAC+DSP soundcard overlay
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			dacplusdsp-codec {
+				#sound-dai-cells = <0>;
+				compatible = "hifiberry,dacplusdsp";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberrydacplusdsp,hifiberrydacplusdsp-soundcard";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-dacplushd-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-dacplushd-overlay.dts
new file mode 100644
index 000000000000..c5583e010339
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-dacplushd-overlay.dts
@@ -0,0 +1,106 @@
+// Definitions for HiFiBerry DAC+ HD
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			dachd_osc: pll_dachd_osc {
+				compatible = "hifiberry,dachd-clk";
+				#clock-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm1792a@4c {
+				compatible = "ti,pcm1792a";
+				#sound-dai-cells = <0>;
+				#clock-cells = <0>;
+				clocks = <&dachd_osc>;
+				reg = <0x4c>;
+				status = "okay";
+			};
+			pll: pll@62 {
+				compatible = "hifiberry,dachd-clk";
+				#clock-cells = <0>;
+				reg = <0x62>;
+				clocks = <&dachd_osc>;
+				status = "okay";
+				common_pll_regs = [
+					02 53 03 00 07 20 0F 00
+					10 0D 11 1D 12 0D 13 8C
+					14 8C 15 8C 16 8C 17 8C
+					18 2A 1C 00 1D 0F 1F 00
+					2A 00 2C 00 2F 00 30 00
+					31 00 32 00 34 00 37 00
+					38 00 39 00 3A 00 3B 01
+					3E 00 3F 00 40 00 41 00
+					5A 00 5B 00 95 00 96 00
+					97 00 98 00 99 00 9A 00
+					9B 00 A2 00 A3 00 A4 00
+					B7 92 ];
+				192k_pll_regs = [
+					1A 0C 1B 35 1E F0 20 09
+					21 50 2B 02 2D 10 2E 40
+					33 01 35 22 36 80 3C 22
+					3D 46 ];
+				96k_pll_regs = [
+					1A 0C 1B 35 1E F0 20 09
+					21 50 2B 02 2D 10 2E 40
+					33 01 35 47 36 00 3C 32
+					3D 46 ];
+				48k_pll_regs = [
+					1A 0C 1B 35 1E F0 20 09
+					21 50 2B 02 2D 10 2E 40
+					33 01 35 90 36 00 3C 42
+					3D 46 ];
+				176k4_pll_regs = [
+					1A 3D 1B 09 1E F3 20 13
+					21 75 2B 04 2D 11 2E E0
+					33 02 35 25 36 C0 3C 22
+					3D 7A ];
+				88k2_pll_regs = [
+					1A 3D 1B 09 1E F3 20 13
+					21 75 2B 04 2D 11 2E E0
+					33 01 35 4D 36 80 3C 32
+					3D 7A ];
+				44k1_pll_regs = [
+					1A 3D 1B 09 1E F3 20 13
+					21 75 2B 04 2D 11 2E E0
+					33 01 35 9D 36 00 3C 42
+					3D 7A ];
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-dacplushd";
+			i2s-controller = <&i2s>;
+			clocks = <&pll 0>;
+			reset-gpio = <&gpio 16 GPIO_ACTIVE_LOW>;
+			status = "okay";
+		};
+	};
+
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-digi-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-digi-overlay.dts
new file mode 100644
index 000000000000..a2309a50e8d8
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-digi-overlay.dts
@@ -0,0 +1,41 @@
+// Definitions for HiFiBerry Digi
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-digi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hifiberry-digi-pro-overlay.dts b/arch/arm/boot/dts/overlays/hifiberry-digi-pro-overlay.dts
new file mode 100644
index 000000000000..83de602e76ba
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hifiberry-digi-pro-overlay.dts
@@ -0,0 +1,43 @@
+// Definitions for HiFiBerry Digi Pro
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "hifiberry,hifiberry-digi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+			clock44-gpio = <&gpio 5 0>;
+			clock48-gpio = <&gpio 6 0>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/highperi-overlay.dts b/arch/arm/boot/dts/overlays/highperi-overlay.dts
new file mode 100644
index 000000000000..46cb76c2d34f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/highperi-overlay.dts
@@ -0,0 +1,63 @@
+/*
+ * highperi.dts
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&soc>;
+		#address-cells = <2>;
+		#size-cells = <1>;
+
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0x7c000000  0x4 0x7c000000  0x04000000>,
+				 <0x40000000  0x4 0xc0000000  0x00800000>;
+		};
+	};
+
+	fragment@1 {
+		target = <&scb>;
+		#address-cells = <2>;
+		#size-cells = <1>;
+
+		__overlay__ {
+			#address-cells = <2>;
+			#size-cells = <2>;
+			ranges = <0x0 0x7c000000  0x4 0x7c000000  0x0 0x04000000>,
+				 <0x0 0x40000000  0x4 0xc0000000  0x0 0x00800000>,
+				 <0x6 0x00000000  0x6 0x00000000  0x0 0x40000000>;
+			dma-ranges = <0x0 0x00000000  0x0 0x00000000  0x2 0x00000000>;
+		};
+	};
+
+	fragment@2 {
+		target = <&v3dbus>;
+		#address-cells = <2>;
+		#size-cells = <1>;
+
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <2>;
+			ranges = <0x7c500000  0x4 0x7c500000  0x0 0x03300000>,
+				 <0x40000000  0x4 0xc0000000  0x0 0x00800000>;
+		};
+	};
+
+	fragment@3 {
+		target = <&emmc2bus>;
+		#address-cells = <2>;
+		#size-cells = <1>;
+
+		__overlay__ {
+			#address-cells = <2>;
+			#size-cells = <1>;
+			ranges = <0x0 0x7e000000  0x4 0x7e000000  0x01800000>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hy28a-overlay.dts b/arch/arm/boot/dts/overlays/hy28a-overlay.dts
new file mode 100644
index 000000000000..5843a5e9c86a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hy28a-overlay.dts
@@ -0,0 +1,93 @@
+/*
+ * Device Tree overlay for HY28A display
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			hy28a_pins: hy28a_pins {
+				brcm,pins = <17 25 18>;
+				brcm,function = <0 1 1>; /* in out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			hy28a: hy28a@0{
+				compatible = "ilitek,ili9320";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&hy28a_pins>;
+
+				spi-max-frequency = <32000000>;
+				spi-cpol;
+				spi-cpha;
+				rotate = <270>;
+				bgr;
+				fps = <50>;
+				buswidth = <8>;
+				startbyte = <0x70>;
+				reset-gpios = <&gpio 25 1>;
+				led-gpios = <&gpio 18 1>;
+				debug = <0>;
+			};
+
+			hy28a_ts: hy28a-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =		<&hy28a>,"spi-max-frequency:0";
+		rotate =	<&hy28a>,"rotate:0";
+		fps =		<&hy28a>,"fps:0";
+		debug =		<&hy28a>,"debug:0";
+		xohms =		<&hy28a_ts>,"ti,x-plate-ohms;0";
+		resetgpio =	<&hy28a>,"reset-gpios:4",
+				<&hy28a_pins>, "brcm,pins:4";
+		ledgpio =	<&hy28a>,"led-gpios:4",
+				<&hy28a_pins>, "brcm,pins:8";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hy28b-2017-overlay.dts b/arch/arm/boot/dts/overlays/hy28b-2017-overlay.dts
new file mode 100644
index 000000000000..95bfb1eadc20
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hy28b-2017-overlay.dts
@@ -0,0 +1,152 @@
+/*
+ * Device Tree overlay for HY28b display shield by Texy.
+ * Modified for 2017 version with ILI9325 D chip
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			hy28b_pins: hy28b_pins {
+				brcm,pins = <17 25 18>;
+				brcm,function = <0 1 1>; /* in out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			hy28b: hy28b@0{
+				compatible = "ilitek,ili9325";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&hy28b_pins>;
+
+				spi-max-frequency = <48000000>;
+				spi-cpol;
+				spi-cpha;
+				rotate = <270>;
+				bgr;
+				fps = <50>;
+				buswidth = <8>;
+				startbyte = <0x70>;
+				reset-gpios = <&gpio 25 1>;
+				led-gpios = <&gpio 18 1>;
+
+				init = <0x10000e5 0x78F0
+					0x1000001 0x0100
+					0x1000002 0x0700
+				        0x1000003 0x1030
+					0x1000004 0x0000
+					0x1000008 0x0207
+					0x1000009 0x0000
+				        0x100000a 0x0000
+					0x100000c 0x0000
+					0x100000d 0x0000
+					0x100000f 0x0000
+				        0x1000010 0x0000
+					0x1000011 0x0007
+					0x1000012 0x0000
+					0x1000013 0x0000
+					0x1000007 0x0001
+				        0x2000032
+				        0x2000032
+				        0x2000032
+				        0x2000032
+					0x1000010 0x1090
+					0x1000011 0x0227
+				        0x2000032
+					0x1000012 0x001f
+				        0x2000032
+				        0x1000013 0x1500
+					0x1000029 0x0027
+					0x100002b 0x000d
+				        0x2000032
+				        0x1000020 0x0000
+					0x1000021 0x0000
+				        0x2000032
+					0x1000030 0x0000
+					0x1000031 0x0707
+					0x1000032 0x0307
+					0x1000035 0x0200
+					0x1000036 0x0008
+					0x1000037 0x0004
+					0x1000038 0x0000
+					0x1000039 0x0707
+					0x100003c 0x0002
+					0x100003d 0x1d04
+					0x1000050 0x0000
+				        0x1000051 0x00ef
+					0x1000052 0x0000
+					0x1000053 0x013f
+					0x1000060 0xa700
+				        0x1000061 0x0001
+					0x100006a 0x0000
+					0x1000080 0x0000
+					0x1000081 0x0000
+				        0x1000082 0x0000
+					0x1000083 0x0000
+					0x1000084 0x0000
+					0x1000085 0x0000
+				        0x1000090 0x0010
+					0x1000092 0x0600
+					0x1000007 0x0133>;
+				debug = <0>;
+			};
+
+			hy28b_ts: hy28b-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed = 	<&hy28b>,"spi-max-frequency:0";
+		rotate = 	<&hy28b>,"rotate:0";
+		fps = 		<&hy28b>,"fps:0";
+		debug = 	<&hy28b>,"debug:0";
+		xohms =		<&hy28b_ts>,"ti,x-plate-ohms;0";
+		resetgpio =	<&hy28b>,"reset-gpios:4",
+				<&hy28b_pins>, "brcm,pins:4";
+		ledgpio =	<&hy28b>,"led-gpios:4",
+				<&hy28b_pins>, "brcm,pins:8";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/hy28b-overlay.dts b/arch/arm/boot/dts/overlays/hy28b-overlay.dts
new file mode 100644
index 000000000000..9edd0848d555
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/hy28b-overlay.dts
@@ -0,0 +1,148 @@
+/*
+ * Device Tree overlay for HY28b display shield by Texy
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			hy28b_pins: hy28b_pins {
+				brcm,pins = <17 25 18>;
+				brcm,function = <0 1 1>; /* in out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			hy28b: hy28b@0{
+				compatible = "ilitek,ili9325";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&hy28b_pins>;
+
+				spi-max-frequency = <48000000>;
+				spi-cpol;
+				spi-cpha;
+				rotate = <270>;
+				bgr;
+				fps = <50>;
+				buswidth = <8>;
+				startbyte = <0x70>;
+				reset-gpios = <&gpio 25 1>;
+				led-gpios = <&gpio 18 1>;
+
+				gamma = "04 1F 4 7 7 0 7 7 6 0\n0F 00 1 7 4 0 0 0 6 7";
+
+				init = <0x10000e7 0x0010
+					0x1000000 0x0001
+					0x1000001 0x0100
+					0x1000002 0x0700
+				        0x1000003 0x1030
+					0x1000004 0x0000
+					0x1000008 0x0207
+					0x1000009 0x0000
+				        0x100000a 0x0000
+					0x100000c 0x0001
+					0x100000d 0x0000
+					0x100000f 0x0000
+				        0x1000010 0x0000
+					0x1000011 0x0007
+					0x1000012 0x0000
+					0x1000013 0x0000
+				        0x2000032
+					0x1000010 0x1590
+					0x1000011 0x0227
+				        0x2000032
+					0x1000012 0x009c
+				        0x2000032
+				        0x1000013 0x1900
+					0x1000029 0x0023
+					0x100002b 0x000e
+				        0x2000032
+				        0x1000020 0x0000
+					0x1000021 0x0000
+				        0x2000032
+					0x1000050 0x0000
+				        0x1000051 0x00ef
+					0x1000052 0x0000
+					0x1000053 0x013f
+					0x1000060 0xa700
+				        0x1000061 0x0001
+					0x100006a 0x0000
+					0x1000080 0x0000
+					0x1000081 0x0000
+				        0x1000082 0x0000
+					0x1000083 0x0000
+					0x1000084 0x0000
+					0x1000085 0x0000
+				        0x1000090 0x0010
+					0x1000092 0x0000
+					0x1000093 0x0003
+					0x1000095 0x0110
+				        0x1000097 0x0000
+					0x1000098 0x0000
+					0x1000007 0x0133
+					0x1000020 0x0000
+				        0x1000021 0x0000
+				        0x2000064>;
+				debug = <0>;
+			};
+
+			hy28b_ts: hy28b-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed = 	<&hy28b>,"spi-max-frequency:0";
+		rotate = 	<&hy28b>,"rotate:0";
+		fps = 		<&hy28b>,"fps:0";
+		debug = 	<&hy28b>,"debug:0";
+		xohms =		<&hy28b_ts>,"ti,x-plate-ohms;0";
+		resetgpio =	<&hy28b>,"reset-gpios:4",
+				<&hy28b_pins>, "brcm,pins:4";
+		ledgpio =	<&hy28b>,"led-gpios:4",
+				<&hy28b_pins>, "brcm,pins:8";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i-sabre-q2m-overlay.dts b/arch/arm/boot/dts/overlays/i-sabre-q2m-overlay.dts
new file mode 100644
index 000000000000..0c4cff354674
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i-sabre-q2m-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for I-Sabre Q2M
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&sound>;
+		frag0: __overlay__ {
+			compatible = "audiophonics,i-sabre-q2m";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			i-sabre-codec@48 {
+				#sound-dai-cells = <0>;
+				compatible = "audiophonics,i-sabre-codec";
+				reg = <0x48>;
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-bcm2708-overlay.dts b/arch/arm/boot/dts/overlays/i2c-bcm2708-overlay.dts
new file mode 100644
index 000000000000..8204b6b3aef8
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-bcm2708-overlay.dts
@@ -0,0 +1,13 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			compatible = "brcm,bcm2708-i2c";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts b/arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts
new file mode 100644
index 000000000000..63231b5d7c0c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-gpio-overlay.dts
@@ -0,0 +1,47 @@
+// Overlay for i2c_gpio bitbanging host bus.
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+
+		__overlay__ {
+			i2c_gpio: i2c@0 {
+				reg = <0xffffffff>;
+				compatible = "i2c-gpio";
+				gpios = <&gpio 23 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN) /* sda */
+					 &gpio 24 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN) /* scl */
+					>;
+				i2c-gpio,delay-us = <2>;        /* ~100 kHz */
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c_gpio = "/i2c@0";
+		};
+	};
+
+	fragment@2 {
+		target-path = "/__symbols__";
+		__overlay__ {
+			i2c_gpio = "/i2c@0";
+		};
+	};
+
+	__overrides__ {
+		i2c_gpio_sda = <&i2c_gpio>,"gpios:4";
+		i2c_gpio_scl = <&i2c_gpio>,"gpios:16";
+		i2c_gpio_delay_us = <&i2c_gpio>,"i2c-gpio,delay-us:0";
+		bus = <&i2c_gpio>, "reg:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-mux-overlay.dts b/arch/arm/boot/dts/overlays/i2c-mux-overlay.dts
new file mode 100644
index 000000000000..112aed91ecb2
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-mux-overlay.dts
@@ -0,0 +1,139 @@
+// Umbrella I2C Mux overlay
+
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pca9542: mux@70 {
+				compatible = "nxp,pca9542";
+				reg = <0x70>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				i2c@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+				};
+				i2c@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pca9545: mux@70 {
+				compatible = "nxp,pca9545";
+				reg = <0x70>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				i2c@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+				};
+				i2c@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+				i2c@2 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <2>;
+				};
+				i2c@3 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <3>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pca9548: mux@70 {
+				compatible = "nxp,pca9548";
+				reg = <0x70>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				i2c@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+				};
+				i2c@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+				i2c@2 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <2>;
+				};
+				i2c@3 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <3>;
+				};
+				i2c@4 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <4>;
+				};
+				i2c@5 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <5>;
+				};
+				i2c@6 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <6>;
+				};
+				i2c@7 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <7>;
+				};
+			};
+		};
+	};
+
+	__overrides__ {
+		pca9542 = <0>, "+0";
+		pca9545 = <0>, "+1";
+		pca9548 = <0>, "+2";
+
+		addr =  <&pca9542>,"reg:0",
+			<&pca9545>,"reg:0",
+			<&pca9548>,"reg:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts b/arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts
new file mode 100644
index 000000000000..9bb16465a50e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts
@@ -0,0 +1,26 @@
+// Definitions for NXP PCA9685A I2C PWM controller on ARM I2C bus.
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pca: pca@40 {
+				compatible = "nxp,pca9685-pwm";
+				#pwm-cells = <2>;
+				reg = <0x40>;
+				status = "okay";
+			};
+		};
+	};
+	__overrides__ {
+		addr = <&pca>,"reg:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-rtc-gpio-overlay.dts b/arch/arm/boot/dts/overlays/i2c-rtc-gpio-overlay.dts
new file mode 100644
index 000000000000..227e3c0fa1cd
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-rtc-gpio-overlay.dts
@@ -0,0 +1,266 @@
+// Definitions for several I2C based Real Time Clocks
+// Available through i2c-gpio
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			i2c_gpio: i2c-gpio-rtc@0 {
+				compatible = "i2c-gpio";
+				gpios = <&gpio 23 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN) /* sda */
+					 &gpio 24 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN) /* scl */
+					>;
+				i2c-gpio,delay-us = <2>;        /* ~100 kHz */
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			abx80x: abx80x@69 {
+				compatible = "abracon,abx80x";
+				reg = <0x69>;
+				abracon,tc-diode = "standard";
+				abracon,tc-resistor = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds1307: ds1307@68 {
+				compatible = "dallas,ds1307";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds1339: ds1339@68 {
+				compatible = "dallas,ds1339";
+				trickle-resistor-ohms = <0>;
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds3231: ds3231@68 {
+				compatible = "maxim,ds3231";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@5 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			mcp7940x: mcp7940x@6f {
+				compatible = "microchip,mcp7940x";
+				reg = <0x6f>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@6 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			mcp7941x: mcp7941x@6f {
+				compatible = "microchip,mcp7941x";
+				reg = <0x6f>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf2127@51 {
+				compatible = "nxp,pcf2127";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@8 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf8523: pcf8523@68 {
+				compatible = "nxp,pcf8523";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf8563: pcf8563@51 {
+				compatible = "nxp,pcf8563";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@10 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			m41t62: m41t62@68 {
+				compatible = "st,m41t62";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@11 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rv3028: rv3028@52 {
+				compatible = "microcrystal,rv3028";
+				reg = <0x52>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@12 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf2129@51 {
+				compatible = "nxp,pcf2129";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@13 {
+		target = <&i2c_gpio>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rv1805: rv1805@69 {
+				compatible = "microcrystal,rv1805";
+				reg = <0x69>;
+				abracon,tc-diode = "standard";
+				abracon,tc-resistor = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		abx80x = <0>,"+1";
+		ds1307 = <0>,"+2";
+		ds1339 = <0>,"+3";
+		ds3231 = <0>,"+4";
+		mcp7940x = <0>,"+5";
+		mcp7941x = <0>,"+6";
+		pcf2127 = <0>,"+7";
+		pcf8523 = <0>,"+8";
+		pcf8563 = <0>,"+9";
+		m41t62 = <0>,"+10";
+		rv3028 = <0>,"+11";
+		pcf2129 = <0>,"+12";
+		rv1805 = <0>,"+13";
+
+		addr = <&abx80x>, "reg:0",
+		       <&ds1307>, "reg:0",
+		       <&ds1339>, "reg:0",
+		       <&ds3231>, "reg:0",
+		       <&mcp7940x>, "reg:0",
+		       <&mcp7941x>, "reg:0",
+		       <&pcf8523>, "reg:0",
+		       <&pcf8563>, "reg:0",
+		       <&m41t62>, "reg:0",
+		       <&rv1805>, "reg:0";
+		trickle-diode-type = <&abx80x>,"abracon,tc-diode",
+				     <&rv1805>,"abracon,tc-diode";
+		trickle-resistor-ohms = <&ds1339>,"trickle-resistor-ohms:0",
+					<&abx80x>,"abracon,tc-resistor:0",
+					<&rv3028>,"trickle-resistor-ohms:0",
+					<&rv1805>,"abracon,tc-resistor:0";
+		backup-switchover-mode = <&rv3028>,"backup-switchover-mode:0";
+		wakeup-source = <&ds1339>,"wakeup-source?",
+				<&ds3231>,"wakeup-source?",
+				<&mcp7940x>,"wakeup-source?",
+				<&mcp7941x>,"wakeup-source?";
+		i2c_gpio_sda = <&i2c_gpio>,"gpios:4";
+		i2c_gpio_scl = <&i2c_gpio>,"gpios:16";
+		i2c_gpio_delay_us = <&i2c_gpio>,"i2c-gpio,delay-us:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts b/arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts
new file mode 100644
index 000000000000..735ca303e4fa
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-rtc-overlay.dts
@@ -0,0 +1,278 @@
+// Definitions for several I2C based Real Time Clocks
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			abx80x: abx80x@69 {
+				compatible = "abracon,abx80x";
+				reg = <0x69>;
+				abracon,tc-diode = "standard";
+				abracon,tc-resistor = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds1307: ds1307@68 {
+				compatible = "dallas,ds1307";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds1339: ds1339@68 {
+				compatible = "dallas,ds1339";
+				trickle-resistor-ohms = <0>;
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds3231: ds3231@68 {
+				compatible = "maxim,ds3231";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			mcp7940x: mcp7940x@6f {
+				compatible = "microchip,mcp7940x";
+				reg = <0x6f>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@5 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			mcp7941x: mcp7941x@6f {
+				compatible = "microchip,mcp7941x";
+				reg = <0x6f>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@6 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf2127@51 {
+				compatible = "nxp,pcf2127";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf8523: pcf8523@68 {
+				compatible = "nxp,pcf8523";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@8 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf8563: pcf8563@51 {
+				compatible = "nxp,pcf8563";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			m41t62: m41t62@68 {
+				compatible = "st,m41t62";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@10 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rv3028: rv3028@52 {
+				compatible = "microcrystal,rv3028";
+				reg = <0x52>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@11 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf2129@51 {
+				compatible = "nxp,pcf2129";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@12 {
+		target = <&i2c_arm>;
+	       __dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcf85363@51 {
+				compatible = "nxp,pcf85363";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@13 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rv1805: rv1805@69 {
+				compatible = "microcrystal,rv1805";
+				reg = <0x69>;
+				abracon,tc-diode = "standard";
+				abracon,tc-resistor = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@14 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sd3078: sd3078@32 {
+				compatible = "whwave,sd3078";
+				reg = <0x32>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		abx80x = <0>,"+0";
+		ds1307 = <0>,"+1";
+		ds1339 = <0>,"+2";
+		ds3231 = <0>,"+3";
+		mcp7940x = <0>,"+4";
+		mcp7941x = <0>,"+5";
+		pcf2127 = <0>,"+6";
+		pcf8523 = <0>,"+7";
+		pcf8563 = <0>,"+8";
+		m41t62 = <0>,"+9";
+		rv3028 = <0>,"+10";
+		pcf2129 = <0>,"+11";
+		pcf85363 = <0>,"+12";
+		rv1805 = <0>,"+13";
+		sd3078 = <0>,"+14";
+
+		addr = <&abx80x>, "reg:0",
+		       <&ds1307>, "reg:0",
+		       <&ds1339>, "reg:0",
+		       <&ds3231>, "reg:0",
+		       <&mcp7940x>, "reg:0",
+		       <&mcp7941x>, "reg:0",
+		       <&pcf8523>, "reg:0",
+		       <&pcf8563>, "reg:0",
+		       <&m41t62>, "reg:0",
+		       <&rv1805>, "reg:0";
+		trickle-diode-type = <&abx80x>,"abracon,tc-diode",
+				     <&rv1805>,"abracon,tc-diode";
+		trickle-resistor-ohms = <&ds1339>,"trickle-resistor-ohms:0",
+					<&abx80x>,"abracon,tc-resistor:0",
+					<&rv3028>,"trickle-resistor-ohms:0",
+					<&rv1805>,"abracon,tc-resistor:0";
+		backup-switchover-mode = <&rv3028>,"backup-switchover-mode:0";
+		wakeup-source = <&ds1339>,"wakeup-source?",
+				<&ds3231>,"wakeup-source?",
+				<&mcp7940x>,"wakeup-source?",
+				<&mcp7941x>,"wakeup-source?",
+				<&m41t62>,"wakeup-source?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c-sensor-overlay.dts b/arch/arm/boot/dts/overlays/i2c-sensor-overlay.dts
new file mode 100644
index 000000000000..ce97837b0db5
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c-sensor-overlay.dts
@@ -0,0 +1,271 @@
+// Definitions for I2C based sensors using the Industrial IO or HWMON interface.
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			bme280: bme280@76 {
+				compatible = "bosch,bme280";
+				reg = <0x76>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			bmp085: bmp085@77 {
+				compatible = "bosch,bmp085";
+				reg = <0x77>;
+				default-oversampling = <3>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			bmp180: bmp180@77 {
+				compatible = "bosch,bmp180";
+				reg = <0x77>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			bmp280: bmp280@76 {
+				compatible = "bosch,bmp280";
+				reg = <0x76>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			htu21: htu21@40 {
+				compatible = "htu21";
+				reg = <0x40>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@5 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			lm75: lm75@4f {
+				compatible = "lm75";
+				reg = <0x4f>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@6 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			si7020: si7020@40 {
+				compatible = "si7020";
+				reg = <0x40>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			tmp102: tmp102@48 {
+				compatible = "ti,tmp102";
+				reg = <0x48>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@8 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			hdc100x: hdc100x@40 {
+				compatible = "hdc100x";
+				reg = <0x40>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			tsl4531: tsl4531@29 {
+				compatible = "tsl4531";
+				reg = <0x29>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@10 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			veml6070: veml6070@38 {
+				compatible = "veml6070";
+				reg = <0x38>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@11 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sht3x: sht3x@44 {
+				compatible = "sht3x";
+				reg = <0x44>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@12 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ds1621: ds1621@48 {
+				compatible = "ds1621";
+				reg = <0x48>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@13 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			max17040: max17040@36 {
+				compatible = "maxim,max17040";
+				reg = <0x36>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@14 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			bme680: bme680@76 {
+				compatible = "bosch,bme680";
+				reg = <0x76>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@15 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sps30: sps30@69 {
+				compatible = "sensirion,sps30";
+				reg = <0x69>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		addr =  <&bme280>,"reg:0", <&bmp280>,"reg:0", <&tmp102>,"reg:0",
+			<&lm75>,"reg:0", <&hdc100x>,"reg:0", <&sht3x>,"reg:0",
+			<&ds1621>,"reg:0", <&bme680>,"reg:0";
+		bme280 = <0>,"+0";
+		bmp085 = <0>,"+1";
+		bmp180 = <0>,"+2";
+		bmp280 = <0>,"+3";
+		htu21 = <0>,"+4";
+		lm75 = <0>,"+5";
+		lm75addr = <&lm75>,"reg:0";
+		si7020 = <0>,"+6";
+		tmp102 = <0>,"+7";
+		hdc100x = <0>,"+8";
+		tsl4531 = <0>,"+9";
+		veml6070 = <0>,"+10";
+		sht3x = <0>,"+11";
+		ds1621 = <0>,"+12";
+		max17040 = <0>,"+13";
+		bme680 = <0>,"+14";
+		sps30 = <0>,"+15";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c0-overlay.dts b/arch/arm/boot/dts/overlays/i2c0-overlay.dts
new file mode 100644
index 000000000000..7c6771f84d8e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c0-overlay.dts
@@ -0,0 +1,74 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-0 = <&i2c0_pins>;
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c0_pins>;
+		pins1: __overlay__ {
+			brcm,pins = <0 1>;
+			brcm,function = <4>; /* alt0 */
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0_pins>;
+		pins2: __dormant__ {
+			brcm,pins = <28 29>;
+			brcm,function = <4>; /* alt0 */
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c0_pins>;
+		pins3: __dormant__ {
+			brcm,pins = <44 45>;
+			brcm,function = <5>; /* alt1 */
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0_pins>;
+		pins4: __dormant__ {
+			brcm,pins = <46 47>;
+			brcm,function = <4>; /* alt0 */
+		};
+	};
+
+	fragment@5 {
+		target = <&i2c0>;
+		__dormant__ {
+			compatible = "brcm,bcm2708-i2c";
+		};
+	};
+
+	fragment@6 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@7 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c0 = "/soc/i2c@7e205000";
+		};
+	};
+	__overrides__ {
+		pins_0_1   = <0>,"+1-2-3-4";
+		pins_28_29 = <0>,"-1+2-3-4";
+		pins_44_45 = <0>,"-1-2+3-4";
+		pins_46_47 = <0>,"-1-2-3+4";
+		combine = <0>, "!5";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c1-overlay.dts b/arch/arm/boot/dts/overlays/i2c1-overlay.dts
new file mode 100644
index 000000000000..addaed73e665
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c1-overlay.dts
@@ -0,0 +1,44 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1_pins>;
+		pins1: __overlay__ {
+			brcm,pins = <2 3>;
+			brcm,function = <4>; /* alt 0 */
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1_pins>;
+		pins2: __dormant__ {
+			brcm,pins = <44 45>;
+			brcm,function = <6>; /* alt 2 */
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c1>;
+		__dormant__ {
+			compatible = "brcm,bcm2708-i2c";
+		};
+	};
+
+	__overrides__ {
+		pins_2_3   = <0>,"=1!2";
+		pins_44_45 = <0>,"!1=2";
+		combine = <0>, "!3";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c3-overlay.dts b/arch/arm/boot/dts/overlays/i2c3-overlay.dts
new file mode 100644
index 000000000000..e24a1df21f99
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c3-overlay.dts
@@ -0,0 +1,36 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&i2c3>;
+		frag0: __overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c3_pins>;
+			clock-frequency = <100000>;
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c3_pins>;
+		__dormant__ {
+			brcm,pins = <2 3>;
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c3_pins>;
+		__overlay__ {
+			brcm,pins = <4 5>;
+		};
+	};
+
+	__overrides__ {
+		pins_2_3 = <0>,"=1!2";
+		pins_4_5 = <0>,"!1=2";
+		baudrate = <&frag0>, "clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c4-overlay.dts b/arch/arm/boot/dts/overlays/i2c4-overlay.dts
new file mode 100644
index 000000000000..14c7f4d1da4c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c4-overlay.dts
@@ -0,0 +1,36 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&i2c4>;
+		frag0: __overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c4_pins>;
+			clock-frequency = <100000>;
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c4_pins>;
+		__dormant__ {
+			brcm,pins = <6 7>;
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c4_pins>;
+		__overlay__ {
+			brcm,pins = <8 9>;
+		};
+	};
+
+	__overrides__ {
+		pins_6_7 = <0>,"=1!2";
+		pins_8_9 = <0>,"!1=2";
+		baudrate = <&frag0>, "clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c5-overlay.dts b/arch/arm/boot/dts/overlays/i2c5-overlay.dts
new file mode 100644
index 000000000000..7953621112de
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c5-overlay.dts
@@ -0,0 +1,36 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&i2c5>;
+		frag0: __overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c5_pins>;
+			clock-frequency = <100000>;
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c5_pins>;
+		__dormant__ {
+			brcm,pins = <10 11>;
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c5_pins>;
+		__overlay__ {
+			brcm,pins = <12 13>;
+		};
+	};
+
+	__overrides__ {
+		pins_10_11 = <0>,"=1!2";
+		pins_12_13 = <0>,"!1=2";
+		baudrate = <&frag0>, "clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2c6-overlay.dts b/arch/arm/boot/dts/overlays/i2c6-overlay.dts
new file mode 100644
index 000000000000..555305a7ee1f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2c6-overlay.dts
@@ -0,0 +1,36 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&i2c6>;
+		frag0: __overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c6_pins>;
+			clock-frequency = <100000>;
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c6_pins>;
+		__dormant__ {
+			brcm,pins = <0 1>;
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c6_pins>;
+		__overlay__ {
+			brcm,pins = <22 23>;
+		};
+	};
+
+	__overrides__ {
+		pins_0_1 = <0>,"=1!2";
+		pins_22_23 = <0>,"!1=2";
+		baudrate = <&frag0>, "clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/i2s-gpio28-31-overlay.dts b/arch/arm/boot/dts/overlays/i2s-gpio28-31-overlay.dts
new file mode 100644
index 000000000000..cf43094c6ff4
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/i2s-gpio28-31-overlay.dts
@@ -0,0 +1,18 @@
+/*
+ * Device tree overlay to move i2s to gpio 28 to 31 on CM
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s_pins>;
+		__overlay__ {
+			brcm,pins = <28 29 30 31>;
+			brcm,function = <6>; /* alt2 */
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ilitek251x-overlay.dts b/arch/arm/boot/dts/overlays/ilitek251x-overlay.dts
new file mode 100644
index 000000000000..551aba591d26
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ilitek251x-overlay.dts
@@ -0,0 +1,45 @@
+// Device tree overlay for I2C connected Ilitek multiple touch controller
+/dts-v1/;
+/plugin/;
+
+ / {
+	compatible = "brcm,bcm2835";
+
+ 	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {		
+			ili251x_pins: ili251x_pins {
+				brcm,pins = <4>; // interrupt
+				brcm,function = <0>; // in
+				brcm,pull = <2>; // pull-up //
+			};
+		};
+	};
+
+ 	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+ 			ili251x: ili251x@41 {
+				compatible = "ilitek,ili251x";
+				reg = <0x41>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&ili251x_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <4 8>; // high-to-low edge triggered
+				touchscreen-size-x = <16384>;
+				touchscreen-size-y = <9600>;
+			};
+		};
+	};
+
+ 	__overrides__ {
+		interrupt = <&ili251x_pins>,"brcm,pins:0",
+			<&ili251x>,"interrupts:0";
+		sizex = <&ili251x>,"touchscreen-size-x:0";
+		sizey = <&ili251x>,"touchscreen-size-y:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/imx219-overlay.dts b/arch/arm/boot/dts/overlays/imx219-overlay.dts
new file mode 100644
index 000000000000..3484bde5a9e8
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/imx219-overlay.dts
@@ -0,0 +1,119 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for IMX219 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			imx219: imx219@10 {
+				compatible = "sony,imx219";
+				reg = <0x10>;
+				status = "okay";
+
+				clocks = <&imx219_clk>;
+				clock-names = "xclk";
+
+				VANA-supply = <&imx219_vana>;	/* 2.8v */
+				VDIG-supply = <&imx219_vdig>;	/* 1.8v */
+				VDDL-supply = <&imx219_vddl>;	/* 1.2v */
+
+				rotation = <180>;
+
+				port {
+					imx219_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1 2>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <297000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&imx219_0>;
+					clock-lanes = <0>;
+					data-lanes = <1 2>;
+					clock-noncontinuous;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path="/";
+		__overlay__ {
+			imx219_vana: fixedregulator@0 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx219_vana";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				gpio = <&gpio 41 GPIO_ACTIVE_HIGH>;
+				enable-active-high;
+			};
+			imx219_vdig: fixedregulator@1 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx219_vdig";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+			imx219_vddl: fixedregulator@2 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx219_vddl";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+			};
+
+			imx219_clk: camera-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <24000000>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&imx219_vana>,"gpio:0";
+			cam0-pwdn      = <&imx219_vana>,"gpio:4";
+		};
+	};
+
+	__overrides__ {
+		rotation = <&imx219>,"rotation:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/imx290-overlay.dts b/arch/arm/boot/dts/overlays/imx290-overlay.dts
new file mode 100644
index 000000000000..e536aa7f9e33
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/imx290-overlay.dts
@@ -0,0 +1,32 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for IMX290 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+#include "imx290_327-overlay.dtsi"
+
+/{
+	compatible = "brcm,bcm2835";
+
+	// Fragment numbers deliberately high to avoid conflicts with the
+	// included imx290_327 overlay file.
+
+	fragment@101 {
+		target = <&imx290>;
+		__overlay__ {
+			compatible = "sony,imx290";
+		};
+	};
+
+	fragment@102 {
+		target = <&imx290>;
+		__dormant__ {
+			compatible = "sony,imx290-mono";
+		};
+	};
+
+	__overrides__ {
+		mono = <0>, "-101+102";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/imx290_327-overlay.dtsi b/arch/arm/boot/dts/overlays/imx290_327-overlay.dtsi
new file mode 100644
index 000000000000..8f1dadb13f6a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/imx290_327-overlay.dtsi
@@ -0,0 +1,145 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Partial definitions for IMX290 or IMX327 camera module on VC I2C bus
+// The compatible string should be set in an overlay that then includes this one
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			imx290: imx290@1a {
+				reg = <0x1a>;
+				status = "okay";
+
+				clocks = <&imx290_clk>;
+				clock-names = "xclk";
+				clock-frequency = <37125000>;
+
+				vdda-supply = <&imx290_vdda>;	/* 2.8v */
+				vdddo-supply = <&imx290_vdddo>;	/* 1.8v */
+				vddd-supply = <&imx290_vddd>;	/* 1.5v */
+
+				port {
+					imx290_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&imx290_0>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path="/";
+		__overlay__ {
+			imx290_vdda: fixedregulator@0 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx290_vdda";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				gpio = <&gpio 41 GPIO_ACTIVE_HIGH>;
+				enable-active-high;
+			};
+			imx290_vdddo: fixedregulator@1 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx290_vdddo";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+			imx290_vddd: fixedregulator@2 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx290_vddd";
+				regulator-min-microvolt = <1500000>;
+				regulator-max-microvolt = <1500000>;
+			};
+
+			imx290_clk: camera-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <37125000>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&imx290_vdda>,"gpio:0";
+			cam0-pwdn      = <&imx290_vdda>,"gpio:4";
+		};
+	};
+
+	fragment@6 {
+		target = <&imx290_0>;
+		__overlay__ {
+			data-lanes = <1 2>;
+			link-frequencies =
+				/bits/ 64 <445500000 297000000>;
+		};
+	};
+
+	fragment@7 {
+		target = <&imx290_0>;
+		__dormant__ {
+			data-lanes = <1 2 3 4>;
+			link-frequencies =
+				/bits/ 64 <222750000 148500000>;
+		};
+	};
+
+	fragment@8 {
+		target = <&csi1_ep>;
+		__overlay__ {
+			data-lanes = <1 2>;
+		};
+	};
+
+	fragment@9 {
+		target = <&csi1_ep>;
+		__dormant__ {
+			data-lanes = <1 2 3 4>;
+		};
+	};
+
+	__overrides__ {
+		4lane = <0>, "-6+7-8+9";
+		clock-frequency = <&imx290_clk>,"clock-frequency:0",
+				  <&imx290>,"clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/imx477-overlay.dts b/arch/arm/boot/dts/overlays/imx477-overlay.dts
new file mode 100644
index 000000000000..1a97eaaf4c82
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/imx477-overlay.dts
@@ -0,0 +1,119 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for IMX477 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			imx477: imx477@1a {
+				compatible = "sony,imx477";
+				reg = <0x1a>;
+				status = "okay";
+
+				clocks = <&imx477_clk>;
+				clock-names = "xclk";
+
+				VANA-supply = <&imx477_vana>;	/* 2.8v */
+				VDIG-supply = <&imx477_vdig>;	/* 1.05v */
+				VDDL-supply = <&imx477_vddl>;	/* 1.8v */
+
+				rotation = <180>;
+
+				port {
+					imx477_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1 2>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <450000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&imx477_0>;
+					clock-lanes = <0>;
+					data-lanes = <1 2>;
+					clock-noncontinuous;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path="/";
+		__overlay__ {
+			imx477_vana: fixedregulator@0 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx477_vana";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				gpio = <&gpio 41 GPIO_ACTIVE_HIGH>;
+				enable-active-high;
+				startup-delay-us = <300000>;
+			};
+			imx477_vdig: fixedregulator@1 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx477_vdig";
+				regulator-min-microvolt = <1050000>;
+				regulator-max-microvolt = <1050000>;
+			};
+			imx477_vddl: fixedregulator@2 {
+				compatible = "regulator-fixed";
+				regulator-name = "imx477_vddl";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+			imx477_clk: camera-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <24000000>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&imx477_vana>,"gpio:0";
+			cam0-pwdn      = <&imx477_vana>,"gpio:4";
+		};
+	};
+
+	__overrides__ {
+		rotation = <&imx477>,"rotation:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/iqaudio-codec-overlay.dts b/arch/arm/boot/dts/overlays/iqaudio-codec-overlay.dts
new file mode 100644
index 000000000000..9110f5d34298
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/iqaudio-codec-overlay.dts
@@ -0,0 +1,42 @@
+// Definitions for IQaudIO CODEC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			da2713@1a {
+				#sound-dai-cells = <0>;
+				compatible = "dlg,da7213";
+				reg = <0x1a>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		iqaudio_dac: __overlay__ {
+			compatible = "iqaudio,iqaudio-codec";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts b/arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts
new file mode 100644
index 000000000000..24073cadd0ef
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/iqaudio-dac-overlay.dts
@@ -0,0 +1,46 @@
+// Definitions for IQaudIO DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		frag2: __overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&frag2>,"iqaudio,24db_digital_gain?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/iqaudio-dacplus-overlay.dts b/arch/arm/boot/dts/overlays/iqaudio-dacplus-overlay.dts
new file mode 100644
index 000000000000..7c70b25e58d7
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/iqaudio-dacplus-overlay.dts
@@ -0,0 +1,49 @@
+// Definitions for IQaudIO DAC+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4c {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4c>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		iqaudio_dac: __overlay__ {
+			compatible = "iqaudio,iqaudio-dac";
+			i2s-controller = <&i2s>;
+			mute-gpios = <&gpio 22 0>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&iqaudio_dac>,"iqaudio,24db_digital_gain?";
+		auto_mute_amp = <&iqaudio_dac>,"iqaudio-dac,auto-mute-amp?";
+		unmute_amp = <&iqaudio_dac>,"iqaudio-dac,unmute-amp?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/iqaudio-digi-wm8804-audio-overlay.dts b/arch/arm/boot/dts/overlays/iqaudio-digi-wm8804-audio-overlay.dts
new file mode 100644
index 000000000000..ee54095c869b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/iqaudio-digi-wm8804-audio-overlay.dts
@@ -0,0 +1,47 @@
+// Definitions for IQAudIO Digi WM8804 audio board
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				status = "okay";
+				DVDD-supply = <&vdd_3v3_reg>;
+				PVDD-supply = <&vdd_3v3_reg>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		wm8804_digi: __overlay__ {
+			compatible = "iqaudio,wm8804-digi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		card_name = <&wm8804_digi>,"wm8804-digi,card-name";
+		dai_name = <&wm8804_digi>,"wm8804-digi,dai-name";
+		dai_stream_name = <&wm8804_digi>,"wm8804-digi,dai-stream-name";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/irs1125-overlay.dts b/arch/arm/boot/dts/overlays/irs1125-overlay.dts
new file mode 100644
index 000000000000..e926e18e71fc
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/irs1125-overlay.dts
@@ -0,0 +1,85 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for IRS1125 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			irs1125: irs1125@3D {
+				compatible = "infineon,irs1125";
+				reg = <0x3D>;
+				status = "okay";
+
+				pwdn-gpios = <&gpio 5 0>;
+				clocks = <&irs1125_clk>;
+
+				port {
+					irs1125_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1 2>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <297000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&irs1125_0>;
+					data-lanes = <1 2>;
+					clock-noncontinuous;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&irs1125>,"pwdn-gpios:0";
+			cam0-pwdn      = <&irs1125>,"pwdn-gpios:4";
+		};
+	};
+
+	fragment@5 {
+		target-path = "/";
+		__overlay__ {
+			irs1125_clk: camera-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <26000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/jedec-spi-nor-overlay.dts b/arch/arm/boot/dts/overlays/jedec-spi-nor-overlay.dts
new file mode 100644
index 000000000000..585c7dbcdf7f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/jedec-spi-nor-overlay.dts
@@ -0,0 +1,309 @@
+// Overlay for JEDEC SPI-NOR Flash Devices (aka m25p80)
+
+// dtparams:
+//     flash-spi<n>-<m>        - Enables flash device on SPI<n>, CS#<m>.
+//     flash-fastr-spi<n>-<m>  - Enables flash device with fast read capability on SPI<n>, CS#<m>.
+//
+// If devices are present on SPI1 or SPI2, those interfaces must be enabled with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+//
+// Example: A single flash device with fast read capability on SPI0, CS#0:
+// dtoverlay=jedec-spi-nor:flash-fastr-spi0-0
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	// disable spi-dev on spi0.0
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi0.1
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi1.0
+	fragment@2 {
+		target-path = "spi1/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi1.1
+	fragment@3 {
+		target-path = "spi1/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi1.2
+	fragment@4 {
+		target-path = "spi1/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi2.0
+	fragment@5 {
+		target-path = "spi2/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi2.1
+	fragment@6 {
+		target-path = "spi2/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi2.2
+	fragment@7 {
+		target-path = "spi2/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// enable flash on spi0.0
+	fragment@8 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_00: spi_nor@0 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi0.1
+	fragment@9 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_01: spi_nor@1 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <1>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi1.0
+	fragment@10 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_10: spi_nor@0 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi1.1
+	fragment@11 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_11: spi_nor@1 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <1>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi1.2
+	fragment@12 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_12: spi_nor@2 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <2>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi2.0
+	fragment@13 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_20: spi_nor@0 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi2.1
+	fragment@14 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_21: spi_nor@1 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <1>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// enable flash on spi2.2
+	fragment@15 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			spi_nor_22: spi_nor@2 {
+				#address-cells = <1>;
+				#size-cells = <1>;
+				compatible = "jedec,spi-nor";
+				reg = <2>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	// Enable fast read for device on spi0.0.
+	// Use default active low interrupt signalling.
+	fragment@16 {
+		target = <&spi_nor_00>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi0.1.
+	// Use default active low interrupt signalling.
+	fragment@17 {
+		target = <&spi_nor_01>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi1.0.
+	// Use default active low interrupt signalling.
+	fragment@18 {
+		target = <&spi_nor_10>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi1.1.
+	// Use default active low interrupt signalling.
+	fragment@19 {
+		target = <&spi_nor_11>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi1.2.
+	// Use default active low interrupt signalling.
+	fragment@20 {
+		target = <&spi_nor_12>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi2.0.
+	// Use default active low interrupt signalling.
+	fragment@21 {
+		target = <&spi_nor_20>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi2.1.
+	// Use default active low interrupt signalling.
+	fragment@22 {
+		target = <&spi_nor_21>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	// Enable fast read for device on spi2.2.
+	// Use default active low interrupt signalling.
+	fragment@23 {
+		target = <&spi_nor_22>;
+		__dormant__ {
+			m25p,fast-read;
+		};
+	};
+
+	__overrides__ {
+		flash-spi0-0       = <0>,"+0+8";
+		flash-spi0-1       = <0>,"+1+9";
+		flash-spi1-0       = <0>,"+2+10";
+		flash-spi1-1       = <0>,"+3+11";
+		flash-spi1-2       = <0>,"+4+12";
+		flash-spi2-0       = <0>,"+5+13";
+		flash-spi2-1       = <0>,"+6+14";
+		flash-spi2-2       = <0>,"+7+15";
+		flash-fastr-spi0-0 = <0>,"+0+8+16";
+		flash-fastr-spi0-1 = <0>,"+1+9+17";
+		flash-fastr-spi1-0 = <0>,"+2+10+18";
+		flash-fastr-spi1-1 = <0>,"+3+11+19";
+		flash-fastr-spi1-2 = <0>,"+4+12+20";
+		flash-fastr-spi2-0 = <0>,"+5+13+21";
+		flash-fastr-spi2-1 = <0>,"+6+14+22";
+		flash-fastr-spi2-2 = <0>,"+7+15+23";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/justboom-both-overlay.dts b/arch/arm/boot/dts/overlays/justboom-both-overlay.dts
new file mode 100644
index 000000000000..9c42670631c0
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/justboom-both-overlay.dts
@@ -0,0 +1,65 @@
+// SPDX-License-Identifier: GPL-2.0
+// Definitions for JustBoom Both (Digi+DAC)
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		frag3: __overlay__ {
+			compatible = "justboom,justboom-both";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&frag3>,"justboom,24db_digital_gain?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/justboom-dac-overlay.dts b/arch/arm/boot/dts/overlays/justboom-dac-overlay.dts
new file mode 100644
index 000000000000..d00515dca419
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/justboom-dac-overlay.dts
@@ -0,0 +1,46 @@
+// Definitions for JustBoom DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pcm5122@4d {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5122";
+				reg = <0x4d>;
+				AVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		frag2: __overlay__ {
+			compatible = "justboom,justboom-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		24db_digital_gain = <&frag2>,"justboom,24db_digital_gain?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/justboom-digi-overlay.dts b/arch/arm/boot/dts/overlays/justboom-digi-overlay.dts
new file mode 100644
index 000000000000..e73336029c54
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/justboom-digi-overlay.dts
@@ -0,0 +1,41 @@
+// Definitions for JustBoom Digi
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "justboom,justboom-digi";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ltc294x-overlay.dts b/arch/arm/boot/dts/overlays/ltc294x-overlay.dts
new file mode 100644
index 000000000000..6d971f3649ca
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ltc294x-overlay.dts
@@ -0,0 +1,86 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ltc2941: ltc2941@64 {
+				compatible = "lltc,ltc2941";
+				reg = <0x64>;
+				lltc,resistor-sense = <50>;
+				lltc,prescaler-exponent = <7>; 
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ltc2942: ltc2942@64 {
+				compatible = "lltc,ltc2942";
+				reg = <0x64>;
+				lltc,resistor-sense = <50>;
+				lltc,prescaler-exponent = <7>; 
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ltc2943: ltc2943@64 {
+				compatible = "lltc,ltc2943";
+				reg = <0x64>;
+				lltc,resistor-sense = <50>;
+				lltc,prescaler-exponent = <7>; 
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c_arm>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ltc2944: ltc2944@64 {
+				compatible = "lltc,ltc2944";
+				reg = <0x64>;
+				lltc,resistor-sense = <50>;
+				lltc,prescaler-exponent = <7>; 
+			};
+		};
+	};
+
+	__overrides__ {
+		ltc2941 = <0>,"+0";
+		ltc2942 = <0>,"+1";
+		ltc2943 = <0>,"+2";
+		ltc2944 = <0>,"+3";
+		resistor-sense = <&ltc2941>, "lltc,resistor-sense:0",
+			         <&ltc2942>, "lltc,resistor-sense:0",
+				 <&ltc2943>, "lltc,resistor-sense:0",
+				 <&ltc2944>, "lltc,resistor-sense:0";
+		prescaler-exponent = <&ltc2941>, "lltc,prescaler-exponent:0",
+			         <&ltc2942>, "lltc,prescaler-exponent:0",
+				 <&ltc2943>, "lltc,prescaler-exponent:0",
+				 <&ltc2944>, "lltc,prescaler-exponent:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/max98357a-overlay.dts b/arch/arm/boot/dts/overlays/max98357a-overlay.dts
new file mode 100644
index 000000000000..9e2afb05b7cb
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/max98357a-overlay.dts
@@ -0,0 +1,84 @@
+// Overlay for Maxim MAX98357A audio DAC
+
+// dtparams:
+//     no-sdmode  - SD_MODE pin not managed by driver.
+//     sdmode-pin - Specify GPIO pin to which SD_MODE is connected (default 4).
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	/* Enable I2S */
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	/* DAC whose SD_MODE pin is managed by driver (via GPIO pin) */
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			max98357a_dac: max98357a {
+				compatible = "maxim,max98357a";
+				#sound-dai-cells = <0>;
+				sdmode-gpios = <&gpio 4 0>;   /* 2nd word overwritten by sdmode-pin parameter */
+				status = "okay";
+			};
+		};
+	};
+
+	/* DAC whose SD_MODE pin is not managed by driver */
+	fragment@2 {
+		target-path = "/";
+		__dormant__ {
+			max98357a_nsd: max98357a {
+				compatible = "maxim,max98357a";
+				#sound-dai-cells = <0>;
+				status = "okay";
+			};
+		};
+	};
+
+	/* Soundcard connecting I2S to DAC with SD_MODE */
+	fragment@3 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "simple-audio-card";
+			simple-audio-card,format = "i2s";
+			simple-audio-card,name = "MAX98357A";
+			status = "okay";
+			simple-audio-card,cpu {
+				sound-dai = <&i2s>;
+			};
+			simple-audio-card,codec {
+				sound-dai = <&max98357a_dac>;
+			};
+		};
+	};
+
+	/* Soundcard connecting I2S to DAC without SD_MODE */
+	fragment@4 {
+		target = <&sound>;
+		__dormant__ {
+			compatible = "simple-audio-card";
+			simple-audio-card,format = "i2s";
+			simple-audio-card,name = "MAX98357A";
+			status = "okay";
+			simple-audio-card,cpu {
+				sound-dai = <&i2s>;
+			};
+			simple-audio-card,codec {
+				sound-dai = <&max98357a_nsd>;
+			};
+		};
+	};
+
+	__overrides__ {
+		no-sdmode  = <0>,"-1+2-3+4";
+		sdmode-pin = <&max98357a_dac>,"sdmode-gpios:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/maxtherm-overlay.dts b/arch/arm/boot/dts/overlays/maxtherm-overlay.dts
new file mode 100644
index 000000000000..34d5727069ec
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/maxtherm-overlay.dts
@@ -0,0 +1,166 @@
+/*
+ * Universal device tree overlay for SPI devices
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target-path = "spi1/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target-path = "spi1/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@4 {
+		target-path = "spi1/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@5 {
+		target-path = "spi2/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@6 {
+		target-path = "spi2/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@7 {
+		target-path = "spi2/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	maxfrag: fragment@8 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			max: maxtherm@0 {
+				compatible = "maxim,max6675";
+				reg = <0>;
+				spi-max-frequency = <500000>;
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855e", "maxim,max31855";
+		};
+	};
+
+	fragment@10 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855j", "maxim,max31855";
+		};
+	};
+
+	fragment@11 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855k", "maxim,max31855";
+		};
+	};
+
+	fragment@12 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855n", "maxim,max31855";
+		};
+	};
+
+	fragment@13 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855r", "maxim,max31855";
+		};
+	};
+
+	fragment@14 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855s", "maxim,max31855";
+		};
+	};
+
+	fragment@15 {
+		target = <&max>;
+		__dormant__ {
+			compatible = "maxim,max31855t", "maxim,max31855";
+		};
+	};
+
+	__overrides__ {
+		spi0-0 = <0>, "+0",
+			 <&maxfrag>,"target:0=",<&spi0>,
+			 <&max>,"reg:0=0";
+		spi0-1 = <0>, "+1",
+			 <&maxfrag>,"target:0=",<&spi0>,
+			 <&max>,"reg:0=1";
+		spi1-0 = <0>, "+2",
+			 <&maxfrag>,"target:0=",<&spi1>,
+			 <&max>,"reg:0=0";
+		spi1-1 = <0>, "+3",
+			 <&maxfrag>,"target:0=",<&spi1>,
+			 <&max>,"reg:0=1";
+		spi1-2 = <0>, "+4",
+			 <&maxfrag>,"target:0=",<&spi1>,
+			 <&max>,"reg:0=2";
+		spi2-0 = <0>, "+5",
+			 <&maxfrag>,"target:0=",<&spi2>,
+			 <&max>,"reg:0=0";
+		spi2-1 = <0>, "+6",
+			 <&maxfrag>,"target:0=",<&spi2>,
+			 <&max>,"reg:0=1";
+		spi2-2 = <0>, "+7",
+			 <&maxfrag>,"target:0=",<&spi2>,
+			 <&max>,"reg:0=2";
+		max6675 = <&max>,"compatible=maxim,max6675";
+		max31855 = <&max>,"compatible=maxim,max31855";
+		max31855e = <0>,"+9";
+		max31855j = <0>,"+10";
+		max31855k = <0>,"+11";
+		max31855n = <0>,"+12";
+		max31855r = <0>,"+13";
+		max31855s = <0>,"+14";
+		max31855t = <0>,"+15";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/mbed-dac-overlay.dts b/arch/arm/boot/dts/overlays/mbed-dac-overlay.dts
new file mode 100644
index 000000000000..840dd9b31db4
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mbed-dac-overlay.dts
@@ -0,0 +1,64 @@
+// Definitions for mbed DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+                        #size-cells = <0>;
+			status = "okay";
+
+			tlv320aic23: codec@1a {
+				#sound-dai-cells = <0>;
+				reg = <0x1a>;
+				compatible = "ti,tlv320aic23";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "simple-audio-card";
+			i2s-controller = <&i2s>;
+			status = "okay";
+
+			simple-audio-card,name = "mbed-DAC";
+
+			simple-audio-card,widgets =
+				"Microphone", "Mic Jack",
+				"Line", "Line In",
+				"Headphone", "Headphone Jack";
+
+			simple-audio-card,routing =
+				"Headphone Jack", "LHPOUT",
+				"Headphone Jack", "RHPOUT",
+				"LLINEIN", "Line In",
+				"RLINEIN", "Line In",
+				"MICIN", "Mic Jack";
+
+			simple-audio-card,format = "i2s";
+
+			simple-audio-card,cpu {
+				sound-dai = <&i2s>;
+			};
+
+			sound_master: simple-audio-card,codec {
+				sound-dai = <&tlv320aic23>;
+				system-clock-frequency = <12288000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/mcp23017-overlay.dts b/arch/arm/boot/dts/overlays/mcp23017-overlay.dts
new file mode 100644
index 000000000000..c546d8ba7e6d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp23017-overlay.dts
@@ -0,0 +1,69 @@
+// Definitions for MCP23017 Gpio Extender from Microchip Semiconductor
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			mcp23017_pins: mcp23017_pins@20 {
+				brcm,pins = <4>;
+				brcm,function = <0>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp23017: mcp@20 {
+				compatible = "microchip,mcp23017";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&mcp23017>;
+		__dormant__ {
+			compatible = "microchip,mcp23008";
+		};
+	};
+
+	fragment@4 {
+		target = <&mcp23017>;
+		mcp23017_irq: __overlay__ {
+			#interrupt-cells=<2>;
+			interrupt-parent = <&gpio>;
+			interrupts = <4 2>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	__overrides__ {
+		gpiopin = <&mcp23017_pins>,"brcm,pins:0",
+				<&mcp23017_irq>,"interrupts:0";
+		addr = <&mcp23017>,"reg:0", <&mcp23017_pins>,"reg:0";
+		mcp23008 = <0>,"=3";
+		noints = <0>,"!1!4";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/mcp23s17-overlay.dts b/arch/arm/boot/dts/overlays/mcp23s17-overlay.dts
new file mode 100644
index 000000000000..484d64b225fb
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp23s17-overlay.dts
@@ -0,0 +1,732 @@
+// Overlay for MCP23S08/17 GPIO Extenders from Microchip Semiconductor
+
+// dtparams:
+//     s08-spi<n>-<m>-present  - 4-bit integer, bitmap indicating MCP23S08 devices present on SPI<n>, CS#<m>.
+//     s17-spi<n>-<m>-present  - 8-bit integer, bitmap indicating MCP23S17 devices present on SPI<n>, CS#<m>.
+//     s08-spi<n>-<m>-int-gpio - integer, enables interrupts on a single MCP23S08 device on SPI<n>, CS#<m>, specifies the GPIO pin to which INT output is connected.
+//     s17-spi<n>-<m>-int-gpio - integer, enables mirrored interrupts on a single MCP23S17 device on SPI<n>, CS#<m>, specifies the GPIO pin to which either INTA or INTB output is connected.
+//
+// If devices are present on SPI1 or SPI2, those interfaces must be enabled with one of the spi1-1/2/3cs and/or spi2-1/2/3cs overlays.
+// If interrupts are enabled for a device on a given CS# on a SPI bus, that device must be the only one present on that SPI bus/CS#.
+//
+// Example 1: A single MCP23S17 device on SPI0, CS#0 with its SPI addr set to 0 and INTA output connected to GPIO25:
+// dtoverlay=mcp23s17:s17-spi0-0-present=1,s17-spi0-0-int-gpio=25
+//
+// Example 2: Two MCP23S08 devices on SPI1, CS#0 with their addrs set to 2 and 3. Three MCP23S17 devices on SPI1, CS#1 with their addrs set to 0, 1 and 7:
+// dtoverlay=spi1-2cs
+// dtoverlay=mcp23s17:s08-spi1-0-present=12,s17-spi1-1-present=131
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	// disable spi-dev on spi0.0
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi0.1
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi1.0
+	fragment@2 {
+		target-path = "spi1/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi1.1
+	fragment@3 {
+		target-path = "spi1/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi1.2
+	fragment@4 {
+		target-path = "spi1/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi2.0
+	fragment@5 {
+		target-path = "spi2/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi2.1
+	fragment@6 {
+		target-path = "spi2/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// disable spi-dev on spi2.2
+	fragment@7 {
+		target-path = "spi2/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	// enable one or more mcp23s08s on spi0.0
+	fragment@8 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_00: mcp23s08@0 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi0-0-present parameter */
+     				reg = <0>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi0-0-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi0.1
+	fragment@9 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_01: mcp23s08@1 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi0-1-present parameter */
+     				reg = <1>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi0-1-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi1.0
+	fragment@10 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_10: mcp23s08@0 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi1-0-present parameter */
+     				reg = <0>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi1-0-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi1.1
+	fragment@11 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_11: mcp23s08@1 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi1-1-present parameter */
+     				reg = <1>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi1-1-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi1.2
+	fragment@12 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_12: mcp23s08@2 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi1-2-present parameter */
+     				reg = <2>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi1-2-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi2.0
+	fragment@13 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_20: mcp23s08@0 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi2-0-present parameter */
+     				reg = <0>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi2-0-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi2.1
+	fragment@14 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_21: mcp23s08@1 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi2-1-present parameter */
+     				reg = <1>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi2-1-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s08s on spi2.2
+	fragment@15 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s08_22: mcp23s08@2 {
+				compatible = "microchip,mcp23s08";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s08-spi2-2-present parameter */
+     				reg = <2>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s08-spi2-2-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi0.0
+	fragment@16 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_00: mcp23s17@0 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi0-0-present parameter */
+     				reg = <0>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi0-0-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi0.1
+	fragment@17 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_01: mcp23s17@1 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi0-1-present parameter */
+     				reg = <1>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi0-1-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi1.0
+	fragment@18 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_10: mcp23s17@0 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi1-0-present parameter */
+     				reg = <0>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi1-0-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi1.1
+	fragment@19 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_11: mcp23s17@1 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi1-1-present parameter */
+     				reg = <1>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi1-1-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi1.2
+	fragment@20 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_12: mcp23s17@2 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi1-2-present parameter */
+     				reg = <2>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi1-2-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi2.0
+	fragment@21 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_20: mcp23s17@0 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi2-0-present parameter */
+     				reg = <0>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi2-0-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi2.1
+	fragment@22 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_21: mcp23s17@1 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi2-1-present parameter */
+     				reg = <1>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi2-1-int-gpio parameter */
+			};
+		};
+	};
+
+	// enable one or more mcp23s17s on spi2.2
+	fragment@23 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+			mcp23s17_22: mcp23s17@2 {
+				compatible = "microchip,mcp23s17";
+  				gpio-controller;
+  				#gpio-cells = <2>;
+    				microchip,spi-present-mask = <0x00>;  /* overwritten by mcp23s17-spi2-2-present parameter */
+     				reg = <2>;
+    				spi-max-frequency = <500000>;
+				status = "okay";
+				#interrupt-cells=<2>;
+				interrupts = <0 2>;  /* 1st word overwritten by mcp23s17-spi2-2-int-gpio parameter */
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi0.0 as a input with no pull-up/down
+	fragment@24 {
+		target = <&gpio>;
+		__dormant__ {
+			spi0_0_int_pins: spi0_0_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi0-0-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi0.1 as a input with no pull-up/down
+	fragment@25 {
+		target = <&gpio>;
+		__dormant__ {
+			spi0_1_int_pins: spi0_1_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi0-1-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi1.0 as a input with no pull-up/down
+	fragment@26 {
+		target = <&gpio>;
+		__dormant__ {
+			spi1_0_int_pins: spi1_0_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi1-0-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi1.1 as a input with no pull-up/down
+	fragment@27 {
+		target = <&gpio>;
+		__dormant__ {
+			spi1_1_int_pins: spi1_1_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi1-1-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi1.2 as a input with no pull-up/down
+	fragment@28 {
+		target = <&gpio>;
+		__dormant__ {
+			spi1_2_int_pins: spi1_2_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi1-2-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi2.0 as a input with no pull-up/down
+	fragment@29 {
+		target = <&gpio>;
+		__dormant__ {
+			spi2_0_int_pins: spi2_0_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi2-0-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi2.1 as a input with no pull-up/down
+	fragment@30 {
+		target = <&gpio>;
+		__dormant__ {
+			spi2_1_int_pins: spi2_1_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi2-1-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to INT(A/B) output of mcp23s08/17 on spi2.2 as a input with no pull-up/down
+	fragment@31 {
+		target = <&gpio>;
+		__dormant__ {
+			spi2_2_int_pins: spi2_2_int_pins {
+				brcm,pins = <0>;  /* overwritten by mcp23s08/17-spi2-2-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi0.0.
+	// Use default active low interrupt signalling.
+	fragment@32 {
+		target = <&mcp23s08_00>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi0.1.
+	// Use default active low interrupt signalling.
+	fragment@33 {
+		target = <&mcp23s08_01>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi1.0.
+	// Use default active low interrupt signalling.
+	fragment@34 {
+		target = <&mcp23s08_10>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi1.1.
+	// Use default active low interrupt signalling.
+	fragment@35 {
+		target = <&mcp23s08_11>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi1.2.
+	// Use default active low interrupt signalling.
+	fragment@36 {
+		target = <&mcp23s08_12>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi2.0.
+	// Use default active low interrupt signalling.
+	fragment@37 {
+		target = <&mcp23s08_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi2.1.
+	// Use default active low interrupt signalling.
+	fragment@38 {
+		target = <&mcp23s08_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s08 on spi2.2.
+	// Use default active low interrupt signalling.
+	fragment@39 {
+		target = <&mcp23s08_22>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi0.0.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Use default active low interrupt signalling.
+	fragment@40 {
+		target = <&mcp23s17_00>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi0.1.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@41 {
+		target = <&mcp23s17_01>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi1.0.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@42 {
+		target = <&mcp23s17_10>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi1.1.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@43 {
+		target = <&mcp23s17_11>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi1.2.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@44 {
+		target = <&mcp23s17_12>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi2.0.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@45 {
+		target = <&mcp23s17_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi2.1.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@46 {
+		target = <&mcp23s17_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	// Enable interrupts for a mcp23s17 on spi2.2.
+	// Enable mirroring so that either INTA or INTB output of mcp23s17 can be connected to the GPIO pin.
+	// Configure INTA/B outputs of mcp23s08/17 as active low.
+	fragment@47 {
+		target = <&mcp23s17_22>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			microchip,irq-mirror;
+		};
+	};
+
+	__overrides__ {
+		s08-spi0-0-present = <0>,"+0+8",  <&mcp23s08_00>,"microchip,spi-present-mask:0";
+		s08-spi0-1-present = <0>,"+1+9",  <&mcp23s08_01>,"microchip,spi-present-mask:0";
+		s08-spi1-0-present = <0>,"+2+10", <&mcp23s08_10>,"microchip,spi-present-mask:0";
+		s08-spi1-1-present = <0>,"+3+11", <&mcp23s08_11>,"microchip,spi-present-mask:0";
+		s08-spi1-2-present = <0>,"+4+12", <&mcp23s08_12>,"microchip,spi-present-mask:0";
+		s08-spi2-0-present = <0>,"+5+13", <&mcp23s08_20>,"microchip,spi-present-mask:0";
+		s08-spi2-1-present = <0>,"+6+14", <&mcp23s08_21>,"microchip,spi-present-mask:0";
+		s08-spi2-2-present = <0>,"+7+15", <&mcp23s08_22>,"microchip,spi-present-mask:0";
+		s17-spi0-0-present = <0>,"+0+16", <&mcp23s17_00>,"microchip,spi-present-mask:0";
+		s17-spi0-1-present = <0>,"+1+17", <&mcp23s17_01>,"microchip,spi-present-mask:0";
+		s17-spi1-0-present = <0>,"+2+18", <&mcp23s17_10>,"microchip,spi-present-mask:0";
+		s17-spi1-1-present = <0>,"+3+19", <&mcp23s17_11>,"microchip,spi-present-mask:0";
+		s17-spi1-2-present = <0>,"+4+20", <&mcp23s17_12>,"microchip,spi-present-mask:0";
+		s17-spi2-0-present = <0>,"+5+21", <&mcp23s17_20>,"microchip,spi-present-mask:0";
+		s17-spi2-1-present = <0>,"+6+22", <&mcp23s17_21>,"microchip,spi-present-mask:0";
+		s17-spi2-2-present = <0>,"+7+23", <&mcp23s17_22>,"microchip,spi-present-mask:0";
+		s08-spi0-0-int-gpio = <0>,"+24+32", <&spi0_0_int_pins>,"brcm,pins:0", <&mcp23s08_00>,"interrupts:0";
+		s08-spi0-1-int-gpio = <0>,"+25+33", <&spi0_1_int_pins>,"brcm,pins:0", <&mcp23s08_01>,"interrupts:0";
+		s08-spi1-0-int-gpio = <0>,"+26+34", <&spi1_0_int_pins>,"brcm,pins:0", <&mcp23s08_10>,"interrupts:0";
+		s08-spi1-1-int-gpio = <0>,"+27+35", <&spi1_1_int_pins>,"brcm,pins:0", <&mcp23s08_11>,"interrupts:0";
+		s08-spi1-2-int-gpio = <0>,"+28+36", <&spi1_2_int_pins>,"brcm,pins:0", <&mcp23s08_12>,"interrupts:0";
+		s08-spi2-0-int-gpio = <0>,"+29+37", <&spi2_0_int_pins>,"brcm,pins:0", <&mcp23s08_20>,"interrupts:0";
+		s08-spi2-1-int-gpio = <0>,"+30+38", <&spi2_1_int_pins>,"brcm,pins:0", <&mcp23s08_21>,"interrupts:0";
+		s08-spi2-2-int-gpio = <0>,"+31+39", <&spi2_2_int_pins>,"brcm,pins:0", <&mcp23s08_22>,"interrupts:0";
+		s17-spi0-0-int-gpio = <0>,"+24+40", <&spi0_0_int_pins>,"brcm,pins:0", <&mcp23s17_00>,"interrupts:0";
+		s17-spi0-1-int-gpio = <0>,"+25+41", <&spi0_1_int_pins>,"brcm,pins:0", <&mcp23s17_01>,"interrupts:0";
+		s17-spi1-0-int-gpio = <0>,"+26+42", <&spi1_0_int_pins>,"brcm,pins:0", <&mcp23s17_10>,"interrupts:0";
+		s17-spi1-1-int-gpio = <0>,"+27+43", <&spi1_1_int_pins>,"brcm,pins:0", <&mcp23s17_11>,"interrupts:0";
+		s17-spi1-2-int-gpio = <0>,"+28+44", <&spi1_2_int_pins>,"brcm,pins:0", <&mcp23s17_12>,"interrupts:0";
+		s17-spi2-0-int-gpio = <0>,"+29+45", <&spi2_0_int_pins>,"brcm,pins:0", <&mcp23s17_20>,"interrupts:0";
+		s17-spi2-1-int-gpio = <0>,"+30+46", <&spi2_1_int_pins>,"brcm,pins:0", <&mcp23s17_21>,"interrupts:0";
+		s17-spi2-2-int-gpio = <0>,"+31+47", <&spi2_2_int_pins>,"brcm,pins:0", <&mcp23s17_22>,"interrupts:0";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/mcp2515-can0-overlay.dts b/arch/arm/boot/dts/overlays/mcp2515-can0-overlay.dts
new file mode 100755
index 000000000000..46f143d809cc
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp2515-can0-overlay.dts
@@ -0,0 +1,73 @@
+/*
+ * Device tree overlay for mcp251x/can0 on spi0.0
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+    /* disable spi-dev for spi0.0 */
+    fragment@0 {
+        target = <&spi0>;
+        __overlay__ {
+            status = "okay";
+        };
+    };
+
+    fragment@1 {
+	target = <&spidev0>;
+	__overlay__ {
+	    status = "disabled";
+	};
+    };
+
+    /* the interrupt pin of the can-controller */
+    fragment@2 {
+        target = <&gpio>;
+        __overlay__ {
+            can0_pins: can0_pins {
+                brcm,pins = <25>;
+                brcm,function = <0>; /* input */
+            };
+        };
+    };
+
+    /* the clock/oscillator of the can-controller */
+    fragment@3 {
+        target-path = "/";
+        __overlay__ {
+            /* external oscillator of mcp2515 on SPI0.0 */
+            can0_osc: can0_osc {
+                compatible = "fixed-clock";
+                #clock-cells = <0>;
+                clock-frequency  = <16000000>;
+            };
+        };
+    };
+
+    /* the spi config of the can-controller itself binding everything together */
+    fragment@4 {
+        target = <&spi0>;
+        __overlay__ {
+            /* needed to avoid dtc warning */
+            #address-cells = <1>;
+            #size-cells = <0>;
+            can0: mcp2515@0 {
+                reg = <0>;
+                compatible = "microchip,mcp2515";
+                pinctrl-names = "default";
+                pinctrl-0 = <&can0_pins>;
+                spi-max-frequency = <10000000>;
+                interrupt-parent = <&gpio>;
+                interrupts = <25 8>; /* IRQ_TYPE_LEVEL_LOW */
+                clocks = <&can0_osc>;
+            };
+        };
+    };
+    __overrides__ {
+        oscillator = <&can0_osc>,"clock-frequency:0";
+        spimaxfrequency = <&can0>,"spi-max-frequency:0";
+        interrupt = <&can0_pins>,"brcm,pins:0",<&can0>,"interrupts:0";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/mcp2515-can1-overlay.dts b/arch/arm/boot/dts/overlays/mcp2515-can1-overlay.dts
new file mode 100644
index 000000000000..0a8dd576818e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp2515-can1-overlay.dts
@@ -0,0 +1,73 @@
+/*
+ * Device tree overlay for mcp251x/can1 on spi0.1 edited by petit_miner
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+    /* disable spi-dev for spi0.1 */
+    fragment@0 {
+        target = <&spi0>;
+        __overlay__ {
+            status = "okay";
+        };
+    };
+
+    fragment@1 {
+	target = <&spidev1>;
+	__overlay__ {
+	    status = "disabled";
+	};
+    };
+
+    /* the interrupt pin of the can-controller */
+    fragment@2 {
+        target = <&gpio>;
+        __overlay__ {
+            can1_pins: can1_pins {
+                brcm,pins = <25>;
+                brcm,function = <0>; /* input */
+            };
+        };
+    };
+
+    /* the clock/oscillator of the can-controller */
+    fragment@3 {
+        target-path = "/";
+        __overlay__ {
+            /* external oscillator of mcp2515 on spi0.1 */
+            can1_osc: can1_osc {
+                compatible = "fixed-clock";
+                #clock-cells = <0>;
+                clock-frequency  = <16000000>;
+            };
+        };
+    };
+
+    /* the spi config of the can-controller itself binding everything together */
+    fragment@4 {
+        target = <&spi0>;
+        __overlay__ {
+            /* needed to avoid dtc warning */
+            #address-cells = <1>;
+            #size-cells = <0>;
+            can1: mcp2515@1 {
+                reg = <1>;
+                compatible = "microchip,mcp2515";
+                pinctrl-names = "default";
+                pinctrl-0 = <&can1_pins>;
+                spi-max-frequency = <10000000>;
+                interrupt-parent = <&gpio>;
+                interrupts = <25 8>; /* IRQ_TYPE_LEVEL_LOW */
+                clocks = <&can1_osc>;
+            };
+        };
+    };
+    __overrides__ {
+        oscillator = <&can1_osc>,"clock-frequency:0";
+        spimaxfrequency = <&can1>,"spi-max-frequency:0";
+        interrupt = <&can1_pins>,"brcm,pins:0",<&can1>,"interrupts:0";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/mcp3008-overlay.dts b/arch/arm/boot/dts/overlays/mcp3008-overlay.dts
new file mode 100755
index 000000000000..957fdb9310af
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp3008-overlay.dts
@@ -0,0 +1,205 @@
+/*
+ * Device tree overlay for Microchip mcp3008 10-Bit A/D Converters
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target-path = "spi1/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target-path = "spi1/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@4 {
+		target-path = "spi1/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@5 {
+		target-path = "spi2/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@6 {
+		target-path = "spi2/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@7 {
+		target-path = "spi2/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@8 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_00: mcp3008@0 {
+				compatible = "microchip,mcp3008";
+				reg = <0>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_01: mcp3008@1 {
+				compatible = "microchip,mcp3008";
+				reg = <1>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@10 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_10: mcp3008@0 {
+				compatible = "microchip,mcp3008";
+				reg = <0>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@11 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_11: mcp3008@1 {
+				compatible = "microchip,mcp3008";
+				reg = <1>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@12 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_12: mcp3008@2 {
+				compatible = "microchip,mcp3008";
+				reg = <2>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@13 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_20: mcp3008@0 {
+				compatible = "microchip,mcp3008";
+				reg = <0>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@14 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_21: mcp3008@1 {
+				compatible = "microchip,mcp3008";
+				reg = <1>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@15 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3008_22: mcp3008@2 {
+				compatible = "microchip,mcp3008";
+				reg = <2>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	__overrides__ {
+		spi0-0-present = <0>, "+0+8";
+		spi0-1-present = <0>, "+1+9";
+		spi1-0-present = <0>, "+2+10";
+		spi1-1-present = <0>, "+3+11";
+		spi1-2-present = <0>, "+4+12";
+		spi2-0-present = <0>, "+5+13";
+		spi2-1-present = <0>, "+6+14";
+		spi2-2-present = <0>, "+7+15";
+		spi0-0-speed = <&mcp3008_00>, "spi-max-frequency:0";
+		spi0-1-speed = <&mcp3008_01>, "spi-max-frequency:0";
+		spi1-0-speed = <&mcp3008_10>, "spi-max-frequency:0";
+		spi1-1-speed = <&mcp3008_11>, "spi-max-frequency:0";
+		spi1-2-speed = <&mcp3008_12>, "spi-max-frequency:0";
+		spi2-0-speed = <&mcp3008_20>, "spi-max-frequency:0";
+		spi2-1-speed = <&mcp3008_21>, "spi-max-frequency:0";
+		spi2-2-speed = <&mcp3008_22>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/mcp3202-overlay.dts b/arch/arm/boot/dts/overlays/mcp3202-overlay.dts
new file mode 100755
index 000000000000..8e4e9f60f285
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp3202-overlay.dts
@@ -0,0 +1,205 @@
+/*
+ * Device tree overlay for Microchip mcp3202 12-Bit A/D Converters
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target-path = "spi1/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target-path = "spi1/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@4 {
+		target-path = "spi1/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@5 {
+		target-path = "spi2/spidev@0";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@6 {
+		target-path = "spi2/spidev@1";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@7 {
+		target-path = "spi2/spidev@2";
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@8 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_00: mcp3202@0 {
+				compatible = "mcp3202";
+				reg = <0>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@9 {
+		target = <&spi0>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_01: mcp3202@1 {
+				compatible = "mcp3202";
+				reg = <1>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@10 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_10: mcp3202@0 {
+				compatible = "mcp3202";
+				reg = <0>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@11 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_11: mcp3202@1 {
+				compatible = "mcp3202";
+				reg = <1>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@12 {
+		target = <&spi1>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_12: mcp3202@2 {
+				compatible = "mcp3202";
+				reg = <2>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@13 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_20: mcp3202@0 {
+				compatible = "mcp3202";
+				reg = <0>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@14 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_21: mcp3202@1 {
+				compatible = "mcp3202";
+				reg = <1>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	fragment@15 {
+		target = <&spi2>;
+		__dormant__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mcp3202_22: mcp3202@2 {
+				compatible = "mcp3202";
+				reg = <2>;
+				spi-max-frequency = <1600000>;
+			};
+		};
+	};
+
+	__overrides__ {
+		spi0-0-present = <0>, "+0+8";
+		spi0-1-present = <0>, "+1+9";
+		spi1-0-present = <0>, "+2+10";
+		spi1-1-present = <0>, "+3+11";
+		spi1-2-present = <0>, "+4+12";
+		spi2-0-present = <0>, "+5+13";
+		spi2-1-present = <0>, "+6+14";
+		spi2-2-present = <0>, "+7+15";
+		spi0-0-speed = <&mcp3202_00>, "spi-max-frequency:0";
+		spi0-1-speed = <&mcp3202_01>, "spi-max-frequency:0";
+		spi1-0-speed = <&mcp3202_10>, "spi-max-frequency:0";
+		spi1-1-speed = <&mcp3202_11>, "spi-max-frequency:0";
+		spi1-2-speed = <&mcp3202_12>, "spi-max-frequency:0";
+		spi2-0-speed = <&mcp3202_20>, "spi-max-frequency:0";
+		spi2-1-speed = <&mcp3202_21>, "spi-max-frequency:0";
+		spi2-2-speed = <&mcp3202_22>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/mcp342x-overlay.dts b/arch/arm/boot/dts/overlays/mcp342x-overlay.dts
new file mode 100644
index 000000000000..714eca5a4b5e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mcp342x-overlay.dts
@@ -0,0 +1,164 @@
+// Overlay for MCP3421-8 ADCs from Microchip Semiconductor
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3421: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3421";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3422: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3422";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3423: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3423";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3424: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3424";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3425: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3425","mcp3425";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@5 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3426: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3426";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@6 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3427: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3427";
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			mcp3428: mcp@68 {
+				reg = <0x68>;
+				compatible = "microchip,mcp3428";
+
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		addr = <&mcp3421>,"reg:0",
+		       <&mcp3422>,"reg:0",
+		       <&mcp3423>,"reg:0",
+		       <&mcp3424>,"reg:0",
+		       <&mcp3425>,"reg:0",
+		       <&mcp3426>,"reg:0",
+		       <&mcp3427>,"reg:0",
+		       <&mcp3428>,"reg:0";
+		mcp3421 = <0>,"=0";
+		mcp3422 = <0>,"=1";
+		mcp3423 = <0>,"=2";
+		mcp3424 = <0>,"=3";
+		mcp3425 = <0>,"=4";
+		mcp3426 = <0>,"=5";
+		mcp3427 = <0>,"=6";
+		mcp3428 = <0>,"=7";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/media-center-overlay.dts b/arch/arm/boot/dts/overlays/media-center-overlay.dts
new file mode 100644
index 000000000000..1b56963f4f16
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/media-center-overlay.dts
@@ -0,0 +1,134 @@
+/*
+ * Device Tree overlay for Media Center HAT by Pi Supply
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+
+			spidev@1{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			rpi_display_pins: rpi_display_pins {
+				brcm,pins = <12 23 24 25>;
+				brcm,function = <1 1 1 0>; /* out out out in */
+				brcm,pull = <0 0 0 2>; /* - - - up */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rpidisplay: rpi-display@0{
+				compatible = "ilitek,ili9341";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&rpi_display_pins>;
+
+				spi-max-frequency = <32000000>;
+				rotate = <90>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				reset-gpios = <&gpio 23 1>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 12 0>;
+				debug = <0>;
+			};
+
+			rpidisplay_ts: rpi-display-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <25 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 25 1>;
+				ti,x-plate-ohms = /bits/ 16 <60>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target-path = "/";
+		__overlay__ {
+			lirc_rpi: lirc_rpi {
+				compatible = "rpi,lirc-rpi";
+				pinctrl-names = "default";
+				pinctrl-0 = <&lirc_pins>;
+				status = "okay";
+
+				// Override autodetection of IR receiver circuit
+				// (0 = active high, 1 = active low, -1 = no override )
+				rpi,sense = <0xffffffff>;
+
+				// Software carrier
+				// (0 = off, 1 = on)
+				rpi,softcarrier = <1>;
+
+				// Invert output
+				// (0 = off, 1 = on)
+				rpi,invert = <0>;
+
+				// Enable debugging messages
+				// (0 = off, 1 = on)
+				rpi,debug = <0>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&gpio>;
+		__overlay__ {
+			lirc_pins: lirc_pins {
+				brcm,pins = <6 5>;
+				brcm,function = <1 0>; // out in
+				brcm,pull = <0 1>; // off down
+			};
+		};
+	};
+
+	__overrides__ {
+		speed =     <&rpidisplay>,"spi-max-frequency:0";
+		rotate =    <&rpidisplay>,"rotate:0";
+		fps =       <&rpidisplay>,"fps:0";
+		debug =     <&rpidisplay>,"debug:0", 
+		            <&lirc_rpi>,"rpi,debug:0";
+		xohms =     <&rpidisplay_ts>,"ti,x-plate-ohms;0";
+		swapxy =    <&rpidisplay_ts>,"ti,swap-xy?";
+		backlight = <&rpidisplay>,"led-gpios:4",
+		            <&rpi_display_pins>,"brcm,pins:0";
+
+		gpio_out_pin =  <&lirc_pins>,"brcm,pins:0";
+		gpio_in_pin =   <&lirc_pins>,"brcm,pins:4";
+		gpio_in_pull =  <&lirc_pins>,"brcm,pull:4";
+
+		sense =         <&lirc_rpi>,"rpi,sense:0";
+		softcarrier =   <&lirc_rpi>,"rpi,softcarrier:0";
+		invert =        <&lirc_rpi>,"rpi,invert:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/merus-amp-overlay.dts b/arch/arm/boot/dts/overlays/merus-amp-overlay.dts
new file mode 100644
index 000000000000..4501fbdc253d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/merus-amp-overlay.dts
@@ -0,0 +1,60 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for Infineon Merus-Amp
+/dts-v1/;
+/plugin/;
+#include <dt-bindings/pinctrl/bcm2835.h>
+#include <dt-bindings/gpio/gpio.h>
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			merus_amp_pins: merus_amp_pins {
+				brcm,pins = <23>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <2>; /* up */
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			merus_amp: ma120x0p@20 {
+				#sound-dai-cells = <0>;
+				compatible = "ma,ma120x0p";
+				reg = <0x20>;
+				status = "okay";
+				pinctrl-names = "default";
+				pinctrl-0 = <&merus_amp_pins>;
+				enable_gp-gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
+				mute_gp-gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
+				booster_gp-gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
+				error_gp-gpios = <&gpio 23 GPIO_ACTIVE_HIGH>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "merus,merus-amp";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/midi-uart0-overlay.dts b/arch/arm/boot/dts/overlays/midi-uart0-overlay.dts
new file mode 100644
index 000000000000..f7e44d29e101
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/midi-uart0-overlay.dts
@@ -0,0 +1,36 @@
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/clock/bcm2835.h>
+
+/*
+ * Fake a higher clock rate to get a larger divisor, and thereby a lower
+ * baudrate. The real clock is 48MHz, which we scale so that requesting
+ * 38.4kHz results in an actual 31.25kHz.
+ *
+ *   48000000*38400/31250 = 58982400
+ */
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			midi_clk: midi_clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-output-names = "uart0_pclk";
+				clock-frequency = <58982400>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&uart0>;
+		__overlay__ {
+			clocks = <&midi_clk>,
+			         <&clocks BCM2835_CLOCK_VPU>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/midi-uart1-overlay.dts b/arch/arm/boot/dts/overlays/midi-uart1-overlay.dts
new file mode 100644
index 000000000000..e0bc410acbff
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/midi-uart1-overlay.dts
@@ -0,0 +1,43 @@
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/clock/bcm2835-aux.h>
+
+/*
+ * Fake a higher clock rate to get a larger divisor, and thereby a lower
+ * baudrate. The real clock is 48MHz, which we scale so that requesting
+ * 38.4kHz results in an actual 31.25kHz.
+ *
+ *   48000000*38400/31250 = 58982400
+ */
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/clocks";
+		__overlay__ {
+			midi_clk: clock@5 {
+				compatible = "fixed-factor-clock";
+				#clock-cells = <0>;
+				clocks = <&aux BCM2835_AUX_CLOCK_UART>;
+				clock-mult = <38400>;
+				clock-div  = <31250>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		__overlay__ {
+			clocks = <&midi_clk>;
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			clock-output-names = "aux_uart", "aux_spi1", "aux_spi2";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/miniuart-bt-overlay.dts b/arch/arm/boot/dts/overlays/miniuart-bt-overlay.dts
new file mode 100644
index 000000000000..da49f14a0940
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/miniuart-bt-overlay.dts
@@ -0,0 +1,93 @@
+/dts-v1/;
+/plugin/;
+
+/* Switch Pi3 Bluetooth function to use the mini-UART (ttyS0) and restore
+   UART0/ttyAMA0 over GPIOs 14 & 15. Note that this may reduce the maximum
+   usable baudrate.
+
+   It is also necessary to edit /lib/systemd/system/hciuart.service and
+   replace ttyAMA0 with ttyS0, unless you have a system with udev rules
+   that create /dev/serial0 and /dev/serial1, in which case use /dev/serial1
+   instead because it will always be correct.
+
+   If cmdline.txt uses the alias serial0 to refer to the user-accessable port
+   then the firmware will replace with the appropriate port whether or not
+   this overlay is used.
+*/
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&uart0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&bt>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&uart1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins &bt_pins &fake_bt_cts>;
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&uart0_pins>;
+		__overlay__ {
+			brcm,pins;
+			brcm,function;
+			brcm,pull;
+		};
+	};
+
+	fragment@4 {
+		target = <&uart1_pins>;
+		__overlay__ {
+			brcm,pins = <32 33>;
+			brcm,function = <2>; /* alt5=UART1 */
+			brcm,pull = <0 2>;
+		};
+	};
+
+	fragment@5 {
+		target = <&gpio>;
+		__overlay__ {
+			fake_bt_cts: fake_bt_cts {
+				brcm,pins = <31>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@6 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial0 = "/soc/serial@7e201000";
+			serial1 = "/soc/serial@7e215040";
+		};
+	};
+
+	fragment@7 {
+		target = <&minibt>;
+		minibt_frag: __overlay__ {
+		};
+	};
+
+	__overrides__ {
+		krnbt = <&minibt_frag>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/mmc-overlay.dts b/arch/arm/boot/dts/overlays/mmc-overlay.dts
new file mode 100644
index 000000000000..c1a2f691aa1e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mmc-overlay.dts
@@ -0,0 +1,46 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&mmc>;
+		frag0: __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&mmc_pins>;
+			bus-width = <4>;
+			brcm,overclock-50 = <0>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			mmc_pins: mmc_pins {
+				brcm,pins = <48 49 50 51 52 53>;
+				brcm,function = <7>; /* alt3 */
+				brcm,pull = <0 2 2 2 2 2>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sdhost>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&mmcnr>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	__overrides__ {
+		overclock_50     = <&frag0>,"brcm,overclock-50:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/mpu6050-overlay.dts b/arch/arm/boot/dts/overlays/mpu6050-overlay.dts
new file mode 100644
index 000000000000..3109d90562ae
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mpu6050-overlay.dts
@@ -0,0 +1,28 @@
+// Definitions for MPU6050
+/dts-v1/;
+/plugin/;
+
+/ {
+        compatible = "brcm,bcm2835";
+
+        fragment@0 {
+                target = <&i2c1>;
+                __overlay__ {
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+                        status = "okay";
+                        clock-frequency = <400000>;
+
+                        mpu6050: mpu6050@68 {
+                                compatible = "invensense,mpu6050";
+                                reg = <0x68>;
+                                interrupt-parent = <&gpio>;
+                                interrupts = <4 1>;
+                        };
+                };
+        };
+
+        __overrides__ {
+                interrupt = <&mpu6050>,"interrupts:0";
+        };
+};
diff --git a/arch/arm/boot/dts/overlays/mz61581-overlay.dts b/arch/arm/boot/dts/overlays/mz61581-overlay.dts
new file mode 100644
index 000000000000..6e00e8b2ddf2
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/mz61581-overlay.dts
@@ -0,0 +1,117 @@
+/*
+ * Device Tree overlay for MZ61581-PI-EXT 2014.12.28 by Tontec
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			mz61581_pins: mz61581_pins {
+				brcm,pins = <4 15 18 25>;
+				brcm,function = <0 1 1 1>; /* in out out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mz61581: mz61581@0{
+				compatible = "samsung,s6d02a1";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&mz61581_pins>;
+
+				spi-max-frequency = <128000000>;
+				spi-cpol;
+				spi-cpha;
+
+				width = <320>;
+				height = <480>;
+				rotate = <270>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				txbuflen = <32768>;
+
+				reset-gpios = <&gpio 15 1>;
+				dc-gpios = <&gpio 25 0>;
+				led-gpios = <&gpio 18 0>;
+
+				init = <0x10000b0 00
+					0x1000011
+					0x20000ff
+					0x10000b3 0x02 0x00 0x00 0x00
+					0x10000c0 0x13 0x3b 0x00 0x02 0x00 0x01 0x00 0x43
+					0x10000c1 0x08 0x16 0x08 0x08
+					0x10000c4 0x11 0x07 0x03 0x03
+					0x10000c6 0x00
+					0x10000c8 0x03 0x03 0x13 0x5c 0x03 0x07 0x14 0x08 0x00 0x21 0x08 0x14 0x07 0x53 0x0c 0x13 0x03 0x03 0x21 0x00
+					0x1000035 0x00
+					0x1000036 0xa0
+					0x100003a 0x55
+					0x1000044 0x00 0x01
+					0x10000d0 0x07 0x07 0x1d 0x03
+					0x10000d1 0x03 0x30 0x10
+					0x10000d2 0x03 0x14 0x04
+					0x1000029
+					0x100002c>;
+
+				/* This is a workaround to make sure the init sequence slows down and doesn't fail */
+				debug = <3>;
+			};
+
+			mz61581_ts: mz61581_ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <4 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 4 0>;
+
+				ti,x-plate-ohms = /bits/ 16 <60>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =   <&mz61581>, "spi-max-frequency:0";
+		rotate =  <&mz61581>, "rotate:0";
+		fps =     <&mz61581>, "fps:0";
+		txbuflen = <&mz61581>, "txbuflen:0";
+		debug =   <&mz61581>, "debug:0";
+		xohms =   <&mz61581_ts>,"ti,x-plate-ohms;0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ov5647-overlay.dts b/arch/arm/boot/dts/overlays/ov5647-overlay.dts
new file mode 100644
index 000000000000..fd1e7a457f69
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ov5647-overlay.dts
@@ -0,0 +1,92 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for OV5647 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ov5647: ov5647@36 {
+				compatible = "ovti,ov5647";
+				reg = <0x36>;
+				status = "okay";
+
+				pwdn-gpios = <&gpio 41 1>, <&gpio 32 1>;
+				clocks = <&ov5647_clk>;
+
+				rotation = <0>;
+
+				port {
+					ov5647_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1 2>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <297000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&ov5647_0>;
+					data-lanes = <1 2>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&ov5647>,"pwdn-gpios:0";
+			cam0-pwdn      = <&ov5647>,"pwdn-gpios:4";
+			cam0-led-ctrl  = <&ov5647>,"pwdn-gpios:12";
+			cam0-led       = <&ov5647>,"pwdn-gpios:16";
+		};
+	};
+
+	fragment@5 {
+		target-path = "/";
+		__overlay__ {
+			ov5647_clk: camera-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <25000000>;
+			};
+		};
+	};
+
+	__overrides__ {
+		rotation = <&ov5647>,"rotation:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ov7251-overlay.dts b/arch/arm/boot/dts/overlays/ov7251-overlay.dts
new file mode 100644
index 000000000000..f04eafd4adf9
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ov7251-overlay.dts
@@ -0,0 +1,111 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for OV7251 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ov7251: ov7251@60 {
+				compatible = "ovti,ov7251";
+				reg = <0x60>;
+				status = "okay";
+
+				clocks = <&ov7251_clk>;
+				clock-names = "xclk";
+				clock-frequency = <24000000>;
+
+				vdddo-supply = <&ov7251_dovdd>;
+				vdda-supply = <&ov7251_avdd>;
+				vddd-supply = <&ov7251_dvdd>;
+
+				enable-gpios = <&gpio 41 GPIO_ACTIVE_HIGH>;
+
+				port {
+					ov7251_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <456000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&ov7251_0>;
+					data-lanes = <1>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path="/";
+		__overlay__ {
+			ov7251_avdd: fixedregulator@0 {
+				compatible = "regulator-fixed";
+				regulator-name = "ov7251_avdd";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+			};
+			ov7251_dovdd: fixedregulator@1 {
+				compatible = "regulator-fixed";
+				regulator-name = "ov7251_dovdd";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+			ov7251_dvdd: fixedregulator@2 {
+				compatible = "regulator-fixed";
+				regulator-name = "ov7251_dvdd";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+			};
+			ov7251_clk: ov7251-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <24000000>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&ov7251>,"enable-gpios:0";
+			cam0-pwdn      = <&ov7251>,"enable-gpios:4";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ov9281-overlay.dts b/arch/arm/boot/dts/overlays/ov9281-overlay.dts
new file mode 100644
index 000000000000..40b298d3dd86
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ov9281-overlay.dts
@@ -0,0 +1,111 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for OV9281 camera module on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ov9281: ov9281@60 {
+				compatible = "ovti,ov9281";
+				reg = <0x60>;
+				status = "okay";
+
+				clocks = <&ov9281_clk>;
+				clock-names = "xvclk";
+
+				avdd-supply = <&ov9281_avdd>;
+				dovdd-supply = <&ov9281_dovdd>;
+				dvdd-supply = <&ov9281_dvdd>;
+
+				port {
+					ov9281_0: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						data-lanes = <1 2>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <400000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&ov9281_0>;
+					data-lanes = <1 2>;
+					clock-noncontinuous;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path="/";
+		__overlay__ {
+			ov9281_avdd: fixedregulator@0 {
+				compatible = "regulator-fixed";
+				regulator-name = "ov9281_avdd";
+				regulator-min-microvolt = <2800000>;
+				regulator-max-microvolt = <2800000>;
+				gpio = <&gpio 41 GPIO_ACTIVE_HIGH>;
+				enable-active-high;
+			};
+			ov9281_dovdd: fixedregulator@1 {
+				compatible = "regulator-fixed";
+				regulator-name = "ov9281_dovdd";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+			};
+			ov9281_dvdd: fixedregulator@2 {
+				compatible = "regulator-fixed";
+				regulator-name = "ov9281_dvdd";
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+			};
+			ov9281_clk: ov9281-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <24000000>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target-path="/__overrides__";
+		__overlay__ {
+			cam0-pwdn-ctrl = <&ov9281_avdd>,"gpio:0";
+			cam0-pwdn      = <&ov9281_avdd>,"gpio:4";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/overlay_map.dts b/arch/arm/boot/dts/overlays/overlay_map.dts
new file mode 100644
index 000000000000..22b0ad1738ec
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/overlay_map.dts
@@ -0,0 +1,141 @@
+/dts-v1/;
+
+/ {
+	bmp085_i2c-sensor {
+		deprecated = "use i2c-sensor,bmp085";
+	};
+
+	highperi {
+		bcm2711;
+	};
+
+	i2c0-bcm2708 {
+		deprecated = "use i2c0";
+	};
+
+	i2c1-bcm2708 {
+		deprecated = "use i2c1";
+	};
+
+	i2c3 {
+		bcm2711;
+	};
+
+	i2c4 {
+		bcm2711;
+	};
+
+	i2c5 {
+		bcm2711;
+	};
+
+	i2c6 {
+		bcm2711;
+	};
+
+	lirc-rpi {
+		deprecated = "use gpio-ir";
+	};
+
+	pi3-act-led {
+		renamed = "act-led";
+	};
+
+	pi3-disable-bt {
+		renamed = "disable-bt";
+	};
+
+	pi3-disable-wifi {
+		renamed = "disable-wifi";
+	};
+
+	pi3-miniuart-bt {
+		renamed = "miniuart-bt";
+	};
+
+	rpivid-v4l2 {
+		bcm2711;
+	};
+
+	sdio-1bit {
+		deprecated = "use sdio,bus_width=1,gpios_22_25";
+	};
+
+	spi0-cs {
+		renamed = "spi0-2cs";
+	};
+
+	spi0-hw-cs {
+		deprecated = "no longer necessary";
+	};
+
+	spi3-1cs {
+		bcm2711;
+	};
+
+	spi3-2cs {
+		bcm2711;
+	};
+
+	spi4-1cs {
+		bcm2711;
+	};
+
+	spi4-2cs {
+		bcm2711;
+	};
+
+	spi5-1cs {
+		bcm2711;
+	};
+
+	spi5-2cs {
+		bcm2711;
+	};
+
+	spi6-1cs {
+		bcm2711;
+	};
+
+	spi6-2cs {
+		bcm2711;
+	};
+
+	uart2 {
+		bcm2711;
+	};
+
+	uart3 {
+		bcm2711;
+	};
+
+	uart4 {
+		bcm2711;
+	};
+
+	uart5 {
+		bcm2711;
+	};
+
+	upstream {
+		bcm2835;
+		bcm2711 = "upstream-pi4";
+	};
+
+	upstream-aux-interrupt {
+		deprecated = "no longer necessary";
+	};
+
+	upstream-pi4 {
+		bcm2711;
+	};
+
+	vc4-kms-v3d {
+		bcm2835;
+		bcm2711 = "vc4-kms-v3d-pi4";
+	};
+
+	vc4-kms-v3d-pi4 {
+		bcm2711;
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/papirus-overlay.dts b/arch/arm/boot/dts/overlays/papirus-overlay.dts
new file mode 100644
index 000000000000..7b6bcfd49c86
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/papirus-overlay.dts
@@ -0,0 +1,89 @@
+/* PaPiRus ePaper Screen by Pi Supply */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			display_temp: lm75@48 {
+				compatible = "lm75b";
+				reg = <0x48>;
+				status = "okay";
+				#thermal-sensor-cells = <0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			thermal-zones {
+				display {
+					polling-delay-passive = <0>;
+					polling-delay = <0>;
+					thermal-sensors = <&display_temp>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+
+			spidev@0{
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			repaper_pins: repaper_pins {
+				brcm,pins = <14 15 23 24 25>;
+				brcm,function = <1 1 1 1 0>; /* out out out out in */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			repaper: repaper@0{
+				compatible = "not_set";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&repaper_pins>;
+
+				spi-max-frequency = <8000000>;
+
+				panel-on-gpios = <&gpio 23 0>;
+				border-gpios = <&gpio 14 0>;
+				discharge-gpios = <&gpio 15 0>;
+				reset-gpios = <&gpio 24 0>;
+				busy-gpios = <&gpio 25 0>;
+
+				repaper-thermal-zone = "display";
+			};
+		};
+	};
+
+	__overrides__ {
+		panel = <&repaper>, "compatible";
+		speed = <&repaper>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pca953x-overlay.dts b/arch/arm/boot/dts/overlays/pca953x-overlay.dts
new file mode 100644
index 000000000000..8b6ee44665ce
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pca953x-overlay.dts
@@ -0,0 +1,240 @@
+// Definitions for NXP PCA953x family of I2C GPIO controllers on ARM I2C bus.
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			pca: pca@20 {
+				compatible = "nxp,pca9534";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca6416";
+		};
+	};
+	fragment@2 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9505";
+		};
+	};
+	fragment@3 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9535";
+		};
+	};
+	fragment@4 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9536";
+		};
+	};
+	fragment@5 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9537";
+		};
+	};
+	fragment@6 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9538";
+		};
+	};
+	fragment@7 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9539";
+		};
+	};
+	fragment@8 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9554";
+		};
+	};
+	fragment@9 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9555";
+		};
+	};
+	fragment@10 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9556";
+		};
+	};
+	fragment@11 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9557";
+		};
+	};
+	fragment@12 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9574";
+		};
+	};
+	fragment@13 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9575";
+		};
+	};
+	fragment@14 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca9698";
+		};
+	};
+	fragment@15 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca16416";
+		};
+	};
+	fragment@16 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca16524";
+		};
+	};
+	fragment@17 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "nxp,pca19555a";
+		};
+	};
+	fragment@18 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "maxim,max7310";
+		};
+	};
+	fragment@19 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "maxim,max7312";
+		};
+	};
+	fragment@20 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "maxim,max7313";
+		};
+	};
+	fragment@21 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "maxim,max7315";
+		};
+	};
+	fragment@22 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "ti,pca6107";
+		};
+	};
+	fragment@23 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "ti,tca6408";
+		};
+	};
+	fragment@24 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "ti,tca6416";
+		};
+	};
+	fragment@25 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "ti,tca6424";
+		};
+	};
+	fragment@26 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "ti,tca9539";
+		};
+	};
+	fragment@27 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "ti,tca9554";
+		};
+	};
+	fragment@28 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "onnn,cat9554";
+		};
+	};
+	fragment@29 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "onnn,pca9654";
+		};
+	};
+	fragment@30 {
+		target = <&pca>;
+		__dormant__ {
+			compatible = "exar,xra1202";
+		};
+	};
+
+	__overrides__ {
+		addr = <&pca>,"reg:0";
+		pca6416 = <0>, "+1";
+		pca9505 = <0>, "+2";
+		pca9535 = <0>, "+3";
+		pca9536 = <0>, "+4";
+		pca9537 = <0>, "+5";
+		pca9538 = <0>, "+6";
+		pca9539 = <0>, "+7";
+		pca9554 = <0>, "+8";
+		pca9555 = <0>, "+9";
+		pca9556 = <0>, "+10";
+		pca9557 = <0>, "+11";
+		pca9574 = <0>, "+12";
+		pca9575 = <0>, "+13";
+		pca9698 = <0>, "+14";
+		pca16416 = <0>, "+15";
+		pca16524 = <0>, "+16";
+		pca19555a = <0>, "+17";
+		max7310 = <0>, "+18";
+		max7312 = <0>, "+19";
+		max7313 = <0>, "+20";
+		max7315 = <0>, "+21";
+		pca6107 = <0>, "+22";
+		tca6408 = <0>, "+23";
+		tca6416 = <0>, "+24";
+		tca6424 = <0>, "+25";
+		tca9539 = <0>, "+26";
+		tca9554 = <0>, "+27";
+		cat9554 = <0>, "+28";
+		pca9654 = <0>, "+29";
+		xra1202 = <0>, "+30";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pibell-overlay.dts b/arch/arm/boot/dts/overlays/pibell-overlay.dts
new file mode 100644
index 000000000000..9333a9b09772
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pibell-overlay.dts
@@ -0,0 +1,81 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+
+    fragment@0 {
+        target-path = "/";
+        __overlay__ {
+            codec_out: spdif-transmitter {
+                #address-cells = <0>;
+                #size-cells = <0>;
+                #sound-dai-cells = <0>;
+                compatible = "linux,spdif-dit";
+                status = "okay";
+            };
+
+            codec_in: card-codec {
+                #sound-dai-cells = <0>;
+                compatible = "invensense,ics43432";
+                status = "okay";
+            };
+        };
+    };
+
+    fragment@1 {
+        target = <&i2s>;
+        __overlay__ {
+            #sound-dai-cells = <0>;
+            status = "okay";
+        };
+    };
+
+    fragment@2 {
+        target = <&sound>;
+        snd: __overlay__ {
+            compatible = "simple-audio-card";
+            simple-audio-card,name = "PiBell";
+
+            status="okay";
+
+            capture_link: simple-audio-card,dai-link@0 {
+                format = "i2s";
+
+                r_cpu_dai: cpu {
+                    sound-dai = <&i2s>;
+
+/* example TDM slot configuration
+                    dai-tdm-slot-num = <2>;
+                    dai-tdm-slot-width = <32>;
+*/
+                };
+
+                r_codec_dai: codec {
+                    sound-dai = <&codec_in>;
+                };
+            };
+
+            playback_link: simple-audio-card,dai-link@1 {
+                format = "i2s";
+
+                p_cpu_dai: cpu {
+                    sound-dai = <&i2s>;
+
+/* example TDM slot configuration
+                    dai-tdm-slot-num = <2>;
+                    dai-tdm-slot-width = <32>;
+*/
+                };
+
+                p_codec_dai: codec {
+                    sound-dai = <&codec_out>;
+                };
+            };
+        };
+    };
+
+    __overrides__ {
+        alsaname = <&snd>, "simple-audio-card,name";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/pifacedigital-overlay.dts b/arch/arm/boot/dts/overlays/pifacedigital-overlay.dts
new file mode 100644
index 000000000000..532a858683d6
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pifacedigital-overlay.dts
@@ -0,0 +1,144 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * PiFace Digital, Device Tree Overlay.
+ * Copyright (C) 2020 Thomas Preston <thomas.preston@codethink.co.uk>
+ *
+ * The PiFace Digital is a convenient breakout board for the Microchip mcp23s17
+ * SPI GPIO port expander.
+ *
+ * The first eight GPIOs 0..7 (bank A) are connected to eight output terminals
+ * and LEDs, plus two relays on the first two outputs. These output loads are
+ * active-high.
+ *
+ * The next eight GPIOs 8..15 (bank B) are connected to eight input terminals
+ * with four on-board switches connecting them to ground. Inputs devices are
+ * therefore expected to bridge terminals to ground, so the mcp23s17 pullups are
+ * activated for GPIO bank B.
+ *
+ * On PiFace Digital, the mcp23s17 is connected to the Raspberry Pi's SPI0 CS0
+ * bus. Each SPI bus supports up to eight addressable child devices. The PiFace
+ * Digital only supports addresses 0-4, which can be configured by jumpers JP1
+ * and JP2.
+ *
+ * You can tell the driver about these jumper configurations with the
+ * spi-present-mask bitmask:
+ *
+ *     | JP1 | JP2 | dtoverlay line in /boot/config.txt         |
+ *     | --- | --- | ------------------------------------------ |
+ *     |  0  |  0  | dtoverlay=pifacedigital                    |
+ *     |  0  |  0  | dtoverlay=pifacedigital:spi-present-mask=1 |
+ *     |  0  |  1  | dtoverlay=pifacedigital:spi-present-mask=2 |
+ *     |  1  |  0  | dtoverlay=pifacedigital:spi-present-mask=4 |
+ *     |  1  |  1  | dtoverlay=pifacedigital:spi-present-mask=8 |
+ *
+ * # Example
+ * Set the dtoverlay config in /boot/config.txt and power off the Raspberry Pi:
+ *
+ *     $ grep pifacedigital /boot/config.txt
+ *     dtoverlay=pifacedigital
+ *     $ sudo systemctl poweroff
+ *
+ * Attach the PiFace Digital and power on the Raspberry Pi.
+ * Then use the libgpiod tools to query the device:
+ *
+ *     $ sudo apt install gpiod
+ *     $ gpiodetect | grep mcp23s17
+ *     gpiochip2 [mcp23s17.0] (16 lines)
+ *
+ * Set GPIO outputs 0, 2 and 5:
+ *
+ *     $ gpioset gpiochip2 0=1 2=1 5=1
+ *
+ * Get GPIO status (input GPIO 8..15 are high, because they are active-low):
+ *
+ *     $ gpioget gpiochip2 {8..15}
+ *     1 1 1 1 1 1 1 1
+ *
+ * And even monitor interrupts:
+ *
+ *     $ gpiomon gpiochip2 {8..15}
+ *     event: FALLING EDGE offset: 11 timestamp: [1597361662.926741667]
+ *     event:  RISING EDGE offset: 11 timestamp: [1597361663.062555051]
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	/* Disable exposing /dev/spidev0.0 */
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	/* Add the PiFace Digital device node to the spi0.0 device. */
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pfdigital: pifacedigital@0 {
+				compatible = "microchip,mcp23s17";
+				reg = <0>;
+
+				/* Set devices present with 8-bit mask. */
+				microchip,spi-present-mask = <0x01>;
+				spi-max-frequency = <500000>;
+
+				gpio-controller;
+				#gpio-cells = <2>;
+
+				/* This device can pass through interrupts. */
+				interrupt-controller;
+				#interrupt-cells = <2>;
+
+				/* INTB is connected to GPIO 25.
+				 * 0x8 active-low level-sensitive
+				 */
+				interrupts = <25 0x8>;
+				interrupt-parent = <&gpio>;
+
+				/* Configure pull-ups on bank B GPIOs */
+				pinctrl-0 = <&pfdigital_irq &pfdigital_pullups>;
+				pinctrl-names = "default";
+				pfdigital_pullups: pinmux {
+					pins =
+						"gpio8",
+						"gpio9",
+						"gpio10",
+						"gpio11",
+						"gpio12",
+						"gpio13",
+						"gpio14",
+						"gpio15";
+					bias-pull-up;
+				};
+			};
+		};
+	};
+
+	/* PiFace Digital mcp23s17 INTB pin is connected to GPIO 25. The INTB
+	 * pin is configured active-low (0 on interrupt), so expect to see
+	 * FALLING_EDGE when inputs are bridged to ground (switch is pressed).
+	 */
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			pfdigital_irq: pifacedigital_irq {
+				brcm,pins = <25>;
+				brcm,function = <0>; /* input */
+			};
+		};
+	};
+
+	__overrides__ {
+		spi-present-mask = <&pfdigital>, "microchip,spi-present-mask:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/piglow-overlay.dts b/arch/arm/boot/dts/overlays/piglow-overlay.dts
new file mode 100644
index 000000000000..075bceef158c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/piglow-overlay.dts
@@ -0,0 +1,97 @@
+// Definitions for SN3218 LED driver from Si-En Technology on PiGlow
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sn3218@54 {
+				compatible = "si-en,sn3218";
+				reg = <0x54>;
+				#address-cells = <1>;
+				#size-cells = <0>;
+				status = "okay";
+
+				led@1 {
+					reg = <1>;
+					label = "piglow:red:led1";
+				};
+				led@2 {
+					reg = <2>;
+					label = "piglow:orange:led2";
+				};
+				led@3 {
+					reg = <3>;
+					label = "piglow:yellow:led3";
+				};
+				led@4 {
+					reg = <4>;
+					label = "piglow:green:led4";
+				};
+				led@5 {
+					reg = <5>;
+					label = "piglow:blue:led5";
+				};
+				led@6 {
+					reg = <6>;
+					label = "piglow:green:led6";
+				};
+				led@7 {
+					reg = <7>;
+					label = "piglow:red:led7";
+				};
+				led@8 {
+					reg = <8>;
+					label = "piglow:orange:led8";
+				};
+				led@9 {
+					reg = <9>;
+					label = "piglow:yellow:led9";
+				};
+				led@10 {
+					reg = <10>;
+					label = "piglow:white:led10";
+				};
+				led@11 {
+					reg = <11>;
+					label = "piglow:white:led11";
+				};
+				led@12 {
+					reg = <12>;
+					label = "piglow:blue:led12";
+				};
+				led@13 {
+					reg = <13>;
+					label = "piglow:white:led13";
+				};
+				led@14 {
+					reg = <14>;
+					label = "piglow:green:led14";
+				};
+				led@15 {
+					reg = <15>;
+					label = "piglow:blue:led15";
+				};
+				led@16 {
+					reg = <16>;
+					label = "piglow:yellow:led16";
+				};
+				led@17 {
+					reg = <17>;
+					label = "piglow:orange:led17";
+				};
+				led@18 {
+					reg = <18>;
+					label = "piglow:red:led18";
+				};
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/piscreen-overlay.dts b/arch/arm/boot/dts/overlays/piscreen-overlay.dts
new file mode 100644
index 000000000000..1ac75a248fab
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/piscreen-overlay.dts
@@ -0,0 +1,102 @@
+/*
+ * Device Tree overlay for PiScreen 3.5" display shield by Ozzmaker
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			piscreen_pins: piscreen_pins {
+				brcm,pins = <17 25 24 22>;
+				brcm,function = <0 1 1 1>; /* in out out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			piscreen: piscreen@0{
+				compatible = "ilitek,ili9486";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&piscreen_pins>;
+
+				spi-max-frequency = <24000000>;
+				rotate = <270>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				regwidth = <16>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 22 0>;
+				debug = <0>;
+
+				init = <0x10000b0 0x00
+				        0x1000011
+					0x20000ff
+					0x100003a 0x55
+					0x1000036 0x28
+					0x10000c2 0x44
+					0x10000c5 0x00 0x00 0x00 0x00
+					0x10000e0 0x0f 0x1f 0x1c 0x0c 0x0f 0x08 0x48 0x98 0x37 0x0a 0x13 0x04 0x11 0x0d 0x00
+					0x10000e1 0x0f 0x32 0x2e 0x0b 0x0d 0x05 0x47 0x75 0x37 0x06 0x10 0x03 0x24 0x20 0x00
+					0x10000e2 0x0f 0x32 0x2e 0x0b 0x0d 0x05 0x47 0x75 0x37 0x06 0x10 0x03 0x24 0x20 0x00
+					0x1000011
+					0x1000029>;
+			};
+
+			piscreen_ts: piscreen-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,swap-xy;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =		<&piscreen>,"spi-max-frequency:0";
+		rotate =	<&piscreen>,"rotate:0";
+		fps =		<&piscreen>,"fps:0";
+		debug =		<&piscreen>,"debug:0";
+		xohms =		<&piscreen_ts>,"ti,x-plate-ohms;0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/piscreen2r-overlay.dts b/arch/arm/boot/dts/overlays/piscreen2r-overlay.dts
new file mode 100644
index 000000000000..9d2b51101969
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/piscreen2r-overlay.dts
@@ -0,0 +1,106 @@
+ /*
+ * Device Tree overlay for PiScreen2 3.5" TFT with resistive touch  by Ozzmaker.com
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			piscreen2_pins: piscreen2_pins {
+				brcm,pins = <17 25 24 22>;
+				brcm,function = <0 1 1 1>; /* in out out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			piscreen2: piscreen2@0{
+				compatible = "ilitek,ili9486";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&piscreen2_pins>;
+				bgr;
+				spi-max-frequency = <64000000>;
+				rotate = <90>;
+				fps = <30>;
+				buswidth = <8>;
+				regwidth = <16>;
+				txbuflen = <32768>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 22 0>;
+				debug = <0>;
+
+                                init = <0x10000b0 0x00
+                                        0x1000011
+                                        0x20000ff
+                                        0x100003a 0x55
+                                        0x1000036 0x28
+                                        0x10000c0 0x11 0x09
+                                        0x10000c1 0x41
+                                        0x10000c5 0x00 0x00 0x00 0x00
+                                        0x10000b6 0x00 0x02
+                                        0x10000f7 0xa9 0x51 0x2c 0x2
+                                        0x10000be 0x00 0x04
+                                        0x10000e9 0x00
+                                        0x1000011
+                                        0x1000029>;
+
+			};
+
+			piscreen2_ts: piscreen2-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <17 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 17 0>;
+				ti,swap-xy;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =		<&piscreen2>,"spi-max-frequency:0";
+		rotate =	<&piscreen2>,"rotate:0";
+		fps =		<&piscreen2>,"fps:0";
+		debug =		<&piscreen2>,"debug:0";
+		xohms =		<&piscreen2_ts>,"ti,x-plate-ohms;0";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/pisound-overlay.dts b/arch/arm/boot/dts/overlays/pisound-overlay.dts
new file mode 100644
index 000000000000..49efb2b768fb
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pisound-overlay.dts
@@ -0,0 +1,120 @@
+/*
+ * Pisound Linux kernel module.
+ * Copyright (C) 2016-2017  Vilniaus Blokas UAB, https://blokas.io/pisound
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * as published by the Free Software Foundation; version 2 of the
+ * License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA  02110-1301, USA.
+ */
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pisound_spi: pisound_spi@0{
+				compatible = "blokaslabs,pisound-spi";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&spi0_pins>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@4 {
+		target-path = "/";
+		__overlay__ {
+			pcm5102a-codec {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm5102a";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@5 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "blokaslabs,pisound";
+			i2s-controller = <&i2s>;
+			status = "okay";
+
+			pinctrl-0 = <&pisound_button_pins>;
+
+			osr-gpios =
+				<&gpio 13 GPIO_ACTIVE_HIGH>,
+				<&gpio 26 GPIO_ACTIVE_HIGH>,
+				<&gpio 16 GPIO_ACTIVE_HIGH>;
+
+			reset-gpios =
+				<&gpio 12 GPIO_ACTIVE_HIGH>,
+				<&gpio 24 GPIO_ACTIVE_HIGH>;
+
+			data_available-gpios = <&gpio 25 GPIO_ACTIVE_HIGH>;
+
+			button-gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	fragment@6 {
+		target = <&gpio>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pisound_button_pins>;
+
+			pisound_button_pins: pisound_button_pins {
+				brcm,pins = <17>;
+				brcm,function = <0>; // Input
+				brcm,pull = <2>; // Pull-Up
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pitft22-overlay.dts b/arch/arm/boot/dts/overlays/pitft22-overlay.dts
new file mode 100644
index 000000000000..589ad13795b1
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pitft22-overlay.dts
@@ -0,0 +1,69 @@
+/*
+ * Device Tree overlay for pitft by Adafruit
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+        compatible = "brcm,bcm2835";
+
+        fragment@0 {
+                target = <&spi0>;
+                __overlay__ {
+                        status = "okay";
+
+                        spidev@0{
+                                status = "disabled";
+                        };
+
+                        spidev@1{
+                                status = "disabled";
+                        };
+                };
+        };
+
+        fragment@1 {
+                target = <&gpio>;
+                __overlay__ {
+                        pitft_pins: pitft_pins {
+                                brcm,pins = <25>;
+                                brcm,function = <1>; /* out */
+                                brcm,pull = <0>; /* none */
+                        };
+                };
+        };
+
+        fragment@2 {
+                target = <&spi0>;
+                __overlay__ {
+                        /* needed to avoid dtc warning */
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+
+                        pitft: pitft@0{
+                                compatible = "ilitek,ili9340";
+                                reg = <0>;
+                                pinctrl-names = "default";
+                                pinctrl-0 = <&pitft_pins>;
+
+                                spi-max-frequency = <32000000>;
+                                rotate = <90>;
+                                fps = <25>;
+                                bgr;
+                                buswidth = <8>;
+                                dc-gpios = <&gpio 25 0>;
+                                debug = <0>;
+                        };
+
+                };
+        };
+
+        __overrides__ {
+                speed =   <&pitft>,"spi-max-frequency:0";
+                rotate =  <&pitft>,"rotate:0";
+                fps =     <&pitft>,"fps:0";
+                debug =   <&pitft>,"debug:0";
+        };
+};
diff --git a/arch/arm/boot/dts/overlays/pitft28-capacitive-overlay.dts b/arch/arm/boot/dts/overlays/pitft28-capacitive-overlay.dts
new file mode 100644
index 000000000000..33901ee1db7a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pitft28-capacitive-overlay.dts
@@ -0,0 +1,91 @@
+/*
+ * Device Tree overlay for Adafruit PiTFT 2.8" capacitive touch screen
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+        compatible = "brcm,bcm2835";
+
+        fragment@0 {
+                target = <&spi0>;
+                __overlay__ {
+                        status = "okay";
+                };
+        };
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+        fragment@2 {
+                target = <&gpio>;
+                __overlay__ {
+                        pitft_pins: pitft_pins {
+                                brcm,pins = <24 25>;
+                                brcm,function = <0 1>; /* in out */
+                                brcm,pull = <2 0>; /* pullup none */
+                        };
+                };
+        };
+
+        fragment@3 {
+                target = <&spi0>;
+                __overlay__ {
+                        /* needed to avoid dtc warning */
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+
+                        pitft: pitft@0{
+                                compatible = "ilitek,ili9340";
+                                reg = <0>;
+                                pinctrl-names = "default";
+                                pinctrl-0 = <&pitft_pins>;
+
+                                spi-max-frequency = <32000000>;
+                                rotate = <90>;
+                                fps = <25>;
+                                bgr;
+                                buswidth = <8>;
+                                dc-gpios = <&gpio 25 0>;
+                                debug = <0>;
+                        };
+                };
+        };
+
+        fragment@4 {
+                target = <&i2c1>;
+                __overlay__ {
+                        /* needed to avoid dtc warning */
+                        #address-cells = <1>;
+                        #size-cells = <0>;
+
+                        ft6236: ft6236@38 {
+                                compatible = "focaltech,ft6236";
+                                reg = <0x38>;
+
+                                interrupt-parent = <&gpio>;
+                                interrupts = <24 2>;
+                                touchscreen-size-x = <240>;
+                                touchscreen-size-y = <320>;
+                        };
+                };
+        };
+
+        __overrides__ {
+                speed =   <&pitft>,"spi-max-frequency:0";
+                rotate =  <&pitft>,"rotate:0";
+                fps =     <&pitft>,"fps:0";
+                debug =   <&pitft>,"debug:0";
+                touch-sizex = <&ft6236>,"touchscreen-size-x?";
+                touch-sizey = <&ft6236>,"touchscreen-size-y?";
+                touch-invx  = <&ft6236>,"touchscreen-inverted-x?";
+                touch-invy  = <&ft6236>,"touchscreen-inverted-y?";
+                touch-swapxy = <&ft6236>,"touchscreen-swapped-x-y?";
+        };
+};
diff --git a/arch/arm/boot/dts/overlays/pitft28-resistive-overlay.dts b/arch/arm/boot/dts/overlays/pitft28-resistive-overlay.dts
new file mode 100644
index 000000000000..4a4a3f44c29d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pitft28-resistive-overlay.dts
@@ -0,0 +1,119 @@
+/*
+ * Device Tree overlay for Adafruit PiTFT 2.8" resistive touch screen
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			pitft_pins: pitft_pins {
+				brcm,pins = <24 25>;
+				brcm,function = <0 1>; /* in out */
+				brcm,pull = <2 0>; /* pullup none */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pitft: pitft@0{
+				compatible = "ilitek,ili9340";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pitft_pins>;
+
+				spi-max-frequency = <32000000>;
+				rotate = <90>;
+				fps = <25>;
+				bgr;
+				buswidth = <8>;
+				dc-gpios = <&gpio 25 0>;
+				debug = <0>;
+			};
+
+			pitft_ts@1 {
+				compatible = "st,stmpe610";
+				reg = <1>;
+
+				spi-max-frequency = <500000>;
+				irq-gpio = <&gpio 24 0x2>; /* IRQF_TRIGGER_FALLING */
+				interrupts = <24 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				interrupt-controller;
+
+				stmpe_touchscreen {
+					compatible = "st,stmpe-ts";
+					st,sample-time = <4>;
+					st,mod-12b = <1>;
+					st,ref-sel = <0>;
+					st,adc-freq = <2>;
+					st,ave-ctrl = <3>;
+					st,touch-det-delay = <4>;
+					st,settling = <2>;
+					st,fraction-z = <7>;
+					st,i-drive = <0>;
+				};
+
+				stmpe_gpio: stmpe_gpio {
+					#gpio-cells = <2>;
+					compatible = "st,stmpe-gpio";
+					/*
+					 * only GPIO2 is wired/available
+					 * and it is wired to the backlight
+					 */
+					st,norequest-mask = <0x7b>;
+				};
+			};
+		};
+	};
+
+	fragment@5 {
+		target-path = "/soc";
+		__overlay__ {
+			backlight {
+				compatible = "gpio-backlight";
+				gpios = <&stmpe_gpio 2 0>;
+				default-on;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed =   <&pitft>,"spi-max-frequency:0";
+		rotate =  <&pitft>,"rotate:0";
+		fps =     <&pitft>,"fps:0";
+		debug =   <&pitft>,"debug:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pitft35-resistive-overlay.dts b/arch/arm/boot/dts/overlays/pitft35-resistive-overlay.dts
new file mode 100644
index 000000000000..37629f18a740
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pitft35-resistive-overlay.dts
@@ -0,0 +1,119 @@
+/*
+ * Device Tree overlay for Adafruit PiTFT 3.5" resistive touch screen
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			pitft_pins: pitft_pins {
+				brcm,pins = <24 25>;
+				brcm,function = <0 1>; /* in out */
+				brcm,pull = <2 0>; /* pullup none */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pitft: pitft@0{
+				compatible = "himax,hx8357d", "adafruit,yx350hv15";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&pitft_pins>;
+
+				spi-max-frequency = <32000000>;
+				rotate = <90>;
+				fps = <25>;
+				bgr;
+				buswidth = <8>;
+				dc-gpios = <&gpio 25 0>;
+				debug = <0>;
+			};
+
+			pitft_ts@1 {
+				compatible = "st,stmpe610";
+				reg = <1>;
+
+				spi-max-frequency = <500000>;
+				irq-gpio = <&gpio 24 0x2>; /* IRQF_TRIGGER_FALLING */
+				interrupts = <24 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				interrupt-controller;
+
+				stmpe_touchscreen {
+					compatible = "st,stmpe-ts";
+					st,sample-time = <4>;
+					st,mod-12b = <1>;
+					st,ref-sel = <0>;
+					st,adc-freq = <2>;
+					st,ave-ctrl = <3>;
+					st,touch-det-delay = <4>;
+					st,settling = <2>;
+					st,fraction-z = <7>;
+					st,i-drive = <0>;
+				};
+
+				stmpe_gpio: stmpe_gpio {
+					#gpio-cells = <2>;
+					compatible = "st,stmpe-gpio";
+					/*
+					 * only GPIO2 is wired/available
+					 * and it is wired to the backlight
+					 */
+					st,norequest-mask = <0x7b>;
+				};
+			};
+		};
+	};
+
+	fragment@5 {
+		target-path = "/soc";
+		__overlay__ {
+			backlight {
+				compatible = "gpio-backlight";
+				gpios = <&stmpe_gpio 2 0>;
+				default-on;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed =   <&pitft>,"spi-max-frequency:0";
+		rotate =  <&pitft>,"rotate:0";
+		fps =     <&pitft>,"fps:0";
+		debug =   <&pitft>,"debug:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pps-gpio-overlay.dts b/arch/arm/boot/dts/overlays/pps-gpio-overlay.dts
new file mode 100644
index 000000000000..524a1c1d3670
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pps-gpio-overlay.dts
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			pps: pps@12 {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&gpio 18 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			pps_pins: pps_pins@12 {
+				brcm,pins =     <18>;
+				brcm,function = <0>;    // in
+				brcm,pull =     <0>;    // off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin = <&pps>,"gpios:4",
+			  <&pps>,"reg:0",
+			  <&pps_pins>,"brcm,pins:0",
+			  <&pps_pins>,"reg:0";
+		assert_falling_edge = <&pps>,"assert-falling-edge?";
+		capture_clear = <&pps>,"capture-clear?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts b/arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts
new file mode 100644
index 000000000000..4ddbbfa04065
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pwm-2chan-overlay.dts
@@ -0,0 +1,49 @@
+/dts-v1/;
+/plugin/;
+
+/*
+This is the 2-channel overlay - only use it if you need both channels.
+
+Legal pin,function combinations for each channel:
+  PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+  PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+
+N.B.:
+  1) Pin 18 is the only one available on all platforms, and
+     it is the one used by the I2S audio interface.
+     Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+  2) The onboard analogue audio output uses both PWM channels.
+  3) So be careful mixing audio and PWM.
+*/
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			pwm_pins: pwm_pins {
+				brcm,pins = <18 19>;
+				brcm,function = <2 2>; /* Alt5 */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&pwm>;
+		frag1: __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm_pins>;
+			assigned-clock-rates = <100000000>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		pin   = <&pwm_pins>,"brcm,pins:0";
+		pin2  = <&pwm_pins>,"brcm,pins:4";
+		func  = <&pwm_pins>,"brcm,function:0";
+		func2 = <&pwm_pins>,"brcm,function:4";
+		clock = <&frag1>,"assigned-clock-rates:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pwm-ir-tx-overlay.dts b/arch/arm/boot/dts/overlays/pwm-ir-tx-overlay.dts
new file mode 100644
index 000000000000..119caf746b3b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pwm-ir-tx-overlay.dts
@@ -0,0 +1,40 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			pwm0_pins: pwm0_pins {
+				brcm,pins = <18>;
+				brcm,function = <2>; /* Alt5 */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm0_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			pwm-ir-transmitter {
+				compatible = "pwm-ir-tx";
+				pwms = <&pwm 0 100>;
+			};
+		};
+	};
+
+	__overrides__ {
+		gpio_pin = <&pwm0_pins>, "brcm,pins:0";
+		func = <&pwm0_pins>,"brcm,function:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/pwm-overlay.dts b/arch/arm/boot/dts/overlays/pwm-overlay.dts
new file mode 100644
index 000000000000..92876ab3bc8c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pwm-overlay.dts
@@ -0,0 +1,45 @@
+/dts-v1/;
+/plugin/;
+
+/*
+Legal pin,function combinations for each channel:
+  PWM0: 12,4(Alt0) 18,2(Alt5) 40,4(Alt0)            52,5(Alt1)
+  PWM1: 13,4(Alt0) 19,2(Alt5) 41,4(Alt0) 45,4(Alt0) 53,5(Alt1)
+
+N.B.:
+  1) Pin 18 is the only one available on all platforms, and
+     it is the one used by the I2S audio interface.
+     Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
+  2) The onboard analogue audio output uses both PWM channels.
+  3) So be careful mixing audio and PWM.
+*/
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			pwm_pins: pwm_pins {
+				brcm,pins = <18>;
+				brcm,function = <2>; /* Alt5 */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&pwm>;
+		frag1: __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm_pins>;
+			assigned-clock-rates = <100000000>;
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		pin   = <&pwm_pins>,"brcm,pins:0";
+		func  = <&pwm_pins>,"brcm,function:0";
+		clock = <&frag1>,"assigned-clock-rates:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/qca7000-overlay.dts b/arch/arm/boot/dts/overlays/qca7000-overlay.dts
new file mode 100644
index 000000000000..9a451202a2eb
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/qca7000-overlay.dts
@@ -0,0 +1,55 @@
+// Overlay for the Qualcomm Atheros QCA7000 on I2SE's PLC Stamp micro EVK
+// Visit: https://www.i2se.com/product/plc-stamp-micro-evk for details
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			eth1: qca7000@0 {
+				compatible = "qca,qca7000";
+				reg = <0>; /* CE0 */
+				pinctrl-names = "default";
+				pinctrl-0 = <&eth1_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <23 0x1>; /* rising edge */
+				spi-max-frequency = <12000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			eth1_pins: eth1_pins {
+				brcm,pins = <23>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&eth1>, "interrupts:0",
+		          <&eth1_pins>, "brcm,pins:0";
+		speed   = <&eth1>, "spi-max-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rotary-encoder-overlay.dts b/arch/arm/boot/dts/overlays/rotary-encoder-overlay.dts
new file mode 100644
index 000000000000..ea1d952734e9
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rotary-encoder-overlay.dts
@@ -0,0 +1,59 @@
+// Device tree overlay for GPIO connected rotary encoder.
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			rotary_pins: rotary_pins@4 {
+				brcm,pins = <4 17>; /* gpio 4 17 */
+				brcm,function = <0 0>; /* input */
+				brcm,pull = <2 2>; /* pull-up */
+			};
+
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			rotary: rotary@4 {
+				compatible = "rotary-encoder";
+				status = "okay";
+				pinctrl-names = "default";
+				pinctrl-0 = <&rotary_pins>;
+				gpios = <&gpio 4 0>, <&gpio 17 0>;
+				linux,axis = <0>; /* REL_X */
+				rotary-encoder,encoding = "gray";
+				rotary-encoder,steps = <24>; /* 24 default */
+				rotary-encoder,steps-per-period = <1>; /* corresponds to full period mode. See README */
+			};
+		};
+
+	};  
+
+	__overrides__ {
+		pin_a =		    <&rotary>,"gpios:4",
+				    <&rotary_pins>,"brcm,pins:0",
+				    /* modify reg values to allow multiple instantiation */
+				    <&rotary>,"reg:0",
+				    <&rotary_pins>,"reg:0";
+		pin_b =		    <&rotary>,"gpios:16",
+				    <&rotary_pins>,"brcm,pins:4";
+		relative_axis =     <&rotary>,"rotary-encoder,relative-axis?";
+		linux_axis =        <&rotary>,"linux,axis:0";
+		rollover =          <&rotary>,"rotary-encoder,rollover?";
+		steps-per-period =  <&rotary>,"rotary-encoder,steps-per-period:0";
+		steps =             <&rotary>,"rotary-encoder,steps:0";
+		wakeup =            <&rotary>,"wakeup-source?";
+		encoding =          <&rotary>,"rotary-encoder,encoding";
+                /* legacy parameters*/
+		rotary0_pin_a =     <&rotary>,"gpios:4",
+		                    <&rotary_pins>,"brcm,pins:0";
+		rotary0_pin_b =     <&rotary>,"gpios:16",
+		                    <&rotary_pins>,"brcm,pins:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-backlight-overlay.dts b/arch/arm/boot/dts/overlays/rpi-backlight-overlay.dts
new file mode 100644
index 000000000000..cac5e44c6ec5
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-backlight-overlay.dts
@@ -0,0 +1,21 @@
+/*
+ * Devicetree overlay for mailbox-driven Raspberry Pi DSI Display
+ * backlight controller
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			rpi_backlight: rpi_backlight {
+				compatible = "raspberrypi,rpi-backlight";
+				firmware = <&firmware>;
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-cirrus-wm5102-overlay.dts b/arch/arm/boot/dts/overlays/rpi-cirrus-wm5102-overlay.dts
new file mode 100644
index 000000000000..ed0c2745399f
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-cirrus-wm5102-overlay.dts
@@ -0,0 +1,172 @@
+// Definitions for the Cirrus Logic Audio Card
+/dts-v1/;
+/plugin/;
+#include <dt-bindings/pinctrl/bcm2835.h>
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/mfd/arizona.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			wlf_5102_pins: wlf_5102_pins {
+				brcm,pins = <17 22 27>;
+				brcm,function = <
+					BCM2835_FSEL_GPIO_OUT
+					BCM2835_FSEL_GPIO_OUT
+					BCM2835_FSEL_GPIO_IN
+				>;
+			};
+			wlf_8804_pins: wlf_8804_pins {
+				brcm,pins = <8>;
+				brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0_cs_pins>;
+		__overlay__ {
+			brcm,pins = <7>;
+			brcm,function = <BCM2835_FSEL_GPIO_OUT>;
+		};
+	};
+
+
+	fragment@3 {
+		target-path = "/";
+		__overlay__ {
+			rpi_cirrus_reg_1v8: rpi_cirrus_reg_1v8 {
+				compatible = "regulator-fixed";
+				regulator-name = "RPi-Cirrus 1v8";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-always-on;
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@5 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@6 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+			cs-gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
+
+			wm5102@0{
+				compatible = "wlf,wm5102";
+				reg = <0>;
+
+				pinctrl-names = "default";
+				pinctrl-0 = <&wlf_5102_pins>;
+
+				spi-max-frequency = <500000>;
+
+				interrupt-parent = <&gpio>;
+				interrupts = <27 8>;
+				interrupt-controller;
+				#interrupt-cells = <2>;
+
+				gpio-controller;
+				#gpio-cells = <2>;
+
+				LDOVDD-supply = <&rpi_cirrus_reg_1v8>;
+				AVDD-supply = <&rpi_cirrus_reg_1v8>;
+				DBVDD1-supply = <&rpi_cirrus_reg_1v8>;
+				DBVDD2-supply = <&vdd_3v3_reg>;
+				DBVDD3-supply = <&vdd_3v3_reg>;
+				CPVDD-supply = <&rpi_cirrus_reg_1v8>;
+				SPKVDDL-supply = <&vdd_5v0_reg>;
+				SPKVDDR-supply = <&vdd_5v0_reg>;
+				DCVDD-supply = <&arizona_ldo1>;
+
+				reset-gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
+				wlf,ldoena = <&gpio 22 GPIO_ACTIVE_HIGH>;
+				wlf,gpio-defaults = <
+					ARIZONA_GP_DEFAULT
+					ARIZONA_GP_DEFAULT
+					ARIZONA_GP_DEFAULT
+					ARIZONA_GP_DEFAULT
+					ARIZONA_GP_DEFAULT
+				>;
+				wlf,micd-configs = <0 1 0>;
+				wlf,dmic-ref = <
+					ARIZONA_DMIC_MICVDD
+					ARIZONA_DMIC_MICBIAS2
+					ARIZONA_DMIC_MICVDD
+					ARIZONA_DMIC_MICVDD
+				>;
+				wlf,inmode = <
+					ARIZONA_INMODE_DIFF
+					ARIZONA_INMODE_DMIC
+					ARIZONA_INMODE_SE
+					ARIZONA_INMODE_DIFF
+				>;
+				status = "okay";
+
+				arizona_ldo1: ldo1 {
+					regulator-name = "LDO1";
+					// default constraints as in
+					// arizona-ldo1.c
+					regulator-min-microvolt = <1200000>;
+					regulator-max-microvolt = <1800000>;
+				};
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			wm8804@3b {
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				status = "okay";
+
+				pinctrl-names = "default";
+				pinctrl-0 = <&wlf_8804_pins>;
+
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+				wlf,reset-gpio = <&gpio 8 GPIO_ACTIVE_HIGH>;
+			};
+		};
+	};
+
+	fragment@8 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "wlf,rpi-cirrus";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-dac-overlay.dts b/arch/arm/boot/dts/overlays/rpi-dac-overlay.dts
new file mode 100644
index 000000000000..07a915342702
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-dac-overlay.dts
@@ -0,0 +1,34 @@
+// Definitions for RPi DAC
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pcm1794a-codec {
+				#sound-dai-cells = <0>;
+				compatible = "ti,pcm1794a";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "rpi,rpi-dac";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-display-overlay.dts b/arch/arm/boot/dts/overlays/rpi-display-overlay.dts
new file mode 100644
index 000000000000..de87432ff2be
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-display-overlay.dts
@@ -0,0 +1,91 @@
+/*
+ * Device Tree overlay for rpi-display by Watterott
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			rpi_display_pins: rpi_display_pins {
+				brcm,pins = <18 23 24 25>;
+				brcm,function = <1 1 1 0>; /* out out out in */
+				brcm,pull = <0 0 0 2>; /* - - - up */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rpidisplay: rpi-display@0{
+				compatible = "ilitek,ili9341";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&rpi_display_pins>;
+
+				spi-max-frequency = <32000000>;
+				rotate = <270>;
+				bgr;
+				fps = <30>;
+				buswidth = <8>;
+				reset-gpios = <&gpio 23 1>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 18 0>;
+				debug = <0>;
+			};
+
+			rpidisplay_ts: rpi-display-ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+
+				spi-max-frequency = <2000000>;
+				interrupts = <25 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 25 1>;
+				ti,x-plate-ohms = /bits/ 16 <60>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+	__overrides__ {
+		speed =     <&rpidisplay>,"spi-max-frequency:0";
+		rotate =    <&rpidisplay>,"rotate:0";
+		fps =       <&rpidisplay>,"fps:0";
+		debug =     <&rpidisplay>,"debug:0";
+		xohms =     <&rpidisplay_ts>,"ti,x-plate-ohms;0";
+		swapxy =    <&rpidisplay_ts>,"ti,swap-xy?";
+		backlight = <&rpidisplay>,"led-gpios:4",
+		            <&rpi_display_pins>,"brcm,pins:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts b/arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts
new file mode 100644
index 000000000000..8483c4f4b2eb
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-ft5406-overlay.dts
@@ -0,0 +1,25 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/soc/firmware";
+		__overlay__ {
+			ts: touchscreen {
+				compatible = "raspberrypi,firmware-ts";
+				touchscreen-size-x = <800>;
+				touchscreen-size-y = <480>;
+			};
+		};
+	};
+
+	__overrides__ {
+		touchscreen-size-x = <&ts>,"touchscreen-size-x:0";
+		touchscreen-size-y = <&ts>,"touchscreen-size-y:0";
+		touchscreen-inverted-x = <&ts>,"touchscreen-inverted-x?";
+		touchscreen-inverted-y = <&ts>,"touchscreen-inverted-y?";
+		touchscreen-swapped-x-y = <&ts>,"touchscreen-swapped-x-y?";
+        };
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-poe-overlay.dts b/arch/arm/boot/dts/overlays/rpi-poe-overlay.dts
new file mode 100644
index 000000000000..544038b614e1
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-poe-overlay.dts
@@ -0,0 +1,95 @@
+/*
+ * Overlay for the Raspberry Pi POE HAT.
+ */
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			fan0: rpi-poe-fan@0 {
+				compatible = "raspberrypi,rpi-poe-fan";
+				firmware = <&firmware>;
+				cooling-min-state = <0>;
+				cooling-max-state = <4>;
+				#cooling-cells = <2>;
+				cooling-levels = <0 31 63 150 255>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&cpu_thermal>;
+		__overlay__ {
+			trips {
+				trip0: trip0 {
+					temperature = <40000>;
+					hysteresis = <2000>;
+					type = "active";
+				};
+				trip1: trip1 {
+					temperature = <45000>;
+					hysteresis = <2000>;
+					type = "active";
+				};
+				trip2: trip2 {
+					temperature = <50000>;
+					hysteresis = <2000>;
+					type = "active";
+				};
+				trip3: trip3 {
+					temperature = <55000>;
+					hysteresis = <5000>;
+					type = "active";
+				};
+			};
+			cooling-maps {
+				map0 {
+					trip = <&trip0>;
+					cooling-device = <&fan0 0 1>;
+				};
+				map1 {
+					trip = <&trip1>;
+					cooling-device = <&fan0 1 2>;
+				};
+				map2 {
+					trip = <&trip2>;
+					cooling-device = <&fan0 2 3>;
+				};
+				map3 {
+					trip = <&trip3>;
+					cooling-device = <&fan0 3 4>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target-path = "/__overrides__";
+		__overlay__ {
+			poe_fan_temp0 =		<&trip0>,"temperature:0";
+			poe_fan_temp0_hyst =	<&trip0>,"hysteresis:0";
+			poe_fan_temp1 =		<&trip1>,"temperature:0";
+			poe_fan_temp1_hyst =	<&trip1>,"hysteresis:0";
+			poe_fan_temp2 =		<&trip2>,"temperature:0";
+			poe_fan_temp2_hyst =	<&trip2>,"hysteresis:0";
+			poe_fan_temp3 =		<&trip3>,"temperature:0";
+			poe_fan_temp3_hyst =	<&trip3>,"hysteresis:0";
+		};
+	};
+
+	__overrides__ {
+		poe_fan_temp0 =		<&trip0>,"temperature:0";
+		poe_fan_temp0_hyst =	<&trip0>,"hysteresis:0";
+		poe_fan_temp1 =		<&trip1>,"temperature:0";
+		poe_fan_temp1_hyst =	<&trip1>,"hysteresis:0";
+		poe_fan_temp2 =		<&trip2>,"temperature:0";
+		poe_fan_temp2_hyst =	<&trip2>,"hysteresis:0";
+		poe_fan_temp3 =		<&trip3>,"temperature:0";
+		poe_fan_temp3_hyst =	<&trip3>,"hysteresis:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-proto-overlay.dts b/arch/arm/boot/dts/overlays/rpi-proto-overlay.dts
new file mode 100644
index 000000000000..9cda044a0f62
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-proto-overlay.dts
@@ -0,0 +1,39 @@
+// Definitions for Rpi-Proto
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8731@1a {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8731";
+				reg = <0x1a>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "rpi,rpi-proto";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-sense-overlay.dts b/arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
new file mode 100644
index 000000000000..89d8d2ea6b2e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-sense-overlay.dts
@@ -0,0 +1,47 @@
+// rpi-sense HAT
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rpi-sense@46 {
+				compatible = "rpi,rpi-sense";
+				reg = <0x46>;
+				keys-int-gpios = <&gpio 23 1>;
+				status = "okay";
+			};
+
+			lsm9ds1-magn@1c {
+				compatible = "st,lsm9ds1-magn";
+				reg = <0x1c>;
+				status = "okay";
+			};
+
+			lsm9ds1-accel6a {
+				compatible = "st,lsm9ds1-accel";
+				reg = <0x6a>;
+				status = "okay";
+			};
+
+			lps25h-press@5c {
+				compatible = "st,lps25h-press";
+				reg = <0x5c>;
+				status = "okay";
+			};
+
+			hts221-humid@5f {
+				compatible = "st,hts221-humid", "st,hts221";
+				reg = <0x5f>;
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rpi-tv-overlay.dts b/arch/arm/boot/dts/overlays/rpi-tv-overlay.dts
new file mode 100644
index 000000000000..3c97a545d820
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpi-tv-overlay.dts
@@ -0,0 +1,34 @@
+// rpi-tv HAT
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			cxd2880@0 {
+				compatible = "sony,cxd2880";
+				reg = <0>; /* CE0 */
+				spi-max-frequency = <50000000>;
+				status = "okay";
+			};
+		};
+	};
+
+};
diff --git a/arch/arm/boot/dts/overlays/rpivid-v4l2-overlay.dts b/arch/arm/boot/dts/overlays/rpivid-v4l2-overlay.dts
new file mode 100644
index 000000000000..0a611b31b9d4
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rpivid-v4l2-overlay.dts
@@ -0,0 +1,61 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for Raspberry Pi video decode engine
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&scb>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <2>;
+			#size-cells = <2>;
+
+			codec@7eb10000 {
+				compatible = "raspberrypi,rpivid-vid-decoder";
+				reg = <0x0 0x7eb10000  0x0 0x1000>,  /* INTC */
+				      <0x0 0x7eb00000  0x0 0x10000>; /* HEVC */
+				reg-names = "intc",
+					    "hevc";
+
+				interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
+
+				clocks = <&hevc_clk>;
+				clock-names = "hevc";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&scb>;
+		__overlay__ {
+			hevc-decoder@7eb00000 {
+				status = "disabled";
+			};
+			rpivid-local-intc@7eb10000 {
+				status = "disabled";
+			};
+			h264-decoder@7eb20000 {
+				status = "disabled";
+			};
+			vp9-decoder@7eb30000 {
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			hevc_clk: hevc_clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <500000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/rra-digidac1-wm8741-audio-overlay.dts b/arch/arm/boot/dts/overlays/rra-digidac1-wm8741-audio-overlay.dts
new file mode 100644
index 000000000000..87e9a326eff1
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/rra-digidac1-wm8741-audio-overlay.dts
@@ -0,0 +1,49 @@
+// Definitions for RRA DigiDAC1 Audio card
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			wm8804@3b {
+				#sound-dai-cells = <0>;
+				compatible = "wlf,wm8804";
+				reg = <0x3b>;
+				status = "okay";
+				PVDD-supply = <&vdd_3v3_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+			};
+
+			wm8742: wm8741@1a {
+				compatible = "wlf,wm8741";
+				reg = <0x1a>;
+				status = "okay";
+				AVDD-supply = <&vdd_5v0_reg>;
+				DVDD-supply = <&vdd_3v3_reg>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "rra,digidac1-soundcard";
+			i2s-controller = <&i2s>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sainsmart18-overlay.dts b/arch/arm/boot/dts/overlays/sainsmart18-overlay.dts
new file mode 100644
index 000000000000..c51f1c030a55
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sainsmart18-overlay.dts
@@ -0,0 +1,52 @@
+/*
+ * Device Tree overlay for the Sainsmart 1.8" TFT LCD with ST7735R chip 160x128
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			ss18: sainsmart18@0 {
+				compatible = "fbtft,sainsmart18";
+				reg = <0>;
+				pinctrl-names = "default";
+				spi-max-frequency = <40000000>;
+				rotate = <90>;
+				buswidth = <8>;
+				fps = <50>;
+				height = <160>;
+				width = <128>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				debug = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed     = <&ss18>,"spi-max-frequency:0";
+		rotate    = <&ss18>,"rotate:0";
+		fps       = <&ss18>,"fps:0";
+		bgr       = <&ss18>,"bgr?";
+		debug     = <&ss18>,"debug:0";
+		dc_pin    = <&ss18>,"dc-gpios:4";
+		reset_pin = <&ss18>,"reset-gpios:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts b/arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts
new file mode 100644
index 000000000000..04d74d62897b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sc16is750-i2c-overlay.dts
@@ -0,0 +1,43 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sc16is750: sc16is750@48 {
+				compatible = "nxp,sc16is750";
+				reg = <0x48>; /* i2c address */
+				clocks = <&sc16is750_clk>;
+				interrupt-parent = <&gpio>;
+				interrupts = <24 2>; /* IRQ_TYPE_EDGE_FALLING */
+				gpio-controller;
+				#gpio-cells = <2>;
+				i2c-max-frequency = <400000>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			sc16is750_clk: sc16is750_i2c_clk@48 {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <14745600>;
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&sc16is750>,"interrupts:0";
+		addr = <&sc16is750>,"reg:0", <&sc16is750_clk>,"name";
+		xtal = <&sc16is750_clk>,"clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sc16is752-i2c-overlay.dts b/arch/arm/boot/dts/overlays/sc16is752-i2c-overlay.dts
new file mode 100644
index 000000000000..da05e981314c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sc16is752-i2c-overlay.dts
@@ -0,0 +1,43 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_arm>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sc16is752: sc16is752@48 {
+				compatible = "nxp,sc16is752";
+				reg = <0x48>; /* i2c address */
+				clocks = <&sc16is752_clk>;
+				interrupt-parent = <&gpio>;
+				interrupts = <24 2>; /* IRQ_TYPE_EDGE_FALLING */
+				gpio-controller;
+				#gpio-cells = <2>;
+				i2c-max-frequency = <400000>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			sc16is752_clk: sc16is752_i2c_clk@48 {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <14745600>;
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&sc16is752>,"interrupts:0";
+		addr = <&sc16is752>,"reg:0",<&sc16is752_clk>,"name";
+		xtal = <&sc16is752_clk>,"clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sc16is752-spi0-overlay.dts b/arch/arm/boot/dts/overlays/sc16is752-spi0-overlay.dts
new file mode 100644
index 000000000000..a49a04722b99
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sc16is752-spi0-overlay.dts
@@ -0,0 +1,49 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			sc16is752: sc16is752@0 {
+				compatible = "nxp,sc16is752";
+				reg = <0>; /* CE0 */
+				clocks = <&sc16is752_clk>;
+				interrupt-parent = <&gpio>;
+				interrupts = <24 2>; /* IRQ_TYPE_EDGE_FALLING */
+				gpio-controller;
+				#gpio-cells = <2>;
+				spi-max-frequency = <4000000>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target-path = "/";
+		__overlay__ {
+			sc16is752_clk: sc16is752_spi0_0_clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <14745600>;
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&sc16is752>,"interrupts:0";
+		xtal = <&sc16is752_clk>,"clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sc16is752-spi1-overlay.dts b/arch/arm/boot/dts/overlays/sc16is752-spi1-overlay.dts
new file mode 100644
index 000000000000..730c6e8cd614
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sc16is752-spi1-overlay.dts
@@ -0,0 +1,67 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi1_pins: spi1_pins {
+				brcm,pins = <19 20 21>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi1_cs_pins: spi1_cs_pins {
+				brcm,pins = <18>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins &spi1_cs_pins>;
+			cs-gpios = <&gpio 18 1>;
+			status = "okay";
+
+			sc16is752: sc16is752@0 {
+				compatible = "nxp,sc16is752";
+				reg = <0>; /* CE0 */
+				clocks = <&sc16is752_clk>;
+				interrupt-parent = <&gpio>;
+				interrupts = <24 2>; /* IRQ_TYPE_EDGE_FALLING */
+				gpio-controller;
+				#gpio-cells = <2>;
+				spi-max-frequency = <4000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target-path = "/";
+		__overlay__ {
+			sc16is752_clk: sc16is752_spi1_0_clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <14745600>;
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&sc16is752>,"interrupts:0";
+		xtal = <&sc16is752_clk>,"clock-frequency:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sdhost-overlay.dts b/arch/arm/boot/dts/overlays/sdhost-overlay.dts
new file mode 100644
index 000000000000..0b72b4eeac88
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sdhost-overlay.dts
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/* Provide backwards compatible aliases for the old sdhost dtparams. */
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&sdhost>;
+		frag0: __overlay__ {
+			brcm,overclock-50 = <0>;
+			brcm,pio-limit = <1>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&mmc>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&mmcnr>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	__overrides__ {
+		overclock_50     = <&frag0>,"brcm,overclock-50:0";
+		force_pio        = <&frag0>,"brcm,force-pio?";
+		pio_limit        = <&frag0>,"brcm,pio-limit:0";
+		debug            = <&frag0>,"brcm,debug?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sdio-overlay.dts b/arch/arm/boot/dts/overlays/sdio-overlay.dts
new file mode 100644
index 000000000000..873e49056379
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sdio-overlay.dts
@@ -0,0 +1,77 @@
+/dts-v1/;
+/plugin/;
+
+/* Enable SDIO from MMC interface via various GPIO groups */
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&mmcnr>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&mmc>;
+		sdio_ovl: __overlay__ {
+			pinctrl-0 = <&sdio_ovl_pins>;
+			pinctrl-names = "default";
+			non-removable;
+			bus-width = <4>;
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			sdio_ovl_pins: sdio_ovl_pins {
+				brcm,pins = <22 23 24 25 26 27>;
+				brcm,function = <7>; /* ALT3 = SD1 */
+				brcm,pull = <0 2 2 2 2 2>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&sdio_ovl_pins>;
+		__dormant__ {
+			brcm,pins = <22 23 24 25>;
+			brcm,pull = <0 2 2 2>;
+		};
+	};
+
+	fragment@4 {
+		target = <&sdio_ovl_pins>;
+		__dormant__ {
+			brcm,pins = <34 35 36 37>;
+			brcm,pull = <0 2 2 2>;
+		};
+	};
+
+	fragment@5 {
+		target = <&sdio_ovl_pins>;
+		__dormant__ {
+			brcm,pins = <34 35 36 37 38 39>;
+			brcm,pull = <0 2 2 2 2 2>;
+		};
+	};
+
+	fragment@6 {
+		target-path = "/aliases";
+		__overlay__ {
+			mmc1 = "/soc/mmc@7e300000";
+		};
+	};
+
+	__overrides__ {
+		poll_once = <&sdio_ovl>,"non-removable?";
+		bus_width = <&sdio_ovl>,"bus-width:0";
+		sdio_overclock = <&sdio_ovl>,"brcm,overclock-50:0";
+		gpios_22_25 = <0>,"=3";
+		gpios_34_37 = <0>,"=4";
+		gpios_34_39 = <0>,"=5";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sdtweak-overlay.dts b/arch/arm/boot/dts/overlays/sdtweak-overlay.dts
new file mode 100644
index 000000000000..38157d2f9bf3
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sdtweak-overlay.dts
@@ -0,0 +1,25 @@
+/dts-v1/;
+/plugin/;
+
+/* Provide backwards compatible aliases for the old sdhost dtparams. */
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&sdhost>;
+		frag0: __overlay__ {
+			brcm,overclock-50 = <0>;
+			brcm,pio-limit = <1>;
+		};
+	};
+
+	__overrides__ {
+		overclock_50     = <&frag0>,"brcm,overclock-50:0";
+		force_pio        = <&frag0>,"brcm,force-pio?";
+		pio_limit        = <&frag0>,"brcm,pio-limit:0";
+		debug            = <&frag0>,"brcm,debug?";
+		enable           = <&frag0>,"status";
+		poll_once        = <&frag0>,"non-removable?";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sh1106-spi-overlay.dts b/arch/arm/boot/dts/overlays/sh1106-spi-overlay.dts
new file mode 100644
index 000000000000..57a0cc9b1741
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sh1106-spi-overlay.dts
@@ -0,0 +1,84 @@
+/*
+ * Device Tree overlay for SH1106 based SPI OLED display
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			sh1106_pins: sh1106_pins {
+                                brcm,pins = <25 24>;
+                                brcm,function = <1 1>; /* out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sh1106: sh1106@0{
+				compatible = "sinowealth,sh1106";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&sh1106_pins>;
+
+				spi-max-frequency = <4000000>;
+				bgr = <0>;
+				bpp = <1>;
+				rotate = <0>;
+				fps = <25>;
+				buswidth = <8>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				debug = <0>;
+
+				sinowealth,height = <64>;
+				sinowealth,width = <128>;
+				sinowealth,page-offset = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed     = <&sh1106>,"spi-max-frequency:0";
+		rotate    = <&sh1106>,"rotate:0";
+		fps       = <&sh1106>,"fps:0";
+		debug     = <&sh1106>,"debug:0";
+		dc_pin    = <&sh1106>,"dc-gpios:4",
+		            <&sh1106_pins>,"brcm,pins:4";
+		reset_pin = <&sh1106>,"reset-gpios:4",
+		            <&sh1106_pins>,"brcm,pins:0";
+		height    = <&sh1106>,"sinowealth,height:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/smi-dev-overlay.dts b/arch/arm/boot/dts/overlays/smi-dev-overlay.dts
new file mode 100644
index 000000000000..bafab6c92506
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/smi-dev-overlay.dts
@@ -0,0 +1,20 @@
+// Description: Overlay to enable character device interface for SMI.
+// Author:	Luke Wren <luke@raspberrypi.org>
+
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&soc>;
+		__overlay__ {
+			smi_dev {
+				compatible = "brcm,bcm2835-smi-dev";
+				smi_handle = <&smi>;
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/smi-nand-overlay.dts b/arch/arm/boot/dts/overlays/smi-nand-overlay.dts
new file mode 100644
index 000000000000..ae1e50329d66
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/smi-nand-overlay.dts
@@ -0,0 +1,66 @@
+// Description: Overlay to enable NAND flash through
+// the secondary memory interface
+// Author:	Luke Wren
+
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&smi>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&smi_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&soc>;
+		__overlay__ {
+			nand: flash@0 {
+				compatible = "brcm,bcm2835-smi-nand";
+				smi_handle = <&smi>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				status = "okay";
+
+				partition@0 {
+					label = "stage2";
+					// 128k
+					reg = <0 0x20000>;
+					read-only;
+				};
+				partition@1 {
+					label = "firmware";
+					// 16M
+					reg = <0x20000 0x1000000>;
+					read-only;
+				};
+				partition@2 {
+					label = "root";
+					// 2G (will need to use 64 bit for >=4G)
+					reg = <0x1020000 0x80000000>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			smi_pins: smi_pins {
+				brcm,pins = <0 1 2 3 4 5 6 7 8 9 10 11
+					12 13 14 15>;
+				/* Alt 1: SMI */
+				brcm,function = <5 5 5 5 5 5 5 5 5 5 5
+					5 5 5 5 5>;
+				/* /CS, /WE and /OE are pulled high, as they are
+				   generally active low signals */
+				brcm,pull = <2 2 2 2 2 2 2 2 0 0 0 0 0 0 0 0>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/smi-overlay.dts b/arch/arm/boot/dts/overlays/smi-overlay.dts
new file mode 100644
index 000000000000..bb8c7830df23
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/smi-overlay.dts
@@ -0,0 +1,37 @@
+// Description:	Overlay to enable the secondary memory interface peripheral
+// Author:	Luke Wren
+
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&smi>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&smi_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			smi_pins: smi_pins {
+				/* Don't configure the top two address bits, as
+				   these are already used as ID_SD and ID_SC */
+				brcm,pins = <2 3 4 5 6 7 8 9 10 11 12 13 14 15
+					     16 17 18 19 20 21 22 23 24 25>;
+				/* Alt 1: SMI */
+				brcm,function = <5 5 5 5 5 5 5 5 5 5 5 5 5 5 5
+						 5 5 5 5 5 5 5 5 5>;
+				/* /CS, /WE and /OE are pulled high, as they are
+				   generally active low signals */
+				brcm,pull = <2 2 2 2 2 2 0 0 0 0 0 0 0 0 0 0 0
+					     0 0 0 0 0 0 0>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi-gpio35-39-overlay.dts b/arch/arm/boot/dts/overlays/spi-gpio35-39-overlay.dts
new file mode 100644
index 000000000000..a132b8637c31
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi-gpio35-39-overlay.dts
@@ -0,0 +1,31 @@
+/*
+ * Device tree overlay to move spi0 to gpio 35 to 39 on CM
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			cs-gpios = <&gpio 36 1>, <&gpio 35 1>;
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0_cs_pins>;
+		__overlay__ {
+			brcm,pins = <36 35>;
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0_pins>;
+		__overlay__ {
+			brcm,pins = <37 38 39>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi-gpio40-45-overlay.dts b/arch/arm/boot/dts/overlays/spi-gpio40-45-overlay.dts
new file mode 100644
index 000000000000..9ebcaf1b5ea0
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi-gpio40-45-overlay.dts
@@ -0,0 +1,36 @@
+/*
+ * Boot EEPROM overlay
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			cs-gpios = <&gpio 43 1>, <&gpio 44 1>, <&gpio 45 1>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0_cs_pins>;
+		__overlay__ {
+			brcm,pins = <45 44 43>;
+			brcm,function = <1>; /* output */
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0_pins>;
+		__overlay__ {
+			brcm,pins = <40 41 42>;
+			brcm,function = <3>; /* alt4 */
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi-rtc-overlay.dts b/arch/arm/boot/dts/overlays/spi-rtc-overlay.dts
new file mode 100644
index 000000000000..9664afc9845c
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi-rtc-overlay.dts
@@ -0,0 +1,33 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			rtc-pcf2123@0 {
+				compatible = "nxp,rtc-pcf2123";
+				spi-max-frequency = <5000000>;
+				spi-cs-high = <1>;
+				reg = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		pcf2123 = <0>, "=0=1";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi0-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi0-1cs-overlay.dts
new file mode 100644
index 000000000000..e6eb66e2076a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi0-1cs-overlay.dts
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <8>;
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		frag1: __overlay__ {
+			cs-gpios = <&gpio 8 1>;
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&spi0_pins>;
+		__dormant__ {
+			brcm,pins = <10 11>;
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		no_miso = <0>,"=3";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi0-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi0-2cs-overlay.dts
new file mode 100644
index 000000000000..df6519537c3a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi0-2cs-overlay.dts
@@ -0,0 +1,37 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <8 7>;
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		frag1: __overlay__ {
+			cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0_pins>;
+		__dormant__ {
+			brcm,pins = <10 11>;
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&frag0>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		no_miso = <0>,"=2";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi1-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi1-1cs-overlay.dts
new file mode 100644
index 000000000000..ea2794bc5fd5
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi1-1cs-overlay.dts
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi1_pins: spi1_pins {
+				brcm,pins = <19 20 21>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi1_cs_pins: spi1_cs_pins {
+				brcm,pins = <18>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins &spi1_cs_pins>;
+			cs-gpios = <&gpio 18 1>;
+			status = "okay";
+
+			spidev1_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&spi1_cs_pins>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs0_spidev = <&spidev1_0>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi1-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi1-2cs-overlay.dts
new file mode 100644
index 000000000000..dab34ee79ae2
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi1-2cs-overlay.dts
@@ -0,0 +1,69 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi1_pins: spi1_pins {
+				brcm,pins = <19 20 21>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi1_cs_pins: spi1_cs_pins {
+				brcm,pins = <18 17>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins &spi1_cs_pins>;
+			cs-gpios = <&gpio 18 1>, <&gpio 17 1>;
+			status = "okay";
+
+			spidev1_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev1_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&spi1_cs_pins>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&spi1_cs_pins>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs0_spidev = <&spidev1_0>,"status";
+		cs1_spidev = <&spidev1_1>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi1-3cs-overlay.dts b/arch/arm/boot/dts/overlays/spi1-3cs-overlay.dts
new file mode 100644
index 000000000000..bc7e7d04324b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi1-3cs-overlay.dts
@@ -0,0 +1,81 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi1_pins: spi1_pins {
+				brcm,pins = <19 20 21>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi1_cs_pins: spi1_cs_pins {
+				brcm,pins = <18 17 16>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins &spi1_cs_pins>;
+			cs-gpios = <&gpio 18 1>, <&gpio 17 1>, <&gpio 16 1>;
+			status = "okay";
+
+			spidev1_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev1_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev1_2: spidev@2 {
+				compatible = "spidev";
+				reg = <2>;      /* CE2 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&spi1_cs_pins>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&spi1_cs_pins>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs2_pin  = <&spi1_cs_pins>,"brcm,pins:8",
+			   <&frag1>,"cs-gpios:28";
+		cs0_spidev = <&spidev1_0>,"status";
+		cs1_spidev = <&spidev1_1>,"status";
+		cs2_spidev = <&spidev1_2>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi2-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi2-1cs-overlay.dts
new file mode 100644
index 000000000000..2a29750462af
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi2-1cs-overlay.dts
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi2_pins: spi2_pins {
+				brcm,pins = <40 41 42>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi2_cs_pins: spi2_cs_pins {
+				brcm,pins = <43>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi2>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi2_pins &spi2_cs_pins>;
+			cs-gpios = <&gpio 43 1>;
+			status = "okay";
+
+			spidev2_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&spi2_cs_pins>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs0_spidev = <&spidev2_0>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi2-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi2-2cs-overlay.dts
new file mode 100644
index 000000000000..642678fc9ddd
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi2-2cs-overlay.dts
@@ -0,0 +1,69 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi2_pins: spi2_pins {
+				brcm,pins = <40 41 42>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi2_cs_pins: spi2_cs_pins {
+				brcm,pins = <43 44>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi2>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi2_pins &spi2_cs_pins>;
+			cs-gpios = <&gpio 43 1>, <&gpio 44 1>;
+			status = "okay";
+
+			spidev2_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev2_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&spi2_cs_pins>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&spi2_cs_pins>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs0_spidev = <&spidev2_0>,"status";
+		cs1_spidev = <&spidev2_1>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi2-3cs-overlay.dts b/arch/arm/boot/dts/overlays/spi2-3cs-overlay.dts
new file mode 100644
index 000000000000..28d40c6c3c37
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi2-3cs-overlay.dts
@@ -0,0 +1,81 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&gpio>;
+		__overlay__ {
+			spi2_pins: spi2_pins {
+				brcm,pins = <40 41 42>;
+				brcm,function = <3>; /* alt4 */
+			};
+
+			spi2_cs_pins: spi2_cs_pins {
+				brcm,pins = <43 44 45>;
+				brcm,function = <1>; /* output */
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi2>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi2_pins &spi2_cs_pins>;
+			cs-gpios = <&gpio 43 1>, <&gpio 44 1>, <&gpio 45 1>;
+			status = "okay";
+
+			spidev2_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev2_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev2_2: spidev@2 {
+				compatible = "spidev";
+				reg = <2>;      /* CE2 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&aux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&spi2_cs_pins>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&spi2_cs_pins>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs2_pin  = <&spi2_cs_pins>,"brcm,pins:8",
+			   <&frag1>,"cs-gpios:28";
+		cs0_spidev = <&spidev2_0>,"status";
+		cs1_spidev = <&spidev2_1>,"status";
+		cs2_spidev = <&spidev2_2>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi3-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi3-1cs-overlay.dts
new file mode 100644
index 000000000000..335af8637051
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi3-1cs-overlay.dts
@@ -0,0 +1,44 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi3_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <0>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi3>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi3_pins &spi3_cs_pins>;
+			cs-gpios = <&gpio 0 1>;
+			status = "okay";
+
+			spidev3_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs0_spidev = <&spidev3_0>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi3-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi3-2cs-overlay.dts
new file mode 100644
index 000000000000..ce65da27f767
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi3-2cs-overlay.dts
@@ -0,0 +1,56 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi3_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <0 24>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi3>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi3_pins &spi3_cs_pins>;
+			cs-gpios = <&gpio 0 1>, <&gpio 24 1>;
+			status = "okay";
+
+			spidev3_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev3_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&frag0>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs0_spidev = <&spidev3_0>,"status";
+		cs1_spidev = <&spidev3_1>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi4-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi4-1cs-overlay.dts
new file mode 100644
index 000000000000..85d70b40352b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi4-1cs-overlay.dts
@@ -0,0 +1,44 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi4_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <4>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi4>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi4_pins &spi4_cs_pins>;
+			cs-gpios = <&gpio 4 1>;
+			status = "okay";
+
+			spidev4_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs0_spidev = <&spidev4_0>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi4-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi4-2cs-overlay.dts
new file mode 100644
index 000000000000..8bc2215a6a7e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi4-2cs-overlay.dts
@@ -0,0 +1,56 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi4_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <4 25>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi4>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi4_pins &spi4_cs_pins>;
+			cs-gpios = <&gpio 4 1>, <&gpio 25 1>;
+			status = "okay";
+
+			spidev4_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev4_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&frag0>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs0_spidev = <&spidev4_0>,"status";
+		cs1_spidev = <&spidev4_1>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi5-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi5-1cs-overlay.dts
new file mode 100644
index 000000000000..c0f8cb8510ee
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi5-1cs-overlay.dts
@@ -0,0 +1,44 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi5_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <12>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi5>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi5_pins &spi5_cs_pins>;
+			cs-gpios = <&gpio 12 1>;
+			status = "okay";
+
+			spidev5_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs0_spidev = <&spidev5_0>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi5-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi5-2cs-overlay.dts
new file mode 100644
index 000000000000..7758b9c00b4e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi5-2cs-overlay.dts
@@ -0,0 +1,56 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi5_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <12 26>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi5>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi5_pins &spi5_cs_pins>;
+			cs-gpios = <&gpio 12 1>, <&gpio 26 1>;
+			status = "okay";
+
+			spidev5_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev5_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&frag0>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs0_spidev = <&spidev5_0>,"status";
+		cs1_spidev = <&spidev5_1>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi6-1cs-overlay.dts b/arch/arm/boot/dts/overlays/spi6-1cs-overlay.dts
new file mode 100644
index 000000000000..8c8a953eca01
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi6-1cs-overlay.dts
@@ -0,0 +1,44 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi6_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <18>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi6>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi6_pins &spi6_cs_pins>;
+			cs-gpios = <&gpio 18 1>;
+			status = "okay";
+
+			spidev6_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs0_spidev = <&spidev6_0>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/spi6-2cs-overlay.dts b/arch/arm/boot/dts/overlays/spi6-2cs-overlay.dts
new file mode 100644
index 000000000000..2ff897f21aed
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/spi6-2cs-overlay.dts
@@ -0,0 +1,56 @@
+/dts-v1/;
+/plugin/;
+
+
+/ {
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&spi6_cs_pins>;
+		frag0: __overlay__ {
+			brcm,pins = <18 27>;
+			brcm,function = <1>; /* output */
+		};
+	};
+
+	fragment@1 {
+		target = <&spi6>;
+		frag1: __overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			pinctrl-names = "default";
+		        pinctrl-0 = <&spi6_pins &spi6_cs_pins>;
+			cs-gpios = <&gpio 18 1>, <&gpio 27 1>;
+			status = "okay";
+
+			spidev6_0: spidev@0 {
+				compatible = "spidev";
+				reg = <0>;      /* CE0 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+
+			spidev6_1: spidev@1 {
+				compatible = "spidev";
+				reg = <1>;      /* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <125000000>;
+				status = "okay";
+			};
+		};
+	};
+
+	__overrides__ {
+		cs0_pin  = <&frag0>,"brcm,pins:0",
+			   <&frag1>,"cs-gpios:4";
+		cs1_pin  = <&frag0>,"brcm,pins:4",
+			   <&frag1>,"cs-gpios:16";
+		cs0_spidev = <&spidev6_0>,"status";
+		cs1_spidev = <&spidev6_1>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ssd1306-overlay.dts b/arch/arm/boot/dts/overlays/ssd1306-overlay.dts
new file mode 100644
index 000000000000..84cf10e489d3
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ssd1306-overlay.dts
@@ -0,0 +1,36 @@
+// Overlay for SSD1306 128x64 and 128x32 OLED displays
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+
+    fragment@0 {
+	target = <&i2c1>;
+	__overlay__ {
+	    status = "okay";
+
+	    #address-cells = <1>;
+	    #size-cells = <0>;
+
+	    ssd1306: oled@3c{
+		compatible = "solomon,ssd1306fb-i2c";
+		reg = <0x3c>;
+		solomon,width = <128>;
+		solomon,height = <64>;
+		solomon,page-offset = <0>;
+	    };
+	};
+    };
+
+    __overrides__ {
+	address = <&ssd1306>,"reg:0";
+	width = <&ssd1306>,"solomon,width:0";
+	height = <&ssd1306>,"solomon,height:0";
+	offset = <&ssd1306>,"solomon,page-offset:0";
+	normal = <&ssd1306>,"solomon,segment-no-remap?";
+	sequential = <&ssd1306>,"solomon,com-seq?";
+	remapped = <&ssd1306>,"solomon,com-lrremap?";
+	inverted = <&ssd1306>,"solomon,com-invdir?";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/ssd1306-spi-overlay.dts b/arch/arm/boot/dts/overlays/ssd1306-spi-overlay.dts
new file mode 100644
index 000000000000..ffc90c7cecf6
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ssd1306-spi-overlay.dts
@@ -0,0 +1,84 @@
+/*
+ * Device Tree overlay for SSD1306 based SPI OLED display
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			ssd1306_pins: ssd1306_pins {
+                                brcm,pins = <25 24>;
+                                brcm,function = <1 1>; /* out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			ssd1306: ssd1306@0{
+				compatible = "solomon,ssd1306";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&ssd1306_pins>;
+
+				spi-max-frequency = <10000000>;
+				bgr = <0>;
+				bpp = <1>;
+				rotate = <0>;
+				fps = <25>;
+				buswidth = <8>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				debug = <0>;
+
+				solomon,height = <64>;
+				solomon,width = <128>;
+				solomon,page-offset = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed     = <&ssd1306>,"spi-max-frequency:0";
+		rotate    = <&ssd1306>,"rotate:0";
+		fps       = <&ssd1306>,"fps:0";
+		debug     = <&ssd1306>,"debug:0";
+		dc_pin    = <&ssd1306>,"dc-gpios:4",
+		            <&ssd1306_pins>,"brcm,pins:4";
+		reset_pin = <&ssd1306>,"reset-gpios:4",
+		            <&ssd1306_pins>,"brcm,pins:0";
+		height    = <&ssd1306>,"solomon,height:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/ssd1351-spi-overlay.dts b/arch/arm/boot/dts/overlays/ssd1351-spi-overlay.dts
new file mode 100644
index 000000000000..ffc872c60648
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/ssd1351-spi-overlay.dts
@@ -0,0 +1,83 @@
+/*
+ * Device Tree overlay for SSD1351 based SPI OLED display
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			ssd1351_pins: ssd1351_pins {
+                                brcm,pins = <25 24>;
+                                brcm,function = <1 1>; /* out out */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			ssd1351: ssd1351@0{
+				compatible = "solomon,ssd1351";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&ssd1351_pins>;
+
+				spi-max-frequency = <4500000>;
+				bgr = <0>;
+				bpp = <16>;
+				rotate = <0>;
+				fps = <25>;
+				buswidth = <8>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				debug = <0>;
+
+				solomon,height = <128>;
+				solomon,width = <128>;
+				solomon,page-offset = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		speed     = <&ssd1351>,"spi-max-frequency:0";
+		rotate    = <&ssd1351>,"rotate:0";
+		fps       = <&ssd1351>,"fps:0";
+		debug     = <&ssd1351>,"debug:0";
+		dc_pin    = <&ssd1351>,"dc-gpios:4",
+		            <&ssd1351_pins>,"brcm,pins:4";
+		reset_pin = <&ssd1351>,"reset-gpios:4",
+		            <&ssd1351_pins>,"brcm,pins:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/superaudioboard-overlay.dts b/arch/arm/boot/dts/overlays/superaudioboard-overlay.dts
new file mode 100755
index 000000000000..bad61535981e
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/superaudioboard-overlay.dts
@@ -0,0 +1,73 @@
+// Definitions for SuperAudioBoard
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&sound>;
+		__overlay__ {
+			compatible = "simple-audio-card";
+			i2s-controller = <&i2s>;
+			status = "okay";
+
+			simple-audio-card,name = "SuperAudioBoard";
+
+			simple-audio-card,widgets =
+				"Line", "Line In",
+				"Line", "Line Out";
+
+			simple-audio-card,routing =
+				"Line Out","AOUTA+",
+				"Line Out","AOUTA-",
+				"Line Out","AOUTB+",
+				"Line Out","AOUTB-",
+				"AINA","Line In",
+				"AINB","Line In";
+
+			simple-audio-card,format = "i2s";
+
+			simple-audio-card,bitclock-master = <&sound_master>;
+			simple-audio-card,frame-master = <&sound_master>;
+
+			simple-audio-card,cpu {
+				sound-dai = <&i2s>;
+				dai-tdm-slot-num = <2>;
+				dai-tdm-slot-width = <32>;
+			};
+
+			sound_master: simple-audio-card,codec {
+				sound-dai = <&cs4271>;
+				system-clock-frequency = <24576000>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+    
+	fragment@2 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			cs4271: cs4271@10 {
+				#sound-dai-cells = <0>;
+				compatible = "cirrus,cs4271";
+				reg = <0x10>;
+				status = "okay";
+				reset-gpio = <&gpio 26 0>; /* Pin 26, active high */
+			};
+		};
+	};
+	__overrides__ {
+		gpiopin = <&cs4271>,"reset-gpio:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/sx150x-overlay.dts b/arch/arm/boot/dts/overlays/sx150x-overlay.dts
new file mode 100644
index 000000000000..1d1069345da2
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/sx150x-overlay.dts
@@ -0,0 +1,1706 @@
+// Definitions for SX150x I2C GPIO Expanders from Semtech
+
+// dtparams:
+//     sx150<x>-<n>-<m>          - Enables SX150X device on I2C#<n> with slave address <m>. <x> may be 1-9.
+//                                 <n> may be 0 or 1.  Permissible values of <m> (which is denoted in hex)
+//                                 depend on the device variant.
+//                                 For SX1501, SX1502, SX1504 and SX1505, <m> may be 20 or 21.
+//                                 For SX1503 and SX1506, <m> may be 20.
+//                                 For SX1507 and SX1509, <m> may be 3E, 3F, 70 or 71.
+//                                 For SX1508, <m> may be 20, 21, 22 or 23.
+//     sx150<x>-<n>-<m>-int-gpio - Integer, enables interrupts on SX150X device on I2C#<n> with slave address <m>,
+//                                 specifies the GPIO pin to which NINT output of SX150X is connected.
+//
+//
+// Example 1: A single SX1505 device on I2C#1 with its slave address set to 0x20 and NINT output connected to GPIO25:
+// dtoverlay=sx150x:sx1505-1-20,sx1505-1-20-int-gpio=25
+//
+// Example 2: Two SX1507 devices on I2C#0 with their slave addresses set to 0x3E and 0x70 (interrupts not used):
+// dtoverlay=sx150x:sx1507-0-3E,sx1507-0-70
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	// Enable I2C#0 interface
+	fragment@0 {
+		target = <&i2c0>;
+		__dormant__ {
+			status = "okay";
+		};
+	};
+
+	// Enable I2C#1 interface
+	fragment@1 {
+		target = <&i2c1>;
+		__dormant__ {
+			status = "okay";
+		};
+	};
+
+	// Enable a SX1501 on I2C#0 at slave addr 0x20
+	fragment@2 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1501_0_20: sx150x@20 {
+				compatible = "semtech,sx1501q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1501-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1501 on I2C#1 at slave addr 0x20
+	fragment@3 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1501_1_20: sx150x@20 {
+				compatible = "semtech,sx1501q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1501-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1501 on I2C#0 at slave addr 0x21
+	fragment@4 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1501_0_21: sx150x@21 {
+				compatible = "semtech,sx1501q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1501-0-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1501 on I2C#1 at slave addr 0x21
+	fragment@5 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1501_1_21: sx150x@21 {
+				compatible = "semtech,sx1501q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1501-1-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1502 on I2C#0 at slave addr 0x20
+	fragment@6 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1502_0_20: sx150x@20 {
+				compatible = "semtech,sx1502q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1502-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1502 on I2C#1 at slave addr 0x20
+	fragment@7 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1502_1_20: sx150x@20 {
+				compatible = "semtech,sx1502q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1502-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1502 on I2C#0 at slave addr 0x21
+	fragment@8 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1502_0_21: sx150x@21 {
+				compatible = "semtech,sx1502q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1502-0-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1502 on I2C#1 at slave addr 0x21
+	fragment@9 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1502_1_21: sx150x@21 {
+				compatible = "semtech,sx1502q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1501-1-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1503 on I2C#0 at slave addr 0x20
+	fragment@10 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1503_0_20: sx150x@20 {
+				compatible = "semtech,sx1503q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1503-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1503 on I2C#1 at slave addr 0x20
+	fragment@11 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1503_1_20: sx150x@20 {
+				compatible = "semtech,sx1503q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1503-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1504 on I2C#0 at slave addr 0x20
+	fragment@12 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1504_0_20: sx150x@20 {
+				compatible = "semtech,sx1504q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1504-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1504 on I2C#1 at slave addr 0x20
+	fragment@13 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1504_1_20: sx150x@20 {
+				compatible = "semtech,sx1504q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1504-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1504 on I2C#0 at slave addr 0x21
+	fragment@14 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1504_0_21: sx150x@21 {
+				compatible = "semtech,sx1504q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1504-0-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1504 on I2C#1 at slave addr 0x21
+	fragment@15 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1504_1_21: sx150x@21 {
+				compatible = "semtech,sx1504q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1504-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1505 on I2C#0 at slave addr 0x20
+	fragment@16 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1505_0_20: sx150x@20 {
+				compatible = "semtech,sx1505q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1505-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1505 on I2C#1 at slave addr 0x20
+	fragment@17 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1505_1_20: sx150x@20 {
+				compatible = "semtech,sx1505q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1505-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1505 on I2C#0 at slave addr 0x21
+	fragment@18 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1505_0_21: sx150x@21 {
+				compatible = "semtech,sx1505q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1505-0-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1505 on I2C#1 at slave addr 0x21
+	fragment@19 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1505_1_21: sx150x@21 {
+				compatible = "semtech,sx1505q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1505-1-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1506 on I2C#0 at slave addr 0x20
+	fragment@20 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1506_0_20: sx150x@20 {
+				compatible = "semtech,sx1506q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1506-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1506 on I2C#1 at slave addr 0x20
+	fragment@21 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1506_1_20: sx150x@20 {
+				compatible = "semtech,sx1506q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1506-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#0 at slave addr 0x3E
+	fragment@22 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_0_3E: sx150x@3E {
+				compatible = "semtech,sx1507q";
+				reg = <0x3E>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507_0_3E-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#1 at slave addr 0x3E
+	fragment@23 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_1_3E: sx150x@3E {
+				compatible = "semtech,sx1507q";
+				reg = <0x3E>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507_1_3E-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#0 at slave addr 0x3F
+	fragment@24 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_0_3F: sx150x@3F {
+				compatible = "semtech,sx1507q";
+				reg = <0x3F>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507_0_3F-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#1 at slave addr 0x3F
+	fragment@25 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_1_3F: sx150x@3F {
+				compatible = "semtech,sx1507q";
+				reg = <0x3F>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507_1_3F-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#0 at slave addr 0x70
+	fragment@26 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_0_70: sx150x@70 {
+				compatible = "semtech,sx1507q";
+				reg = <0x70>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507-0-70-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#1 at slave addr 0x70
+	fragment@27 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_1_70: sx150x@70 {
+				compatible = "semtech,sx1507q";
+				reg = <0x70>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507-1-70-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#0 at slave addr 0x71
+	fragment@28 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_0_71: sx150x@71 {
+				compatible = "semtech,sx1507q";
+				reg = <0x71>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507-0-71-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1507 on I2C#1 at slave addr 0x71
+	fragment@29 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1507_1_71: sx150x@71 {
+				compatible = "semtech,sx1507q";
+				reg = <0x71>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1507-1-71-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#0 at slave addr 0x20
+	fragment@30 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_0_20: sx150x@20 {
+				compatible = "semtech,sx1508q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-0-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#1 at slave addr 0x20
+	fragment@31 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_1_20: sx150x@20 {
+				compatible = "semtech,sx1508q";
+				reg = <0x20>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-1-20-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#0 at slave addr 0x21
+	fragment@32 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_0_21: sx150x@21 {
+				compatible = "semtech,sx1508q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-0-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#1 at slave addr 0x21
+	fragment@33 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_1_21: sx150x@21 {
+				compatible = "semtech,sx1508q";
+				reg = <0x21>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-1-21-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#0 at slave addr 0x22
+	fragment@34 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_0_22: sx150x@22 {
+				compatible = "semtech,sx1508q";
+				reg = <0x22>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-0-22-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#1 at slave addr 0x22
+	fragment@35 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_1_22: sx150x@22 {
+				compatible = "semtech,sx1508q";
+				reg = <0x22>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-1-22-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#0 at slave addr 0x23
+	fragment@36 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_0_23: sx150x@23 {
+				compatible = "semtech,sx1508q";
+				reg = <0x23>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-0-23-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1508 on I2C#1 at slave addr 0x23
+	fragment@37 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1508_1_23: sx150x@23 {
+				compatible = "semtech,sx1508q";
+				reg = <0x23>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1508-1-23-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#0 at slave addr 0x3E
+	fragment@38 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_0_3E: sx150x@3E {
+				compatible = "semtech,sx1509q";
+				reg = <0x3E>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509_0_3E-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#1 at slave addr 0x3E
+	fragment@39 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_1_3E: sx150x@3E {
+				compatible = "semtech,sx1509q";
+				reg = <0x3E>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509_1_3E-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#0 at slave addr 0x3F
+	fragment@40 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_0_3F: sx150x@3F {
+				compatible = "semtech,sx1509q";
+				reg = <0x3F>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509_0_3F-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#1 at slave addr 0x3F
+	fragment@41 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_1_3F: sx150x@3F {
+				compatible = "semtech,sx1509q";
+				reg = <0x3F>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509_1_3F-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#0 at slave addr 0x70
+	fragment@42 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_0_70: sx150x@70 {
+				compatible = "semtech,sx1509q";
+				reg = <0x70>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509-0-70-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#1 at slave addr 0x70
+	fragment@43 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_1_70: sx150x@70 {
+				compatible = "semtech,sx1509q";
+				reg = <0x70>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509-1-70-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#0 at slave addr 0x71
+	fragment@44 {
+		target = <&i2c0>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_0_71: sx150x@71 {
+				compatible = "semtech,sx1509q";
+				reg = <0x71>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509-0-71-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable a SX1509 on I2C#1 at slave addr 0x71
+	fragment@45 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			sx1509_1_71: sx150x@71 {
+				compatible = "semtech,sx1509q";
+				reg = <0x71>;
+				gpio-controller;
+				#gpio-cells = <2>;
+				#interrupt-cells = <2>;
+				interrupts = <25 2>; /* 1st word overwritten by sx1509-1-71-int-gpio parameter
+				                        2nd word is 2 for falling-edge triggered */
+				status = "okay";
+			};
+		};
+	};
+
+	// Enable interrupts for a SX1501 on I2C#0 at slave addr 0x20
+	fragment@46 {
+		target = <&sx1501_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1501 on I2C#1 at slave addr 0x20
+	fragment@47 {
+		target = <&sx1501_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1501 on I2C#0 at slave addr 0x21
+	fragment@48 {
+		target = <&sx1501_0_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1501 on I2C#1 at slave addr 0x21
+	fragment@49 {
+		target = <&sx1501_1_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1502 on I2C#0 at slave addr 0x20
+	fragment@50 {
+		target = <&sx1502_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1502 on I2C#1 at slave addr 0x20
+	fragment@51 {
+		target = <&sx1502_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1502 on I2C#0 at slave addr 0x21
+	fragment@52 {
+		target = <&sx1502_0_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1502 on I2C#1 at slave addr 0x21
+	fragment@53 {
+		target = <&sx1502_1_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1503 on I2C#0 at slave addr 0x20
+	fragment@54 {
+		target = <&sx1503_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1503 on I2C#1 at slave addr 0x20
+	fragment@55 {
+		target = <&sx1503_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1504 on I2C#0 at slave addr 0x20
+	fragment@56 {
+		target = <&sx1504_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1504 on I2C#1 at slave addr 0x20
+	fragment@57 {
+		target = <&sx1504_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1504 on I2C#0 at slave addr 0x21
+	fragment@58 {
+		target = <&sx1504_0_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1504 on I2C#1 at slave addr 0x21
+	fragment@59 {
+		target = <&sx1504_1_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1505 on I2C#0 at slave addr 0x20
+	fragment@60 {
+		target = <&sx1505_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1505 on I2C#1 at slave addr 0x20
+	fragment@61 {
+		target = <&sx1505_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1505 on I2C#0 at slave addr 0x21
+	fragment@62 {
+		target = <&sx1505_0_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1505 on I2C#1 at slave addr 0x21
+	fragment@63 {
+		target = <&sx1505_1_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1506 on I2C#0 at slave addr 0x20
+	fragment@64 {
+		target = <&sx1506_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1506 on I2C#1 at slave addr 0x20
+	fragment@65 {
+		target = <&sx1506_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#0 at slave addr 0x3E
+	fragment@66 {
+		target = <&sx1507_0_3E>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_3E_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#1 at slave addr 0x3E
+	fragment@67 {
+		target = <&sx1507_1_3E>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_3E_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#0 at slave addr 0x3F
+	fragment@68 {
+		target = <&sx1507_0_3F>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_3F_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#1 at slave addr 0x3F
+	fragment@69 {
+		target = <&sx1507_1_3F>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_3F_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#0 at slave addr 0x70
+	fragment@70 {
+		target = <&sx1507_0_70>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_70_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#1 at slave addr 0x70
+	fragment@71 {
+		target = <&sx1507_1_70>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_70_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#0 at slave addr 0x71
+	fragment@72 {
+		target = <&sx1507_0_71>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_71_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1507 on I2C#1 at slave addr 0x71
+	fragment@73 {
+		target = <&sx1507_1_71>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_71_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#0 at slave addr 0x20
+	fragment@74 {
+		target = <&sx1508_0_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#1 at slave addr 0x20
+	fragment@75 {
+		target = <&sx1508_1_20>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_20_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#0 at slave addr 0x21
+	fragment@76 {
+		target = <&sx1508_0_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#1 at slave addr 0x21
+	fragment@77 {
+		target = <&sx1508_1_21>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_21_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#0 at slave addr 0x22
+	fragment@78 {
+		target = <&sx1508_0_22>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_22_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#1 at slave addr 0x22
+	fragment@79 {
+		target = <&sx1508_1_22>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_22_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#0 at slave addr 0x23
+	fragment@80 {
+		target = <&sx1508_0_23>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_23_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1508 on I2C#1 at slave addr 0x23
+	fragment@81 {
+		target = <&sx1508_1_23>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_23_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#0 at slave addr 0x3E
+	fragment@82 {
+		target = <&sx1509_0_3E>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_3E_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#1 at slave addr 0x3E
+	fragment@83 {
+		target = <&sx1509_1_3E>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_3E_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#0 at slave addr 0x3F
+	fragment@84 {
+		target = <&sx1509_0_3F>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_3F_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#1 at slave addr 0x3F
+	fragment@85 {
+		target = <&sx1509_1_3F>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_3F_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#0 at slave addr 0x70
+	fragment@86 {
+		target = <&sx1509_0_70>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_70_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#1 at slave addr 0x70
+	fragment@87 {
+		target = <&sx1509_1_70>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_70_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#0 at slave addr 0x71
+	fragment@88 {
+		target = <&sx1509_0_71>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_0_71_pins>;
+		};
+	};
+
+	// Enable interrupts for a SX1509 on I2C#1 at slave addr 0x71
+	fragment@89 {
+		target = <&sx1509_1_71>;
+		__dormant__ {
+			interrupt-parent = <&gpio>;
+			interrupt-controller;
+			pinctrl-names = "default";
+			pinctrl-0 = <&sx150x_1_71_pins>;
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x20
+        // Configure as a input with no pull-up/down
+	fragment@90 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_20_pins: sx150x_0_20_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-20-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x20
+        // Configure as a input with no pull-up/down
+	fragment@91 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_20_pins: sx150x_1_20_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-20-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x21
+        // Configure as a input with no pull-up/down
+	fragment@92 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_21_pins: sx150x_0_21_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-21-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x21
+        // Configure as a input with no pull-up/down
+	fragment@93 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_21_pins: sx150x_1_21_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-21-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x22
+        // Configure as a input with no pull-up/down
+	fragment@94 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_22_pins: sx150x_0_22_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-22-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x22
+        // Configure as a input with no pull-up/down
+	fragment@95 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_22_pins: sx150x_1_22_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-22-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x23
+        // Configure as a input with no pull-up/down
+	fragment@96 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_23_pins: sx150x_0_23_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-23-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x23
+        // Configure as a input with no pull-up/down
+	fragment@97 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_23_pins: sx150x_1_23_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-23-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x3E
+        // Configure as a input with no pull-up/down
+	fragment@98 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_3E_pins: sx150x_0_3E_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-3E-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x3E
+        // Configure as a input with no pull-up/down
+	fragment@99 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_3E_pins: sx150x_1_3E_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-3E-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x3F
+        // Configure as a input with no pull-up/down
+	fragment@100 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_3F_pins: sx150x_0_3F_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-3F-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x3F
+        // Configure as a input with no pull-up/down
+	fragment@101 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_3F_pins: sx150x_1_3F_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-3F-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x70
+        // Configure as a input with no pull-up/down
+	fragment@102 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_70_pins: sx150x_0_70_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-70-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x70
+        // Configure as a input with no pull-up/down
+	fragment@103 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_70_pins: sx150x_1_70_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-70-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#0 interface at slave addr 0x71
+        // Configure as a input with no pull-up/down
+	fragment@104 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_0_71_pins: sx150x_0_71_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-0-71-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	// Configure GPIO pin connected to NINT output of a SX150x on I2C#1 interface at slave addr 0x71
+        // Configure as a input with no pull-up/down
+	fragment@105 {
+		target = <&gpio>;
+		__dormant__ {
+			sx150x_1_71_pins: sx150x_1_71_pins {
+				brcm,pins = <0>;  /* overwritten by sx150x-1-71-int-gpio parameter */
+				brcm,function = <0>;
+				brcm,pull = <0>;
+			};
+		};
+	};
+
+	__overrides__ {
+		sx1501-0-20          = <0>,"+0+2";
+		sx1501-1-20          = <0>,"+1+3";
+		sx1501-0-21          = <0>,"+0+4";
+		sx1501-1-21          = <0>,"+1+5";
+		sx1502-0-20          = <0>,"+0+6";
+		sx1502-1-20          = <0>,"+1+7";
+		sx1502-0-21          = <0>,"+0+8";
+		sx1502-1-21          = <0>,"+1+9";
+		sx1503-0-20          = <0>,"+0+10";
+		sx1503-1-20          = <0>,"+1+11";
+		sx1504-0-20          = <0>,"+0+12";
+		sx1504-1-20          = <0>,"+1+13";
+		sx1504-0-21          = <0>,"+0+14";
+		sx1504-1-21          = <0>,"+1+15";
+		sx1505-0-20          = <0>,"+0+16";
+		sx1505-1-20          = <0>,"+1+17";
+		sx1505-0-21          = <0>,"+0+18";
+		sx1505-1-21          = <0>,"+1+19";
+		sx1506-0-20          = <0>,"+0+20";
+		sx1506-1-20          = <0>,"+1+21";
+		sx1507-0-3E          = <0>,"+0+22";
+		sx1507-1-3E          = <0>,"+1+23";
+		sx1507-0-3F          = <0>,"+0+24";
+		sx1507-1-3F          = <0>,"+1+25";
+		sx1507-0-70          = <0>,"+0+26";
+		sx1507-1-70          = <0>,"+1+27";
+		sx1507-0-71          = <0>,"+0+28";
+		sx1507-1-71          = <0>,"+1+29";
+		sx1508-0-20          = <0>,"+0+30";
+		sx1508-1-20          = <0>,"+1+31";
+		sx1508-0-21          = <0>,"+0+32";
+		sx1508-1-21          = <0>,"+1+33";
+		sx1508-0-22          = <0>,"+0+34";
+		sx1508-1-22          = <0>,"+1+35";
+		sx1508-0-23          = <0>,"+0+36";
+		sx1508-1-23          = <0>,"+1+37";
+		sx1509-0-3E          = <0>,"+0+38";
+		sx1509-1-3E          = <0>,"+1+39";
+		sx1509-0-3F          = <0>,"+0+40";
+		sx1509-1-3F          = <0>,"+1+41";
+		sx1509-0-70          = <0>,"+0+42";
+		sx1509-1-70          = <0>,"+1+43";
+		sx1509-0-71          = <0>,"+0+44";
+		sx1509-1-71          = <0>,"+1+45";
+		sx1501-0-20-int-gpio = <0>,"+46+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1501_0_20>,"interrupts:0";
+		sx1501-1-20-int-gpio = <0>,"+47+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1501_1_20>,"interrupts:0";
+		sx1501-0-21-int-gpio = <0>,"+48+92",  <&sx150x_0_21_pins>,"brcm,pins:0", <&sx1501_0_21>,"interrupts:0";
+		sx1501-1-21-int-gpio = <0>,"+49+93",  <&sx150x_1_21_pins>,"brcm,pins:0", <&sx1501_1_21>,"interrupts:0";
+		sx1502-0-20-int-gpio = <0>,"+50+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1502_0_20>,"interrupts:0";
+		sx1502-1-20-int-gpio = <0>,"+51+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1502_1_20>,"interrupts:0";
+		sx1502-0-21-int-gpio = <0>,"+52+92",  <&sx150x_0_21_pins>,"brcm,pins:0", <&sx1502_0_21>,"interrupts:0";
+		sx1502-1-21-int-gpio = <0>,"+53+93",  <&sx150x_1_21_pins>,"brcm,pins:0", <&sx1502_1_21>,"interrupts:0";
+		sx1503-0-20-int-gpio = <0>,"+54+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1503_0_20>,"interrupts:0";
+		sx1503-1-20-int-gpio = <0>,"+55+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1503_1_20>,"interrupts:0";
+		sx1504-0-20-int-gpio = <0>,"+56+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1504_0_20>,"interrupts:0";
+		sx1504-1-20-int-gpio = <0>,"+57+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1504_1_20>,"interrupts:0";
+		sx1504-0-21-int-gpio = <0>,"+58+92",  <&sx150x_0_21_pins>,"brcm,pins:0", <&sx1504_0_21>,"interrupts:0";
+		sx1504-1-21-int-gpio = <0>,"+59+93",  <&sx150x_1_21_pins>,"brcm,pins:0", <&sx1504_1_21>,"interrupts:0";
+		sx1505-0-20-int-gpio = <0>,"+60+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1505_0_20>,"interrupts:0";
+		sx1505-1-20-int-gpio = <0>,"+61+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1505_1_20>,"interrupts:0";
+		sx1505-0-21-int-gpio = <0>,"+62+92",  <&sx150x_0_21_pins>,"brcm,pins:0", <&sx1505_0_21>,"interrupts:0";
+		sx1505-1-21-int-gpio = <0>,"+63+93",  <&sx150x_1_21_pins>,"brcm,pins:0", <&sx1505_1_21>,"interrupts:0";
+		sx1506-0-20-int-gpio = <0>,"+64+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1506_0_20>,"interrupts:0";
+		sx1506-1-20-int-gpio = <0>,"+65+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1506_1_20>,"interrupts:0";
+		sx1507-0-3E-int-gpio = <0>,"+66+98",  <&sx150x_0_3E_pins>,"brcm,pins:0", <&sx1507_0_3E>,"interrupts:0";
+		sx1507-1-3E-int-gpio = <0>,"+67+99",  <&sx150x_1_3E_pins>,"brcm,pins:0", <&sx1507_1_3E>,"interrupts:0";
+		sx1507-0-3F-int-gpio = <0>,"+68+100", <&sx150x_0_3F_pins>,"brcm,pins:0", <&sx1507_0_3F>,"interrupts:0";
+		sx1507-1-3F-int-gpio = <0>,"+69+101", <&sx150x_1_3F_pins>,"brcm,pins:0", <&sx1507_1_3F>,"interrupts:0";
+		sx1507-0-70-int-gpio = <0>,"+60+102", <&sx150x_0_70_pins>,"brcm,pins:0", <&sx1507_0_70>,"interrupts:0";
+		sx1507-1-70-int-gpio = <0>,"+71+103", <&sx150x_1_70_pins>,"brcm,pins:0", <&sx1507_1_70>,"interrupts:0";
+		sx1507-0-71-int-gpio = <0>,"+72+104", <&sx150x_0_71_pins>,"brcm,pins:0", <&sx1507_0_71>,"interrupts:0";
+		sx1507-1-71-int-gpio = <0>,"+73+105", <&sx150x_1_71_pins>,"brcm,pins:0", <&sx1507_1_71>,"interrupts:0";
+		sx1508-0-20-int-gpio = <0>,"+74+90",  <&sx150x_0_20_pins>,"brcm,pins:0", <&sx1508_0_20>,"interrupts:0";
+		sx1508-1-20-int-gpio = <0>,"+75+91",  <&sx150x_1_20_pins>,"brcm,pins:0", <&sx1508_1_20>,"interrupts:0";
+		sx1508-0-21-int-gpio = <0>,"+76+92",  <&sx150x_0_21_pins>,"brcm,pins:0", <&sx1508_0_21>,"interrupts:0";
+		sx1508-1-21-int-gpio = <0>,"+77+93",  <&sx150x_1_21_pins>,"brcm,pins:0", <&sx1508_1_21>,"interrupts:0";
+		sx1508-0-22-int-gpio = <0>,"+78+94",  <&sx150x_0_22_pins>,"brcm,pins:0", <&sx1508_0_22>,"interrupts:0";
+		sx1508-1-22-int-gpio = <0>,"+79+95",  <&sx150x_1_22_pins>,"brcm,pins:0", <&sx1508_1_22>,"interrupts:0";
+		sx1508-0-23-int-gpio = <0>,"+80+96",  <&sx150x_0_23_pins>,"brcm,pins:0", <&sx1508_0_23>,"interrupts:0";
+		sx1508-1-23-int-gpio = <0>,"+81+97",  <&sx150x_1_23_pins>,"brcm,pins:0", <&sx1508_1_23>,"interrupts:0";
+		sx1509-0-3E-int-gpio = <0>,"+82+98",  <&sx150x_0_3E_pins>,"brcm,pins:0", <&sx1509_0_3E>,"interrupts:0";
+		sx1509-1-3E-int-gpio = <0>,"+83+99",  <&sx150x_1_3E_pins>,"brcm,pins:0", <&sx1509_1_3E>,"interrupts:0";
+		sx1509-0-3F-int-gpio = <0>,"+84+100", <&sx150x_0_3F_pins>,"brcm,pins:0", <&sx1509_0_3F>,"interrupts:0";
+		sx1509-1-3F-int-gpio = <0>,"+85+101", <&sx150x_1_3F_pins>,"brcm,pins:0", <&sx1509_1_3F>,"interrupts:0";
+		sx1509-0-70-int-gpio = <0>,"+86+102", <&sx150x_0_70_pins>,"brcm,pins:0", <&sx1509_0_70>,"interrupts:0";
+		sx1509-1-70-int-gpio = <0>,"+87+103", <&sx150x_1_70_pins>,"brcm,pins:0", <&sx1509_1_70>,"interrupts:0";
+		sx1509-0-71-int-gpio = <0>,"+88+104", <&sx150x_0_71_pins>,"brcm,pins:0", <&sx1509_0_71>,"interrupts:0";
+		sx1509-1-71-int-gpio = <0>,"+89+105", <&sx150x_1_71_pins>,"brcm,pins:0", <&sx1509_1_71>,"interrupts:0";
+	};
+};
+
diff --git a/arch/arm/boot/dts/overlays/tc358743-audio-overlay.dts b/arch/arm/boot/dts/overlays/tc358743-audio-overlay.dts
new file mode 100644
index 000000000000..047695bb0c71
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/tc358743-audio-overlay.dts
@@ -0,0 +1,52 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions to add I2S audio from the Toshiba TC358743 HDMI to CSI2 bridge.
+// Requires tc358743 overlay to have been loaded to actually function.
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2s>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			tc358743_codec: tc358743-codec {
+				#sound-dai-cells = <0>;
+				compatible = "linux,spdif-dir";
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&sound>;
+		sound_overlay: __overlay__ {
+			compatible = "simple-audio-card";
+			simple-audio-card,format = "i2s";
+			simple-audio-card,name = "tc358743";
+			simple-audio-card,bitclock-master = <&dailink0_slave>;
+			simple-audio-card,frame-master = <&dailink0_slave>;
+			status = "okay";
+
+			simple-audio-card,cpu {
+				sound-dai = <&i2s>;
+				dai-tdm-slot-num = <2>;
+				dai-tdm-slot-width = <32>;
+			};
+			dailink0_slave: simple-audio-card,codec {
+				sound-dai = <&tc358743_codec>;
+			};
+		};
+	};
+
+	__overrides__ {
+		card-name = <&sound_overlay>,"simple-audio-card,name";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/tc358743-overlay.dts b/arch/arm/boot/dts/overlays/tc358743-overlay.dts
new file mode 100644
index 000000000000..a1f8af36d2e7
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/tc358743-overlay.dts
@@ -0,0 +1,107 @@
+// SPDX-License-Identifier: GPL-2.0-only
+// Definitions for Toshiba TC358743 HDMI to CSI2 bridge on VC I2C bus
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&i2c_csi_dsi>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "okay";
+
+			tc358743@0f {
+				compatible = "toshiba,tc358743";
+				reg = <0x0f>;
+				status = "okay";
+
+				clocks = <&tc358743_clk>;
+				clock-names = "refclk";
+
+				port {
+					tc358743: endpoint {
+						remote-endpoint = <&csi1_ep>;
+						clock-lanes = <0>;
+						clock-noncontinuous;
+						link-frequencies =
+							/bits/ 64 <486000000>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&csi1>;
+		__overlay__ {
+			status = "okay";
+
+			port {
+				csi1_ep: endpoint {
+					remote-endpoint = <&tc358743>;
+				};
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&tc358743>;
+		__overlay__ {
+			data-lanes = <1 2>;
+		};
+	};
+
+	fragment@3 {
+		target = <&tc358743>;
+		__dormant__ {
+			data-lanes = <1 2 3 4>;
+		};
+	};
+
+	fragment@4 {
+		target = <&i2c0if>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target = <&i2c0mux>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@6 {
+		target-path = "/";
+		__overlay__ {
+			tc358743_clk: bridge-clk {
+				compatible = "fixed-clock";
+				#clock-cells = <0>;
+				clock-frequency = <27000000>;
+			};
+		};
+	};
+
+	fragment@7 {
+		target = <&csi1_ep>;
+		__overlay__ {
+			data-lanes = <1 2>;
+		};
+	};
+
+	fragment@8 {
+		target = <&csi1_ep>;
+		__dormant__ {
+			data-lanes = <1 2 3 4>;
+		};
+	};
+
+	__overrides__ {
+		4lane = <0>, "-2+3-7+8";
+		link-frequency = <&tc358743>,"link-frequencies#0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/tinylcd35-overlay.dts b/arch/arm/boot/dts/overlays/tinylcd35-overlay.dts
new file mode 100644
index 000000000000..a102b09e3ab5
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/tinylcd35-overlay.dts
@@ -0,0 +1,222 @@
+/*
+ * tinylcd35-overlay.dts
+ *
+ * -------------------------------------------------
+ * www.tinlylcd.com
+ * -------------------------------------------------
+ * Device---Driver-----BUS       GPIO's
+ * display  tinylcd35  spi0.0    25 24 18
+ * touch    ads7846    spi0.1    5
+ * rtc      ds1307     i2c1-0068
+ * rtc      pcf8563    i2c1-0051
+ * keypad   gpio-keys  --------- 17 22 27 23 28
+ *
+ *
+ * TinyLCD.com 3.5 inch TFT
+ *
+ *  Version 001
+ *  5/3/2015  -- Noralf Trønnes     Initial Device tree framework
+ *  10/3/2015 -- tinylcd@gmail.com  added ds1307 support.
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			tinylcd35_pins: tinylcd35_pins {
+				brcm,pins = <25 24 18>;
+				brcm,function = <1>; /* out */
+			};
+			tinylcd35_ts_pins: tinylcd35_ts_pins {
+				brcm,pins = <5>;
+				brcm,function = <0>; /* in */
+			};
+			keypad_pins: keypad_pins {
+				brcm,pins = <4 17 22 23 27>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <1>; /* down */
+			};
+		};
+	};
+
+	fragment@4 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			tinylcd35: tinylcd35@0{
+				compatible = "neosec,tinylcd";
+				reg = <0>;
+				pinctrl-names = "default";
+				pinctrl-0 = <&tinylcd35_pins>,
+					    <&tinylcd35_ts_pins>;
+
+				spi-max-frequency = <48000000>;
+				rotate = <270>;
+				fps = <20>;
+				bgr;
+				buswidth = <8>;
+				reset-gpios = <&gpio 25 1>;
+				dc-gpios = <&gpio 24 0>;
+				led-gpios = <&gpio 18 0>;
+				debug = <0>;
+
+				init = <0x10000B0 0x80
+					0x10000C0 0x0A 0x0A
+					0x10000C1 0x01 0x01
+					0x10000C2 0x33
+					0x10000C5 0x00 0x42 0x80
+					0x10000B1 0xD0 0x11
+					0x10000B4 0x02
+					0x10000B6 0x00 0x22 0x3B
+					0x10000B7 0x07
+					0x1000036 0x58
+					0x10000F0 0x36 0xA5 0xD3
+					0x10000E5 0x80
+					0x10000E5 0x01
+					0x10000B3 0x00
+					0x10000E5 0x00
+					0x10000F0 0x36 0xA5 0x53
+					0x10000E0 0x00 0x35 0x33 0x00 0x00 0x00 0x00 0x35 0x33 0x00 0x00 0x00
+					0x100003A 0x55
+					0x1000011
+					0x2000001
+					0x1000029>;
+			};
+
+			tinylcd35_ts: tinylcd35_ts@1 {
+				compatible = "ti,ads7846";
+				reg = <1>;
+				status = "disabled";
+
+				spi-max-frequency = <2000000>;
+				interrupts = <5 2>; /* high-to-low edge triggered */
+				interrupt-parent = <&gpio>;
+				pendown-gpio = <&gpio 5 0>;
+				ti,x-plate-ohms = /bits/ 16 <100>;
+				ti,pressure-max = /bits/ 16 <255>;
+			};
+		};
+	};
+
+	/*  RTC    */
+
+	fragment@5 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			pcf8563: pcf8563@51 {
+				compatible = "nxp,pcf8563";
+				reg = <0x51>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@6 {
+		target = <&i2c1>;
+		__dormant__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			ds1307: ds1307@68 {
+				compatible = "dallas,ds1307";
+				reg = <0x68>;
+				status = "okay";
+			};
+		};
+	};
+
+	/*
+	 * Values for input event code is found under the
+	 * 'Keys and buttons' heading in include/uapi/linux/input.h
+	 */
+	fragment@7 {
+		target-path = "/soc";
+		__overlay__ {
+			keypad: keypad {
+				compatible = "gpio-keys";
+				pinctrl-names = "default";
+				pinctrl-0 = <&keypad_pins>;
+				status = "disabled";
+				autorepeat;
+
+				button@17 {
+					label = "GPIO KEY_UP";
+					linux,code = <103>;
+					gpios = <&gpio 17 0>;
+				};
+				button@22 {
+					label = "GPIO KEY_DOWN";
+					linux,code = <108>;
+					gpios = <&gpio 22 0>;
+				};
+				button@27 {
+					label = "GPIO KEY_LEFT";
+					linux,code = <105>;
+					gpios = <&gpio 27 0>;
+				};
+				button@23 {
+					label = "GPIO KEY_RIGHT";
+					linux,code = <106>;
+					gpios = <&gpio 23 0>;
+				};
+				button@4 {
+					label = "GPIO KEY_ENTER";
+					linux,code = <28>;
+					gpios = <&gpio 4 0>;
+				};
+			};
+		};
+	};
+
+	__overrides__ {
+		speed =      <&tinylcd35>,"spi-max-frequency:0";
+		rotate =     <&tinylcd35>,"rotate:0";
+		fps =        <&tinylcd35>,"fps:0";
+		debug =      <&tinylcd35>,"debug:0";
+		touch =      <&tinylcd35_ts>,"status";
+		touchgpio =  <&tinylcd35_ts_pins>,"brcm,pins:0",
+			     <&tinylcd35_ts>,"interrupts:0",
+			     <&tinylcd35_ts>,"pendown-gpio:4";
+		xohms =      <&tinylcd35_ts>,"ti,x-plate-ohms;0";
+		rtc-pcf =    <0>,"=5";
+		rtc-ds =     <0>,"=6";
+		keypad =     <&keypad>,"status";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/tpm-slb9670-overlay.dts b/arch/arm/boot/dts/overlays/tpm-slb9670-overlay.dts
new file mode 100644
index 000000000000..e69188503ca3
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/tpm-slb9670-overlay.dts
@@ -0,0 +1,44 @@
+/*
+ * Device Tree overlay for the Infineon SLB9670 Trusted Platform Module add-on
+ * boards, which can be used as a secure key storage and hwrng.
+ * available as "Iridium SLB9670" by Infineon and "LetsTrust TPM" by pi3g.
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev1>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+			slb9670: slb9670@1 {
+				compatible = "infineon,slb9670";
+				reg = <1>;	/* CE1 */
+				#address-cells = <1>;
+				#size-cells = <0>;
+				spi-max-frequency = <32000000>;
+				status = "okay";
+			};
+
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/uart0-overlay.dts b/arch/arm/boot/dts/overlays/uart0-overlay.dts
new file mode 100755
index 000000000000..73d563bbaabf
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart0-overlay.dts
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&uart0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			uart0_pins: uart0_pins {
+				brcm,pins = <14 15>;
+				brcm,function = <4>; /* alt0 */
+				brcm,pull = <0 2>;
+			};
+		};
+	};
+
+	__overrides__ {
+		txd0_pin = <&uart0_pins>,"brcm,pins:0";
+		rxd0_pin = <&uart0_pins>,"brcm,pins:4";
+		pin_func = <&uart0_pins>,"brcm,function:0";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/uart1-overlay.dts b/arch/arm/boot/dts/overlays/uart1-overlay.dts
new file mode 100644
index 000000000000..986d725a2652
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart1-overlay.dts
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&uart1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			uart1_pins: uart1_pins {
+				brcm,pins = <14 15>;
+				brcm,function = <2>; /* alt5 */
+				brcm,pull = <0 2>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target-path = "/chosen";
+		__overlay__ {
+			bootargs = "8250.nr_uarts=1";
+		};
+	};
+
+	__overrides__ {
+		txd1_pin = <&uart1_pins>,"brcm,pins:0";
+		rxd1_pin = <&uart1_pins>,"brcm,pins:4";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/uart2-overlay.dts b/arch/arm/boot/dts/overlays/uart2-overlay.dts
new file mode 100644
index 000000000000..9face240aca1
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart2-overlay.dts
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&uart2>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart2_pins>;
+		__dormant__ {
+			brcm,pins = <0 1 2 3>;
+			brcm,pull = <0 2 2 0>;
+		};
+	};
+
+	__overrides__ {
+		ctsrts = <0>,"=1";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/uart3-overlay.dts b/arch/arm/boot/dts/overlays/uart3-overlay.dts
new file mode 100644
index 000000000000..ae9f9fe5ea1d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart3-overlay.dts
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&uart3>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart3_pins>;
+		__dormant__ {
+			brcm,pins = <4 5 6 7>;
+			brcm,pull = <0 2 2 0>;
+		};
+	};
+
+	__overrides__ {
+		ctsrts = <0>,"=1";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/uart4-overlay.dts b/arch/arm/boot/dts/overlays/uart4-overlay.dts
new file mode 100644
index 000000000000..ac004ffbadbf
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart4-overlay.dts
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&uart4>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart4_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart4_pins>;
+		__dormant__ {
+			brcm,pins = <8 9 10 11>;
+			brcm,pull = <0 2 2 0>;
+		};
+	};
+
+	__overrides__ {
+		ctsrts = <0>,"=1";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/uart5-overlay.dts b/arch/arm/boot/dts/overlays/uart5-overlay.dts
new file mode 100644
index 000000000000..04eaf376effe
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/uart5-overlay.dts
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2711";
+
+	fragment@0 {
+		target = <&uart5>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart5_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart5_pins>;
+		__dormant__ {
+			brcm,pins = <12 13 14 15>;
+			brcm,pull = <0 2 2 0>;
+		};
+	};
+
+	__overrides__ {
+		ctsrts = <0>,"=1";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/udrc-overlay.dts b/arch/arm/boot/dts/overlays/udrc-overlay.dts
new file mode 100644
index 000000000000..ae7c37996894
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/udrc-overlay.dts
@@ -0,0 +1,128 @@
+#include <dt-bindings/clock/bcm2835.h>
+/*
+ * Device tree overlay for the Universal Digital Radio Controller
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "brcm,bcm2835";
+    fragment@0 {
+        target = <&i2s>;
+        __overlay__ {
+            clocks = <&clocks BCM2835_CLOCK_PCM>;
+            clock-names = "pcm";
+            status = "okay";
+        };
+    };
+
+    fragment@1 {
+        target-path = "/";
+        __overlay__ {
+            regulators {
+                compatible = "simple-bus";
+                #address-cells = <1>;
+                #size-cells = <0>;
+
+                udrc0_ldoin: udrc0_ldoin {
+                    compatible = "regulator-fixed";
+                    regulator-name = "ldoin";
+                    regulator-min-microvolt = <3300000>;
+                    regulator-max-microvolt = <3300000>;
+                    regulator-always-on;
+                };
+            };
+        };
+    };
+
+    fragment@2 {
+        target = <&i2c1>;
+        __overlay__ {
+            #address-cells = <1>;
+            #size-cells = <0>;
+            status = "okay";
+            clocks = <&clocks BCM2835_CLOCK_VPU>;
+            clock-frequency = <400000>;
+
+            tlv320aic32x4: tlv320aic32x4@18 {
+                compatible = "ti,tlv320aic32x4";
+                #sound-dai-cells = <0>;
+                reg = <0x18>;
+                status = "okay";
+
+                clocks = <&clocks BCM2835_CLOCK_GP0>;
+                clock-names = "mclk";
+                assigned-clocks = <&clocks BCM2835_CLOCK_GP0>;
+                assigned-clock-rates = <25000000>;
+
+                pinctrl-names = "default";
+                pinctrl-0 = <&gpclk0_pin &aic3204_reset>;
+
+                reset-gpios = <&gpio 13 0>;
+
+                iov-supply = <&udrc0_ldoin>;
+                ldoin-supply = <&udrc0_ldoin>;
+            };
+        };
+    };
+
+    fragment@3 {
+        target = <&sound>;
+        snd: __overlay__ {
+            compatible = "simple-audio-card";
+            i2s-controller = <&i2s>;
+            status = "okay";
+
+            simple-audio-card,name = "udrc";
+            simple-audio-card,format = "i2s";
+
+            simple-audio-card,bitclock-master = <&dailink0_master>;
+            simple-audio-card,frame-master = <&dailink0_master>;
+
+            simple-audio-card,widgets =
+                "Line", "Line In",
+                "Line", "Line Out";
+
+            simple-audio-card,routing =
+                "IN1_R", "Line In",
+                "IN1_L", "Line In",
+                "CM_L", "Line In",
+                "CM_R", "Line In",
+                "Line Out", "LOR",
+                "Line Out", "LOL";
+
+            dailink0_master: simple-audio-card,cpu {
+                sound-dai = <&i2s>;
+            };
+
+            simple-audio-card,codec {
+                sound-dai = <&tlv320aic32x4>;
+            };
+        };
+    };
+
+    fragment@4 {
+        target = <&gpio>;
+        __overlay__ {
+            gpclk0_pin: gpclk0_pin {
+                brcm,pins = <4>;
+                brcm,function = <4>;
+            };
+
+            aic3204_reset: aic3204_reset {
+                brcm,pins = <13>;
+                brcm,function = <1>;
+                brcm,pull = <1>;
+            };
+
+            aic3204_gpio: aic3204_gpio {
+                brcm,pins = <26>;
+            };
+        };
+    };
+
+    __overrides__ {
+        alsaname = <&snd>, "simple-audio-card,name";
+    };
+};
diff --git a/arch/arm/boot/dts/overlays/upstream-overlay.dts b/arch/arm/boot/dts/overlays/upstream-overlay.dts
new file mode 100644
index 000000000000..2e9dcd4f5f0a
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/upstream-overlay.dts
@@ -0,0 +1,113 @@
+// redo: ovmerge -c vc4-kms-v3d-overlay.dts,cma-default dwc2-overlay.dts,dr_mode=otg
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/clock/bcm2835.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+	fragment@0 {
+		target = <&cma>;
+		__dormant__ {
+			size = <0x10000000>;
+		};
+	};
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@2 {
+		target = <&fb>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+	fragment@3 {
+		target = <&pixelvalve0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@4 {
+		target = <&pixelvalve1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@5 {
+		target = <&pixelvalve2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@6 {
+		target = <&hvs>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@7 {
+		target = <&hdmi>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@8 {
+		target = <&v3d>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@9 {
+		target = <&vc4>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@10 {
+		target = <&clocks>;
+		__overlay__ {
+			claim-clocks = <BCM2835_PLLD_DSI0 BCM2835_PLLD_DSI1 BCM2835_PLLH_AUX BCM2835_PLLH_PIX>;
+		};
+	};
+	fragment@11 {
+		target = <&vec>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@12 {
+		target = <&txp>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@13 {
+		target = <&hdmi>;
+		__dormant__ {
+			dmas;
+		};
+	};
+	fragment@14 {
+		target = <&audio>;
+		__overlay__ {
+			brcm,disable-hdmi;
+		};
+	};
+	fragment@15 {
+		target = <&usb>;
+		#address-cells = <1>;
+		#size-cells = <1>;
+		__overlay__ {
+			compatible = "brcm,bcm2835-usb";
+			dr_mode = "otg";
+			g-np-tx-fifo-size = <32>;
+			g-rx-fifo-size = <558>;
+			g-tx-fifo-size = <512 512 512 512 512 256 256>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/upstream-pi4-overlay.dts b/arch/arm/boot/dts/overlays/upstream-pi4-overlay.dts
new file mode 100644
index 000000000000..6195e02bf9ff
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/upstream-pi4-overlay.dts
@@ -0,0 +1,161 @@
+// redo: ovmerge -c vc4-kms-v3d-pi4-overlay.dts,cma-default dwc2-overlay.dts,dr_mode=otg
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/clock/bcm2835.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+	fragment@0 {
+		target = <&cma>;
+		__dormant__ {
+			size = <0x10000000>;
+		};
+	};
+	fragment@1 {
+		target = <&ddc0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@2 {
+		target = <&ddc1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@3 {
+		target = <&hdmi0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@4 {
+		target = <&hdmi1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@5 {
+		target = <&hvs>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@6 {
+		target = <&pixelvalve0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@7 {
+		target = <&pixelvalve1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@8 {
+		target = <&pixelvalve2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@9 {
+		target = <&pixelvalve3>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@10 {
+		target = <&pixelvalve4>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@11 {
+		target = <&v3d>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@12 {
+		target = <&vc4>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@13 {
+		target = <&txp>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@14 {
+		target = <&fb>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+	fragment@15 {
+		target = <&firmwarekms>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+	fragment@16 {
+		target = <&vec>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+	fragment@17 {
+		target = <&hdmi0>;
+		__dormant__ {
+			dmas;
+		};
+	};
+	fragment@18 {
+		target = <&hdmi1>;
+		__dormant__ {
+			dmas;
+		};
+	};
+	fragment@19 {
+		target = <&audio>;
+		__overlay__ {
+			brcm,disable-hdmi;
+		};
+	};
+	fragment@20 {
+		target = <&dvp>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+	fragment@21 {
+		target = <&pixelvalve3>;
+		__dormant__ {
+			status = "okay";
+		};
+	};
+	fragment@22 {
+		target = <&vec>;
+		__dormant__ {
+			status = "okay";
+		};
+	};
+	fragment@23 {
+		target = <&usb>;
+		#address-cells = <1>;
+		#size-cells = <1>;
+		__overlay__ {
+			compatible = "brcm,bcm2835-usb";
+			dr_mode = "otg";
+			g-np-tx-fifo-size = <32>;
+			g-rx-fifo-size = <558>;
+			g-tx-fifo-size = <512 512 512 512 512 256 256>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/vc4-fkms-v3d-overlay.dts b/arch/arm/boot/dts/overlays/vc4-fkms-v3d-overlay.dts
new file mode 100644
index 000000000000..ca344492bed8
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/vc4-fkms-v3d-overlay.dts
@@ -0,0 +1,40 @@
+/*
+ * vc4-fkms-v3d-overlay.dts
+ */
+
+/dts-v1/;
+/plugin/;
+
+#include "cma-overlay.dts"
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@1 {
+		target = <&fb>;
+		__overlay__  {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&firmwarekms>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&v3d>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target = <&vc4>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/vc4-kms-kippah-7inch-overlay.dts b/arch/arm/boot/dts/overlays/vc4-kms-kippah-7inch-overlay.dts
new file mode 100644
index 000000000000..b03394844abd
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/vc4-kms-kippah-7inch-overlay.dts
@@ -0,0 +1,43 @@
+/*
+ * vc4-kms-v3d-overlay.dts
+ */
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/pinctrl/bcm2835.h>
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+			panel: panel {
+				compatible = "ontat,yx700wv03", "simple-panel";
+
+				port {
+					panel_in: endpoint {
+						remote-endpoint = <&dpi_out>;
+					};
+				};
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&dpi>;
+		__overlay__  {
+			status = "okay";
+
+			pinctrl-names = "default";
+			pinctrl-0 = <&dpi_18bit_gpio0>;
+
+			port {
+				dpi_out: endpoint@0 {
+					remote-endpoint = <&panel_in>;
+				};
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts b/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
new file mode 100644
index 000000000000..6d34a2bff49b
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
@@ -0,0 +1,122 @@
+/*
+ * vc4-kms-v3d-overlay.dts
+ */
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/clock/bcm2835.h>
+
+#include "cma-overlay.dts"
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&fb>;
+		__overlay__  {
+			status = "disabled";
+		};
+	};
+
+	fragment@3 {
+		target = <&pixelvalve0>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target = <&pixelvalve1>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target = <&pixelvalve2>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@6 {
+		target = <&hvs>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@7 {
+		target = <&hdmi>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@8 {
+		target = <&v3d>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@9 {
+		target = <&vc4>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@10 {
+		target = <&clocks>;
+		__overlay__  {
+			claim-clocks = <
+				BCM2835_PLLD_DSI0
+				BCM2835_PLLD_DSI1
+				BCM2835_PLLH_AUX
+				BCM2835_PLLH_PIX
+			>;
+		};
+	};
+
+	fragment@11 {
+		target = <&vec>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@12 {
+		target = <&txp>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@13 {
+		target = <&hdmi>;
+		__dormant__  {
+			dmas;
+		};
+	};
+
+	fragment@14 {
+		target = <&audio>;
+		__overlay__  {
+		    brcm,disable-hdmi;
+		};
+	};
+
+	__overrides__ {
+		audio   = <0>,"!13", <0>,"=14";
+		noaudio = <0>,"=13", <0>,"!14";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts b/arch/arm/boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts
new file mode 100644
index 000000000000..f721f12d729d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/vc4-kms-v3d-pi4-overlay.dts
@@ -0,0 +1,186 @@
+/*
+ * vc4-kms-v3d-pi4-overlay.dts
+ */
+
+/dts-v1/;
+/plugin/;
+
+#include <dt-bindings/clock/bcm2835.h>
+
+#include "cma-overlay.dts"
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@1 {
+		target = <&ddc0>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&ddc1>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@3 {
+		target = <&hdmi0>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@4 {
+		target = <&hdmi1>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@5 {
+		target = <&hvs>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@6 {
+		target = <&pixelvalve0>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@7 {
+		target = <&pixelvalve1>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@8 {
+		target = <&pixelvalve2>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@9 {
+		target = <&pixelvalve3>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@10 {
+		target = <&pixelvalve4>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@11 {
+		target = <&v3d>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@12 {
+		target = <&vc4>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@13 {
+		target = <&txp>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@14 {
+		target = <&fb>;
+		__overlay__  {
+			status = "disabled";
+		};
+	};
+
+	fragment@15 {
+		target = <&firmwarekms>;
+		__overlay__  {
+			status = "disabled";
+		};
+	};
+
+	fragment@16 {
+		target = <&vec>;
+		__overlay__  {
+			status = "disabled";
+		};
+	};
+
+	fragment@17 {
+		target = <&hdmi0>;
+		__dormant__  {
+			dmas;
+		};
+	};
+
+	fragment@18 {
+		target = <&hdmi1>;
+		__dormant__  {
+			dmas;
+		};
+	};
+
+	fragment@19 {
+		target = <&audio>;
+		__overlay__  {
+		    brcm,disable-hdmi;
+		};
+	};
+
+	fragment@20 {
+		target = <&dvp>;
+		__overlay__  {
+			status = "okay";
+		};
+	};
+
+	fragment@21 {
+		target = <&pixelvalve3>;
+		__dormant__  {
+			status = "okay";
+		};
+	};
+
+	fragment@22 {
+		target = <&vec>;
+		__dormant__  {
+			status = "okay";
+		};
+	};
+
+	__overrides__ {
+		audio   = <0>,"!17";
+		audio1   = <0>,"!18";
+		noaudio = <0>,"=17", <0>,"=18", <0>,"!19";
+		composite = <0>, "!1",
+			    <0>, "!2",
+			    <0>, "!3",
+			    <0>, "!4",
+			    <0>, "!6",
+			    <0>, "!7",
+			    <0>, "!8",
+			    <0>, "!9",
+			    <0>, "!10",
+			    <0>, "!16",
+			    <0>, "=21",
+			    <0>, "=22";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/vga666-overlay.dts b/arch/arm/boot/dts/overlays/vga666-overlay.dts
new file mode 100644
index 000000000000..a4968d180a5d
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/vga666-overlay.dts
@@ -0,0 +1,30 @@
+/dts-v1/;
+/plugin/;
+
+/{
+	compatible = "brcm,bcm2835";
+
+	// There is no VGA driver module, but we need a platform device
+	// node (that doesn't already use pinctrl) to hang the pinctrl
+	// reference on - leds will do
+
+	fragment@0 {
+		target = <&leds>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&vga666_pins>;
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			vga666_pins: vga666_pins {
+				brcm,pins = <2 3 4 5 6 7 8 9 10 11 12
+					     13 14 15 16 17 18 19 20 21>;
+				brcm,function = <6>; /* alt2 */
+				brcm,pull = <0>; /* no pull */
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/w1-gpio-overlay.dts b/arch/arm/boot/dts/overlays/w1-gpio-overlay.dts
new file mode 100644
index 000000000000..f44e325bc1f2
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/w1-gpio-overlay.dts
@@ -0,0 +1,40 @@
+// Definitions for w1-gpio module (without external pullup)
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+
+			w1: onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&gpio 4 0>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			w1_pins: w1_pins@0 {
+				brcm,pins = <4>;
+				brcm,function = <0>; // in (initially)
+				brcm,pull = <0>; // off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin =       <&w1>,"gpios:4",
+				<&w1>,"reg:0",
+				<&w1_pins>,"brcm,pins:0",
+				<&w1_pins>,"reg:0";
+		pullup;		// Silently ignore unneeded parameter
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/w1-gpio-pullup-overlay.dts b/arch/arm/boot/dts/overlays/w1-gpio-pullup-overlay.dts
new file mode 100644
index 000000000000..953c6a1aeab9
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/w1-gpio-pullup-overlay.dts
@@ -0,0 +1,42 @@
+// Definitions for w1-gpio module (with external pullup)
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target-path = "/";
+		__overlay__ {
+
+			w1: onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&gpio 4 0>, <&gpio 5 1>;
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&gpio>;
+		__overlay__ {
+			w1_pins: w1_pins@0 {
+				brcm,pins = <4 5>;
+				brcm,function = <0 1>; // in out
+				brcm,pull = <0 0>; // off off
+			};
+		};
+	};
+
+	__overrides__ {
+		gpiopin =       <&w1>,"gpios:4",
+				<&w1>,"reg:0",
+				<&w1_pins>,"brcm,pins:0",
+				<&w1_pins>,"reg:0";
+		extpullup =     <&w1>,"gpios:16",
+				<&w1_pins>,"brcm,pins:4";
+		pullup;		// Silently ignore unneeded parameter
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/w5500-overlay.dts b/arch/arm/boot/dts/overlays/w5500-overlay.dts
new file mode 100644
index 000000000000..4d3e66296753
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/w5500-overlay.dts
@@ -0,0 +1,63 @@
+// Overlay for the Wiznet w5500 Ethernet Controller
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&spidev0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@1 {
+		target = <&spidev1>;
+		__dormant__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+			/* needed to avoid dtc warning */
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			status = "okay";
+
+			eth1: w5500@0{
+				compatible = "wiznet,w5500";
+				reg = <0>; /* CE0 */
+				pinctrl-names = "default";
+				pinctrl-0 = <&eth1_pins>;
+				interrupt-parent = <&gpio>;
+				interrupts = <25 0x8>;
+				spi-max-frequency = <30000000>;
+//				local-mac-address = [aa bb cc dd ee ff];
+				status = "okay";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&gpio>;
+		__overlay__ {
+			eth1_pins: eth1_pins {
+				brcm,pins = <25>;
+				brcm,function = <0>; /* in */
+				brcm,pull = <0>; /* none */
+			};
+		};
+	};
+
+	__overrides__ {
+		int_pin = <&eth1>, "interrupts:0",
+		          <&eth1_pins>, "brcm,pins:0";
+		speed   = <&eth1>, "spi-max-frequency:0";
+		cs      = <&eth1>, "reg:0",
+			  <0>, "!0=1";
+	};
+};
diff --git a/arch/arm/boot/dts/overlays/wittypi-overlay.dts b/arch/arm/boot/dts/overlays/wittypi-overlay.dts
new file mode 100644
index 000000000000..71ce806186de
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/wittypi-overlay.dts
@@ -0,0 +1,44 @@
+/*
+ * Device Tree overlay for Witty Pi extension board by UUGear
+ *
+ */
+
+/dts-v1/;
+/plugin/;
+
+/ {
+
+	compatible = "brcm,bcm2835";
+
+	fragment@0 {
+		target = <&leds>;
+		__overlay__ {
+			compatible = "gpio-leds";
+			wittypi_led: wittypi_led {
+				label = "wittypi_led";
+				linux,default-trigger = "default-on";
+				gpios = <&gpio 17 0>;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			rtc: ds1337@68 {
+				compatible = "dallas,ds1337";
+				reg = <0x68>;
+				wakeup-source;
+			};
+		};
+	};
+
+	__overrides__ {
+		led_gpio =	<&wittypi_led>,"gpios:4";
+		led_trigger =	<&wittypi_led>,"linux,default-trigger";
+	};
+
+};
diff --git a/arch/arm64/boot/dts/Makefile b/arch/arm64/boot/dts/Makefile
index 9b1170658d60..cc6c25629057 100644
--- a/arch/arm64/boot/dts/Makefile
+++ b/arch/arm64/boot/dts/Makefile
@@ -30,3 +30,5 @@ subdir-y += ti
 subdir-y += toshiba
 subdir-y += xilinx
 subdir-y += zte
+
+subdir-y += overlays
diff --git a/arch/arm64/boot/dts/broadcom/Makefile b/arch/arm64/boot/dts/broadcom/Makefile
index cb7de8d99223..c3eaf8d63ee4 100644
--- a/arch/arm64/boot/dts/broadcom/Makefile
+++ b/arch/arm64/boot/dts/broadcom/Makefile
@@ -1,9 +1,21 @@
 # SPDX-License-Identifier: GPL-2.0
-dtb-$(CONFIG_ARCH_BCM2835) += bcm2711-rpi-4-b.dtb \
-			      bcm2837-rpi-3-a-plus.dtb \
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2837-rpi-3-a-plus.dtb \
 			      bcm2837-rpi-3-b.dtb \
 			      bcm2837-rpi-3-b-plus.dtb \
 			      bcm2837-rpi-cm3-io3.dtb
+dtb-$(CONFIG_ARCH_BCM2709) += bcm2710-rpi-2-b.dtb
+dtb-$(CONFIG_ARCH_BCM2709) += bcm2710-rpi-3-b.dtb
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2710-rpi-2-b.dtb
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2710-rpi-3-b.dtb
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2711-rpi-4-b.dtb
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2710-rpi-3-b-plus.dtb
+dtb-$(CONFIG_ARCH_BCM2709) += bcm2710-rpi-cm3.dtb
+dtb-$(CONFIG_ARCH_BCM2835) += bcm2710-rpi-cm3.dtb
 
 subdir-y	+= northstar2
 subdir-y	+= stingray
+
+# Enable fixups to support overlays on BCM2835 platforms
+ifeq ($(CONFIG_ARCH_BCM2835),y)
+	DTC_FLAGS ?= -@
+endif
diff --git a/arch/arm64/boot/dts/broadcom/bcm2710-rpi-2-b.dts b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-2-b.dts
new file mode 100644
index 000000000000..116cdbf94b9b
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-2-b.dts
@@ -0,0 +1,3 @@
+#define RPI364
+
+#include "../../../../arm/boot/dts/bcm2710-rpi-2-b.dts"
diff --git a/arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b-plus.dts b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b-plus.dts
new file mode 100644
index 000000000000..d9242ff77079
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b-plus.dts
@@ -0,0 +1,3 @@
+#define RPI364
+
+#include "../../../../arm/boot/dts/bcm2710-rpi-3-b-plus.dts"
diff --git a/arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b.dts b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b.dts
new file mode 100644
index 000000000000..deb33441da95
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-3-b.dts
@@ -0,0 +1,3 @@
+#define RPI364
+
+#include "../../../../arm/boot/dts/bcm2710-rpi-3-b.dts"
diff --git a/arch/arm64/boot/dts/broadcom/bcm2710-rpi-cm3.dts b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-cm3.dts
new file mode 100644
index 000000000000..1c2560017c02
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm2710-rpi-cm3.dts
@@ -0,0 +1,3 @@
+#define RPI364
+
+#include "../../../../arm/boot/dts/bcm2710-rpi-cm3.dts"
diff --git a/arch/arm64/boot/dts/broadcom/bcm2711-rpi-4-b.dts b/arch/arm64/boot/dts/broadcom/bcm2711-rpi-4-b.dts
index d24c53682e44..1fd86f81f542 100644
--- a/arch/arm64/boot/dts/broadcom/bcm2711-rpi-4-b.dts
+++ b/arch/arm64/boot/dts/broadcom/bcm2711-rpi-4-b.dts
@@ -1,2 +1,3 @@
-// SPDX-License-Identifier: GPL-2.0
-#include "arm/bcm2711-rpi-4-b.dts"
+#define RPI364
+
+#include "../../../../arm/boot/dts/bcm2711-rpi-4-b.dts"
diff --git a/arch/arm64/boot/dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi b/arch/arm64/boot/dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi
new file mode 120000
index 000000000000..e5c400284467
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi
@@ -0,0 +1 @@
+../../../../arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi
\ No newline at end of file
diff --git a/arch/arm64/boot/dts/broadcom/bcm283x-rpi-lan7515.dtsi b/arch/arm64/boot/dts/broadcom/bcm283x-rpi-lan7515.dtsi
new file mode 120000
index 000000000000..fc4c05bbe7fd
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm283x-rpi-lan7515.dtsi
@@ -0,0 +1 @@
+../../../../arm/boot/dts/bcm283x-rpi-lan7515.dtsi
\ No newline at end of file
diff --git a/arch/arm64/boot/dts/overlays b/arch/arm64/boot/dts/overlays
new file mode 120000
index 000000000000..ded08646b6f6
--- /dev/null
+++ b/arch/arm64/boot/dts/overlays
@@ -0,0 +1 @@
+../../../arm/boot/dts/overlays
\ No newline at end of file
diff --git a/scripts/Makefile.dtbinst b/scripts/Makefile.dtbinst
index 50d580d77ae9..079b83308011 100644
--- a/scripts/Makefile.dtbinst
+++ b/scripts/Makefile.dtbinst
@@ -18,9 +18,10 @@ include scripts/Kbuild.include
 include $(src)/Makefile
 
 dtbs    := $(addprefix $(dst)/, $(dtb-y) $(if $(CONFIG_OF_ALL_DTBS),$(dtb-)))
+dtbos   := $(addprefix $(dst)/, $(dtbo-y) $(if $(CONFIG_OF_ALL_DTBS),$(dtb-)))
 subdirs := $(addprefix $(obj)/, $(subdir-y) $(subdir-m))
 
-__dtbs_install: $(dtbs) $(subdirs)
+__dtbs_install: $(dtbs) $(dtbos) $(subdirs)
 	@:
 
 quiet_cmd_dtb_install = INSTALL $@
@@ -29,6 +30,9 @@ quiet_cmd_dtb_install = INSTALL $@
 $(dst)/%.dtb: $(obj)/%.dtb
 	$(call cmd,dtb_install)
 
+$(dst)/%.dtbo: $(obj)/%.dtbo
+	$(call cmd,dtb_install)
+
 PHONY += $(subdirs)
 $(subdirs):
 	$(Q)$(MAKE) $(dtbinst)=$@ dst=$(patsubst $(obj)/%,$(dst)/%,$@)
diff --git a/scripts/Makefile.lib b/scripts/Makefile.lib
index 94133708889d..9c0df5bde46c 100644
--- a/scripts/Makefile.lib
+++ b/scripts/Makefile.lib
@@ -281,6 +281,7 @@ DTC_FLAGS += -Wno-interrupt_provider
 ifeq ($(findstring 1,$(KBUILD_EXTRA_WARN)),)
 DTC_FLAGS += -Wno-unit_address_vs_reg \
 	-Wno-unit_address_format \
+	-Wno-gpios_property \
 	-Wno-avoid_unnecessary_addr_size \
 	-Wno-alias_paths \
 	-Wno-graph_child_address \
@@ -341,6 +342,18 @@ endef
 $(obj)/%.dt.yaml: $(src)/%.dts $(DTC) $(DT_TMP_SCHEMA) FORCE
 	$(call if_changed_rule,dtc,yaml)
 
+quiet_cmd_dtco = DTCO    $@
+cmd_dtco = mkdir -p $(dir ${dtc-tmp}) ; \
+	$(CPP) $(dtc_cpp_flags) -x assembler-with-cpp -o $(dtc-tmp) $< ; \
+	$(DTC) -@ -H epapr -O dtb -o $@ -b 0 \
+		-i $(dir $<) $(DTC_FLAGS) \
+		-Wno-interrupts_property \
+		-d $(depfile).dtc.tmp $(dtc-tmp) ; \
+	cat $(depfile).pre.tmp $(depfile).dtc.tmp > $(depfile)
+
+$(obj)/%.dtbo: $(src)/%-overlay.dts FORCE
+	$(call if_changed_dep,dtco)
+
 dtc-tmp = $(subst $(comma),_,$(dot-target).dts.tmp)
 
 # Bzip2
-- 
2.30.2

