// SPDX-License-Identifier: GPL-2.0-or-later

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "compex,wpj558-16m", "qca,qca9558";
	model = "Compex WPJ558 (16MB flash)";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_sig4;
		led-failsafe = &led_sig4;
		led-running = &led_sig4;
		led-upgrade = &led_sig4;
	};

	leds {
		compatible = "gpio-leds";

		sig1 {
			label = "red:sig1";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		sig2 {
			label = "yellow:sig2";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		sig3 {
			label = "green:sig3";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led_sig4: sig4 {
			label = "green:sig4";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	beeper {
		compatible = "gpio-beeper";
		gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x030000>;
				read-only;
			};

			firmware@30000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x030000 0xfc0000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x0c 0x07600000 /* PORT6 PAD MODE CTRL */
			0x50 0xcc35cc35 /* LED_CTRL0 */
			0x54 0x00000000 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x03ffff00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x0000007e /* PORT6 STATUS */
		>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x56000000 0x00000101 0x00001616>;
	phy-handle = <&phy0>;

	nvmem-cells = <&macaddr_uboot_2e010>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&pcie0 {
	status = "okay";
};

&uboot {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_uboot_2e010: macaddr@2e010 {
		reg = <0x2e010 0x6>;
	};
};
