// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "cn7130_ubnt_edgerouter-e300.dtsi"

/ {
	compatible = "ubnt,edgerouter-6p", "cavium,cn7130";
	model = "Ubiquiti EdgeRouter 6P";
};

&smi0 {
	phy8: ethernet-phy@8 {
		device_type = "ethernet-phy";
		interrupts = <17 8>;
		interrupt-parent = <&gpio>;
		compatible = "vitesse,vsc8514", "ethernet-phy-ieee802.3-c22";
		reg = <8>;
	};

	phy9: ethernet-phy@9 {
		device_type = "ethernet-phy";
		interrupts = <17 8>;
		interrupt-parent = <&gpio>;
		compatible = "vitesse,vsc8514", "ethernet-phy-ieee802.3-c22";
		reg = <9>;
	};
};

&pip {
	interface@0 {
		ethernet@0 {
			label = "lan5";
			status = "okay";
			phy-mode = "sgmii";
			phy-handle = <&phy4>;
			nvmem-cells = <&macaddr_eeprom_0>;
			nvmem-cell-names = "mac-address";
		};
	};

	interface@1 {
		status = "okay";

		ethernet@0 {
			label = "lan3";
			status = "okay";
			phy-mode = "sgmii";
			phy-handle = <&phy8>;
			nvmem-cells = <&macaddr_eeprom_0>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <(4)>;
		};

		ethernet@1 {
			label = "lan4";
			status = "okay";
			phy-mode = "sgmii";
			phy-handle = <&phy9>;
			nvmem-cells = <&macaddr_eeprom_0>;
			nvmem-cell-names = "mac-address";
			mac-address-increment = <(5)>;
		};
	};
};

&eeprom {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_eeprom_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
