From 05a1c88d9b8dd344edfce3eaa00a3cac866cf3ad Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 29 Apr 2020 21:47:25 +0100
Subject: [PATCH] media: i2c: ov5647: Neither analogue gain nor
 exposure need EXECUTE_ON_WRITE

The controls for analogue gain and exposure were defined with
V4L2_CTRL_FLAG_EXECUTE_ON_WRITE. This is not required as we only need
to send changes to the sensor.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/i2c/ov5647.c | 27 ++++++++++++---------------
 1 file changed, 12 insertions(+), 15 deletions(-)

--- a/drivers/media/i2c/ov5647.c
+++ b/drivers/media/i2c/ov5647.c
@@ -1472,7 +1472,6 @@ static int ov5647_probe(struct i2c_clien
 	struct v4l2_subdev *sd;
 	struct device_node *np = client->dev.of_node;
 	u32 xclk_freq;
-	struct v4l2_ctrl *ctrl;
 	int hblank;
 
 	sensor = devm_kzalloc(dev, sizeof(*sensor), GFP_KERNEL);
@@ -1525,20 +1524,18 @@ static int ov5647_probe(struct i2c_clien
 			       V4L2_EXPOSURE_MANUAL,  /* max */
 			       0,                     /* skip_mask */
 			       V4L2_EXPOSURE_MANUAL); /* default */
-	ctrl = v4l2_ctrl_new_std(&sensor->ctrls, &ov5647_ctrl_ops,
-				 V4L2_CID_EXPOSURE,
-				 4,     /* min lines */
-				 65535, /* max lines (4+8+4 bits)*/
-				 1,     /* step */
-				 1000); /* default number of lines */
-	ctrl->flags |= V4L2_CTRL_FLAG_EXECUTE_ON_WRITE;
-	ctrl = v4l2_ctrl_new_std(&sensor->ctrls, &ov5647_ctrl_ops,
-				 V4L2_CID_ANALOGUE_GAIN,
-				 16,   /* min, 16 = 1.0x */
-				 1023, /* max (10 bits) */
-				 1,    /* step */
-				 32);  /* default, 32 = 2.0x */
-	ctrl->flags |= V4L2_CTRL_FLAG_EXECUTE_ON_WRITE;
+	v4l2_ctrl_new_std(&sensor->ctrls, &ov5647_ctrl_ops,
+			  V4L2_CID_EXPOSURE,
+			  4,     /* min lines */
+			  65535, /* max lines (4+8+4 bits)*/
+			  1,     /* step */
+			  1000); /* default number of lines */
+	v4l2_ctrl_new_std(&sensor->ctrls, &ov5647_ctrl_ops,
+			  V4L2_CID_ANALOGUE_GAIN,
+			  16,   /* min, 16 = 1.0x */
+			  1023, /* max (10 bits) */
+			  1,    /* step */
+			  32);  /* default, 32 = 2.0x */
 
 	/* Set the default mode before we init the subdev */
 	sensor->mode = OV5647_DEFAULT_MODE;
