From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] ARM: dts: BCM5301X: Update Northstar pinctrl binding
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---

--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -422,7 +422,7 @@
 		#size-cells = <1>;
 
 		cru@100 {
-			compatible = "simple-bus";
+			compatible = "syscon", "simple-mfd";
 			reg = <0x100 0x1a4>;
 			ranges;
 			#address-cells = <1>;
@@ -448,10 +448,9 @@
 						     "sata1", "sata2";
 			};
 
-			pinctrl: pin-controller@1c0 {
+			pinctrl: pin-controller {
 				compatible = "brcm,bcm4708-pinmux";
-				reg = <0x1c0 0x24>;
-				reg-names = "cru_gpio_control";
+				offset = <0xc0>;
 
 				spi-pins {
 					groups = "spi_grp";
