// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6328.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Innacomm W3400V6";
	compatible = "innacomm,w3400v6", "brcm,bcm6328";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wps {
			label = "wps";
			gpios = <&pinctrl 15 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 23 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <16666667>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "brcm,bcm963xx-cfe-nor-partitions";
		};
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds>;

	led@1 {
		reg = <1>;
		active-low;
		label = "green:inet";
	};

	led@2 {
		reg = <2>;
		active-low;
		label = "red:inet";
	};

	led@3 {
		reg = <3>;
		active-low;
		label = "green:dsl";
	};

	led_power_green: led@4 {
		reg = <4>;
		active-low;
		label = "green:power";
		default-state = "on";
	};

	led_power_red: led@5 {
		reg = <5>;
		active-low;
		label = "red:power";
	};

	led@11 {
		reg = <11>;
		active-low;
		label = "green:wps";
	};
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio1", "gpio2", "gpio3",
		       "gpio4", "gpio5", "gpio11";
	};
};

&uart0 {
	status = "okay";
};
