// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "D-Link DIR-859 A1";
	compatible = "dlink,dir-859-a1", "qca,qca9563";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		wps {
			label = "green:wps";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		led_power: power {
			label = "green:power";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		internet {
			label = "green:internet";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	gpio-export {
		compatible = "gpio-export";
		#size-cells = <0>;

		gpio_switch_reset {
			gpio-export,name = "dir-859-a1:reset:switch";
			gpio-export,output = <1>;
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
		};
	};
};

&pcie {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "bootloader";
				reg = <0x000000 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "bdcfg";
				reg = <0x040000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "devdata";
				reg = <0x050000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "devconf";
				reg = <0x060000 0x10000>;
				read-only;
			};

			partition@70000 {
				compatible = "seama";
				label = "firmware";
				reg = <0x070000 0xf80000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0>;

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,mib-poll-interval = <500>;

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x10 0x81000080 /* POWER_ON_STRAP */
			0x50 0xcc35cc35 /* LED_CTRL0 */
			0x54 0xcb37cb37 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x00f3cf00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};
