#include "rt3050.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "alphanetworks,asl26555", "ralink,rt3050-soc";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 10 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		eth {
			label = "green:eth";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
		};

		wan-red {
			label = "red:wan";
			gpios = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		};

		wan-green {
			label = "green:wan";
			gpios = <&gpio0 2 GPIO_ACTIVE_HIGH>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio0 7 GPIO_ACTIVE_HIGH>;
		};

		led_power_green: power-green {
			label = "green:power";
			gpios = <&gpio0 8 GPIO_ACTIVE_HIGH>;
		};

		power-red {
			label = "red:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_HIGH>;
		};

		3g-green {
			label = "green:3g";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
			trigger-sources = <&otg_port1>;
			linux,default-trigger = "usbport";
		};

		3g-red {
			label = "red:3g";
			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "jtag", "rgmii", "mdio", "uartf";
		function = "gpio";
	};
};

&esw {
	mediatek,portmap = <0x1e>;
};

&wmac {
	ralink,mtd-eeprom = <&devdata 0x4000>;
};

&otg {
	status = "okay";
};
