From 2d5ba37461013253d2ff0a3641b727fd32ea97a9 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Tue, 23 Feb 2021 18:44:53 +0100
Subject: [PATCH 1/3] usb: ehci: add spurious flag to disable overcurrent
 checking
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This patch adds an ignore_oc flag which can be set by EHCI controller
not supporting or wanting to disable overcurrent checking. The EHCI
platform data in include/linux/usb/ehci_pdriver.h is also augmented to
take advantage of this new flag.

Signed-off-by: Florian Fainelli <florian@openwrt.org>
Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Link: https://lore.kernel.org/r/20210223174455.1378-2-noltari@gmail.com
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/ehci-hcd.c      | 2 +-
 drivers/usb/host/ehci-hub.c      | 4 ++--
 drivers/usb/host/ehci-platform.c | 2 ++
 drivers/usb/host/ehci.h          | 1 +
 include/linux/usb/ehci_pdriver.h | 1 +
 5 files changed, 7 insertions(+), 3 deletions(-)

--- a/drivers/usb/host/ehci-hcd.c
+++ b/drivers/usb/host/ehci-hcd.c
@@ -651,7 +651,7 @@ static int ehci_run (struct usb_hcd *hcd
 		"USB %x.%x started, EHCI %x.%02x%s\n",
 		((ehci->sbrn & 0xf0)>>4), (ehci->sbrn & 0x0f),
 		temp >> 8, temp & 0xff,
-		ignore_oc ? ", overcurrent ignored" : "");
+		(ignore_oc || ehci->spurious_oc) ? ", overcurrent ignored" : "");
 
 	ehci_writel(ehci, INTR_MASK,
 		    &ehci->regs->intr_enable); /* Turn On Interrupts */
--- a/drivers/usb/host/ehci-hub.c
+++ b/drivers/usb/host/ehci-hub.c
@@ -643,7 +643,7 @@ ehci_hub_status_data (struct usb_hcd *hc
 	 * always set, seem to clear PORT_OCC and PORT_CSC when writing to
 	 * PORT_POWER; that's surprising, but maybe within-spec.
 	 */
-	if (!ignore_oc)
+	if (!ignore_oc && !ehci->spurious_oc)
 		mask = PORT_CSC | PORT_PEC | PORT_OCC;
 	else
 		mask = PORT_CSC | PORT_PEC;
@@ -1013,7 +1013,7 @@ int ehci_hub_control(
 		if (temp & PORT_PEC)
 			status |= USB_PORT_STAT_C_ENABLE << 16;
 
-		if ((temp & PORT_OCC) && !ignore_oc){
+		if ((temp & PORT_OCC) && (!ignore_oc && !ehci->spurious_oc)){
 			status |= USB_PORT_STAT_C_OVERCURRENT << 16;
 
 			/*
--- a/drivers/usb/host/ehci-platform.c
+++ b/drivers/usb/host/ehci-platform.c
@@ -319,6 +319,8 @@ static int ehci_platform_probe(struct pl
 		hcd->has_tt = 1;
 	if (pdata->reset_on_resume)
 		priv->reset_on_resume = true;
+	if (pdata->spurious_oc)
+		ehci->spurious_oc = 1;
 
 #ifndef CONFIG_USB_EHCI_BIG_ENDIAN_MMIO
 	if (ehci->big_endian_mmio) {
--- a/drivers/usb/host/ehci.h
+++ b/drivers/usb/host/ehci.h
@@ -218,6 +218,7 @@ struct ehci_hcd {			/* one per controlle
 	unsigned		frame_index_bug:1; /* MosChip (AKA NetMos) */
 	unsigned		need_oc_pp_cycle:1; /* MPC834X port power */
 	unsigned		imx28_write_fix:1; /* For Freescale i.MX28 */
+	unsigned		spurious_oc:1;
 
 	/* required for usb32 quirk */
 	#define OHCI_CTRL_HCFS          (3 << 6)
--- a/include/linux/usb/ehci_pdriver.h
+++ b/include/linux/usb/ehci_pdriver.h
@@ -50,6 +50,7 @@ struct usb_ehci_pdata {
 	unsigned	no_io_watchdog:1;
 	unsigned	reset_on_resume:1;
 	unsigned	dma_mask_64:1;
+	unsigned	spurious_oc:1;
 
 	/* Turn on all power and clocks */
 	int (*power_on)(struct platform_device *pdev);
