From d946085ff5a331de64e91a2e3c96b9ca79d740f5 Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Mon, 15 Jun 2020 00:10:34 +0200
Subject: [PATCH] ath9k: enabled MFP capability unconditionally

ath9k will already fallback on software-crypto for chipsets not
supporting IEEE802.11w (MFP). So advertising MFP is not dependent
on disabling HW crypto for all traffic entirely.

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 drivers/net/wireless/ath/ath9k/init.c | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

--- a/drivers/net/wireless/ath/ath9k/init.c
+++ b/drivers/net/wireless/ath/ath9k/init.c
@@ -924,6 +924,7 @@ static void ath9k_set_hw_capab(struct at
 	ieee80211_hw_set(hw, HOST_BROADCAST_PS_BUFFERING);
 	ieee80211_hw_set(hw, SUPPORT_FAST_XMIT);
 	ieee80211_hw_set(hw, SUPPORTS_CLONED_SKBS);
+	ieee80211_hw_set(hw, MFP_CAPABLE);
 
 	if (ath9k_ps_enable)
 		ieee80211_hw_set(hw, SUPPORTS_PS);
@@ -936,9 +937,6 @@ static void ath9k_set_hw_capab(struct at
 				IEEE80211_RADIOTAP_MCS_HAVE_STBC;
 	}
 
-	if (AR_SREV_9160_10_OR_LATER(sc->sc_ah) || ath9k_modparam_nohwcrypt)
-		ieee80211_hw_set(hw, MFP_CAPABLE);
-
 	hw->wiphy->features |= NL80211_FEATURE_ACTIVE_MONITOR |
 			       NL80211_FEATURE_AP_MODE_CHAN_WIDTH_CHANGE |
 			       NL80211_FEATURE_P2P_GO_CTWIN;
