--- a/drivers/net/wireless/broadcom/b43/main.c
+++ b/drivers/net/wireless/broadcom/b43/main.c
@@ -114,7 +114,7 @@ static int b43_modparam_pio = 0;
 module_param_named(pio, b43_modparam_pio, int, 0644);
 MODULE_PARM_DESC(pio, "Use PIO accesses by default: 0=DMA, 1=PIO");
 
-static int modparam_allhwsupport = !IS_ENABLED(CPTCFG_BRCMSMAC);
+static int modparam_allhwsupport = 1;
 module_param_named(allhwsupport, modparam_allhwsupport, int, 0444);
 MODULE_PARM_DESC(allhwsupport, "Enable support for all hardware (even it if overlaps with the brcmsmac driver)");
 
