// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7100.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "siemens,ws-ap3610", "qca,ar7161";
	model = "Siemens WS-AP3610";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
		label-mac-device = &eth0;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-output-names = "ref";
		clock-frequency = <40000000>;
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: led_power_green {
			label = "green:power";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};

		led_power_red: led_power_red {
			label = "red:power";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		led_wlan5_blue {
			label = "blue:wlan5";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led_wlan5_green {
			label = "green:wlan5";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		led_wlan2_blue {
			label = "blue:wlan2";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led_wlan2_green {
			label = "green:wlan2";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie0 {
	status = "okay";
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		/*
		 * When the compatible-is missing, PHY autodetection
		 * is performed, but the PHY-ID reads all 0xff.
		 *
		 * Linux does not create the device in this case,
		 * and the reset is never even de-asserted.
		 */
		compatible = "ethernet-phy-id0143.bca2",
				"ethernet-phy-ieee802.3-c22";
		reg = <0>;

		resets = <&rst 8>;
		reset-names = "phy";
		reset-assert-us = <10000>;
		reset-deassert-us = <10000>;
	};
};

&eth0 {
	status = "okay";

	phy-mode = "rgmii-id";
	phy-handle = <&phy0>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-bak";
				reg = <0x40000 0x40000>;
				read-only;
			};

			partition@80000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x80000 0xe00000>;
			};

			partition@e80000 {
				label = "cfg1";
				reg = <0xe80000 0x40000>;
				read-only;
			};

			partition@ec0000 {
				label = "cfg2";
				reg = <0xec0000 0x40000>;
				read-only;
			};

			partition@f00000 {
				label = "nvram1";
				reg = <0xf00000 0x40000>;
				read-only;
			};

			partition@f40000 {
				label = "nvram2";
				reg = <0xf40000 0x40000>;
				read-only;
			};

			partition@f80000 {
				label = "rsvd1";
				reg = <0xf80000 0x40000>;
				read-only;
			};

			partition@fc0000 {
				label = "rsvd2";
				reg = <0xfc0000 0x40000>;
				read-only;
			};
		};
	};
};
