From 3f911800613a3417101563b488c51a9b310ba7fa Mon Sep 17 00:00:00 2001
From: Vladimir Oltean <vladimir.oltean@nxp.com>
Date: Fri, 27 Dec 2019 20:14:57 +0200
Subject: [PATCH] net: dsa: Pass pcs_poll flag from driver to PHYLINK

The DSA drivers that implement .phylink_mac_link_state should normally
register an interrupt for the PCS, from which they should call
phylink_mac_change(). However not all switches implement this, and those
who don't should set this flag in dsa_switch in the .setup callback, so
that PHYLINK will poll for a few ms until the in-band AN link timer
expires and the PCS state settles.

Signed-off-by: Vladimir Oltean <vladimir.oltean@nxp.com>

Conflicts:
	include/net/dsa.h

trivially with upstream commit 05f294a85235 ("net: dsa: allocate ports
on touch") which was merged in v5.4-rc3.
---
 include/net/dsa.h | 5 +++++
 net/dsa/port.c    | 1 +
 2 files changed, 6 insertions(+)

--- a/include/net/dsa.h
+++ b/include/net/dsa.h
@@ -291,6 +291,11 @@ struct dsa_switch {
 	 */
 	bool			vlan_filtering;
 
+	/* MAC PCS does not provide link state change interrupt, and requires
+	 * polling. Flag passed on to PHYLINK.
+	 */
+	bool			pcs_poll;
+
 	/* Dynamically allocated ports, keep last */
 	size_t num_ports;
 	struct dsa_port ports[];
--- a/net/dsa/port.c
+++ b/net/dsa/port.c
@@ -639,6 +639,7 @@ static int dsa_port_phylink_register(str
 
 	dp->pl_config.dev = ds->dev;
 	dp->pl_config.type = PHYLINK_DEV;
+	dp->pl_config.pcs_poll = ds->pcs_poll;
 
 	dp->pl = phylink_create(&dp->pl_config, of_fwnode_handle(port_dn),
 				mode, &dsa_port_phylink_mac_ops);
