#
# Copyright (C) 2012-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
iom,ix2-200)
	ucidef_set_led_timer "health" "health" "status:white:rebuild_led" "200" "800"
	;;
linksys,e4200-v2|\
linksys,ea4500)
	ucidef_set_led_default "pulse" "pulse" "viper:white:pulse" "1"
	;;
esac

board_config_flush

exit 0
