#
# Updated 97/06/13 to livingston-radius-2.01 miquels@cistron.nl
#
#	This file contains dictionary translations for parsing
#	requests and generating responses.  All transactions are
#	composed of Attribute/Value Pairs.  The value of each attribute
#	is specified as one of 4 data types.  Valid data types are:
#
#	string - 0-253 octets
#	ipaddr - 4 octets in network byte order
#	integer - 32 bit value in big endian order (high byte first)
#	date - 32 bit value in big endian order - seconds since
#					00:00:00 GMT,  Jan.  1,  1970
#
#	Enumerated values are stored in the user file with dictionary
#	VALUE translations for easy administration.
#
#	Example:
#
#	ATTRIBUTE	  VALUE
#	---------------   -----
#	Framed-Protocol = PPP
#	7		= 1	(integer encoding)
#

# The dictionary format now supports vendor-specific attributes.
# Vendors are introduced like this:
#
#	VENDOR vendor_name vendor_number
#
# For example:
#
#	VENDOR RoaringPenguin 10055
#
# Vendor-specific attributes have a fifth field with the name of the
# vendor.  For example:
#
#       ATTRIBUTE RP-Upstream-Speed-Limit 1 integer RoaringPenguin
#
# introduces a Roaring Penguin vendor-specific attribbute with name
# RP-Upstream-Speed-Limit, number 1, type integer and vendor RoaringPenguin.

#
#	Following are the proper new names. Use these.
#
ATTRIBUTE	User-Name		1	string
ATTRIBUTE	Password		2	string
ATTRIBUTE	CHAP-Password		3	string
ATTRIBUTE	NAS-IP-Address		4	ipaddr
ATTRIBUTE	NAS-Port-Id		5	integer
ATTRIBUTE	Service-Type		6	integer
ATTRIBUTE	Framed-Protocol		7	integer
ATTRIBUTE	Framed-IP-Address	8	ipaddr
ATTRIBUTE	Framed-IP-Netmask	9	ipaddr
ATTRIBUTE	Framed-Routing		10	integer
ATTRIBUTE	Filter-Id		11	string
ATTRIBUTE	Framed-MTU		12	integer
ATTRIBUTE	Framed-Compression	13	integer
ATTRIBUTE	Login-IP-Host		14	ipaddr
ATTRIBUTE	Login-Service		15	integer
ATTRIBUTE	Login-TCP-Port		16	integer
ATTRIBUTE	Reply-Message		18	string
ATTRIBUTE	Callback-Number		19	string
ATTRIBUTE	Callback-Id		20	string
ATTRIBUTE	Framed-Route		22	string
ATTRIBUTE	Framed-IPX-Network	23	ipaddr
ATTRIBUTE	State			24	string
ATTRIBUTE	Class			25	string
ATTRIBUTE	Session-Timeout		27	integer
ATTRIBUTE	Idle-Timeout		28	integer
ATTRIBUTE	Termination-Action	29	integer
ATTRIBUTE	Called-Station-Id	30	string
ATTRIBUTE	Calling-Station-Id	31	string
ATTRIBUTE	NAS-Identifier		32	string
ATTRIBUTE	Acct-Status-Type	40	integer
ATTRIBUTE	Acct-Delay-Time		41	integer
ATTRIBUTE	Acct-Input-Octets	42	integer
ATTRIBUTE	Acct-Output-Octets	43	integer
ATTRIBUTE	Acct-Session-Id		44	string
ATTRIBUTE	Acct-Authentic		45	integer
ATTRIBUTE	Acct-Session-Time	46	integer
ATTRIBUTE	Acct-Input-Packets	47	integer
ATTRIBUTE	Acct-Output-Packets	48	integer
ATTRIBUTE	Acct-Terminate-Cause	49	integer
ATTRIBUTE	Chap-Challenge		60	string
ATTRIBUTE	NAS-Port-Type		61	integer
ATTRIBUTE	Port-Limit		62	integer
ATTRIBUTE	Connect-Info		77	string

# RFC 2869
ATTRIBUTE	Acct-Interim-Interval	85	integer

#
#	Experimental Non Protocol Attributes used by Cistron-Radiusd
#
ATTRIBUTE	Huntgroup-Name		221	string
ATTRIBUTE	User-Category		1029	string
ATTRIBUTE	Group-Name		1030	string
ATTRIBUTE	Simultaneous-Use	1034	integer
ATTRIBUTE	Strip-User-Name		1035	integer
ATTRIBUTE	Fall-Through		1036	integer
ATTRIBUTE	Add-Port-To-IP-Address	1037	integer
ATTRIBUTE	Exec-Program		1038	string
ATTRIBUTE	Exec-Program-Wait	1039	string
ATTRIBUTE	Hint			1040	string

#
#	Non-Protocol Attributes
#	These attributes are used internally by the server
#
ATTRIBUTE	Expiration		  21	date
ATTRIBUTE	Auth-Type		1000	integer
ATTRIBUTE	Menu			1001	string
ATTRIBUTE	Termination-Menu	1002	string
ATTRIBUTE	Prefix			1003	string
ATTRIBUTE	Suffix			1004	string
ATTRIBUTE	Group			1005	string
ATTRIBUTE	Crypt-Password		1006	string
ATTRIBUTE	Connect-Rate		1007	integer

#
#       Experimental, implementation specific attributes
#
# Limit session traffic
ATTRIBUTE	Session-Octets-Limit	227	integer
# What to assume as limit - 0 in+out, 1 in, 2 out, 3 max(in,out)
ATTRIBUTE	Octets-Direction	228	integer

#
#	Integer Translations
#

#	User Types

VALUE		Service-Type		Login-User		1
VALUE		Service-Type		Framed-User		2
VALUE		Service-Type		Callback-Login-User	3
VALUE		Service-Type		Callback-Framed-User	4
VALUE		Service-Type		Outbound-User		5
VALUE		Service-Type		Administrative-User	6
VALUE		Service-Type		NAS-Prompt-User		7

#	Framed Protocols

VALUE		Framed-Protocol		PPP			1
VALUE		Framed-Protocol		SLIP			2

#	Framed Routing Values

VALUE		Framed-Routing		None			0
VALUE		Framed-Routing		Broadcast		1
VALUE		Framed-Routing		Listen			2
VALUE		Framed-Routing		Broadcast-Listen	3

#	Framed Compression Types

VALUE		Framed-Compression	None			0
VALUE		Framed-Compression	Van-Jacobson-TCP-IP	1

#	Login Services

VALUE		Login-Service		Telnet			0
VALUE		Login-Service		Rlogin			1
VALUE		Login-Service		TCP-Clear		2
VALUE		Login-Service		PortMaster		3

#	Status Types

VALUE		Acct-Status-Type	Start			1
VALUE		Acct-Status-Type	Stop			2
VALUE		Acct-Status-Type	Accounting-On		7
VALUE		Acct-Status-Type	Accounting-Off		8

#	Authentication Types

VALUE		Acct-Authentic		RADIUS			1
VALUE		Acct-Authentic		Local			2
VALUE		Acct-Authentic		PowerLink128		100

#	Termination Options

VALUE		Termination-Action	Default			0
VALUE		Termination-Action	RADIUS-Request		1

#	NAS Port Types, available in 3.3.1 and later

VALUE		NAS-Port-Type		Async			0
VALUE		NAS-Port-Type		Sync			1
VALUE		NAS-Port-Type		ISDN			2
VALUE		NAS-Port-Type		ISDN-V120		3
VALUE		NAS-Port-Type		ISDN-V110		4

#	Acct Terminate Causes, available in 3.3.2 and later

VALUE           Acct-Terminate-Cause    User-Request            1
VALUE           Acct-Terminate-Cause    Lost-Carrier            2
VALUE           Acct-Terminate-Cause    Lost-Service            3
VALUE           Acct-Terminate-Cause    Idle-Timeout            4
VALUE           Acct-Terminate-Cause    Session-Timeout         5
VALUE           Acct-Terminate-Cause    Admin-Reset             6
VALUE           Acct-Terminate-Cause    Admin-Reboot            7
VALUE           Acct-Terminate-Cause    Port-Error              8
VALUE           Acct-Terminate-Cause    NAS-Error               9
VALUE           Acct-Terminate-Cause    NAS-Request             10
VALUE           Acct-Terminate-Cause    NAS-Reboot              11
VALUE           Acct-Terminate-Cause    Port-Unneeded           12
VALUE           Acct-Terminate-Cause    Port-Preempted          13
VALUE           Acct-Terminate-Cause    Port-Suspended          14
VALUE           Acct-Terminate-Cause    Service-Unavailable     15
VALUE           Acct-Terminate-Cause    Callback                16
VALUE           Acct-Terminate-Cause    User-Error              17
VALUE           Acct-Terminate-Cause    Host-Request            18

#
#	Non-Protocol Integer Translations
#

VALUE		Auth-Type		Local			0
VALUE		Auth-Type		System			1
VALUE		Auth-Type		SecurID			2
VALUE		Auth-Type		Crypt-Local		3
VALUE		Auth-Type		Reject			4

#
#	Cistron extensions
#
VALUE		Auth-Type		Pam			253
VALUE		Auth-Type		None			254

#
#	Experimental Non-Protocol Integer Translations for Cistron-Radiusd
#
VALUE		Fall-Through		No			0
VALUE		Fall-Through		Yes			1
VALUE		Add-Port-To-IP-Address	No			0
VALUE		Add-Port-To-IP-Address	Yes			1

#
#	Configuration Values
#	uncomment these two lines to turn account expiration on
#

#VALUE		Server-Config		Password-Expiration	30
#VALUE		Server-Config		Password-Warning	5

#       Octets-Direction
VALUE		Octets-Direction        Sum			0
VALUE		Octets-Direction        Input			1
VALUE		Octets-Direction        Output			2
VALUE		Octets-Direction        MaxOveral		3
VALUE		Octets-Direction        MaxSession		4

INCLUDE /etc/ppp/radius/dictionary.microsoft
